SECTION III.  EMISSIONS UNITS AND SPECIFIC CONDITIONS.
Subsection C.  Emissions Unit XXX
Company Name
Plant Name
Facility ID No. XXXXXXX
County Name County
Initial Title V Air Operation Permit Revision/Renewal
Permit No. XXXXXXX-XXX-AV
(Renewal/Revision of Title V Air Operation Permit No. XXXXXXX-ZZZ-AV)
[image: ]
Permitting Authority:
State of Florida
District/Local Office
Permitting Authority
Address
Telephone:  (xxx) xxx-xxxx
Fax:  (xxx) xxx-xxxx
Compliance Authority:
Compliance Authority Name
Compliance Authority
Address
Telephone:  (xxx) xxx-xxxx
Email (preferred):  District@dep.state.fl.us 
	

19

Title V Air Operation Permit Revision/Renewal
Permit No. XXXXXXX-XXX-AV
Table of Contents
Section	Page Number
Placard Page 	 1
I. Facility Information.
A. Facility Description. 	 2
B. Summary of Emissions Units. 	 2
C. Applicable Regulations. 	 2
II. Facility-wide Conditions. 	 3
III. Emissions Units and Conditions.
A. Brief EU Description. 	 5
B. Brief EU Description. 	 8
C. Brief EU Description. 	 X
D. Brief EU Description. 	 X
IV. Appendices. 	 21
Appendix A, Glossary.
Appendix CAM, Compliance Assurance Monitoring Plan.
Appendix CEMS.  (Only if in AC for facility)
Appendix CP, Compliance Plan (If required)
Appendix I, List of Insignificant Emissions Units and/or Activities.
Appendix NESHAP, Subpart A – General Provisions. (Include for all units that are subject to a NESHAP)
Appendix NESHAP, ____
Appendix NSPS, Subpart A – General Provisions.  (Include for all units that are subject to an NSPS subpart)
Appendix NSPS, Subpart ____
Appendix RR, Facility-wide Reporting Requirements.
[bookmark: OLE_LINK1][bookmark: OLE_LINK2]Appendix TR, Facility-wide Testing Requirements.
Appendix TV, Title V General Conditions.
Appendix U, List of Unregulated Emissions Units and/or Activities.
Referenced Attachments. At End
Figure 1, Summary Report-Gaseous and Opacity Excess Emission and 
Monitoring System Performance (40 CFR 60, July, 1996).  (Include if NSPS Subpart A is included)
Table H, Permit History.
Table 1, Summary of Air Pollutant Standards and Terms.
Table 2, Compliance Requirements.
Etc.

Company Name	Site Name


i
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The purpose of this permit is to renew the or to issue the initial Title V air operation permit for the above referenced facility.  The existing PLANT NAME is located in NAME County at ADDRESS, CITY.  UTM Coordinates are:  Zone 17, XXXXXXX.  Latitude is:  XXXX North; and, Longitude is:  XXXXX West.
The Title V air operation permit is issued under the provisions of Chapter 403, Florida Statutes (F.S.), and Florida Administrative Code (F.A.C.) Chapters 62-4, 62-210, 62-213 and 62-214.  The above named permittee is hereby authorized to operate the facility in accordance with the terms and conditions of this permit.
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(Draft/Proposed)
(Signature)
XXX/xx/xx
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[bookmark: SectionIA]Subsection A.  Facility Description.
{FACILITY DESCRIPTION.}
[bookmark: SectionIB]Subsection B.  Summary of Emissions Units.
	EU No.
	Brief Description

	Regulated Emissions Units

	001
	

	002
	

	003
	

	Unregulated Emissions Units and Activities 
(see Appendix U, List of Unregulated Emissions Units and/or Activities)

	00X
	

	00X
	


Also included in this permit are miscellaneous insignificant emissions units and/or activities (see Appendix I, List of Insignificant Emissions Units and/or Activities).
Subsection C.  Applicable Regulations.
Based on the initial Title V air operation permit renewal/revision application received APPLICATION REC’D DATE, this facility is/is not a major source of hazardous air pollutants (HAP).  The existing facility is a prevention of significant deterioration (PSD) major source of air pollutants in accordance with Rule 62-212.400, F.A.C.  A summary of applicable regulations is shown in the following table.  
	Regulation
	EU No(s).

	Federal Rule Citations

	40 CFR 60, Subpart A, NSPS General Provisions
	

	40 CFR 60, Subpart ___  
	

	40 CFR 63, Subpart ___
	

	40 CFR 75 Acid Rain Monitoring Provisions
	

	40 
	

	State Rule Citations

	State Rule Citations (list all that apply, main rule, not all #’s, i.e. 62-296.405, 62-296.406, BACT, etc.)
	

	(etc.)
	

	
	

	
	



SECTION I.  FACILITY INFORMATION.

Facility Name	Permit No. 9999999-999-AV
Plant Name	Initial Title V Air Operation Permit Renewal/Revision
Page 12 of 17
[bookmark: SectionII]The following conditions apply facility-wide to all emission units and activities:
FW1. Appendices.  The permittee shall comply with all documents identified in Section X, Appendices, listed in the Table of Contents.  Each document is an enforceable part of this permit unless otherwise indicated.  [Rule 62-213.440, F.A.C.]
Emissions and Controls
FW2. Not federally Enforceable.  Objectionable Odor Prohibited.  No person shall cause, suffer, allow or permit the discharge of air pollutants, which cause or contribute to an objectionable odor.  An “objectionable odor” means any odor present in the outdoor atmosphere which by itself or in combination with other odors, is or may be harmful or injurious to human health or welfare, which unreasonably interferes with the comfortable use and enjoyment of life or property, or which creates a nuisance.  [Rule 62-296.320(2) and 62-210.200(Definitions), F.A.C.]
If the facility includes a landfill, insert the following odor remediation plan requirement from the waste rules.
FW3. Odor Remediation Plan.  The facility shall be operated to control objectionable odors in accordance with subsection 62-296.320(2), F.A.C.  After being notified by the Department that objectionable odors have been confirmed beyond the landfill property boundary, the owner or operator shall:
a. Immediately take steps to reduce the objectionable odors.  Such steps may include applying or increasing initial cover, reducing the size of the working face, and ceasing operations in the areas where odors have been detected;
b. Submit to the Department for approval an odor remediation plan for the gas releases.  The plan shall describe the nature and extent of the problem and the proposed long-term remedy.  The remedy shall be initiated within 30 days of approval.
c. Implement a routine odor monitoring program to determine the timing and extent of any off-site odors, and to evaluate the effectiveness of the odor remediation plan.
[Rule 62-701.530(3)(b), F.A.C.]
FW4. General Volatile Organic Compounds (VOC) Emissions or Organic Solvents (OS) Emissions.  The permittee shall allow no person to store, pump, handle, process, load, unload or use in any process or installation, volatile organic compounds or organic solvents without applying known and existing vapor emission control devices or systems deemed necessary and ordered by the Department.  Customize as appropriate according to underlying AC permit condition(s) or include the Permitting Note shown below.  [Rule 62-296.320(1), F.A.C.]
{Permitting Note:  Nothing is deemed necessary and ordered at this time.}
FW5. General Visible Emissions.  No person shall cause, let, permit, suffer or allow to be discharged into the atmosphere the emissions of air pollutants from any activity equal to or greater than 20% opacity.  This regulation does not impose a specific testing requirement.  [Rule 62-296.320(4)(b), F.A.C.]
If in Hillsborough County, use this alternate condition instead of the version of FW4. above:
General Visible Emissions.  No person shall cause, let, permit, suffer or allow to be discharged into the atmosphere the emissions of air pollutants from any activity equal to or greater than 20% opacity.  Emissions from the following types of activities in Hillsborough County are further subject to a general 5% opacity standard:  loading or unloading of materials to or from containers such as rail cars, trucks, ships, storage structures and stockpiles; permanent conveyor systems; storage of materials in structures such as silos or enclosed bins, which have a storage capacity of fifty cubic yards or more; crushing, grinding, sizing and screening operations; and, static drop transfer points.  These regulations do not impose a specific testing requirement.  [Rules 62-296.320(4)(b)1, F.A.C. and Rule 1-3.52, HCEPC] 
FW6. Unconfined Particulate Matter.  No person shall cause, let, permit, suffer or allow the emissions of unconfined particulate matter from any activity, including vehicular movement; transportation of materials; construction; alteration; demolition or wrecking; or industrially related activities such as loading, unloading, storing or handling; without taking reasonable precautions to prevent such emissions.  Reasonable precautions to prevent emissions of unconfined particulate matter at this facility include:
a. (Insert from application).
b. (Insert from application).
c. (Insert from application).
d. (Etc.).
[Rule 62-296.320(4)(c), F.A.C.; and, proposed by applicant in Title V air operation permit renewal application received Month Day, Year.]
Reports and Fees 
See Appendix RR, Facility-wide Reporting Requirements for additional details.
FW7. Electronic Annual Operating Report and Title V Annual Emissions Fees.  The information required by the Annual Operating Report for Air Pollutant Emitting Facility [Including Title V Source Emissions Fee Calculation] (DEP Form No. 62-210.900(5)) shall be submitted by April 1 of each year, for the previous calendar year, to the Department of Environmental Protection’s (DEP) Division of Air Resource Management.  Each Title V source shall submit the annual operating report using the DEP’s Electronic Annual Operating Report (EAOR) software, unless the Title V source claims a technical or financial hardship by submitting DEP Form No. 62-210.900(5) to the DEP Division of Air Resource Management instead of using the reporting software.  Emissions shall be computed in accordance with the provisions of subsection 62-210.370(2), F.A.C.  Each Title V source must pay between January 15 and April 1 of each year an annual emissions fee in an amount determined as set forth in subsection 62-213.205(1), F.A.C.  The annual fee shall only apply to those regulated pollutants, except carbon monoxide and greenhouse gases, for which an allowable numeric emission-limiting standard is specified in the source’s most recent construction permit or operation permit.  Upon completing the required EAOR entries, the EAOR Title V Fee Invoice can be printed by the source showing which of the reported emissions are subject to the fee and the total Title V Annual Emissions Fee that is due.  The submission of the annual Title V emissions fee payment is also due (postmarked) by April 1st of each year.  A copy of the system-generated EAOR Title V Annual Emissions Fee Invoice and the indicated total fee shall be submitted to:  Major Air Pollution Source Annual Emissions Fee, Post Office Box 3070, Tallahassee, Florida 32315-3070.  Additional information is available by accessing the Title V Annual Emissions Fee On-line Information Center at the following Internet web site:  http://www.dep.state.fl.us/air/emission/tvfee.htm.  [Rules 62-210.370(3), 62-210.900 & 62-213.205, F.A.C.; and, §403.0872(11), Florida Statutes (2013)]
{Permitting Note:  Resources to help you complete your AOR are available on the electronic AOR (EAOR) website at:  http://www.dep.state.fl.us/air/emission/eaor.  If you have questions or need assistance after reviewing the information posted on the EAOR website, please contact the Department by phone at (850) 717-9000 or email at eaor@dep.state.fl.us.}
{Permitting Note:  The Title V Annual Emissions Fee form (DEP Form No. 62-213.900(1)) has been repealed.  A separate Annual Emissions Fee form is no longer required to be submitted by March 1st each year.}
FW8. Annual Statement of Compliance.  The permittee shall submit an annual statement of compliance to the compliance authority at the address shown on the cover of this permit and to the US. EPA at the address shown below within 60 days after the end of each calendar year during which the Title V air operation permit was effective.  (See also Appendix RR, Conditions RR1 and RR7.)  [Rules 62-213.440(3)(a)2. & 3. and (b), F.A.C.]
U.S. Environmental Protection Agency, Region 4
Atlanta Federal Center
61 Forsyth Street, SW
Atlanta, Georgia  30303
Attn:  Air Enforcement Branch
FW9. Prevention of Accidental Releases (Section 112(r) of CAA).
a. As required by Section 112(r)(7)(B)(iii) of the CAA and 40 CFR 68, the owner or operator shall submit an updated Risk Management Plan (RMP) to the Chemical Emergency Preparedness and Prevention Office (CEPPO) RMP Reporting Center.  (See paragraph e., below.)
b. As required under Section 252.941(1)(c), F.S., the owner or operator shall report to the appropriate representative of the Division of Emergency Management, as established by department rule, within one working day of discovery of an accidental release of a regulated substance from the stationary source, if the owner or operator is required to report the release to the United States Environmental Protection Agency under Section 112(r)(6) of the CAA.
c. The owner or operator shall submit the required annual registration fee to the Division of Emergency Management on or before April 1, in accordance with Part IV, Chapter 252, F.S., and Rule 27P-21, F.A.C.
d. Any required written reports, notifications, certifications, and data required to be sent to the Division of Emergency Management, should be sent to:  Division of Emergency Management, 2555 Shumard Oak Boulevard, Tallahassee, FL  32399-2100, Telephone:  (850) 413-9970, Fax:  (850) 488-1739.
e. Any Risk Management Plans, original submittals, revisions, or updates to submittals, should be sent electronically through EPA’s Central Data Exchange system at the following address:  https://cdx.epa.gov.  Information on electronically submitting risk management plans using the Central Data Exchange system is available at:  http://www2.epa.gov/rmp.  The RMP Reporting Center can be contacted at:  RMP Reporting Center, Post Office Box 10162, Fairfax, VA  22038, Telephone:  (703) 227-7650.
f. Any required reports to be sent to the National Response Center, should be sent to:  National Response Center, EPA Office of Solid Waste and Emergency Response, 1200 Pennsylvania Avenue Northwest, Mail Code:  USEPA (5101T), Washington, DC  20460, Telephone:  (800) 424-8802.
g. Send the required annual registration fee using approved forms made payable to:  Cashier, Division of Emergency Management, State Emergency Response Commission, 2555 Shumard Oak Boulevard, Tallahassee, FL  32399-2149
[Part IV, Chapter 252, F.S.; and, Rule 27P-21, F.A.C.]
-OR-
FW9.   Prevention of Accidental Releases (Section 112(r) of CAA).  If, and when, the facility becomes subject to 112(r), the permittee shall:
a. Submit its Risk Management Plan (RMP) to the Chemical Emergency Preparedness and Prevention Office (CEPPO) RMP Reporting Center.  Any Risk Management Plans, original submittals, revisions or updates to submittals, should be sent electronically through EPA’s Central Data Exchange system at the following address:  https://cdx.epa.gov.  Information on electronically submitting risk management plans using the Central Data Exchange system is available at:  http://www2.epa.gov/rmp.  The RMP Reporting Center can be contacted at:  RMP Reporting Center, Post Office Box 10162, Fairfax, VA  22038, Telephone:  (703) 227-7650.
b. Submit to the permitting authority Title V certification forms or a compliance schedule in accordance with Rule 62-213.440(2), F.A.C.
[40 CFR 68]
FW10. [bookmark: _Hlk509406950][bookmark: _GoBack]Semi-Annual Reports.  The permittee shall monitor compliance with the terms and conditions of this permit and shall submit reports at least every six months to the compliance office.  Each semi-annual report shall cover the 6-month periods of January 1 – June 30 and July 1 – December 31.  The reports shall be submitted by the 60th day following the end of each calendar half (i.e., March 1st and August 29th of every year).  All instances of deviations from permit requirements (including conditions in the referenced Appendices) must be clearly identified in such reports, including reference to the specific requirement and the duration of such deviation.  If there are no deviations during the reporting period, the report shall so indicate.  Any semi-annual reporting requirements contained in applicable federal NSPS or NESHAP requirements may be submitted as part of this report.  The submittal dates specified above shall replace the submittal dates specified in the federal rules.  All additional reports submitted as part of this report should be clearly identified according to the specific federal requirement.  All reports shall include a certification by a responsible official, pursuant to subsection 62-213.420(4), F.A.C.  (See also Conditions RR2. – RR4. of Appendix RR, Facility-wide Reporting Requirements, for additional reporting requirements related to deviations.)  [Rule 62-213.440(1)(b)3.a., F.A.C.; and, 40 CFR 60.19(d), 40 CFR 61.10(h) & 40 CFR 63.10(a)(5)]
{Permitting Note:  EPA has clarified that, pursuant to 40 CFR 70.6(a)(3), the word “monitoring” is used in a broad sense and means monitoring (i.e., paying attention to) the compliance of the source with all emissions limitations, standards, and work practices specified in the permit.}
Other Requirements
FW11. Etc. (Make sure that anything added here is truly a facility-wide requirement, including being applicable to all of the insignificant and unregulated emissions units and activities.)
SECTION II.  FACILITY-WIDE CONDITIONS.

The specific conditions in this section apply to the following emissions unit(s):
	

EU No.
	Brief Description

	XXX
	Brief description of emissions unit(s)

	YYY
	Brief description of emissions unit(s)


(Insert a DETAILED description of the emissions unit(s), including a description of any control devices, continuous emissions monitors, rules that specifically apply to this/these unit(s), start up date, stack parameters, etc.)
{Permitting Note:  This/These emission unit(s) is/or regulated under…}
Essential Potential to Emit (PTE) Parameters
A.1. Permitted Capacity.  The maximum allowable heat input rate is as follows:
	Unit No.
	MMBtu/hr Heat Input (or other regulated capacity)
	Fuel Type

	(list)
	
	

	
	
	

	
	
	


[Rules 62-4.160(2), 62-204.800, 62-210.200(PTE), 62-214.330 & 62-296.405, F.A.C.; and, Permit No(s). XXXXXXX-XXX-AC.]
A.2. Emissions Unit Operating Rate Limitation After Testing.  See the related testing provisions in Appendix TR, Facility-wide Testing Requirements.  [Rule 62-297.310(3), F.A.C.]
A.3. Methods of Operation. [Example]
a. Fuels.  The fuels that are allowed to be burned in this unit/these units are:
(1) Coal, primary fuel,
(2) Natural gas,
(3) New No. 2 fuel oil, 
(4) Biomass. 
(5) On-specification used oil (see Specific Condition A.XX.),  
(6) And/or on-site generated “oil contaminated soil”, which is periodically combusted for energy recovery purposes.
b. Other.
(1) Supplemental injection of “GAM 60” for purposes of maintaining boiler tube temperatures.
(2) Supplemental injection of sodium carbonate or sodium sulfate at a rate of 440 pounds per hour as necessary to enhance the operation of the particulate control devices on these units.
c. Etc.
[Rule 62-213.410, F.A.C.; Applicant’s request in Title V permit renewal application received Month DD, YYYY; and, Permit No(s). XXXXXXX-XXX-AC.]
A.4. Hours of Operation.  This/These emissions unit(s) may operate continuously (i.e., 8,760) without restriction or <enter limit from AC permit>.  [Rule 62-210.200(PTE), F.A.C.; and, Permit No. XXXXXXX-XXX-AC]
Control Technology
A.5. (If in AC permits)
Emission Limitations and Standards
{Permitting Note:  The attached Table 1, Summary of Air Pollutant Standards, summarizes information for convenience purposes only.  This table does not supersede any of the terms or conditions of this permit.}
Unless otherwise specified, the averaging time(s) for Specific Condition(s) [A].[#].-[A].[#]. [is/are] based on the specified averaging time of the applicable test method.
A.6. Visible Emissions.  Visible emissions shall not exceed _____.  Specify compliance method (CEMS, stack test, etc.), averaging times and correction factors as established by AC permit.  [Rule Citations]
A.7. NOX Emissions.  Nitrogen oxide (NOX) emissions shall not exceed _____.  Specify compliance method (CEMS, stack test, etc.), averaging times and correction factors as established by AC permit.  [Rule Citations]
A.8. PM Emissions.  Particulate matter (PM) emissions shall not exceed _____.  Specify compliance method (CEMS, stack test, etc.), averaging times and correction factors as established by AC permit.  [Rule Citations]
A.9. Etc.
Excess Emissions
Rule 62-210.700 (Excess Emissions), F.A.C. cannot vary any requirement of an NSPS, NESHAP or Acid Rain program provision.
A.10. Excess Emissions.  (Insert as applicable – for most units unless AC specifically over rides.  If only NSPS limits in permit, then 62-210.700 provisions do not apply.) Excess emissions resulting from startup, shutdown or malfunction of any emissions unit shall be permitted provided (1) best practices to minimize emissions are adhered to and (2) the duration of excess emissions shall be minimized but in no case exceed two hours in any 24-hour period unless specifically authorized by the Department for longer duration.  Excess emissions that are caused entirely or in part by poor maintenance, poor operation, or any other equipment or process failure that may reasonably be prevented during startup, shutdown or malfunction shall be prohibited.  [Rule 62-210.700(1), F.A.C.; and, Permit No. XXXXXXX-XXX-AC]
A.11. Excess Emissions Allowed.  (Insert as applicable – only for existing fossil fuel steam generators, i.e. 62-296.405 boilers) Excess emissions resulting from startup or shutdown shall be permitted provided that best operational practices to minimize emissions are adhered to and the duration of excess emissions shall be minimized.  [Rule 62-210.700(2), F.A.C.; and, Permit No. XXXXXXX-XXX-AC]
A.12. Other State Excess Emissions from 62-210.700(1) – (7) that specifically apply to this/these units.
A.13. NSPS Excess emissions conditions that specifically apply to this/these units.
A.14. AC/PSD established excess emissions conditions.  (Note that these conditions may alter the standard conditions from 62-210.700 or may be in addition to them.  If they alter/replace the conditions of 62-210.700, then customize condition A.10 accordingly.  Do not leave the full rule language if the AC changes it but do include the changed language from the AC.)  [Rule 62-210.700(6), F.A.C.; and, Permit No. XXXXXXX-XXX-AC]
Monitoring of Operations
A.15. CAM Plan.  This/these emissions unit(s) is/are subject to the Compliance Assurance Monitoring (CAM) requirements contained in the attached Appendix CAM.  Failure to adhere to the monitoring requirements specified does not necessarily indicate an exceedance of a specific emissions limitation; however, it may constitute good reason to require compliance testing pursuant to Rule 62-297.310(8)(c), F.A.C.  [40 CFR 64; and, Rules 62-204.800 and 62-213.440(1)(b)1.a., F.A.C.] (Delete condition if not subject to CAM)
A.16. Other required operational monitoring specific to this/these unit(s) that isn’t in any appendix.
Continuous Emissions Monitoring Requirements 
[List continuous monitoring requirements specific to this/these unit(s) that aren’t in any appendix.]
A.17. NOX CEMS.
A.18. SO2 CEMS
A.19. Etc.
Test Methods and Procedures
{Permitting Note:  The attached Table 2, Summary of Compliance Requirements, summarizes information for convenience purposes only.  This table does not supersede any of the terms or conditions of this permit.}
A.20. Test Methods.  When required, tests shall be performed in accordance with the following reference methods: [List only those that apply.]
	Method
	Description of Method and Comments

	1-4
	Traverse Points, Velocity and Flow Rate, Gas Analysis, and Moisture Content

	5B
	Method for Determining Particulate Matter Emissions (All PM is assumed to be PM10.)

	7E
	Determination of Nitrogen Oxide Emissions from Stationary Sources

	9
	Visual Determination of the Opacity of Emissions from Stationary Sources

	10
	Determination of Carbon Monoxide Emissions from Stationary Sources
{Note:  The method shall be based on a continuous sampling train.}

	18
	Measurement of Gaseous Organic Compound Emissions by Gas Chromatography

	19
	Determination of Sulfur Dioxide Removal Efficiency and Particulate Matter, Sulfur Dioxide, and Nitrogen Oxides Emission Rates (Optional F-factor method may be used to determine flow rate and gas analysis to calculate mass emissions in lieu of Methods 1-4.)

	20
	Determination of Nitrogen Oxides, Sulfur Dioxide and Diluent Emissions from Stationary Gas Turbines

	25A
	Method for Determining Gaseous Organic Concentrations (Flame Ionization)

	CTM-027
	Conditional EPA Test Method 027, Measurement of Ammonia Slip (or equivalent method)


The above methods are described in 40 CFR 60, Appendix A, and adopted by reference in Rule 62-204.800, F.A.C.  No other methods may be used unless prior written approval is received from the Department.  [Rule 62-204.800, F.A.C., and, AC No. XXX, etc. list as appropriate]
A.21. Common Testing Requirements.  Unless otherwise specified, tests shall be conducted in accordance with the requirements and procedures specified in Appendix TR, Facility-Wide Testing Requirements, of this permit.  [Rule 62-297.310, F.A.C.]
[bookmark: _Hlk9346819]{Permitting Note:  Air compliance test notifications can now be completed online in the Department’s Business Portal.  To access this online process, go to http://www.fldepportal.com/go/home and sign in (or register if you’re a new user) from the link in the upper right corner of the page.  On the Welcome page select the Submit option, then select Registration/Notification, and then click on Air Compliance Test Notifications.  Once in the process, just carefully read the instructions on each screen (and under the Help tabs) to complete the notification.}
A.22. Annual Compliance Tests Required.  During each calendar year (January 1st to December 31st), each EU shall be tested to demonstrate compliance with the emissions standards for __, __ and__.  [Rule 62-297.310(8), F.A.C.] [Include if not exempted pursuant to subparagraph 62-297.310(8)(a)5., F.A.C.]
A.23. Compliance Tests Prior To Renewal.  (If same as Annual tests in A.23., then blend together as one condition.)  Except as provided in subparagraph 62-297.310(8)(b)3., F.A.C. (see condition TR7.b.(3) in Appendix TR – Facility-wide Testing Requirements), in addition to the annual compliance tests specified above, compliance tests shall also be performed for __, __ and__ prior to obtaining a renewed operation permit to demonstrate compliance with the emission limits in Specific Conditions A.X. – A.Y.  [Rules 62-210.300(2)(a) and 62-297.310(8)(b), F.A.C.]
{Permitting Note:  Tests which are only required once during the term of a permit prior to obtaining a renewed permit should be performed roughly five years from the previous test.}
A.24. Additional Compliance Test Requirements.  Insert additional tests or test provisions/requirements as required by other applicable regulations. [Rule ____]
Recordkeeping and Reporting Requirements
A.25. Reporting Schedule.  The following reports and notifications shall be submitted to the Compliance Authority:  (Include here reports that are specific to the unit based on state rule, federal rule or AC permit, and that are not already covered by Appendix RR.)
	Report
	Reporting Deadline
	Related Condition(s)

	Notice of ___
	Reporting frequency of document
	A.XX.

	Notice of ___
	Reporting frequency of document
	A.YY.


[Rule 62-213.440(1)(b), F.A.C.]
A.26. Other Reporting Requirements.  See Appendix RR, Facility-Wide Reporting Requirements, for additional reporting requirements.  [Rule 62-213.440(1)(b), F.A.C.]
A.27. Specific Reporting Requirement.
A.28. Etc.
Other Requirements
A.29. Compliance Plan.  Based on the application, this/these emissions unit(s) were not in compliance with all applicable requirements at the time the application was submitted.  Appendix CP, Compliance Plan, is a part of this permit.  [Rule 62-213.440(2), F.A.C.]
A.30. Etc.
SECTION III.  EMISSIONS UNITS AND SPECIFIC CONDITIONS.
Subsection A.  Emissions Unit XXX

The specific conditions in this section apply to the following emissions unit(s):
	

EU No.
	Brief Description

	ZZZ
	{Description of emissions unit, fuel, capacity, controls, monitors, stack parameters, etc.}


Essential Potential to Emit (PTE) Parameters
Same as Subsection A.  Repeat as needed.
[bookmark: _Hlk512258552][bookmark: _Hlk512258553]SECTION III.  EMISSIONS UNITS AND SPECIFIC CONDITIONS.
Subsection B.  Emissions Unit XXX

Subsection C.  The specific conditions in this section apply to the following emissions units:
	

EU No.
	Brief Description

	XXX
	{Description of emissions unit, fuel, capacity, controls, monitors, stack parameters, etc.}

	YYY
	{Description of emissions unit, fuel, capacity, controls, monitors, stack parameters, etc.}

	ZZZ
	{Description of emissions unit, fuel, capacity, controls, monitors, stack parameters, etc.}
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