	ESTIMATED POLLUTANT LOAD REDUCTION: 

	

KILOGRAMS/YR

		BMP’s Installed
	TSS
kg/yr
	TP
kg/yr
	TN
kg/yr
	BOD
kg/yr
	Fecal Coliform
TC/yr
	Other
kg/yr

	Alum Injection
	
	
	
	
	Total Count
	     

	Pollutant Loads
	Pre-Project
	64,997
	1,440
	5,218
	21,839
	9.07E+13
	     

	
	Post-Project
	14,496
	380
	3,937
	14,689
	1.73E+13
	     

	
	Load Reduction
	50,501
	1,060
	1,281
	7,150
	7.34E+13
	     

	
	% Reduction
	78%
	74%
	25%
	33%
	81%
	     

	
	
	
	
	
	
	






POUNDS/YR
	



BMPs Installed
	TSS
lbs/yr
	TP
lbs/yr
	TN
lbs/yr
	BOD
lbs/yr
	Fecal Coliform 
	Other
lbs/yr

	Alum Injection
	
	
	
	
	 (total count)
	

	Pollutant Loads
	Pre-Project
	143,318
	3,175
	11,506
	48,155
	9.07E+13
	N/A

	
	Post-Project
	31,964
	838
	8,681
	32,389
	1.73E+13
	N/A

	
	Load Reduction
	111,355
	2,337
	2,825
	15,766
	7.34E+13
	N/A

	
	% Reduction
	78%
	74%
	25%
	33%
	81%
	N/A



