[bookmark: _GoBack]For the problem that flow paths passing through water bodies, you may take a look at Section 3.4.5 (page 3-10) of the user manual (http://people.sc.fsu.edu/~mye/ArcNLET/users_manual.pdf).

Another relevant section is about post-processing plumes described in Section 3.3.2 (page 3-16) of the technical manual (http://people.sc.fsu.edu/~mye/ArcNLET/technical_manual.pdf).

For the option of sink filling for flat area, the description is given in Section 2.3.2 (page 2-7) of the technical manual (http://people.sc.fsu.edu/~mye/ArcNLET/technical_manual.pdf). However, if the area is too flat, a solution is to run the Groundwater Flow and Particle Tracking modules for an area larger than the domain of interest so that the reasonably large DEM difference is available. In fact, this is always necessary to avoid effect of domain boundary on the smoothing.
