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[bookmark: _Hlk30963953]Background
The Indian River Lagoon (IRL) is a 156-mile-long estuary along Florida's east coast. The impaired portions of the IRL are directly adjacent to lands in only Volusia, Brevard, Indian River, and St. Lucie counties. The northern portion of the watershed extends to near the Ponce De Leon Inlet in Volusia County and the southern portion to near the Fort Pierce Inlet at the Indian River County–St. Lucie County boundary line. Because of the large geographical extent of the IRL Basin and the hydrological differences throughout the basin, the Florida Department of Environmental Protection (DEP) determined the best way to address the total maximum daily loads (TMDLs) and impairments for the IRL Basin would be to divide the watershed into 3 subbasins: (1) Central IRL (CIRL), (2) North IRL (NIRL), and (3) Banana River Lagoon (BRL). Separate basin management action plans (BMAPs) were developed for each subbasin; this document focuses solely on the NIRL Subbasin. The main stem of the NIRL Subbasin extends from Turnbull Creek in Volusia County to the Melbourne Causeway in Brevard County (Figure ES-1). 
Intense and extensive algal blooms in the IRL began in 2011 and have returned periodically. Harmful algal blooms (HABs) cause shading that stresses seagrass in the IRL, adverse effects on wildlife, and in some cases, detrimental effects on human health. The St. Johns River Water Management District (SJRWMD) launched the Indian River Lagoon Protection Initiative in 2013, including a multiyear investigation that increased the understanding of these blooms. This and other research indicate it is important to persevere with projects that decrease nutrient loads to the IRL, because that approach will limit the severity of HABs and their impacts on the system.
TMDLs
A TMDL is a water quality restoration goal establishing the maximum amount of a pollutant that a waterbody can assimilate without causing exceedances of water quality standards. The nutrient TMDLs for the main stem of the IRL were adopted by DEP in March 2009. The TMDLs focus on the water quality conditions necessary for seagrass regrowth at water depth limits where seagrass historically grew in the lagoon, based on a multiyear composite of seagrass coverage. The median depth limits of seagrass coverage in the IRL decreased over the years because of changes in water quality conditions resulting from anthropogenic influences. As polluted runoff reaches the lagoon, it contributes to conditions that prevent the seagrass from growing in deeper water. 
Additionally, TMDLs were adopted in 2013 for two tributaries to the NIRL, are now addressed in this BMAP. For Addison Creek (waterbody identification [WBID] number 3028), no further nutrient load reductions were requested beyond those already established for the main stem seagrass nutrient TMDLs. For the Eau Gallie River (WBID 3082), the total nitrogen (TN) and total phosphorus (TP) target loads defined in the TMDLs are different from the main stem. The tidal portion of the Eau Gallie River consistently showed high annual average chlorophyll a concentrations, and so the loading targets for the Eau Gallie are the natural background nutrient condition, which require a 51 % TN reduction and a 58 % TP reduction of nonpoint source loads based on the Hydrological Simulation Program–Fortran Model for the period from 1996 to 2005. 
NIRL BMAP
In addition to dividing the overall IRL Watershed into subbasins, the NIRL was further divided into "project zones." The project zone boundaries are based on the distinct hydrology in different areas of the basin and their corresponding annual residence times. These zones are important because the flushing times vary greatly among locations and consequently affect how nutrient reductions will impact these distinct areas of the basin. The project zones identify large areas where projects should be implemented to ensure that the load reductions achieve the desired response for each subbasin.NIRL Subbasin was split into two project zones, as follows:
North A – Turnbull Creek to NASA Causeway (State Road 405).
North B – NASA Causeway to Melbourne Causeway (U.S. Highway 192).
DEP first adopted the NIRL BMAP in 2013 to implement total nitrogen TN and total phosphorus TP TMDLs. BMAPs are designed to be implemented in a phased approach. In 2018, DEP and several local stakeholders were developing several components of an updated BMAP, including the local completion and DEP review of a new water quality model, the Spatial Watershed Iterative Loading (SWIL) Model. The SWIL Model was developed through cooperative funding provided by Brevard County, all of its cities, and Florida Department of Transportation (FDOT) District 5, as well as support from the U.S. Air Force, in an effort to update the data being used to predict loading. In this BMAP update, the SWIL Model is used to estimate loading to the CIRL. The percent reductions adopted in the original TMDL rules are applied as the water quality targets.
[bookmark: _Hlk30945209]This 2020 BMAP was developed based on several changes since the 2013 BMAP was adopted, including updated modeling efforts, boundary adjustments, updated allocations and load reductions to the responsible stakeholders, updated management actions to achieve nutrient reductions, and a revised monitoring plan to continue to track trends in water quality. This update sets a deadline for achieving load reductions no later than 2035, which is 22 years after the initial BMAP adoption in 2013.
As part of the adaptive management process for this BMAP, DEP will explore refinements to the SWIL Model used to develop BMAP allocations and estimate project credits. This effort could include updates to some of the SWIL Model input layers (e.g. land use, soils, etc.), the verification of watershed boundaries in some areas, revisions to the model period of record, and the validation of predicted flows in selected calibration basins. There are also several optional tasks that could streamline efforts during the load allocation and project calculation processes. The SWIL Model revisions may change the loading estimates presented in this BMAP, and may therefore result in changes to allocations in future iterations of the BMAP. Although the direction and magnitude of those changes is uncertain, DEP anticipates that some may be higher, and some may be lower.
[bookmark: _Hlk30944942]Summary of Load Reductions
[bookmark: _Hlk55386468][bookmark: _Hlk30946315]DEP requested stakeholders provide information on management actions, including projects, programs, and activities, that may reduce nutrient loads to the NIRL. Management actions are included in the BMAP to address nutrient loads to the lagoon and have to meet several criteria to be considered eligible for credit. The estimated reductions of activities completed to date are provided in Table ES-1. Figure ES-2 and Figure ES-3 show progress towards the TN and TP TMDL load reductions through July 31, 2020. 
[bookmark: _Hlk30946333]To achieve the TMDLs, stakeholders must identify and submit additional local projects as well as determine the significant funding that will be necessary. Enhancements to programs addressing basinwide sources will also be required. 
[bookmark: _Ref55404098][bookmark: _Ref56177168][bookmark: _Ref55404094][bookmark: _Toc58513897][bookmark: _Toc58745907][bookmark: _Toc56428109][bookmark: _Toc58576480]Table ES-1. Progress to date in the NIRL BMAP area by project zone
lbs/yr = pounds per year
	Project Zone
	TN Reduction (lbs/yr)
	% Achieved towards TN Target
	TP Reduction (lbs/yr)
	% Achieved towards TP Target

	A
	41,071
	34.6
	7,845
	39.9

	B
	65,340
	48.8
	14,709
	57.6

	Total
	106,411
	42.1
	22,554
	49.9



Source Requirements 
Florida law (Section 403.086, Florida Statutes [F.S.], and Chapter 2020-150, Laws of Florida) requires all domestic wastewater facilities directly discharging to surface waters of the state within or connected to the IRL to meet advanced wastewater treatment requirements no later than July 1, 2025. Additionally, this BMAP sets TN and TP effluent limits in the NIRL for individually permitted domestic wastewater facilities and their associated rapid rate land application (RRLA) effluent disposal systems and reuse activities, unless the owner or operator can demonstrate reasonable assurance that the discharge or associated RRLA or reuse activity would not cause or contribute to a failure to achieve the TMDLs or an exceedance of water quality standards. Local governments must also develop remediation plans to address loads from wastewater facilities and septic systems in the BMAP area. 
[bookmark: _Hlk55303799][bookmark: _Hlk56792767]Agricultural nonpoint sources are a contributor of TN and TP loading to the NIRL. Since the adoption of the NIRL BMAP in 2013, some agricultural producers have enrolled in the Florida Department of Agriculture and Consumer Services (FDACS) Best Management Practices (BMP) Program. However, enrollment still falls well short of the full participation requirement under law, and for those producers that have enrolled, the onsite verification of BMP implementation is inconsistent and incomplete. Sufficient agricultural BMP enrollment and implementation verification will be necessary to achieve the TMDLs. FDACS continues to work to improve enrollment percentages in the basin and will be undertaking implementation verification site visits on enrolled producers at least every two years to carry out its statutory authority and fulfill its statutory obligations to facilitate enrollment and implementation verification, pursuant to Paragraphs 403.067(7)(c) and 403.067(7)(d), F.S.
Within five years of the adoption of this BMAP, DEP will evaluate any entity located in the BMAP area that serves a minimum resident population of at least 1,000 individuals who are not currently covered by a municipal separate storm sewer system (MS4) permit and designate eligible entities as regulated MS4s, in accordance with Chapter 62-624, Florida Administrative Code (F.A.C.). In accordance with Subsection 373.4131(6), F.S., DEP and the water management districts are planning to update the stormwater design and operation requirements in Environmental Resource Permit rules and incorporate the most recent scientific information available to improve nutrient reduction benefits.
Water Quality Monitoring
The updated NIRL BMAP monitoring network consists of seven stations sampled by the SJRWMD. The monitoring plan also includes research priorities to better understand the lagoon, nutrient sources, and the responses of seagrass to nutrient loading, both internal and external, to the lagoon.
BMAP Cost
The project costs provided for the BMAP may include capital costs as well as those associated with construction, routine operations and maintenance, and monitoring. Many BMAP projects were built to achieve multiple objectives, and not just nutrient reductions. Funds for some projects have already been spent, others have been obligated to ongoing projects, and the remainder are yet to be appropriated.
The funding sources for the projects range from local public and private contributions to state and federal legislative appropriations. DEP will continue to work with stakeholders to explore new opportunities for funding assistance to ensure that the activities listed in this BMAP can be maintained at the necessary level of effort and that additional projects can be constructed by 2035.
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Draft Upper Ocklawaha Basin Management Action Plan Supplemental Report, September 2017
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[bookmark: _Ref58426346][bookmark: _Toc58513898][bookmark: _Toc58683281][bookmark: _Toc58684140][bookmark: _Toc58576017][bookmark: _Toc58605336]Figure ES-2. Estimated progress towards the NIRL BMAP TN milestones with projects completed through July 31, 2020
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[bookmark: _Ref58426356][bookmark: _Toc58513899][bookmark: _Toc58683282][bookmark: _Toc58684141][bookmark: _Toc58576018][bookmark: _Toc58605337]Figure ES-3. Estimated progress towards meeting the NIRL BMAP TP milestones with projects completed through July 31, 2020



[bookmark: _Toc31199644][bookmark: _Toc58684879][bookmark: _Toc58592533][bookmark: _Hlk30964138]Background Information
[bookmark: _Toc31199645][bookmark: _Hlk30964215][bookmark: _Hlk480550256][bookmark: _Hlk494377065][bookmark: _Toc58684880][bookmark: _Toc58592534] Water Quality Standards and Total Maximum Daily Loads (TMDLs)
[bookmark: _GoBack]Florida's water quality standards are designed to ensure that surface waters fully support their designated uses, such as drinking water, aquatic life, recreation, and agriculture. Currently, most surface waters in Florida, including many of those in the North Indian River Lagoon (NIRL), are categorized as Class III waters, meaning they must be suitable for recreation and must support fish consumption and the propagation and maintenance of a healthy, well-balanced population of fish and wildlife. In addition, many waterbody segments (also known as waterbody identification units, WBIDs) are categorized as Class II waters, which have a designated use of shellfish propagation or harvesting. Table 1 lists all designated use classifications for Florida surface waters.
[bookmark: _Ref159826726][bookmark: _Toc159826834][bookmark: _Toc233423663][bookmark: _Toc335996805][bookmark: _Toc483903005][bookmark: _Toc486848062][bookmark: _Toc21362559][bookmark: _Toc31199806][bookmark: _Toc58513900][bookmark: _Toc58745908][bookmark: _Toc58576652][bookmark: _Toc58605272]Table 1. Designated use attainment categories for Florida surface waters
1 Class I, I-Treated, and II waters additionally include all Class III uses.
	Classification
	Description

	Class I1
	Potable water supplies

	Class I-Treated1
	Treated potable water supplies

	Class II1
	Shellfish propagation or harvesting

	Class III
	Fish consumption; recreation, propagation and maintenance of a healthy, 
well-balanced population of fish and wildlife

	Class III-Limited
	Fish consumption, recreation or limited recreation, and/or propagation and maintenance of a limited population of fish and wildlife

	Class IV
	Agricultural water supplies

	Class V
	Navigation, utility, and industrial use (no current Class V designations)



[bookmark: _Hlk52103699]Class II waters in the NIRL may be used for aquaculture. The WBIDs that are designated as Class II waters are listed in Table 2. If not listed, the remaining WBIDs are Class III waters.
[bookmark: _Ref55405071][bookmark: _Toc58513901][bookmark: _Toc58745909]Table 2. Class II waters in the NIRL
	Classification
	WBID Number
	WBID Name

	Class II
	2924
	Mosquito Lagoon

	Class II
	2942A
	Turnbull Creek (Marine Segment)

	Class II
	2963A1
	Indian River Above Sebastian Inlet

	Class II
	2963B1
	Indian River Above Melbourne Causeway

	Class II
	2963C1
	Indian River Below 520 Causeway

	Class II
	2963D1
	Indian River Above 520 Causeway

	Class II
	2963EA
	Indian River Above Nasa Causeway

	Class II
	2963F2
	Big Flounder Creek

	Class II
	2963F3
	Indian River Above Max Brewer Causeway

	Class II
	3057A
	Banana River Below 520 Causeway



[bookmark: _Ref55407092]Section 303(d) of the federal Clean Water Act (CWA) requires that each state must identify its impaired waters every two years, including estuaries, lakes, rivers, and streams, that do not meet their designated uses. Florida Department of Environmental Protection (DEP) staff in the Division of Environmental Assessment and Restoration are responsible for assessing Florida's waters for inclusion on the Verified List of Impaired Waters (when a causative pollutant for the impairment has been identified) and Study List (when a causative pollutant for the impairment has not been identified and additional study is needed). These lists are then provided to the U.S. Environmental Protection Agency (EPA) as an update to the state’s 303(d) list. In 2009, DEP adopted, by Secretarial Order, revisions to the Verified List of Impaired Waters for the NIRL that identified several estuarine segments as impaired for dissolved oxygen (DO) and nutrients. The DO impairment was based on low DO concentrations measured in milligrams per liter (mg/L), and the nutrient impairment was based on an imbalance in flora and fauna because of decreases in seagrass distribution.
[bookmark: _Ref55413831][bookmark: _Toc58592535][bookmark: _Toc31199646][bookmark: _Toc58684881][bookmark: _Hlk52109647]NIRL TMDLs
TMDLs are water quality restoration goals establishing the maximum amount of a pollutant that a waterbody can assimilate without causing exceedances of water quality standards. The IRL TMDLs focus on the water quality conditions necessary for seagrass regrowth at water depth limits where seagrass historically grew in the lagoon, based on a multiyear composite of seagrass coverage. The median depth limits of seagrass coverage in the IRL decreased over the years (see Section 4.2) due to changes in water quality conditions resulting from anthropogenic influences. 
As polluted runoff reaches the lagoon, it contributes to conditions that prevent the seagrass from growing in deeper water because of elevated light attenuation. The full restoration depth-limit target for seagrass was established for each segment based on a deep edge boundary delineating the composite of 7 years of historical seagrass data for the period from 1943 to 1999. The restoration targets were set at depths where the deep edge of the seagrass beds previously grew and created a maximum depth limit for seagrass distribution. The TMDL targets allowed for a 10 % departure (shoreward) from the full restoration target seagrass depth. The 10 % departure in target depths was selected to be consistent with the water quality criteria in Chapter 62-302, Florida Administrative Code (F.A.C.), which allows for up to a 10 % reduction in the photo compensation point. 
To determine nutrient targets and reductions needed to improve lagoon water quality in each subbasin, regression relationships were used between 4 years of loading levels and the same years' seagrass depth limit (the percent departure from the full restoration). Total nitrogen (TN) and total phosphorus (TP) targets were developed from the median concentrations observed where seagrass depth limits were within the 10 % departure (shoreward) from their full restoration levels. These targets should result in nutrient reductions that allow seagrass to grow almost to the depths previously seen in the area. Table 3 lists the TMDLs and pollutant load allocations adopted by rule for the NIRL.
[bookmark: _Ref55405147]

[bookmark: _Ref55408247][bookmark: _Toc58513902][bookmark: _Toc58745910][bookmark: _Toc58576482][bookmark: _Toc58576654][bookmark: _Toc58605274]Table 3. NIRL TMDLs
NPDES = National Pollutant Discharge Elimination System.
	WBID
	Waterbody
	NPDES 
Stormwater TN 
(% reduction)
	NPDES 
Stormwater TP 
(% reduction)

	2963F
	Indian River above Max Brewer
	35
	47

	2963E
	Indian River above NASA Causeway
	35
	47

	2963D
	Indian River above 520 Causeway
	36
	53

	2963B+2963C
	Indian River above Melbourne Causeway
	36
	48



Additionally, this BMAP addresses adopted TMDLs for two tributaries to the NIRL. A summary of reductions for the NIRL Tributaries appears in Table 4. For Addison Creek (WBID 3028), no further nutrient load reductions were requested beyond those already established for the main stem seagrass nutrient TMDLs. For the Eau Gallie River (WBID 3082), the total nitrogen (TN) and total phosphorus (TP) target loads defined in the TMDLs are different from the main stem; there is also a biochemical oxygen demand (BOD) TMDL for the Eau Gallie River. The tidal portion of the Eau Gallie River consistently showed high annual average chlorophyll a concentrations, and so the loading targets for the Eau Gallie are the natural background nutrient condition, which require a 51 % TN reduction and a 58 % TP reduction of nonpoint source loads based on the Hydrological Simulation Program–Fortran (HSPF) Model for the period from 1996 to 2005.
[bookmark: _Ref55408393][bookmark: _Ref58921916][bookmark: _Toc58513903][bookmark: _Toc58745911][bookmark: _Toc58576483][bookmark: _Toc58576655][bookmark: _Toc58605275]Table 4. NIRL Tributary TMDLs
	WBID
	Waterbody
	NPDES 
Stormwater TN 
(% reduction)
	NPDES 
Stormwater TP 
(% reduction)
	Project Zone

	3028
	Addison Creek
	35
	47
	A

	3082
	Eau Gallie River
	51
	58
	B



[bookmark: _Hlk30964386][bookmark: _Toc31199647][bookmark: _Toc58684882][bookmark: _Toc58592536] NIRL Basin Management Action Plan (BMAP)
A BMAP is a framework for water quality restoration that contains local and state commitments to reduce pollutant loading through current and future projects and strategies. BMAPs contain a comprehensive set of solutions, such as permit limits on wastewater facilities, urban and agricultural best management practices, (BMPs), and conservation programs designed to achieve pollutant reductions established by a TMDL. These broad-based plans are developed with local stakeholders and rely on local input and commitment for development and successful implementation. BMAPs are adopted by DEP Secretarial Order and are legally enforceable. 
The Florida Watershed Restoration Act (FWRA), Subparagraph 403.067(7)(a)1., Florida Statutes (F.S.), establishes an adaptive management process for BMAPs that continues until the TMDLs are met. This approach allows for incrementally reducing loadings through the implementation of projects and programs, while simultaneously monitoring and conducting studies to better understand water quality dynamics (sources and response variables) in each impaired waterbody. The NIRL BMAP was first adopted in February 2013. An adaptive management process that is statutorily required, such as the changes made in this updated BMAP, will continue until the TMDLs are met.
This document serves as an update to the 2013 BMAP. Figure 1 shows the NIRL BMAP area.
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[bookmark: _Ref55405270][bookmark: _Toc58514012][bookmark: _Toc58683283][bookmark: _Toc58684142][bookmark: _Ref55408511][bookmark: _Toc58575548][bookmark: _Toc58605338]Figure 1. NIRL BMAP area

[bookmark: _Toc31199649][bookmark: _Toc58684883]Pollutant Sources
There are various sources of pollution in the NIRL. Nonpoint (i.e., diffuse) sources in the watershed contribute the majority of the TN and TP loads to the NIRL and include urban and agricultural runoff. For additional information on other sources not directly addressable through anthropogenic activities, please refer to Section 1.2.4. The Mosquito Lagoon, to the north, is being addressed through a reasonable assurance plan.
Chapter 1. [bookmark: _Toc58513554][bookmark: _Toc58513962][bookmark: _Toc58513557][bookmark: _Toc58513965][bookmark: _Toc31199650][bookmark: _Toc58684884][bookmark: _Ref26615642][bookmark: _Toc26616014]
1.1. 
1.2. 
1.2.1. 
[bookmark: _Ref56192457]Agricultural Nonpoint Sources
[bookmark: _Hlk56792793][bookmark: _Hlk56794904][bookmark: _Hlk55303997]The primary agricultural land uses in the NIRL BMAP area are fallow, grazing lands, and citrus. Other agricultural land uses include nurseries, field/row crops, and horse farms/specialty farms. Most of the horse farms are small, noncommercial hobby farms. Because of urban encroachment, citrus health issues (freeze/disease), and the downturn in the economy, a majority of previously existing citrus operations have been destroyed or abandoned, have significantly lowered their production acreage, or have transitioned to another commodity. In recent years, some of this acreage may have also shifted to nonagricultural/urban uses. 
Per Section 403.067, F.S., when DEP adopts a BMAP that includes agriculture, it is the agricultural landowner's responsibility either to implement BMPs adopted by the Florida Department of Agriculture and Consumer Services (FDACS) to help achieve load reductions, or to conduct water quality monitoring pursuant to Chapter 62-307, F.A.C. Landowners that do not enroll in the BMP Program or conduct water quality monitoring are referred to DEP for enforcement action. To date, FDACS' Office of Agricultural Water Policy (OAWP) has adopted BMP manuals by rule for cow/calf, citrus, vegetable and agronomic crops, nurseries, equine, sod, dairy, poultry, and specialty fruit and nut operations.
To enroll in the BMP Program, landowners first meet with OAWP to determine the BMPs that are applicable to that individual operation. The landowner must then submit to OAWP a Notice of Intent (NOI) to implement the BMPs on the checklist from the applicable BMP manual. Because many agricultural operations are diverse and are engaged in the production of multiple commodities, a landowner may be required to sign multiple NOIs for a single parcel.
OAWP is required to verify that landowners are properly implementing the BMPs identified in their NOIs. Rule 5M-1.008, F.A.C., outlines the procedures used to verify the implementation of agricultural BMPs. BMP implementation is verified through site visits conducted by OAWP staff at least every two years, as required by Subparagraph 403.067(7)(d)3, F.S. Producers not properly implementing BMPs according to the process outlined in Chapter 5M-1, F.A.C., are referred to DEP for enforcement action after attempts at corrective and remedial action are exhausted.
[bookmark: _Hlk57985876]FDACS staff conduct site visits to verify that all BMPs are being properly implemented and to review nutrient and irrigation management records. In addition, OAWP verifies that cost-share items are being implemented correctly. Site visits are prioritized based on the date the NOI was signed, the date of the last BMP verification site visit, and whether the operation has received cost-share funding. FDACS undertakes these onsite inspections at least every two years and provides DEP with aggregated information on nutrient amounts being applied. 
Where water quality problems are detected for agricultural nonpoint sources despite the appropriate implementation of adopted BMPs, a reevaluation of the BMPs shall be conducted pursuant to Subparagraph 403.067(7),(c)4, F.S. If the reevaluation determines that the BMPs or other measures require modification, the applicable rule (BMP manual) will be revised to require implementation of the modified practice. Continuing water quality problems may be detected through the monitoring component of the BMAP and other DEP and St. Johns River Water Management District (SJRWMD) activities. If a reevaluation of the BMPs is needed, FDACS will also include DEP, SJRWMD, and other partners in the process. Additional information on the evaluation of BMPs is provided in Section 2.3.1.
Under Paragraph 403.067(7)(c), F.S., the proper implementation of FDACS-adopted, DEP-verified BMPs, in accordance with FDACS rules, provides a presumption of compliance with state water quality standards for the pollutants addressed by the BMPs. For the BMAP, the implementation of agricultural BMPs will be documented based on participation in FDACS' BMP Program. Table 5 and Table 6 summarize the agricultural land use enrolled in BMP programs for the entire NIRL BMAP area and by project zone, respectively. Enrollment is as of July 2020, and the agricultural acreage in each basin is based on the Florida Statewide Agricultural Irrigation Demand (FSAID) VII Geodatabase. Appendix C provides more information on agricultural activities in the NIRL BMAP area.
[bookmark: _Ref55405410][bookmark: _Ref55408758][bookmark: _Toc58513904][bookmark: _Toc58745912][bookmark: _Toc58576484][bookmark: _Toc58576656][bookmark: _Toc58605276]Table 5. Agricultural land use acreage enrolled summary in the BMP Program in the NIRL BMAP area as of July 2020
	Category
	Acres

	FSAID VII agricultural acres in the BMAP area
	7,256

	Total agricultural acres enrolled
	401

	% of FSAID VII agricultural acres enrolled
	6


[bookmark: _Toc31199887]
[bookmark: _Ref55405460][bookmark: _Ref55408767][bookmark: _Toc58513905][bookmark: _Toc58745913][bookmark: _Toc58576485][bookmark: _Toc58576657][bookmark: _Toc58605277]Table 6. Agricultural land use acreage enrolled in the BMP Program in the NIRL BMAP area by project zone
	Project Zone
	Total FSAID VII Agricultural Acres
	Agricultural Acres Enrolled
	% of Agricultural Acreage Enrolled

	A
	5,683
	327
	6

	B
	1,573
	74
	5

	Total
	7,256
	401
	6






UNENROLLED AGRICULTURAL ACREAGE
[bookmark: _Hlk55304214]Agricultural land use designation is not always indicative of current agricultural activity and consequently presents challenges to estimating load allocations accurately as well as enrolling every agricultural acre in an appropriate BMP manual. To characterize unenrolled agricultural acres, OAWP identified FSAID VII features outside the BMP enrollment areas using geographic information system (GIS) software (see Appendix C for details). Table 7 summarizes the results of that analysis.
[bookmark: _Ref55405614][bookmark: _Ref55408932][bookmark: _Ref55405608][bookmark: _Toc58513906][bookmark: _Toc58745914][bookmark: _Toc58576658][bookmark: _Toc58605278]Table 7. Summary of unenrolled agricultural land use acreage in the NIRL BMAP area
Note: Because of geometric variations between shapefiles used in the unenrolled agricultural lands analysis performed by OAWP, the unenrolled agricultural acres differ from subtraction of the FSAID VII Agricultural Acres in the BMAP and the Total Agricultural Acres Enrolled referenced in Table 5.
	Category
	Acres

	Unenrolled agricultural acres
	6,855

	Acres identified within slivers of unenrolled agricultural areas
	164

	Lands without enrollable agricultural activity (e.g., tribal lands, residential development, and parcels with Florida Department of Revenue (DOR) use codes 70-98)
	1,515

	Total lands with potentially enrollable agricultural activities
	5,176




As of July 2020, OAWP had enrolled 401 agricultural acres in BMPs. Considering the results of the analysis shown in Table 7, the total acreage with the potential to have agricultural activities that can be enrolled in FDACS' BMP Program in the watershed is 5,577 acres. Using this adjusted agricultural acreage, 7 % of agricultural acres have been enrolled. 
Analyzing land use data and parcel data is a valuable first step in identifying the agricultural areas that provide the greatest net benefits to water resources for enrollment in FDACS' BMP Program, as well as prioritizing implementation verification visits in a given basin. OAWP will continue to enroll agricultural lands in the BMP Program, focusing on intensive operations, including irrigated acreage, dairies and nurseries, parcels greater than 50 acres in size, and agricultural parcels adjacent to waterways. 
The next step to help prioritize the enrollment efforts could use the parcel loading information derived from the Spatial Watershed Iterative Loading (SWIL) Model. This effort could help FDACS identify specific parcels with the highest modeled nutrient loading. These parcels could then be targeted for the enrollment and implementation of BMPs, as well as the verification of BMP implementation.
AQUACULTURE
Under the CWA, aquaculture activities are defined as a point source. Since 1992, all aquaculture facilities have been regulated by DEP, the water management district, or both, through a general fish farm permit authorized by Section 403.814, F.S. In 1999, the Florida Legislature amended Chapter 597, F.S., Florida Aquaculture Policy Act, to create a program within FDACS requiring Floridians who commercially culture aquatic species to annually acquire an Aquaculture Certificate of Registration and implement Chapter 5L-3, F.A.C., Aquaculture BMPs. Permit holders must reapply to be certified every year.
However, as with agricultural land use in Florida, aquaculture facilities are frequently in and out of production. The facilities for which acreages were provided may no longer be in operation and there may be new companies in different parts of the watershed. In the NIRL subbasin, 85 acres of aquaculture are estimated to be under certification with FDACS' Division of Aquaculture as of September 2020. For the purposes of the BMAP, OAWP delineated the aquaculture facilities using parcel data. Since the acreages were not delineated to just the tank, pond, or pool areas, in most cases these calculations overestimate the acreages of aquaculture activity. 
[bookmark: _Toc31199651][bookmark: _Toc58684885][bookmark: _Toc58592537] Municipal Separate Storm Sewer Systems (MS4s)
Many of the municipalities in the watershed are regulated by the Florida National Pollutant Discharge Elimination System (NPDES) Stormwater Program. An MS4 is a conveyance or system of conveyances, such as roads with stormwater systems, municipal streets, catch basins, curbs, gutters, ditches, constructed channels, or storm drains.
If an MS4 permittee is identified as a contributor in the BMAP, the permitted MS4 must undertake projects specified in the BMAP. The BMAP projects required to be undertaken by MS4s are detailed for each project zone in Chapter 3. Phase I and Phase II MS4s are required to implement stormwater management programs (SWMPs) to reduce pollutants to the maximum extent practicable and address applicable TMDL allocations. Phase I MS4 permits include assessment practices to determine the effectiveness of SWMPs, which can include water quality monitoring. Both Phase I and Phase II MS4 permits include provisions for the modification of SWMP activities, at the time of permit renewal, for consistency with the assumptions and requirements of the adopted BMAP. There are no Phase I MS4 permittees in the NIRL as of September 2020.
PHASE II MS4 STORMWATER PERMIT REQUIREMENTS
Table 8 lists the Phase II MS4s in the NIRL as of September 2020. Under a generic permit, the operators of regulated Phase II MS4s must develop a SWMP that includes BMPs with measurable goals and a schedule for implementation to meet the following six minimum control measures:
Public Education and Outreach – Implement a public education program to distribute educational materials to the community or conduct equivalent outreach activities about the impacts of stormwater discharges on waterbodies and the steps that the public can take to reduce pollutants in stormwater runoff.
Public Participation/Involvement – Implement a public participation/involvement program that complies with state and local public notice requirements.
Illicit Discharge Detection and Elimination – Subsection 62-624.200(2), F.A.C., defines an illicit discharge as "…any discharge to an MS4 that is not composed entirely of stormwater…," except discharges under an NPDES permit, or those listed in rule that do not cause a violation of water quality standards. Illicit discharges can include septic/sanitary sewer discharge, car wash wastewater, laundry wastewater, the improper disposal of auto and household toxics, and spills from roadway accidents.
Develop, if not already completed, a storm sewer system map showing the location of all outfalls, and the names and location of all surface waters of the state that receive discharges from those outfalls.
To the extent allowable under state or local law, effectively prohibit, through ordinance or other regulatory mechanism, nonstormwater discharges into the storm sewer system and implement appropriate enforcement procedures and actions.
Develop and implement a plan to detect and address nonstormwater discharges, including illegal dumping, to the storm sewer system.
Inform public employees, businesses, and the general public of hazards associated with illegal discharges and improper waste disposal.
Construction Site Runoff Control – 
Implement a regulatory mechanism to require erosion and sediment controls, as well as sanctions to ensure compliance, to reduce pollutants in any stormwater runoff to the Phase II MS4 from construction activity that results in a land disturbance greater than or equal to an acre. Construction activity disturbing less than one acre must also be included if that construction activity is part of a larger common plan of development or sale that would disturb one acre or more. 
[bookmark: _Hlk12951020]Develop and implement requirements for construction site operators to implement appropriate erosion and sediment control BMPs.
Implement requirements for construction site operators to control waste such as discarded building materials, concrete truck washout, chemicals, litter, and sanitary waste at the construction site that may cause adverse impacts to water quality.
Develop and implement procedures for site plan review that incorporate the consideration of potential water quality impacts.
[bookmark: _Hlk12951072]Develop and implement procedures for receiving and considering information submitted by the public.
[bookmark: _Hlk12951100]Develop and implement procedures for site inspection and the enforcement of control measures.
Postconstruction Runoff Control – Implement and enforce a program to address the discharges of postconstruction stormwater runoff from areas with new development and redevelopment. (Note: In Florida, Environmental Resource Permits issued by water management districts typically serve as a Qualifying Alternative Program for purposes of this minimum control measure.)
Pollution Prevention/Good Housekeeping – Implement an operations and maintenance program that has the ultimate goal of preventing or reducing pollutant runoff from MS4 operator activities, such as park and open space maintenance, fleet and building maintenance, new construction and land disturbances, stormwater system maintenance, and staff training in pollution prevention.
The "NPDES Generic Permit for Discharge of Stormwater from Phase II MS4s," Paragraph 62-621.300(7)(a), F.A.C., also requires that if the permittee discharges stormwater to a waterbody with an adopted TMDL pursuant to Chapter 62-304, F.A.C., then the permittee must revise its SWMP to address the assigned wasteload in the TMDL. Additionally, in accordance with Section 403.067, F.S., if an MS4 permittee is identified in an area with an adopted BMAP or a BMAP in development, the permittee must comply with the adopted provisions of the BMAP that specify activities to be undertaken by the permittee.
DEP can designate an entity as a regulated Phase II MS4 if its discharges meet the requirements of the rule and are determined to be a significant contributor of pollutants to surface waters of the state in accordance with Rule 62-624.800, F.A.C. A Phase II MS4 can be designated for regulation when a TMDL has been adopted for a waterbody or segment into which the MS4 discharges the pollutant(s) of concern. If an MS4 is designated as a regulated Phase II MS4, it is subject to the conditions of the "NPDES Generic Permit for Stormwater Discharges from Phase II MS4s." A list of those permitted entities can be found in Table 8.
[bookmark: _Ref55405874][bookmark: _Toc58513907]

[bookmark: _Ref58829360][bookmark: _Ref55409148][bookmark: _Toc58745915][bookmark: _Toc58576486][bookmark: _Toc58576659][bookmark: _Toc58605279]Table 8. Entities in the NIRL designated as Phase II MS4s as of September 2020
	Permittee
	Permit Number

	Brevard County
	FLR04E052

	Volusia County
	FLR04E033

	City of Cocoa
	FLR04E032

	City of Edgewater
	FLR04E016

	City of Melbourne
	FLR04E027

	City of Oak Hill
	FLR04E130

	City of Rockledge
	FLR04E047

	City of Titusville
	FLR04E079

	Town of Indialantic
	FLR04E030

	Florida Department of Transportation (FDOT) District 5
	FLR04E024



[bookmark: _Toc31199652][bookmark: _Ref55412195][bookmark: _Toc58684886][bookmark: _Toc58592538]Septic Systems 
Based on data from the Florida Department of Health (FDOH) Florida Water Management Inventory (FLWMI), there are 16,171 known or likely septic systems (onsite sewage treatment and disposal systems [OSTDS]) located throughout the NIRL (Figure 2). Table 9 summarizes the number of septic systems by project zone.
[bookmark: _Ref55406006][bookmark: _Ref55409244][bookmark: _Toc58576487][bookmark: _Toc58576660][bookmark: _Toc58513908][bookmark: _Toc58745916][bookmark: _Toc58605280]Table 9. Septic system counts by project zone
	NIRL Project Zone
	Total Number of Septic Systems

	A
	1,998

	B
	14,173

	Total
	16,171
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[bookmark: _Ref55405975][bookmark: _Ref55409198][bookmark: _Ref55405971][bookmark: _Toc58514013][bookmark: _Toc58683284][bookmark: _Toc58684143][bookmark: _Toc58575549][bookmark: _Toc58576488][bookmark: _Toc58605339]Figure 2. Location of septic systems in the NIRL
[bookmark: _Toc31199653][bookmark: _Toc58684887][bookmark: _Toc58592539]Urban Nonpoint Sources
Subsubparagraph 403.067(7)(b)2.f., F.S., prescribes the pollutant reduction actions required for nonagricultural pollutant sources that are not subject to NPDES permitting. Non-MS4 sources must also implement the pollutant reduction requirements detailed in a BMAP and are subject to enforcement action by DEP or a water management district if they fail to implement their responsibilities under the BMAP. Table 10 lists the urban nonpoint sources in the NIRL.
[bookmark: _Ref55406045][bookmark: _Ref55409326][bookmark: _Toc58513909][bookmark: _Toc58745917][bookmark: _Toc58576489][bookmark: _Toc58576661][bookmark: _Toc58605281]Table 10. Urban nonpoint sources in the NIRL
	Type of Entity
	Participant

	Government Entities and Special Districts
	Kennedy Space Center



[bookmark: _Toc31199654][bookmark: _Ref55412356][bookmark: _Toc58684888][bookmark: _Toc58592540][bookmark: _Hlk58327708]Wastewater Treatment Facilities (WWTFs)
As of September 2020, DEP identified 18 individually permitted wastewater facilities or activities in the NIRL Subbasin. A list of wastewater facilities in the NIRL as of September 2020 is provided below in Table 11 and a map of their locations is shown in Figure 3.
[bookmark: _Ref55406069][bookmark: _Ref55409379][bookmark: _Toc58513910][bookmark: _Toc58745918][bookmark: _Toc58576490][bookmark: _Toc58576662][bookmark: _Toc58605282]Table 11. Wastewater facilities in the NIRL as of September 2020
FPL = Florida Power and Light; RV = Recreational vehicle; VC = Volusia County; BCUD =  Brevard County Utility District
	[bookmark: _Hlk58506605]Facility ID
	Facility Name

	FL0001473
	FPL - Cape Canaveral Power Plant

	FL0021521
	Cocoa, City of - Cocoa Water Reclamation Facility

	FL0021571
	Rockledge, City Of

	FL0103268
	Titusville, City of - North - Osprey WWTF

	FLA010264
	Housing Authority of Brevard County WWTF

	FLA010323
	David B Lee Wastewater Treatment Plant

	FLA010336
	Orlando Utilities Commission - Indian River Plant

	FLA010354
	Canebreaker Condo

	FLA010355
	Tropical Trail Village WWTF

	FLA010358
	Willow Lakes RV Park WWTF

	FLA010361
	River Forest Mobile Home Park WWTF

	FLA010365
	Palm Harbor Mobile Home Park WWTF

	FLA010375
	Oak Point Mobile Home Park WWTF

	FLA010377
	Merritt Island Utility Company WWTF

	FLA010383
	Riverview Mobile Home & RV Park

	FLA011175
	Magnolia Village WWTF

	FLA017413
	VC/Southeast WWTF-7

	FLA102695
	BCUD/Sykes Creek Regional Wastewater Treatment Facility
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[bookmark: _Ref55406096][bookmark: _Ref55409461][bookmark: _Toc58514014][bookmark: _Toc58683285][bookmark: _Toc58684144][bookmark: _Ref55409454][bookmark: _Toc58575550][bookmark: _Toc58605340]Figure 3. Map of wastewater facilities in the NIRL

[bookmark: _Toc58684889][bookmark: _Toc58592541] Milestones and Tracking Progress
[bookmark: _Hlk56089489]The projects and activities in the BMAP are key to the overall goal of recovering seagrass in the lagoon. The estimated benefits of these implemented activities are tracked to show stakeholder efforts by determining a percentage towards the total required reductions to be achieved at each milestone. Additionally, stakeholders provide DEP with reasonable assurance that they have a plan to achieve the individually assigned reductions required in Chapter 2. Section 403.067(7)(a)6, F.S., indicates that an assessment of progress towards the BMAP milestones shall be conducted every five years, and plan revisions made as appropriate. To meet these requirements, DEP has established milestones for the years 2025, 2030, and 2035. The percent reductions in the milestones apply to the total BMAP required reductions, so as various entities implement their projects, the overall milestones are also being met.
The following percent reduction goals are proposed for each milestone and may be adjusted as the BMAP is adaptively managed through future phases:
5-year milestone in 2025: 55 % or 138,872 pounds per year (lbs/yr) of TN and 24,856 lbs/yr of TP. Based on model revisions, reset 10-year and 15-year milestones, as needed.
10-year milestone in 2030: 80 % or 201,996 lbs/yr of TN and 36,154 lbs/yr of TP. 
15-year milestone in 2035: 100 % or 252,495 lbs/yr of TN and 45,193 lbs/yr of TP.
The next milestone is in 2025, by which at least 55 % of the TN and TP required reductions must be met. Figure ES- 2 and Figure ES- 3 show the milestones as well as the cumulative TN and TP reductions over time as projects are completed in each reporting period. The deadline established by this BMAP for achieving the full load reductions is 2035, which is 22 years after the initial adoption of the 2013 BMAP.
[bookmark: _Toc31199655][bookmark: _Toc58684890][bookmark: _Toc58592542]Assumptions
The water quality impacts of BMAP implementation are based on several fundamental assumptions about the pollutants targeted by the TMDLs, modeling approaches, waterbody response, and natural processes. The following assumptions were used during the BMAP process:
Certain BMPs were assigned provisional nutrient reduction benefits for load reductions in this BMAP iteration while additional monitoring and research are conducted to quantify their effectiveness. These estimated reductions may change in future BMAP iterations as additional information becomes available.
Nutrient reduction benefits of the stakeholders' projects were calculated using the best available methodologies. Project-specific monitoring, where available, will be used to verify calculations, and reduction benefits may be adjusted as necessary.
The TMDLs require TN and TP reductions from the watershed to improve water quality, allowing seagrass to grow at greater water depths. High watershed nutrient loadings result in high chlorophyll a concentrations in the lagoon, which may indicate algal growth and a reduction in light availability to the seagrass, thus limiting the depth at which seagrass can grow. Therefore, reducing nutrient loading to the NIRL is an important factor to improving seagrass depth limits. 
The allocations do not require load reductions from areas identified as natural land use areas in the modeled land use/land cover information. These loads are considered uncontrollable, background sources, and the stakeholders are not required to make reductions on natural lands. The BMAP allocations focus on urban and agricultural stormwater sources and septic systems in the watershed.
[bookmark: _Hlk55139183][bookmark: _Toc31199656]Water is exchanged between the NIRL and other nearby waterbodies (the BRL, Central Indian River Lagoon [CIRL], and Mosquito Lagoon), and water quality conditions in the NIRL may be influenced by conditions in nearby waters. To help address these nearby conditions, separate BMAPs have been adopted for these watersheds, and a reasonable assurance plan has been adopted for the Mosquito Lagoon.
[bookmark: _Toc58684891][bookmark: _Toc58592543][bookmark: _Ref58602459][bookmark: _Ref58603290]Considerations
This BMAP requires stakeholders to implement their projects to achieve reductions within the specified period. However, the full implementation of this BMAP will be a long-term, adaptively managed process. While some of the BMAP projects and activities were recently completed or are currently ongoing, several projects require more time to design, secure funding, and construct. Regular followup and continued coordination and communication by the stakeholders will be essential to ensure the implementation of management strategies and assessment of incremental effects.
During the BMAP process, a number of items were identified that should be addressed in future watershed management cycles to ensure that future BMAPs use the most accurate information:
Harmful Algal Blooms (HABs) – HABs cause shading that stresses seagrass in the IRL, adverse effects on wildlife, and in some cases, has detrimental effects on human health. Intense and extensive algal blooms in the IRL began in 2011 and have returned periodically, with clear impacts on the extent, density, and depth where seagrasses grow; some fish kills; and, fortunately, little direct impact on human health. Compared with earlier blooms, the recent blooms have been dominated by smaller species of algae called nanoplankton and picoplankton. SJRWMD launched the Indian River Lagoon Protection Initiative in 2013, including a multiyear investigation that increased the understanding of the blooms. This and other research indicate it is important to persevere with projects that decrease TN and TP loads to the IRL, because that approach will limit the severity of HABs and their impacts on the system.
Land Uses – The loading estimates in the BMAP are based on land uses at a point in time, allowing the model to be calibrated. The loading estimates for this BMAP iteration were based on land use/land cover data from approximately 2015 from the water management district as well as property appraiser data. Land uses in the model will be updated during future model revisions based on the most recent and accurate data available; this may result in changes to loading estimates.
Basin Boundaries – Figure 4 shows the previous and updated BMAP boundary. Overall, 6,516 acres were added to the BMAP area and 904 acres removed, resulting in a net addition of 5,692 acres. When the 2013 basin boundary was developed, there was uncertainty about whether some areas drained to the IRL, to the Upper St. Johns River, or to other adjacent waterbodies. The boundaries were adjusted based on the best information available about the hydrology of the IRL but future adjustments may be made because of flow diversions or updated information.
Jurisdictional Boundaries – Entities may experience shifts in their jurisdictional boundaries over time that require allocation adjustments. Changes to the boundaries and/or allocations for these stakeholders may be made as necessary and reflected in future BMAP iterations.
SWIL Model – The SWIL Model was initially developed through cooperative funding provided by Brevard County, all of its cities, and FDOT District 5, as well as support from the U.S. Air Force for purposes other than the BMAPs, and DEP will explore refinements that may help improve the future use of the SWIL for the IRL BMAPs. This effort could include updates to some of the SWIL Model input layers, the verification of watershed boundaries in some areas, revisions to the model period of record, and the validation of predicted flows in selected calibration basins. There are also several optional tasks that could streamline efforts during the load allocation and project calculation processes. DEP expects the SWIL Model enhancements to change the loading estimates and the NIRL future allocations. Although the direction and magnitude of those changes are not certain, DEP anticipates that some may be higher, and some may be lower.
Community Development District (CDD) Responsibilities – DEP has had several communications with the CDDs located in the NIRL. In the NIRL, CDDs were assigned allocations only if three criteria were met: (1) there is development—i.e., roads and infrastructure—in the CDD area; (2) the CDD does not discharge to an MS4; and (3) the CDD pays a stormwater fee and receives a refund of this fee. CDDs that did not receive an allocation in this BMAP iteration may receive allocations in future BMAP iterations.
Complexity of the Problem – DEP acknowledges the complexity of the dynamics affecting the water quality of the NIRL; therefore, this BMAP is designed to encompass a wide variety of projects and management strategies that will cumulatively act to significantly reduce nutrient loads. In estuarine-based systems, the interaction with ocean waters and freshwater inflows adds variability to the water quality conditions—including those associated with climate change and sea level rise. Other factors such as inconsistency in annual rainfall amounts, changing land uses and farming practices, and internal nutrient sources such as muck deposits also complicate measuring the benefits of projects and management strategies and understanding the relationship between nutrient loading and the biological response of the seagrass deep edge. 
Sea Level Rise – Sea level rise and changes in lagoon water depth over time affect the depth at which seagrass growth is measured for TMDL compliance and for assessing seagrass restoration. Improved depth estimates and seagrass deep edge assessment techniques are needed.
Previous Restoration Efforts – DEP recognizes that stakeholders throughout the watershed have implemented stormwater management projects prior to the implementation of the TMDLs and that these efforts have benefited water quality. Projects completed in 2000 or later are considered for credits and inclusion in the BMAP.
Atmospheric Deposition – Reductions in atmospheric deposition have occurred over time and are expected to continue. This BMAP and all subsequent nutrient reduction requirements and allowable loads factor only those inputs directly from the watershed. DEP will continue to monitor atmospheric deposition and may address it in future BMAP iterations as part of the adaptive management process.
Muck Deposition – Muck deposits contain nutrients that flux into the water column, increasing the abundance of phytoplankton, drift macroalgae, and epiphytes that attenuate light and constrain seagrass growth and propagation. Most IRL muck originates from upland soils and vegetation. For this reason, stringent watershed soil-erosion control and soil/vegetation containment measures are needed. Without such measures in place, muck removal will need to be frequently repeated, which is neither cost-effective nor time efficient. Ideally, muck removal projects should be performed in conjunction with soil and vegetation retention programs, including public awareness activities, that limit the amount of muck material deposited into the IRL. The SWIL Model does not automatically take this process into account; however, guidance documentation has been developed for crediting muck removal projects specifically from the lagoon.
Tributary Water Quality Impairments – DEP has identified nutrient and DO impairments in many of the NIRL tributaries, but has not yet set water quality targets with TMDLs. These waters include Turnbull Creek marine (WBID 2942A), Turnbull Creek freshwater (WBID 2942B), and Horse Creek (WBID 3081). The relationship between the tributary loads and the targets set for the lagoon proper will be defined as tributary TMDLs are developed. As a general principle, when DEP establishes upstream TMDLs, downstream water quality targets are considered. In this case, when DEP establishes NIRL tributary TMDLs, meeting the lagoon's seagrass depth targets will be considered. Future tributary TMDLs may allow the targeting of specific watersheds for nutrient load reductions.
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[bookmark: _Ref55409725][bookmark: _Ref55406482][bookmark: _Toc58514015][bookmark: _Toc58684145][bookmark: _Toc58575551][bookmark: _Toc58576492][bookmark: _Toc58605341]Figure 4. 2013 BMAP area boundary and 2020 BMAP area boundary


[bookmark: _Toc58684892][bookmark: _Toc58592544] Economic Benefits of the IRL System
The IRL is a valuable ecological and economic asset for the state of Florida and the counties that border the lagoon and its tributaries. It is considered one of the most biologically diverse estuaries in North America and was recognized as part of the National Estuary Program (NEP) in 1990. The lagoon directly and indirectly supports a large part of the region's and the state's economy. The basin supports the multimillion-dollar Indian River citrus industry and boat and marine sales industries. Finfish and shellfish harvesting from the lagoon also contribute to local economies.
[bookmark: _Hlk58923356][bookmark: _Hlk58923333]An economic study prepared by the East Coast Florida Regional Planning Council (ECFRPC) and Treasure Coast Regional Planning Council (TCRPC) (ECFRPC and TCRPC 2016) estimated the total annual value of the lagoon's benefits at $7.6 billion, measured in 2014 dollars. This does not include the estimated $934 million in annualized real estate value added for property located on or near the IRL (Hazen and Sawyer 2008). The study area spanned from Ponce de Leon Inlet in Volusia County to Jupiter Inlet in Palm Beach County, and included all of Brevard, Indian River, St. Lucie, and Martin counties. The economic analysis was primarily conducted using the Impact Analysis for Planning (IMPLAN) Regional Economic Input/Output Model. The Model estimates direct, indirect, and induced economic effects, as outlined in Figure 5.
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[bookmark: _Ref56083999][bookmark: _Toc56083961][bookmark: _Ref56083992][bookmark: _Toc58514016][bookmark: _Toc58684146][bookmark: _Toc58575552][bookmark: _Toc58605342]Figure 5. IMPLAN Model calculation process
The primary IRL-related industry groups identified in the study are Living Resources, Marine Industries, Recreation and Visitor-Related, Resource Management, and Defense and Aerospace. The breakdown of the monetary contribution to the IRL regional economy is shown in Figure 6.
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[bookmark: _Ref56084081][bookmark: _Toc56083962][bookmark: _Toc58514017][bookmark: _Toc58684147][bookmark: _Toc58575553][bookmark: _Toc58605343]Figure 6. Total annual economic output by industry group in the IRL region, 2014

Money spent on recreation and visitor-related activities generated $1.57 billion of economic benefit. In 2014, over 7.4 million visitors traveled to the IRL region. Between 2.3 to 3.5 million visitors to the IRL region participate in IRL-related recreation, and each visitor spends an average of about $162 a day. By 2025, the IRL region is anticipated to receive over 11 million visitors annually.
The study also estimated the cost of a sustainable IRL-based economy and return on investment of achieving water quality and seagrass restoration goals for the IRL. The annualized cost of achieving the nutrient load reductions required by the four BMAPs that span the entire area was estimated at $230 million. When compared with the $7.6 billion valuation of the region's average annual economic output, the return on investment from achieving water quality and seagrass restoration goals is 33 to 1. Therefore, investing in projects and programs to improve the lagoon's water quality and seagrass beds is not only important for environmental considerations but also to improve the regional economy.


[bookmark: _Toc31011639][bookmark: _Toc31011849][bookmark: _Toc499899513][bookmark: _Toc31199657][bookmark: _Ref55406134][bookmark: _Ref55408212][bookmark: _Toc58684893][bookmark: _Ref55409503][bookmark: _Ref55413903][bookmark: _Toc58592545]Modeling, Load Estimates, and Restoration Approach
0. [bookmark: _Toc31199658][bookmark: _Toc58684894][bookmark: _Toc58592546] BMAP Modeling
Nutrient loading estimates were originally calculated for the BMAP using the Pollutant Load Screening Model (PLSM), which was expanded by SJRWMD to represent year 2000 loading (Adkins et al. 2004) in most of the IRL Watershed (excluding the IRL south of the Indian River and St. Lucie county boundary). The seagrass depth limits were developed by SJRWMD based on a series of photo-interpreted seagrass coverages from 1943 through 2001. DEP reviewed these models and the seagrass depth limits and used them to develop the IRL TMDLs that were adopted by rule (Gao 2009).
Through cooperative local effects, all the MS4 permittees within the Brevard County section of the IRL (17 entities) partnered to fund a Study Team to create a new watershed model that would update and refine the information that was used in the PLSM and associated TMDLs for the IRL. One outcome of this study was the development of the SWIL Model, which is intended to incorporate more available data, more recent conditions, and more temporally fine datasets. SWIL is a custom ESRI ArcGIS toolset, originally designed to provide a continuous monthly simulation of runoff over a 16-year period (Applied Ecology 2019).
During 2017 and 2018, while DEP prepared to calculate allocations for the Central IRL BMAP, the SWIL Model was proposed as an alternative to the previously used PLSM. Several options were presented for updating allocations during a public meeting in May 2017, and the options were discussed by DEP and stakeholders during and after the meeting. In November 2017, a presentation was made to the IRL National Estuary Program (NEP) Science, Technology, Engineering and Mathematics (STEM) Committee to provide a technical overview of the SWIL. During the annual public meeting for the IRL BMAPs in December 2018, a proposed path forward was presented that included applying the SWIL to calculate allocations for the IRL BMAPs. A technical presentation was given by the model developer at a public webinar in January 2019 to provide stakeholders with an opportunity to discuss the model further. Finally, during the annual public meeting for the IRL BMAPs in December 2019, a summary of the allocation approach using SWIL was presented.
[bookmark: _Toc31199659][bookmark: _Toc58684895][bookmark: _Toc58592547]SWIL Modeling
The initial version of SWIL was developed for the IRL in 2012 (SWIL 1.0). To address several DEP comments and to improve execution and processing time, SWIL 2.0 was released in July 2014. SWIL 3.0 was released in April 2015 with improved model calibration to the measured available gauge data, including a revised method to derive baseflow volumes and loads. SWIL 3.0 also incorporated new evapotranspiration raster datasets. SWIL 4.0 was developed in support of the 3D numerical modeling effort led by the Florida Institute of Technology. Three major changes were performed for SWIL 4.0: (1) Expansion of the model extent to provide nutrient loadings from Ponce Inlet to Fort Pierce; (2) temporal expansion to include 2011 to 2015, for a total model period of 20 years (1995 to 2015); and (3) the addition of a third land use/treatment time step using data from 2010 (Applied Ecology 2019).
[bookmark: _Toc31199660][bookmark: _Toc58684896][bookmark: _Toc58592548]SWIL Calibration
[bookmark: _Hlk58591410][bookmark: _Hlk58402443]The SWIL 3.0 version was used for calibration using flow data primarily from the CIRL. The five gauge stations included in the calibration are located in the following basins: Crane Creek, Hickory Creek, North and South prongs of the Sebastian River, and Fellsmere Canal. Few data were available in the NIRL and none in the BRL, and so the calibration is based primarily on the CIRL conditions. Also, during the calibration process, a change was made to the normalization process of the baseflow volumes by incorporating "groundwater storage depth," an area-weighted groundwater input variable (Applied Ecology, 2015). The calibration was based on simulated 1995-2010 flow volumes compared against measured data at the gauge stations. Since the treatment layer inputs to the model simulation did not incorporate BMPs beyond permit requirements after the year 2000, most projects installed from 2000 onward were not included in the calibration and are not well represented in the SWIL Model loading estimates. Therefore, projects completed from 2000 onward are eligible for BMAP credit.
[bookmark: _Toc31199662][bookmark: _Toc58684897][bookmark: _Toc58592549]Allocation Process
To generate average annual TN and TP loads from the IRL Watershed, SWIL was run using rainfall inputs that were thought to be from a representative period covering various conditions from high to low rainfall years. The outputs from this model run were used to generate a GIS-based Load Estimation Tool (LET) that included annual average loads from the watershed and was the basis of the allocation calculations.
The LET based on the SWIL Model can produce polygon outputs with loading data included. The determination of each entity's loading was performed using the LET and a GIS process. Through a series of GIS steps, polygons were generated for each stakeholder. GIS data were used to clip the area within the BMAP boundary associated with each entity's jurisdictional boundary or the codes from the model land cover data related to natural and agricultural lands. The clipping process was done sequentially, as follows:
Dispersed Water Management (DWM) or Comprehensive Everglades Restoration Plan (CERP) projects.
Roads (FDOT and Florida's Turnpike Enterprise).
Water control districts (WCDs) and water improvement district canals and rights-of-way.
Natural lands (land use codes 3000 [not including 3300], 4000, 5000, and 6000).
Agriculture (land use codes 2000 and 3300).
CDDs, if they meet the criteria.
Municipalities.
Remaining area assigned to each county.
Loads within DWM or CERP project areas were not included in the total loads for the project zone, since these land uses are being converted to treatment projects. Loads from natural land uses were not assigned to any specific entity's starting load. FDOT, agriculture, CDD’s, municipalities, and counties were assigned starting loads based on this sequential process. 
[bookmark: _Toc31199663][bookmark: _Toc58684898][bookmark: _Toc58592550]Project Credit Process
[bookmark: _Toc31199664]The LET was used to calculate updated TN and TP baseloads from all existing project treatment areas in the BMAP. The August 2020 DEP BMP Efficiencies Guidance document was used to determine the appropriate credit calculations for the various project types. Some project types that have credits based on measured data or weighed material, such as street sweeping, did not need to be updated using the LET.
[bookmark: _Hlk52642519][bookmark: _Toc58684899][bookmark: _Toc58592551] Calculation of Starting Loads and Allocations
[bookmark: _Toc478028427][bookmark: _Ref480552768][bookmark: _Toc491243155][bookmark: _Toc491243333][bookmark: _Toc491243372][bookmark: _Toc499899521][bookmark: _Ref505343823]This section describes the process used to calculate the load reductions needed to achieve the TMDLs and to allocate the load reduction requirements to the responsible stakeholders.
[bookmark: _Toc31199665][bookmark: _Toc478028421][bookmark: _Toc491243150][bookmark: _Toc491243328][bookmark: _Toc491243367][bookmark: _Toc499899518][bookmark: _Toc58684900][bookmark: _Toc58592552][bookmark: _Toc31199666]Starting Loads and Allocation of Load Reductions
DEP requested to use the SWIL 4.0 Model to update the load allocations for the second cycle of the IRL BMAPs. To develop the loads that represent updated current conditions, the SWIL Model was customized for this use with the following parameters (Applied Ecology 2018):
A 50 x 50-meter (m) cell size was used, which is a much higher spatial resolution than any previously developed watershed loading models for the IRL.
Land use corresponds to 2015 conditions and is derived from water management district land use data, property appraiser data, and local government natural communities land cover, where available.
Treatment layer (stormwater BMPs) corresponds to development conditions in approximately 2015, excluding any retrofits implemented by the stakeholders in the IRL Watershed. Retrofit projects will need to be retroactively calculated and provided as credits to the stakeholders.
Period of record rainfall that includes 2004 to 2017 data, which allows for a wide range of rainfall conditions to represent the variability in loading to the IRL. 
The outputs of this modeling effort can be described as static feature classes that include more than 1.2 million 50 x 50-m cells (as features) each. Each individual cell is associated with an estimated volume and both nitrogen and phosphorus estimated loading for the selected mean period of record conditions (Applied Ecology 2018). 
For land use and land cover, 2015 conditions were represented as derived from water management district data for nonurban land uses and from local property appraiser datasets for urban land uses. Natural community data from local governments were also incorporated, where available (Brevard County). In addition, field-validated 2015 land use datasets for Patrick Air Force Base, Cape Canaveral Air Force Station, and the Malabar Annex were used in lieu of water management district data (Applied Ecology 2018). Land covers were grouped to reflect the available event mean concentrations (EMCs) and C values that would be applied in the model (Listopad 2020).
DEP used the LET to develop the allocations (see Figure 7 and Figure 8). The percent reduction from the TMDLs was applied to the applicable areas within the BMAP. The TMDL percent reductions are based on segmented areas of the lagoon defined by both DEP WBIDs, along with breaks in the hydrology of the lagoon as defined by the SJRWMD. Areas where segments share hydrologic similarity and similar reduction percentages, as noted by the TMDLs, are defined as segment groups. Additionally, during the first phase of BMAP adoption, the hydrology defined by SJRWMD was used to define project zones in order to assess seagrass compliance. Both project zone and segment groups assist in calculating the required reduction and the allocation of each entity within the BMAP area. The total segment load from the LET was used, and the percent reduction from the TMDLs for that segment was applied to discern the total required reductions per segment. Natural lands had no reductions applied, and so the SWIL loads from natural land uses were held constant. The land cover codes considered to be "natural lands" include 3000 (upland nonforested; not including 3300), 4000 (upland forests), 5000 (water), and 6000 (wetlands). The allowable load in the segment was determined by subtracting the required reductions from the total segment load determined by the LET.
A test was performed to make sure that no reductions would be expected from natural land uses. The weighted average load per acre from natural lands for each segment was compared with the load per acre from the allowable load. If the allowable load per acre was less than the natural land load per acre, the allowable load was increased to equal the natural load per acre times the acres in the segment. This process was performed for both TN and TP loads in each segment. This adjustment was made for both TN and TP for Segment Groups IR1-5 and IR1-8 EauGallie.
Once the total required reductions for each segment were defined, the total anthropogenic load for the segment was examined. Each stakeholder's anthropogenic load was compared with the total anthropogenic load for the segment to determine its contribution to the total anthropogenic load. This percentage was considered to be representative of the stakeholder's loading contribution and that percentage of the segment's required reduction was applied to that stakeholder. If an entity was located in more than one BMAP area, the required reductions were added together to determine that entity’s total required reductions for the project zone. 
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The SWIL Model starting loads for each project zone are described in Table 12.
[bookmark: _Ref55406737][bookmark: _Ref55410146][bookmark: _Toc58576494][bookmark: _Toc58576663][bookmark: _Toc58605283][bookmark: _Toc58513911]Table 12. SWIL Model starting loads (lbs/yr)
	Project Zone
	Starting TN Load 
	% Total Load TN
	Starting TP Load 
	% Total Load TP

	A
	399,161
	53
	46,021
	48

	B
	359,923
	47
	50,203
	52

	Totals
	759,084
	100.00
	96,224
	100.00




Chapter 2. [bookmark: _Toc56186339][bookmark: _Toc56186342][bookmark: _Toc58684901][bookmark: _Toc58592553][bookmark: _Ref480546357][bookmark: _Toc497481328][bookmark: _Toc497741357][bookmark: _Toc499899541]
2.1. 
2.2. 
2.2.1. 
Low Priority Ranking Determination 
[bookmark: _Ref480547283][bookmark: _Ref497750543][bookmark: ch2t14][bookmark: _Toc497481331][bookmark: _Toc497741360][bookmark: _Toc499899547]Several stakeholders contribute less than 0.30 % of both the TN and TP loading from the watershed to the NIRL. The contribution to the overall nutrient loading from these stakeholders is low enough that reductions from these areas would have essentially no impact on the required reductions for the BMAP during this phase of implementation; therefore, these entities are currently considered a low priority for implementing reductions. Low-priority entities will be evaluated in future phases of BMAP implementation, as their contributions may change over time.
Table 13 summarizes the priority evaluation, and those stakeholders meeting the classification requirements for low priority are highlighted in grey. The stakeholder that met the low-priority classification is the City of Oak Hill. This entity is not required to meet the reduction targets for TN and TP in this phase of BMAP implementation but must continue to adhere to all requirements of their MS4 permit or other permits.
BMAP progress will be reviewed over time, and reduction requirements, including for those stakeholders with this low-priority status, will be modified in a future BMAP update as needed. TN and TP reductions may be needed from the low-priority entities in the future. Therefore, although they do not currently have a reduction responsibility, this does not exempt these stakeholders from such requirements in future BMAP updates. Any actions taken by these entities that result in TN and TP reductions will be documented for credit against any reduction requirements allocated in subsequent BMAP updates.
[bookmark: _Ref55406753][bookmark: _Ref55410363]

[bookmark: _Toc58513912][bookmark: _Toc58576495][bookmark: _Toc58576664][bookmark: _Toc58605284]Table 13. Entity contributions to total TN and TP starting loads with low priority ranking cutoff
Note: Grey highlighting and bold indicates jurisdictions meeting the classification requirements for low priority.
N/A = Not applicable
	Entity
	Starting TN Load (lbs/yr)
	Anthropogenic % TN in BMAP
	Starting TP Load (lbs/yr)
	Anthropogenic % TP in BMAP

	Brevard County
	178,194
	38.86
	26,588
	39.70

	City of Melbourne
	77,791
	16.97
	11,420
	17.05

	City of Titusville
	56,775
	12.38
	8,264
	12.34

	Agricultural Producers
	38,099
	8.31
	5,750
	8.59

	City of Rockledge
	27,669
	6.03
	3,982
	5.95

	Volusia County
	23,029
	5.02
	3,309
	4.94

	City of Cocoa
	18,189
	3.97
	2,645
	3.95

	Kennedy Space Center
	18,271
	3.98
	2,251
	3.36

	FDOT District 5
	13,893
	3.03
	1,825
	2.73

	City of Edgewater
	2,704
	0.59
	361
	0.54

	Town of Palm Shores
	1,924
	0.42
	276
	0.41

	Town of Indialantic
	1,623
	0.35
	244
	0.36

	City of Oak Hill
	371
	0.08
	49
	0.07

	Total of Allocated Entities
	458,532
	100.00
	66,964
	100.00

	Natural Lands
	300,552
	N/A
	29,259
	N/A

	Total of BMAP
	759,084
	N/A
	96,224
	N/A




[bookmark: _Toc58684902][bookmark: _Toc58592554]Required Reductions 
The TN and TP reductions required by each entity are shown in Table 14 and Table 15, respectively. 
[bookmark: _Ref55410471][bookmark: _Ref55406797][bookmark: _Toc58513913][bookmark: _Toc58576496][bookmark: _Toc58576665][bookmark: _Toc58605285]Table 14. TN load required reductions by entity (lbs/yr)
Note: Grey highlighting and bold indicates jurisdictions meeting the classification requirements for low priority.
N/A = Not applicable
*Indicates a project zone with a segment group adjustment
	Entity
	Project Zone A
	Project Zone B
	Total

	Brevard County
	27,759
	64,506
	92,265

	City of Melbourne
	0
	34,378
	34,378

	City of Titusville
	37,334
	2,619
	39,953

	Agricultural Producers
	20,550
	4,714
	25,264

	City of Rockledge
	0
	11,322
	11,322

	Volusia County
	16,679
	0
	16,679

	Kennedy Space Center
	9,730
	2,423
	12,153

	City of Cocoa
	0
	8,837
	8,837

	FDOT District 5
	4,325
	3,640
	7,965

	City of Edgewater
	1,959
	0
	1,959

	Town of Palm Shores
	0
	787
	787

	Town of Indialantic
	0
	664
	664

	City of Oak Hill
	269
	0
	N/A

	Total
	118,604*
	133,891*
	252,226



[bookmark: _Ref55406798][bookmark: _Ref55410635][bookmark: _Toc58513914][bookmark: _Toc58576497][bookmark: _Toc58576666][bookmark: _Toc58605286]Table 15. TP load required reductions by entity (lbs/yr)
Note: Grey highlighting indicates jurisdictions meeting the classification requirements for low priority.
N/A = Not applicable
*Indicates a project zone with a segment group adjustment
	Entity
	Project Zone A
	Project Zone B
	Total

	Brevard County
	4,809
	12,667
	17,476

	City of Melbourne
	0
	6,292
	6,292

	City of Titusville
	6,224
	474
	6,698

	Agricultural Producers
	3,522
	958
	4,480

	City of Rockledge
	0
	2,135
	2,135

	Volusia County
	2,724
	0
	2,724

	Kennedy Space Center
	1,422
	353
	1,775

	City of Cocoa
	0
	1,726
	1,726

	FDOT District 5
	631
	641
	1,272

	City of Edgewater
	297
	0
	297

	Town of Palm Shores
	0
	148
	148

	Town of Indialantic
	0
	131
	131

	City of Oak Hill
	40
	0
	0

	Total
	19,669*
	25,524*
	45,154



[bookmark: _Toc31199667][bookmark: _Toc22130773][bookmark: _Toc58684903][bookmark: _Toc58592555] Basinwide Sources Approach
[bookmark: _Hlk58575356]The basinwide sources approach involves tailoring management strategies to the primary sources of anthropogenic nutrient loading throughout the NIRL Subbasin. The primary source categories included in this approach are agricultural runoff, septic systems, urban stormwater, and wastewater. For additional information on other sources not directly addressed through anthropogenic activities, please refer to Section 1.2.4.
[bookmark: _Toc31199668][bookmark: _Ref55405364][bookmark: _Ref55405368][bookmark: _Ref55410486][bookmark: _Ref55486266][bookmark: _Toc58684904][bookmark: _Ref55408626][bookmark: _Ref55408630][bookmark: _Toc58592556]	Agriculture 
[bookmark: _Hlk55304371]When DEP adopts a BMAP that includes agriculture, it is the agricultural landowner's responsibility to properly implement BMPs adopted by FDACS to help achieve load reductions or demonstrate compliance through monitoring. FDACS is responsible for verifying that all eligible landowners are enrolled in appropriate BMP programs. Subparagraph 403.067(7)(d)3, F.S., requires FDACS to perform regular onsite inspections, at least every two years, of all agricultural operations enrolled under a BMP manual to ensure that these practices are being properly implemented. From these inspections, FDACS will provide DEP with an annual summary of aggregated fertilizer use in the BMAP area, quantifying total applications and providing information on applications by project zone. 
It is anticipated that additional enrollment in agricultural BMPs, along with more frequent implementation verification site visits by FDACS, will increase nutrient reductions from agricultural nonpoint sources. However, further reductions, beyond the implementation of required owner-implemented BMPs currently required by the FDACS manuals, may be necessary to achieve the TMDLs. FDACS has committed to updating its existing BMP manuals to incorporate updated BMPs based on the latest scientific and technical research. Subparagraph 403.067(7)(f)1, F.S., requires FDACS to annually develop research plans and legislative budget requests for the following:
Evaluate and suggest enhancements to the existing adopted agricultural BMPs to reduce nutrient runoff.
Develop new BMPs that, if proven effective, may be adopted by rule.
Develop agricultural nutrient runoff reduction projects that willing participants could implement on a site-specific, cooperative basis, in addition to BMPs. 
FDACS also provides funding to some agricultural operations to add other practices beyond owner-implemented BMPs. Examples include drainage improvements, fencing, water control structures, precision agriculture technology, and fertigation. SJRWMD are implementing and/or funding projects that encourage low-input agriculture and the use of water quality improvement technologies. 
If owner-implemented BMPs fail to achieve water quality improvements, a cooperative agricultural regional water quality improvement element may be developed for this BMAP, subject to the conditions outlined in Subparagraph 403.067(7)(e)1, F.S. DEP, FDACS, and agricultural producers will cooperatively develop a regional water quality improvement element in the event of the following:
Agricultural measures have been adopted by FDACS pursuant to Subparagraph 403.067(7)(c)2, F.S., and have been implemented and the waterbody remains impaired. 
Agricultural nonpoint sources contribute to at least 20 % of nonpoint source nutrient discharges.
DEP determines that additional measures, in combination with state-sponsored regional projects and other management strategies included in the BMAP, are necessary to achieve the TMDLs.
Further nutrient reductions can be achieved through the implementation of additional agricultural projects or activities. Other reductions associated with the implementation and modification of BMPs may be realized through ongoing studies, data collection, and water management district initiatives. These additional projects and practices are to be implemented in conjunction with the BMP Program, which will aim to achieve full enrollment with verification to ensure that the BMAP goals are achieved.
[bookmark: _Toc22130774][bookmark: _Toc31199669][bookmark: _Toc58684905][bookmark: _Toc58592557]Septic Systems
[bookmark: _Hlk54969568][bookmark: _Hlk30957683][bookmark: _Hlk25068726]As required in Section 403.067(7) (a) 9.b., F.S., local governments must develop an onsite sewage treatment and disposal system (OSTDS) remediation plan to be adopted as part of the BMAP no later than July 1, 2025. The OSTDS remediation plans must be developed by each local government in cooperation with DEP, FDOH, water management districts, and public and private domestic wastewater facilities.
The OSTDS remediation plan requires entities to identify and address the following:
Cost-effective and financially feasible projects necessary to achieve the nutrient load reductions required for OSTDS (e.g., sewering, advanced septic system retrofits, prohibiting the installation of new conventional septic systems).
An inventory of OSTDS based on the best information available.
OSTDS that would be eliminated through connection to existing or future central domestic wastewater infrastructure in the jurisdiction or domestic wastewater service area of the local government.
OSTDS that would be replaced with or upgraded to enhanced nutrient-reducing systems.
Cost of improvements and sources of funding.
Based on data from FDOH, there are 16,171 known and likely septic systems located throughout the NIRL Subbasin. Table 9 summarizes the count of septic systems by project zone.
Stakeholders will submit projects describing how septic loads are addressed as part of BMAP reporting and estimate the load reductions associated with each project. The estimated reductions to the lagoon from addressing these septic systems will be based on several factors, including how they are addressed (i.e., connecting to central sewer sends the wastewater to a treatment facility, which does not remove 100 % of the nutrient load) and the amount of attenuation that occurs as the effluent travels through the watershed to the lagoon.
[bookmark: _Toc31199670][bookmark: _Toc58684906][bookmark: _Toc58592558]Stormwater
[bookmark: _Hlk22304082]Stormwater from urban areas is a considerable source of nutrient loading to the NIRL, and many of these areas are already regulated under the NPDES Stormwater Program. MS4 permittees are required to develop and implement a stormwater management program. Urban areas located in the BMAP area that are not currently covered by an MS4 permit also significantly contribute, individually or in aggregate, to nutrient loading. Therefore, the NPDES Stormwater Program will, within 5 years of BMAP adoption, evaluate any entity located in the BMAP area that serves a minimum resident population of at least 1,000 individuals that are not currently covered by an MS4 permit and designate eligible entities as regulated MS4s, in accordance with Chapter 62-624, F.A.C. 
In accordance with Subsection 373.4131(6), F.S., DEP and the water management districts are planning to update the stormwater design and operation requirements in Environmental Resource Permit rules. These revisions will incorporate the most recent scientific information available to improve nutrient reduction benefits.
[bookmark: _Toc31199671][bookmark: _Toc58684907][bookmark: _Toc58592559][bookmark: _Hlk58327790]Wastewater Treatment
[bookmark: _Hlk30958195]DEP issues permits for facilities and activities to discharge wastewater to surface waters and groundwaters of the state. DEP is authorized by the EPA to issue permits for discharges to surface waters under the NPDES Program. Permits for discharges to groundwater are issued by DEP under state statutes and rules. These wastewater discharge permits establish specific limitations and requirements based on the location and type of facility or activity releasing industrial or domestic wastewaters from a point source.
[bookmark: _Hlk55323163]As of September 2020, there were 18 individually permitted wastewater facilities or activities in the NIRL Subbasin. All new or existing wastewater facilities that dispose of or discharge effluent in the BMAP area are subject to the BMAP provisions, regardless of whether the facility is listed in this BMAP. A preliminary list of wastewater facilities in the NIRL as of September 2020 is provided in Table 11 and a map of their locations is shown in Figure 3.
In areas where there is anticipated growth in human population, adequate treatment capacity of domestic wastewater is essential. Domestic wastewater is treated through either WWTFs or OSTDS (septic systems). Where sewer lines are available, Florida law (Section 381.00655, F.S.) requires a development or property owner to abandon the use of OSTDS and connect to sanitary sewer lines.
Florida law (Section 403.086, F.S., and Chapter 2020-150, Laws of Florida) requires all existing and new domestic wastewater facilities discharging to surface waters of the state within or connected to the IRL to meet advanced waste treatment requirements, as defined in Section 403.086, F.S., no later than July 1, 2025. Additionally, this BMAP requires all other individually permitted domestic wastewater facilities to meet the effluent limitations listed in Table 16 and Table 17, unless the owner or operator can demonstrate reasonable assurance that the effluent would not cause or contribute to an exceedance of the TMDLs or water quality standards in groundwater. To demonstrate reasonable assurance, the owner or operator must provide relevant water quality data, physical circumstances, or other site-specific credible information needed to show the facility would not cause or contribute to the nutrient loading in the BMAP area. This demonstration may include factors such as dilution; site-specific geological conditions; research/studies, including dye tracer tests; and modeling. If DEP concurs with the reasonable assurance demonstration, the effluent limitations established for discharges to groundwater may be modified or waived for the facility. New effluent limitations will take effect no later than July 1, 2025.
New and existing domestic wastewater facilities must meet the stringent nutrient wastewater limitations set forth in this BMAP. Any such new facilities (those commencing after the adoption of this BMAP) must be capable of meeting the requirements of this BMAP at the time of permit issuance. For existing domestic wastewater facilities, DEP shall modify the permit limitations and requirements to be consistent with this BMAP at the time of the next permit renewal. If the facility needs additional time to meet the new limits, the permit may include a compliance schedule with a completion date not to exceed four and a half years after the effective date of the permit.
Table 16 and Table 17 list the TP and TN effluent limitations, respectively, adopted for this BMAP that apply to domestic wastewater facilities unless the owner or operator can demonstrate reasonable assurance as listed above. The effluent limitations for direct surface water discharges and reclaimed water pipelines apply to individually permitted NPDES facilities at the end-of-pipe. Because the limitations for direct surface water discharges are technically based advanced waste treatment limitations, mixing zones are not authorized for TN and TP. The effluent limitations for discharges to groundwater apply at the compliance well located at the edge of the zone of discharge. The owner or operator may elect to meet the groundwater limitations prior to the edge of the zone of discharge. These effluent limitations are applied as an annual average. For direct surface water discharges, the limitations in Subparagraph 62-600.740(2)(b), F.A.C., will be applied in the permit.
Short-term or intermittent industrial discharges are not significant sources of TN or TP in the NIRL Subbasin and are not subject to the limits in Table 16 and Table 17. Intermittent, rainfall-driven, diffuse overflow releases of wastewater from ponds or basins designed to hold precipitation from a 25-year, 24-hour rainfall event or less frequent rainfall event and that infrequently reaches surface waters are considered insignificant sources of TN and TP, provided the ponds or basins are maintained under normal conditions at or below established water levels. The owners or operators of cooling pond reservoirs must operate each spillway gate either during regular operation or on a test basis to protect the structural integrity of the reservoir. Because of the short duration and low volume of wastewater released during spillway gate testing, releases either on an annual or semiannual basis are considered insignificant sources of TN and TP.
Existing industrial wastewater facilities are not subject to the limits in Table 16 and Table 17. However, these facilities must hold the line and shall not increase the nutrient load to receiving or downstream waters. New industrial wastewater facilities shall meet the limits in Table 16 and Table 17. For industrial wastewater facilities that discharge to surface waters of the state must meet the numeric nutrient criteria in Rules 62-302.531 and 62-302.532, F.A.C.
Additionally, new or renewed wastewater permits in the BMAP area must require at least quarterly sampling of the effluent at the point of discharge or edge of the zone of discharge for TN and TP and the reporting of sampling results in the discharge monitoring reports submitted to DEP.
[bookmark: _Ref55407004][bookmark: _Ref58507323][bookmark: _Ref55412549][bookmark: _Toc58513915][bookmark: _Toc58576498][bookmark: _Toc58576667][bookmark: _Toc58605287]Table 16. TN effluent limits
mg/L = milligrams per liter
mgd = million gallons per day 
RRLA = rapid rate land application
	Permitted Average Daily Flow 
(mgd)
	TN Concentration Limits for Direct Surface Discharge (mg/L)
	TN Concentration Limits for RRLA Effluent Disposal System 
(mg/L)
	TN Concentration Limits for All Other Disposal Methods, Including Reuse (mg/L)

	Greater than or equal to 0.5
	3.0
	3.0
	10.0

	Less than 0.5 and greater than or equal to 0.1
	3.0
	6.0
	10.0

	Less than 0.1
	3.0
	10.0
	10.0



[bookmark: _Ref55407007][bookmark: _Ref55412697][bookmark: _Toc58513916][bookmark: _Toc58576499][bookmark: _Toc58576668][bookmark: _Toc58605288]Table 17. TP effluent limits
	Permitted Average Daily Flow 
(mgd)
	TP Concentration Limits for Direct Surface Discharge (mg/L)
	TP Concentration Limits for RRLA Effluent Disposal System 
(mg/L)
	TP Concentration Limits for All Other Disposal Methods, Including Reuse (mg/L)

	Greater than or equal to 0.5
	1.0
	1.0
	6.0

	Less than 0.5 and greater than or equal to 0.1
	1.0
	3.0
	6.0

	Less than 0.1
	1.0
	6.0
	6.0


[bookmark: _Hlk54969608][bookmark: _Toc31199675]
Pursuant to Subsubparagraph 403.067(7)(a)9., F.S., local governments in BMAPs where DEP determines remediation is necessary to achieve the TMDL must develop wastewater treatment plans to be adopted as part of the BMAP no later than July 1, 2025, when all effluent is required to meet the TN and TP concentrations for Direct Surface Discharge cited in Table 16 and Table 17.
The wastewater treatment plans must be developed by each local government, in cooperation with DEP, the water management district, and the public and private domestic wastewater treatment facilities within the jurisdiction of the local government. A local government is not responsible for a private domestic wastewater facility's compliance with the BMAP unless the facility is operated through a public-private partnership to which the local government is a party.
The wastewater treatment plan requires entities to identify and address the following:
Provide construction, expansion or necessary facility upgrades to achieve the TMDL applicable to the domestic WWTF.
Include the permitted capacity in annual gallons per day for the domestic WWTF.
Include the average nutrient concentration and the estimated average nutrient load of the domestic wastewater.
Provide a project timeline of the date when the construction of any facility improvements will begin and be completed and the date when operations of the improved facility will begin. 
Estimate the cost of improvements.
Identify the responsible parties.
[bookmark: _Toc58684908][bookmark: _Toc58592560] Seagrass and Water Quality Monitoring Plan
This monitoring plan is designed to track seagrass distribution and to identify long-term water quality trends. Sampling stations, parameters, frequency, and other elements of this strategy may be modified as appropriate to match changing environmental conditions, funding resources, and understanding of the IRL system. 
[bookmark: _Toc249759419][bookmark: _Toc323297679][bookmark: _Toc323303041][bookmark: _Toc345583065][bookmark: _Toc58684909][bookmark: _Toc345583023][bookmark: _Toc58592561]Objectives
The primary and secondary monitoring objectives are described as follows:
Primary Monitoring Objective
Track seagrass depth extent responses to BMAP implementation. 
Secondary Monitoring Objective
Track trends in ambient water quality in the NIRL and its watershed, including major tributaries. 
Determine if watershed nutrient loading is decreasing and resulting in improved lagoon water quality, which will allow seagrass to grow to target depths.
Additional information about the seagrass depth and compliance with the TMDL targets is discussed in Section 4.2, including the most recent results based on the 2019 aerial mapping data. To read more about the process for analyzing the seagrass data and depth analysis, see Appendix D. 
[bookmark: _Toc249759420][bookmark: _Toc323297680][bookmark: _Toc345583024][bookmark: _Toc58684910][bookmark: _Toc58592562]Monitoring Parameters, Frequency, and Network
To achieve the primary monitoring objective, the main parameter that will be tracked is the seagrass depth by project zone, which is identified through flyover mapping and aerial photography interpretation. DEP and SJRWMD are partnering to fund and conduct flyovers and mapping. In the past, SJRWMD and partners typically have contracted for seagrass mapping every two to three years, and DEP will continue to work with the District to maintain this frequency for the BMAP monitoring plan as long as resources remain available. 
[bookmark: _Hlk46911094]The aerial photography is taken in spring to early summer, during the seagrass growing season. Field sampling conducted around the time of the flights provides data for assessing the accuracy of the maps, and additional field sampling is conducted to address uncertainty regarding areas mapped as seagrass. Using the aerial photography, a map is created showing seagrass extent in the lagoon. These maps are used in evaluations to assess progress towards the TMDL seagrass depth targets for the NIRL. Additional details on the seagrass assessment methodology are contained in Appendix D.
To achieve the secondary monitoring objective above, the existing SJRWMD monthly stations in the NIRL BMAP will be monitored. On average, seagrass transects are 1 kilometer (km) away from a long-term water quality station. The monitoring strategy for these stations focuses on the following parameters:
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Total Kjeldahl Nitrogen
Nitrite/Nitrate
Ammonia
· Total Nitrogen (TN)
Total Phosphorus (TP)
Orthophosphate 
Chlorophyll -a (corrected) 
Photosynthetically Active Radiation (PAR)
True Color
Turbidity
Total Suspended Solids (TSS)
Dissolved Oxygen
Specific Conductivity
pH
Salinity
Secchi Depth
Depth of Collection
Total Depth of Sample Site
Water Temperature
Field Conditions
Total Organic Carbon
Dissolved Organic Carbon
Silica
Alkalinity
Volatile Suspended Solids


In addition to the SJRWMD water quality monitoring stations, Volusia County collects water quality data at three stations in the NIRL, and the U.S. Geological Survey (USGS) collects flow data at two stations. 
[bookmark: _Ref55407208]Table 18 lists the stations that SJRWMD, Volusia County, and USGS currently sample in the NIRL BMAP; these stations are shown by project zone in Figure 9 and Figure 10. Generally data are collected from three types of stations: flow stations where volume is primarily determined; tributary water quality stations near the junction of tributaries where parameters are sampled as these waters mix with the lagoon; and lagoon water quality stations that measure parameters in the lagoon itself.
[bookmark: _Ref55412959][bookmark: _Toc58513917][bookmark: _Ref55412953][bookmark: _Toc58576500][bookmark: _Toc58576669][bookmark: _Toc58605289]Table 18. Water quality monitoring stations in the NIRL BMAP area
	[bookmark: RANGE!A1:H20]Entity
	Station ID
	Project Zone
	Status
	Latitude
	Longitude
	Station Type
	Frequency

	SJRWMD
	IRLBFRR
	NIRL-A
	Active
	28.7553
	-80.8461
	Tributary Water Quality
	Monthly

	SJRWMD
	IRLI02
	NIRL-A
	Active
	28.7370
	-80.8007
	Lagoon Water Quality
	Monthly

	SJRWMD
	IRLI06
	NIRL-A
	Active
	28.6358
	-80.8020
	Lagoon Water Quality
	Monthly

	SJRWMD
	IRLI07
	NIRL-A
	Active
	28.6035
	-80.7984
	Lagoon Water Quality
	Monthly

	SJRWMD
	IRLI09E
	NIRL-A
	Active
	28.5564
	-80.7416
	Lagoon Water Quality
	Monthly

	USGS
	02248380
	NIRL-A
	Active
	28.7362
	-80.7546
	Flow
	Continuous

	Volusia County
	ODIX
	NIRL-A
	Active
	28.8051
	-80.8604
	Tributary Water Quality
	Bi-monthly

	SJRWMD
	IRLTBC
	NIRL-A
	Active
	28.8209
	-80.8601
	Tributary Water Quality
	Monthly

	Volusia County
	TC2
	NIRL-A
	Active
	28.8252
	-80.8572
	Tributary Water Quality
	Bi-monthly

	SJRWMD
	IRLEGU
	NIRL-B
	Active
	28.1243
	-80.6308
	Tributary Water Quality
	Monthly

	SJRWMD
	IRLI10
	NIRL-B
	Active
	28.5012
	-80.7686
	Lagoon Water Quality
	Monthly

	SJRWMD
	IRLI13
	NIRL-B
	Active
	28.3931
	-80.7359
	Lagoon Water Quality
	Monthly

	SJRWMD
	IRLI15
	NIRL-B
	Active
	28.3353
	-80.7131
	Lagoon Water Quality
	Monthly

	SJRWMD
	IRLI16
	NIRL-B
	Active
	28.2778
	-80.6767
	Lagoon Water Quality
	Monthly

	SJRWMD
	IRLI18
	NIRL-B
	Active
	28.1949
	-80.6487
	Lagoon Water Quality
	Monthly

	SJRWMD
	IRLI21
	NIRL-B
	Active
	28.1253
	-80.6165
	Lagoon Water Quality
	Monthly

	SJRWMD
	IRLUPEGWR
	NIRL-B
	Active
	28.1270
	-80.6454
	Tributary Water Quality
	Monthly

	SJRWMD
	IRLUPHC
	NIRL-B
	Active
	28.1612
	-80.6554
	Tributary Water Quality
	Monthly

	USGS
	02249007
	NIRL-B
	Active
	28.1270
	-80.6454
	Flow
	Continuous
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[bookmark: _Toc249759422][bookmark: _Toc323297681][bookmark: _Toc345583025][image: ]A


[bookmark: _Ref323288967][bookmark: _Ref246149493][bookmark: _Ref323288964][bookmark: _Toc58575556][bookmark: _Toc58605346][bookmark: _Toc58514020][bookmark: _Toc58684150]Figure 9. Monitoring network in NIRL Project Zone A
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[bookmark: _Ref55404163][bookmark: _Toc58575557][bookmark: _Toc58605347][bookmark: _Toc58514021][bookmark: _Toc58684151][bookmark: _Toc58575558][bookmark: _Toc58605348]Figure 10. Monitoring network in NIRL Project Zone B


[bookmark: _Toc58684911][bookmark: _Toc58592563]Data Management and Assessment
[bookmark: _Hlk40702633]In 2017, the Florida Watershed Information Network (WIN) replaced the Florida Storage and Retrieval (STORET) Database. WIN now serves as the primary repository of ambient water quality data for the state of Florida. Water quality data from the WIN Database are used for Impaired Surface Waters Rule (IWR) assessments and TMDL development. Ambient water quality data collected as part of the BMAP will be uploaded into WIN for long-term storage and availability. All BMAP data providers have agreed to upload ambient water quality data to WIN at least quarterly, upon the completion of the appropriate quality assurance/quality control (QA/QC) checks.
Other data relevant to monitoring restoration efforts, such as the extent and abundance of seagrass coverages, groundwater, and storm events, may be collected. Stakeholders agree to provide these data to other BMAP partners upon request, and when appropriate, for inclusion in BMAP data analyses and adaptive management evaluations. Other biological data used to assess the biological health of streams and lakes may be provided to DEP staff in the Watershed Assessment Section. For more information on submitting external biological data, visit the DEP website.
[bookmark: _Hlk40702716]The water quality data will be analyzed periodically to determine trends in water quality in the lagoon. Specific statistical analyses were not identified during BMAP development; however, commonly accepted methods of data analysis will be used.
[bookmark: _Toc220746239][bookmark: _Toc220746709][bookmark: _Toc220917888][bookmark: _Toc220925364][bookmark: _Toc220746241][bookmark: _Toc220746711][bookmark: _Toc220917890][bookmark: _Toc220925366][bookmark: _Toc220746243][bookmark: _Toc220746713][bookmark: _Toc220917892][bookmark: _Toc220925368][bookmark: _Toc220746245][bookmark: _Toc220746715][bookmark: _Toc220917894][bookmark: _Toc220925370][bookmark: _Toc220746247][bookmark: _Toc220746717][bookmark: _Toc220917896][bookmark: _Toc220925372][bookmark: _Toc220746248][bookmark: _Toc220746718][bookmark: _Toc220746801][bookmark: _Toc220917897][bookmark: _Toc220917980][bookmark: _Toc220925373][bookmark: _Toc220925456][bookmark: _Toc219541668][bookmark: _Toc249759423][bookmark: _Toc323297682][bookmark: _Toc345583026][bookmark: _Toc58684912][bookmark: _Toc58592564]Quality Assurance/Quality Control
Stakeholders participating in the monitoring plan must collect water quality data in a manner consistent with the DEP standard operating procedures (SOPs) for QA/QC. The most current version of these procedures can be downloaded from the DEP website. For BMAP-related data analyses, entities should use National Environmental Laboratory Accreditation Council (NELAC) National Environmental Laboratory Accreditation Program (NELAP)–certified laboratories or other labs that meet the certification and other requirements outlined in the DEP SOPs. SJRWMD staff and contractors collect, process, and preserve samples according to SJRWMD's Field Standard Operating Procedures for Surface Water Sampling, Fiscal Year 2020. 
[bookmark: _Toc323297683][bookmark: _Toc345583027][bookmark: _Toc58684913][bookmark: _Toc58592565] Research Priorities
During the BMAP process, the stakeholders identified several research priorities they would like to pursue, if funding becomes available. The investments prompted by the 2011 superbloom generated research topics that include the following:
Collecting data to update the bathymetry for the IRL Basin, which would be used in evaluations of seagrass depth limits.
Continuing coordinated monitoring of phytoplankton, periphyton, drift algae, and macroalgae in the basin to gain insights into the cycling of nutrients as well as toxin production and release.
[bookmark: _Hlk40702924]Data analysis of storm event monitoring at the major outfalls.
Refining load estimates delivered by baseflows and modeling the contributions of baseflows.
Synthesizing data on nutrient flux/internal recycling of legacy nutrient loads held within IRL sediments and exchanged with the water column. 
Completing the development, calibration, and validation of a water quality model that can be used to design, site, and prioritize projects that reduce nutrient loads (e.g., Hydrologic Simulation Program FORTRAN [HSPF] or SWIL Model coupled with the Environmental Fluid Dynamics Code [EFDC] Model, or another model that generates predictions of conditions that may be favorable for seagrass growth).
[bookmark: _Hlk46908385]The stakeholders will continue to work with DEP and IRL NEP to identify other research needs, prioritize these needs, and develop scopes of work to address research priorities as appropriate. This information may be organized in a more detailed research plan that could be used to guide future efforts, as funding becomes available. These research projects are not BMAP requirements but would provide valuable information for future assessments of the health of NIRL. There are reports and peer-reviewed articles that have been completed to address several of these research priorities. References are provided in Chapter 5.
[bookmark: _Toc514422670][bookmark: _Toc408412586][bookmark: _Toc408412610]

[bookmark: _Toc31199679][bookmark: _Ref55405826][bookmark: _Toc58684914][bookmark: _Ref55409041][bookmark: _Toc58592566][bookmark: CH3][bookmark: _Toc478028453][bookmark: _Toc491243167][bookmark: _Toc491243345][bookmark: _Toc491243384][bookmark: _Toc499899528]Project Zones
[bookmark: _Toc31199680]Section 3.1 and Section 3.2 provide specific land use and project information on the two project zones in the NIRL. All projects identified as part of this BMAP are listed by project zone. For projects that treat lands in multiple project zones, the nutrient reductions provided in the table are only the estimated reductions for the project zone specified. To calculate the total benefits from these projects, credits from all project zones treated by the project should be summed. The table of existing and planned projects lists those projects submitted by stakeholders to help meet their obligations under the BMAP. Information in the tables was provided by the lead entity and is subject to change as the project develops and more information becomes available.
It should be noted that only projects completed in 2000 and beyond are eligible for BMAP credit. Since the treatment input data for the hydrology calibration was from an earlier period in the model simulation, most projects beyond permit requirements installed from 2000 onward were not included in the calibration and are not well represented in the SWIL Model loading estimates. Therefore, projects completed from 2000 onward are eligible for BMAP credit. Projects completed prior to 2000 are accounted for in the period of record used for calibration of the SWIL Model.
The projects and management strategies are ranked with a priority of high, medium, or low. Projects with a "completed" status were assigned a low priority. Projects classified as "underway" were assigned a medium priority because some resources have been allocated to these projects, but additional assistance may be needed for the projects to be completed. A high priority was assigned to projects listed as "planned," as well as certain "ongoing" projects (i.e., "street sweeping," "catch basin inserts/inlet filter clean out," "public education efforts," "fertilizer cessation," "fertilizer reduction," or "aquatic vegetation harvesting").
[bookmark: _Ref55407370][bookmark: _Toc58684915] Project Zone A
Project Zone A covers more than 91,000 acres of the NIRL BMAP area. As shown in Table 19, wetlands make up 47.9 % of the project zone, followed by urban areas with 15.0 %. Stakeholders in Project Zone A are Volusia County, Brevard County, FDOT District 5, City of Edgewater, City of Oak Hill, City of Titusville, and Kennedy Space Center. 
[bookmark: _Ref55407445][bookmark: _Toc58513918]

[bookmark: _Ref55413369][bookmark: _Toc58576501][bookmark: _Toc58576670][bookmark: _Toc58605290]Table 19. Summary of land uses in Project Zone A
Note: this does not include the area of the lagoon waterbody
	[bookmark: _Hlk55290627]Level 1 
Land Use Code 
	Land Use Description 
	Acres 
	% Total 

	1000
	Urban
	13,707
	15.0

	2000
	Agricultural
	5,223
	5.7

	3000
	Upland Prairie and Shrublands
	12,752
	13.9

	4000
	Upland Forested Areas
	9,363
	10.2

	5000
	Water
	4,453
	4.9

	6000
	Wetlands
	43,880
	47.9

	7000
	Disturbed Lands
	715
	0.8

	8000
	Transportation
	1,464
	1.6

	Total
	
	91,557
	100.0



DEP asked stakeholders to provide information on management actions, including projects, programs, and activities, that may reduce nutrient loads to the CIRL. Management actions are included in the BMAP to address nutrient loads to the lagoon and have to meet several criteria to be considered eligible for credit. Figure 11 and Figure 12 show progress towards the required TN and TP load reductions allocated to Project Zone A from projects completed through July 31, 2020.



[bookmark: _Toc31199758][image: ]
[bookmark: _Ref58512801][bookmark: _Ref58423787][bookmark: _Toc58514022][bookmark: _Toc58684152][bookmark: _Toc58575560][bookmark: _Toc58605350]Figure 11. Estimated progress towards meeting the Required TN Reductions allocated to NIRL Project Zone A with projects completed through July 31, 2020
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[bookmark: _Ref58512813][bookmark: _Ref58423793][bookmark: _Toc58514023][bookmark: _Toc58684153][bookmark: _Toc58575561][bookmark: _Toc58605351]Figure 12. Estimated progress towards meeting the Required TP Reductions allocated to NIRL Project Zone A with projects completed through July 31, 2020


[bookmark: _Toc58684916][bookmark: _Toc58592568]NIRL Project Zone A Existing and Planned Projects
Table 20 summarizes the existing and planned projects provided by the stakeholders for Project Zone A.
[bookmark: _Ref55484331][bookmark: _Ref55413427][bookmark: _Ref56168816][bookmark: _Toc58513919][bookmark: _Toc58576502][bookmark: _Toc58576671][bookmark: _Toc58605291]Table 20. Existing and planned projects in Project Zone A
[bookmark: _Toc55131116]
	Lead Entity
	Partners
	Project Number
	Project Name
	Project Description
	Project Type
	Project Status
	Estimated Completion Date
	TN Reduction (lbs/yr)
	TP Reduction (lbs/yr)
	Project Zone
	Acres Treated
	Cost Estimate
	Cost Annual O&M
	Funding Source
	Funding Amount
	DEP Contract Agreement Number

	FDACS
	N/A
	FDACS-01
	Credit for Changes in Land Use
	Credit for changes in land use. Project canceled in 2020 since land use changes were incorporated into the load estimation tool (LET).
	Land Use Change
	Canceled
	N/A
	N/A
	N/A
	A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A

	FDACS
	Agricultural Producers
	FDACS-03
	BMP Implementation and Verification
	Enrollment and verification of BMPs by agricultural producers. Acres treated based on FDACS OAWP July 2020 Enrollment and FSAID VII. Reductions based on SWIL Model-LET.
	Agricultural BMPs
	Ongoing
	N/A
	199.2484
	28.57038
	A
	211.2176
	TBD
	TBD
	FDACS
	TBD
	N/A

	FDACS
	Not provided
	FDACS-05
	FDACS Cost Share Projects
	Cost-share projects paid for by FDACS. Acres treated based on FDACS OAWP July 2020 Enrollment. Reductions based on SWIL Model-LET.
	Agricultural BMPs
	Ongoing
	N/A
	0
	0
	A
	TBD
	TBD
	TBD
	FDACS
	TBD
	N/A

	Brevard County
	N/A
	BC-001
	Old Dixie Highway 601
	Sediment trap.
	BMP Cleanout
	Ongoing
	2014
	Not provided
	Not provided
	A
	Not provided
	2000
	2000
	County
	County - $2,000
	N/A

	Brevard County
	DEP/ Titusville
	BC-002
	Chain of Lakes Pond
	Wet detention Regional Pond.
	Wet Detention Pond
	Completed
	2010
	3530.485
	945.2629
	A
	1072.5
	2051405
	Not provided
	DEP
	Not provided
	WM804

	Brevard County
	West Melbourne/ Grant-Valkaria/ Malabar/ Melbourne/ Cocoa/ Indian Harbour Beach (IHB)/ Satellite Beach/ Cocoa Beach/ Cape Canaveral
	BC-003
	Education Efforts
	FYN; landscape, irrigation, fertilizer, and pet waste ordinances; PSAs; pamphlets; website, Illicit Discharge Program.
	Education Efforts
	Ongoing
	N/A
	2299.68
	350.52
	A
	N/A
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Brevard County
	TBD
	BC-004
	Scottsmoor I
	Advanced denitrification and baffle box treatment train.
	BMP Treatment Train
	Underway
	TBD
	1602.542
	435.2317
	A
	530.9
	601664
	1000
	Legislative Funds
	Legislative Funds - $286,648
	LP05118

	Brevard County
	DEP/ City of Titusville
	BC-005
	Chain of Lakes Southern Expansion Phase 1
	Completion of additional detention.
	Wet Detention Pond
	Completed
	2014
	284.4301
	317.1718
	A
	575.2
	3200000
	1000
	DEP
	Not provided
	S0620

	Brevard County
	Not provided
	BC-006
	Chain of Lakes Reuse
	Installing reuse from the pond.
	Stormwater Reuse
	Completed
	2005
	TBD
	TBD
	A
	Not provided
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Brevard County
	TBD
	BC-007
	Scottsmoor C
	Advanced denitrification and baffle box treatment train.
	BMP Treatment Train
	Underway
	2019
	1008.8
	265.2656
	A
	463
	TBD
	1000
	Legislative Funds
	Legislative Funds - $33,7043
	LP05114

	Brevard County
	Not provided
	BC-058
	Street Sweeping
	Monthly street sweeping.
	Street Sweeping
	Ongoing
	N/A
	110
	71
	A
	N/A
	N/A
	21000
	County
	N/A
	N/A

	Brevard County
	N/A
	BC-059
	Baffle Box/Sediment Trap Cleaning
	Quarterly baffle box/sediment trap cleaning.
	BMP Cleanout
	Ongoing
	2015
	Not provided
	Not provided
	A
	N/A
	250000
	250000
	County
	County - $250,000
	N/A

	Brevard County
	DEP
	BC-060
	Huntington Road
	Installation of vegetative floating island into an exiting detention pond.
	Floating Islands/ Managed Aquatic Plant Systems (MAPS)
	Completed
	2016
	248.562
	37.9331
	A
	354.6415
	45788
	9997.5
	DEP/County
	Not provided
	G0430

	Brevard County
	SOIRL
	BC-074
	Flounder Creek Pond Denitrification Retrofit
	Stormwater traditional BMP.
	Biosorption Activated Media (BAM)
	Planned
	TBD
	TBD
	TBD
	A
	320
	157500
	12307.5
	Not provided
	Not provided
	N/A

	Brevard County
	Not provided
	BC-075
	Huntington Creek Pond Denitrification Retrofit
	Not provided.
	Biosorption Activated Media (BAM)
	Planned
	TBD
	TBD
	TBD
	A
	355
	180000
	16662.5
	Not provided
	Not provided
	N/A

	Brevard County
	All Cities
	BC-081
	Education Efforts
	Fertilizer video, rain barrel workshops, Facebook page, bus wrap, and billboard.
	Education Efforts
	Ongoing
	N/A
	N/A
	N/A
	A
	N/A
	50000
	TBD
	SOIRL
	SOIRL - $50,000
	N/A

	Brevard County
	N/A
	BC-092
	Baffle Box/Sediment Trap Cleaning
	Increasing cleanout frequency to quarterly.
	BMP Cleanout
	Ongoing
	N/A
	1
	1
	A
	N/A
	Not provided
	276303.3
	County
	Not provided
	N/A

	Brevard County
	SOIRL
	BC-094
	Johns Rd Pond BAM - BB#62 (Actually located in 51)
	Adding a media to remove nitrogen by denitrification. The media will be added to the side slope of the pond or the bottom of the swale.
	Biosorption Activated Media (BAM)
	Underway
	2020
	TBD
	TBD
	A
	Not provided
	172000
	Not provided
	LF/SOIRL
	58030
	N/A

	Brevard County
	SOIRL
	BC-095
	Burkholm Rd BAM - BB#100
	Adding a media to remove nitrogen by denitrification. The media will be added to the side slope of the pond or the bottom of the swale.
	Biosorption Activated Media (BAM)
	Underway
	2020
	TBD
	TBD
	A
	Not provided
	161000
	Not provided
	LF/SOIRL
	99390
	N/A

	Brevard County
	SOIRL
	BC-096
	Carter Rd BAM- BB#115
	Adding a media to remove nitrogen by denitrification. The media will be added to the side slope of the pond or the bottom of the swale.
	Biosorption Activated Media (BAM)
	Underway
	2020
	TBD
	TBD
	A
	Not provided
	176000
	Not provided
	LF/SOIRL
	97510
	N/A

	Brevard County
	SOIRL
	BC-097
	Wiley Rd BAM - BB#193
	Adding a media to remove nitrogen by denitrification. The media will be added to the side slope of the pond or the bottom of the swale.
	Biosorption Activated Media (BAM)
	Underway
	2020
	TBD
	TBD
	A
	Not provided
	179000
	Not provided
	LF/SOIRL
	117735
	N/A

	Brevard County
	SOIRL
	BC-098
	Broadway Pond BAM - BB#832
	Adding a media to remove nitrogen by denitrification. The media will be added to the side slope of the pond or the bottom of the swale.
	Biosorption Activated Media (BAM)
	Underway
	2020
	TBD
	TBD
	A
	Not provided
	290000
	Not provided
	LF/SOIRL
	77864
	N/A

	Brevard County
	SOIRL/ MRC
	BC-101
	Grass Clippings Campaign Phase 1
	Not provided.
	Enhanced Public Education
	Ongoing
	2019
	N/A
	N/A
	A
	N/A
	6667
	N/A
	SOIRL
	SOIRL - $20,000
	N/A

	Brevard County
	SOIRL
	BC-102
	Education Efforts
	Fertilizer, grass clippings, and septic system maintenance.
	Enhanced Public Education
	Ongoing
	N/A
	N/A
	N/A
	A
	Not provided
	375000
	Not provided
	SOIRL
	SOIRL - $375,000
	N/A

	Brevard County
	SOIRL
	BC-103
	Mims Muck Removal: Outflow Water Nutrient Removal
	Not provided.
	Muck Removal/Restoration Dredging
	Underway
	TBD
	TBD
	TBD
	A
	Not provided
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Brevard County
	LF/ SOIRL
	BC-104
	Countyline Ditch Road - BB#10
	Adding a media to remove nitrogen by denitrification. The media will be added to the side slope of the pond or the bottom of the swale.
	Biosorption Activated Media (BAM)
	Underway
	2020
	TBD
	TBD
	A
	Not provided
	200000
	Not provided
	LF/SOIRL
	107773
	N/A

	Brevard County
	LF/ SOIRL
	BC-105
	BB#141
	Adding a media to remove nitrogen by denitrification. The media will be added to the side slope of the pond or the bottom of the swale.
	Biosorption Activated Media (BAM)
	Underway
	2020
	TBD
	TBD
	A
	Not provided
	164000
	Not provided
	LF/SOIRL
	104174
	N/A

	Brevard County
	LF
	BC-106
	Huntington Road BAM - BB#22
	Adding a media to remove nitrogen by denitrification. The media will be added to the side slope of the pond or the bottom of the swale.
	Biosorption Activated Media (BAM)
	Underway
	2020
	TBD
	TBD
	A
	Not provided
	TBD
	Not provided
	LF/SOIRL
	35000
	N/A

	Brevard County
	Not provided
	BC-107
	Sunste Ave BAM - BB#26
	Adding a media to remove nitrogen by denitrification. The media will be added to the side slope of the pond or the bottom of the swale.
	Biosorption Activated Media (BAM)
	Underway
	2021
	TBD
	TBD
	A
	Not provided
	TBD
	Not provided
	Not provided
	Not provided
	N/A

	City of Titusville
	SOIRL
	BC-83
	Stormwater Project - NIRL - Titusville - St. Teresa Basin
	SOIRL-19.
	Baffle Boxes- Second Generation
	Completed
	2019
	TBD
	TBD
	A
	758.0605
	375250
	Not provided
	DEP TMDL
	DEP TMDL - $272,800
	N/A

	City of Titusville
	SOIRL
	BC-84
	Stormwater Project - NIRL - Titusville - South St Basin
	SOIRL-20.
	Baffle Boxes- Second Generation
	Completed
	2019
	TBD
	TBD
	A
	202.25
	475125
	Not provided
	DEP TMDL
	DEP TMDL - $86,856
	NF025

	City of Titusville
	SOIRL
	BC-85
	Stormwater Project - NIRL - Titusville - La Paloma Basin
	SOIRL-21.
	Baffle Boxes- Second Generation
	Completed
	2019
	TBD
	TBD
	A
	554.8
	375250
	Not provided
	DEP TMDL
	DEP TMDL - $208,296
	N/A

	City of Titusville
	SOIRL
	BC-89
	Wastewater Treatment Facility Upgrade-NIRL-Titusville
	SOIRL-02.
	WWTF Upgrade
	Planned
	2022
	TBD
	N/A
	A
	Not provided
	8000000
	Not provided
	SOIRL/ City
	8000000
	N/A

	City of Titusville
	SOIRL
	BC-99
	Coleman Pond MAPS
	Installation of floating islands within a 1 acre City owned pond located within the Chain of Lakes basin.
	Floating Islands/ Managed Aquatic Plant Systems (MAPS)
	Completed
	2019
	TBD
	TBD
	A
	750
	35000
	Not provided
	SOIRL
	SOIRL - $11,437.5
	N/A

	City of Edgewater
	Not provided
	EW-1
	Education Efforts
	FYN; landscape, irrigation, fertilizer, and pet waste ordinances; PSAs; pamphlets; website, Illicit Discharge Program.
	Education Efforts
	Ongoing
	N/A
	162.2
	21.7
	A
	N/A
	Not provided
	15000
	Not provided
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-01
	Education Efforts
	IDDE training, brochures, and NDPES flyer.
	Education Efforts
	Ongoing
	N/A
	59.72
	7.66
	A
	N/A
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-02
	Street Sweeping
	Street Sweeping
	Street Sweeping
	Ongoing
	N/A
	185
	119
	A
	N/A
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-03
	Fertilizer Cessation
	Elimination of fertilizer use along the rights-of-way.
	Fertilizer Cessation
	Completed
	2005
	595
	0
	A
	N/A
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-23
	FM 406869-4
79000-4068694-02 Pond 12B
	Six lane Brevard C/L to SR44
	Wet Detention Pond
	Completed
	2016
	0.351767
	0.082338
	A
	TBD
	N/A
	N/A
	Florida Legislature
	N/A
	N/A

	FDOT District 5
	N/A
	FDOT-24
	FM 406869-4
79000-4068694-04 Swales
	Six lane Brevard C/L to SR44
	Grass swales without swale blocks or raised culverts
	Completed
	2016
	136.2083
	17.02499
	A
	TBD
	N/A
	N/A
	Florida Legislature
	N/A
	N/A

	FDOT District 5
	N/A
	FDOT-25
	FM240812
79210-3505-01 WRA B
	Add lanes/reconstruct from I-95 to Air Park Rd.
	Wet Detention Pond
	Completed
	2006
	8.766934
	2.479871
	A
	TBD
	N/A
	N/A
	Florida Legislature
	N/A
	N/A

	FDOT District 5
	N/A
	FDOT-26
	FM240812
79210-3505-02 Pond C
	Add lanes/reconstruct from I-95 to Air Park Rd.
	Dry Detention Pond
	Completed
	2006
	8.235103
	0.96799
	A
	TBD
	N/A
	N/A
	Florida Legislature
	N/A
	N/A

	FDOT District 5
	N/A
	FDOT-27
	FM240812
79210-3505-03 Pond D
	Add lanes/reconstruct from I-95 to Air Park Rd.
	Dry Detention Pond
	Completed
	2006
	9.86142
	1.197754
	A
	TBD
	N/A
	N/A
	Florida Legislature
	N/A
	N/A

	FDOT District 5
	N/A
	FDOT-28
	FM240811
79210-3504-01 Pond 1
	Add lanes/reconstruct from Air Park Rd to US 1.
	Wet Detention Pond
	Completed
	2006
	4.535713
	1.60398
	A
	TBD
	N/A
	N/A
	Florida Legislature
	N/A
	N/A

	Kennedy Space Center
	Not provided
	KSC-01
	Landscape Fertilizer Reduction
	Fertilizer use reduced from 60 tons/year in 2000 to 20 tons/year in 2010; formula changed from rapid nitrogen release 16-4-8 to slow nitrogen release, phosphate-free 15-0-15.
	Fertilizer Reduction
	Completed
	2009
	312
	44.2
	A
	N/A
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Kennedy Space Center
	Not provided
	KSC-02
	Citrus Grove Termination Roberts Road
	Grove lease termination resulted in abandonment of previously fertilized areas.
	Land Use Change
	Completed
	2010
	TBD
	TBD
	A
	Not provided
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Kennedy Space Center
	Not provided
	KSC-03
	Citrus Grove Termination Schwartz Road
	Grove lease termination resulted in abandonment of previously fertilized areas. Accounted for in 2020 BMAP update.
	Land Use Change
	Canceled
	2010
	N/A
	N/A
	A
	Not provided
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Kennedy Space Center
	N/A
	KSC-04
	Storage Building L5-0734
	Demolition of facility resulted in loss of impervious area and change of land use.
	Land Use Change
	Completed
	2010
	TBD
	TBD
	A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A

	Kennedy Space Center
	N/A
	KSC-05
	Support Building L5-0683
	Demolition of facility resulted in loss of impervious area and change of land use.
	Land Use Change
	Completed
	2010
	TBD
	TBD
	A
	0.2
	N/A
	N/A
	N/A
	N/A
	N/A

	Kennedy Space Center
	Not provided
	KSC-06
	Shuttle Landing Facility - missing from model
	Runoff is captured and treated before discharging to the lagoon.
	Wet Detention Pond
	Completed
	Prior to 2013
	1598.265
	341.0494
	A
	617.8
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Kennedy Space Center
	Not provided
	KSC-07
	Launch Pad 39A
	This area is a closed basin.
	Non-contributing Basin
	Completed
	2014
	1296.061
	164.5454
	A
	456.5
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Kennedy Space Center
	Not provided
	KSC-08
	Launch Pad 39B
	This area is a closed basin.
	Non-contributing Basin
	Completed
	2014
	2587.278
	287.3302
	A
	549
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Kennedy Space Center
	Not provided
	KSC-09
	Schwartz Road Drainage System - missing from model
	Closed system that ultimately drains to the northwest before discharging to an impoundment area adjacent to the lagoon.
	Impoundment
	Completed
	2014
	1714.045
	228.7809
	A
	1614.1
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Kennedy Space Center
	Not provided
	KSC-10
	Warehouse/Processing Area - missing from model
	Receives treatment from permitted stormwater treatment systems.
	Wet Detention Pond
	Completed
	2014
	35.56989
	7.777276
	A
	15.2
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Kennedy Space Center
	Not provided
	KSC-17a
	NASA Parkway West
	Missing from Model. Ditch along south side of NASA Parkway West, ends before the lagoon.
	Grass Swales without Swale Blocks or Raised Culverts
	Completed
	2014
	48.71653
	10.31643
	A
	23.87923
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Kennedy Space Center
	N/A
	KSC-18
	Demolition of Facility J6-2377
	Demolition of facility resulted in loss of impervious area and change of land use.
	Land Use Change
	Completed
	2014
	TBD
	TBD
	A
	0.1
	N/A
	N/A
	N/A
	N/A
	N/A

	Town of Indialantic
	DEP
	TI-04
	Lily Park
	Stormwater treatment.
	Wet Detention Pond
	Completed
	2016
	TBD
	TBD
	A
	1.93
	173000
	500
	DEP
	DEP - $65,000
	LP05120

	City of Titusville
	Brevard County
	TV-01
	Area 1 Stormwater Improvements
	Upsize existing storm pipes and enclose the Florida Ditch; water directed to TV-02.
	Wet Detention Pond
	Completed
	2010
	1334.346
	365.1335
	A
	432.2
	2151510
	4797
	City/ Brevard County
	City - $1,410,072/ County - $470,000
	N/A

	City of Titusville
	Brevard County/ Parrish Medical Center (PMC)/ Brevard Community College (BCC)/ SJRWMD
	TV-02
	Chain of Lakes Regional Stormwater Pond
	Construction of a regional park featuring wetlands, treatment ponds, and recreational features.
	Wet Detention Pond
	Completed
	2010
	759.2001
	191.2186
	A
	339.8
	3521489
	15620
	City/ Brevard County/ SJRWMD/ PMC/ BCC
	City - $1,210,013/ County - $1,910,709/ SJRWMD - $577,145/ PMC - $350,000/ BCC - $217,500
	N/A

	City of Titusville
	DEP/ SJRWMD
	TV-03
	Draa Field Stormwater Park
	Water quality treatment for Area 2 drainage basin.
	Wet Detention Pond
	Completed
	2016
	394.4124
	103.4624
	A
	105.0747
	1810000
	15000
	DEP/ SJRWMD/ Florida Legislature/ City
	DEP - $388,825/ SJRWMD - $366,000/ Florida Legislature - $800,000/ City - $255,000
	G0416

	City of Titusville
	DEP/ SJRWMD
	TV-04
	St. Johns Basin Stormwater Improvements
	Construction of a 3. 5-acre wet detention pond to treat runoff from mixed use lands prior to discharge to the lagoon.
	Wet Detention Pond
	Completed
	2014
	81.53559
	10.20378
	A
	882.1
	2024000
	8000
	DEP/ Brevard County/ City
	DEP - $681,563/ County - $141,655/ City - $1,314,625
	S0338

	City of Titusville
	DEP/ SJRWMD
	TV-05
	St. Johns Basin Stormwater Improvements
	Installation of a baffle box downstream of the pond to treat runoff from mixed use lands prior to discharge to the lagoon.
	Baffle Boxes- Second Generation
	Completed
	2011
	1553.253
	175.7318
	A
	882.1
	167343
	8000
	DEP/ City
	DEP - $100,000/ City - $67,343
	S0338

	City of Titusville
	DEP/ SJRWMD/ FCT/ Florida Recreation Development Assistance Program (FRDAP)/ FDOT
	TV-06
	Spaceview Park
	Alum treatment.
	Stormwater - Alum Injection System
	Completed
	2007
	571.3578
	142.9964
	A
	110.6
	2727394
	15000
	DEP/ SJRWMD/ FCT/ FRDAP/ FDOT/ City
	DEP - $981,151/ SJRWMD - $83,600/ FCT - $228,375/ FRDAP - $103,956/ FDOT - $72,195/ City - $1,258,116
	G0053

	City of Titusville
	N/A
	TV-07
	Education Efforts
	Irrigation, fertilizer, pet waste management, and landscaping ordinances; pamphlets, presentations, website, Illicit Discharge Program.
	Education Efforts
	Ongoing
	N/A
	3092.94
	495.84
	A
	N/A
	N/A
	5000
	City
	N/A
	N/A

	City of Titusville
	N/A
	TV-08
	Street Sweeping
	Approximately 2,006,375 lbs. of debris were removed in North A during the reporting period.
	Street Sweeping
	Ongoing
	N/A
	1130
	724
	A
	N/A
	188120
	63106
	City
	Not provided
	N/A

	City of Titusville
	N/A
	TV-11
	Senior Center Pond Floating Islands
	Floating islands within a wet detention pond.
	Floating Islands/ Managed Aquatic Plant Systems (MAPS)
	Completed
	2015
	447.3607
	58.35909
	A
	624
	52536
	43720
	City
	City - $52,536
	N/A

	City of Titusville
	DEP
	TV-12
	Senior Center Ponds Littoral Zone Plantings
	Littoral vegetation plantings around an already existing wet detention pond.
	BMP Treatment Train
	Completed
	2016
	N/A
	N/A
	A
	413.6
	50000
	2000
	DEP/ City
	DEP - $21,144/ City - $14,721
	G0433

	City of Titusville
	DEP
	TV-13
	Royal Oak Littoral Zone Plantings
	Littoral vegetation plantings around an already existing wet detention pond.
	BMP Treatment Train
	Completed
	2016
	N/A
	N/A
	A
	123.1
	50000
	2000
	DEP/ City
	DEP - $21,144/ City - $14,721
	G0433

	City of Titusville
	DEP
	TV-14
	Main Street Baffle Box with BAM
	2nd generation baffle box with media.
	Baffle Boxes- Second Generation with Media
	Completed
	2018
	2136.693
	337.6215
	A
	295.96
	393363
	4000
	DEP/ City
	DEP - $176,376/ City - $216,987
	G0442

	City of Titusville
	DEP
	TV-15
	Sycamore Street Baffle Box with BAM
	2nd generation baffle box with media.
	Baffle Boxes- Second Generation with Media
	Completed
	2018
	2051.967
	329.0023
	A
	300.07
	570517.7
	4000
	DEP/ City
	DEP - $176,376/ City - $394,142
	G0442

	City of Titusville
	N/A
	TV-16
	Knox Mc Rae Baffle Box
	2nd generation baffle box with media.
	Baffle Boxes- Second Generation with Media
	Completed
	2018
	308.4667
	51.6468
	A
	37.9
	225000
	4000
	Florida Legislature/ City
	Florida Legislature - $105,000/ City - $120,000
	LP05031

	City of Titusville
	Brevard County
	TV-17
	Coleman Basin TMDL Improvements
	Managed aquatic plant system within a one acre pond.
	Floating Islands/ Managed Aquatic Plant Systems (MAPS)
	Completed
	2019
	636.7672
	93.96413
	A
	107
	11437.5
	12000
	County
	County - $11,438
	N/A

	City of Titusville
	SJRWMD/ Brevard County
	TV-18
	South Street Basin TMDL Improvements
	Three 2nd generation baffle boxes with media.
	Baffle Boxes- Second Generation with Media
	Completed
	2019
	1482.313
	234.8645
	A
	235
	450000
	12000
	City/ SJRWMD/ County
	City - $254,144/ SJRWMD - $110,000/ County - $86,856
	N/A

	City of Titusville
	Brevard County
	TV-19
	St. Theresa Basin TMDL Improvements
	2nd generation baffle box with media.
	Baffle Boxes- Second Generation with Media
	Completed
	2019
	4728.512
	761.7081
	A
	314
	375000
	4000
	City/ County
	City - $102,200/ County - $272,800
	N/A

	City of Titusville
	Brevard County
	TV-20
	La Paloma Basin TMDL Improvements
	2nd generation baffle box with media.
	Baffle Boxes- Second Generation with Media
	Completed
	2019
	3533.862
	562.5211
	A
	488
	375000
	4000
	City/ County
	City - $166,704/ County - $208,296
	N/A

	City of Titusville
	TBD
	TV-21
	THS Basin TMDL Improvements
	Future project.
	Baffle Boxes- Second Generation with Media
	Planned
	2020
	1498.178
	235.5219
	A
	239.65
	TBD
	TBD
	TBD
	TBD
	N/A

	City of Titusville
	TBD
	TV-22
	Brevard Street Basin TMDL Improvements
	Future project.
	BMP Treatment Train
	Planned
	TBD
	TBD
	TBD
	A
	17.71
	TBD
	TBD
	TBD
	TBD
	N/A

	City of Titusville
	TBD
	TV-23
	St. Johns 2nd Baffle Box TMDL Improvements
	Future project.
	BMP Treatment Train
	Planned
	TBD
	TBD
	TBD
	A
	882.1
	TBD
	TBD
	TBD
	TBD
	N/A

	City of Titusville
	Brevard County/ SOIRL
	TV-24
	Marina Basin TMDL Improvements - Osprey Pond MAPS
	Osprey Pond MAPS
	Floating Islands/ Managed Aquatic Plant Systems (MAPS)
	Planned
	2021
	259.7038
	37.84802
	A
	271.17
	60000
	30000
	County
	County - $60,000
	N/A

	City of Titusville
	TBD
	TV-25
	Grace Basin TMDL Improvements
	Future project.
	BMP Treatment Train
	Planned
	TBD
	TBD
	TBD
	A
	17.73
	TBD
	TBD
	TBD
	TBD
	N/A

	City of Titusville
	Private Development
	TV-26
	Miracle City Basin TMDL Improvements
	2nd generation baffle box.
	Baffle Boxes- Second Generation
	Completed
	2018
	10.91436
	1.194394
	A
	2.448
	TBD
	4000
	Private Development
	TBD
	N/A

	City of Titusville
	TBD
	TV-27
	South Marina Basin TMDL Improvements
	Future project.
	BMP Treatment Train
	Planned
	TBD
	TBD
	TBD
	A
	322.88
	TBD
	TBD
	TBD
	TBD
	N/A

	City of Titusville
	TBD
	TV-28
	S.R. 50 Basin TMDL Improvements
	Future project.
	BMP Treatment Train
	Planned
	TBD
	TBD
	TBD
	A
	131.09
	TBD
	TBD
	TBD
	TBD
	N/A

	City of Titusville
	TBD
	TV-29
	Commons Basin TMDL Improvements
	Future project.
	BMP Treatment Train
	Planned
	TBD
	TBD
	TBD
	A
	4.37
	TBD
	TBD
	TBD
	TBD
	N/A

	City of Titusville
	TBD
	TV-30
	Broad Street Basin TMDL Improvements
	Future project.
	BMP Treatment Train
	Planned
	TBD
	TBD
	TBD
	A
	13.44
	TBD
	TBD
	TBD
	TBD
	N/A

	City of Titusville
	TBD
	TV-31
	Riverview Street Basin TMDL Improvements
	Future project.
	BMP Treatment Train
	Planned
	TBD
	TBD
	TBD
	A
	7.32
	TBD
	TBD
	TBD
	TBD
	N/A

	City of Titusville
	TBD
	TV-32
	THS 2 Basin TMDL Improvements
	Future project.
	BMP Treatment Train
	Planned
	TBD
	TBD
	TBD
	A
	26.54
	TBD
	TBD
	TBD
	TBD
	N/A

	City of Titusville
	Brevard County
	TV-33
	Osprey Water Reclamation Nutrient Removal Upgrade
	Nitrogen effluent reduction of reclaimed water from 17.9 mg/l to 6 mg/l.
	WWTF Nutrient Reduction
	Planned
	2022
	TBD
	TBD
	A
	N/A
	8000000
	TBD
	City/ County
	TBD
	N/A

	City of Titusville
	Brevard County
	TV-34
	Draa Field Pond MAPS
	Managed aquatic plant system within a 3 acre pond.
	Floating Islands/ Managed Aquatic Plant Systems (MAPS)
	Planned
	2020
	TBD
	TBD
	A
	105
	60000
	40000
	City/ Brevard County
	City - $28,719 / County - $31,281
	N/A

	City of Titusville
	Brevard County
	TV-35
	Draa Field Vegetation Harvesting
	Aquatic vegetation harvesting of a 3 acre pond.
	Aquatic Vegetation Harvesting
	Planned
	2020
	TBD
	TBD
	A
	3
	50000
	0
	City/ Brevard County
	TBD
	N/A

	Volusia County
	Not provided
	VC-01
	Education Efforts
	Irrigation, fertilizer, pet waste management, and landscaping ordinances; pamphlets, presentations, website, illicit discharge program.
	Education Efforts
	Ongoing
	N/A
	1381.74
	198.54
	A
	N/A
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Volusia County
	Not provided
	VC-02
	Roadside Ditch Cleaning
	Roadside ditch cleaning.
	BMP Cleanout
	Ongoing
	2016
	Not provided
	Not provided
	A
	Not provided
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Volusia County
	Not provided
	VC-03
	Open Channel Cleaning
	Open channel cleaning; digging sediment out of open channels.
	BMP Cleanout
	Ongoing
	2016
	Not provided
	Not provided
	A
	Not provided
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Volusia County
	N/A
	VC-04
	Fertilizer Ordinance
	Fertilizer restrictions including summer ban on nitrogen and phosphorus. Reductions included in VC-01.
	Regulations, Ordinances, and Guidelines
	Ongoing
	N/A
	N/A
	N/A
	A
	N/A
	Not provided
	Not provided
	Volusia County
	N/A
	N/A



[bookmark: _Ref55407383][bookmark: _Toc58684917] Project Zone B
Project Zone B covers more than 49,000 acres of the NIRL BMAP area. As shown in Table 21, urban areas make up the majority of the project zone with 59.3 % of the area, followed by wetlands with 16.5 %. Stakeholders in Project Zone B are Brevard County, FDOT District 5, City of Titusville, City of Cocoa, City of Rockledge, City of Melbourne, Town of Palm Shores, Town of Indialantic, and Kennedy Space Center. 
[bookmark: _Ref55407961][bookmark: _Toc58605292][bookmark: _Toc58513920]Table 21. Summary of land uses in Project Zone B
	Level 1 
Land Use Code 
	Land Use Description 
	Acres 
	% Total 

	1000
	 Urban
	29,544
	59.3

	2000
	Agricultural
	2,310
	4.6

	3000
	Upland Prairie and Shrublands
	2,159
	4.3

	4000
	Upland Forested Areas
	2,570
	5.2

	5000
	Water
	1,815
	3.6

	6000
	Wetlands
	8,198
	16.5

	7000
	Distrurbed Lands
	256
	0.5

	8000
	Transportation
	2,963
	5.9

	Total
	
	49,816
	100.0



[bookmark: _Ref55413501]DEP asked stakeholders to provide information on management actions, including projects, programs, and activities, that may reduce nutrient loads to the CIRL. Management actions are included in the BMAP to address nutrient loads to the lagoon and have to meet several criteria to be considered eligible for credit. Figure 13 and Figure 14 show progress towards the required TN and TP load reductions allocated to Project Zone B from projects completed through July 31, 2020. 



[bookmark: _Ref58513106][bookmark: _Ref58423912][bookmark: _Toc58514024][bookmark: _Toc58684154][bookmark: _Toc58575562][bookmark: _Toc58605352]Figure 13. Estimated progress towards meeting the Required TN Reductions allocated to NIRL Project Zone B with projects completed through July 31, 2020


57 %

[bookmark: _Ref58513112][bookmark: _Ref58423919][bookmark: _Toc58514025][bookmark: _Toc58684155][bookmark: _Toc58575563][bookmark: _Toc58605353]Figure 14. Estimated progress towards meeting the Required TP Reductions allocated to NIRL Project Zone B with projects completed through July 31, 2020



[bookmark: _Toc58684918][bookmark: _Toc58591468][bookmark: _Toc58591598][bookmark: _Toc58592570][bookmark: _Toc58591469][bookmark: _Toc58591599][bookmark: _Toc58592571][bookmark: _Toc58591470][bookmark: _Toc58591600][bookmark: _Toc58592572][bookmark: _Toc58592573]NIRL Project Zone B Existing and Planned Projects
Table 22 summarizes the existing and planned projects provided by the stakeholders for Project Zone B.
[bookmark: _Ref55484530][bookmark: _Ref55413561][bookmark: _Toc58576503][bookmark: _Toc58576672][bookmark: _Toc58605293][bookmark: _Toc58513921][bookmark: _Toc58591473][bookmark: _Toc58591603][bookmark: _Toc58592575][bookmark: _Toc58576505][bookmark: _Toc58576674][bookmark: _Toc58605295]Table 22. Existing and planned projects in Project Zone B
	[bookmark: _Toc55156821][bookmark: _Toc55156933][bookmark: _Toc55157009][bookmark: TB83][bookmark: _Toc55131123][bookmark: _Toc55131124][bookmark: _Toc55131125][bookmark: _Toc55131126][bookmark: _Toc55131127][bookmark: _Toc55131128][bookmark: _Toc55131129][bookmark: _Toc55131130][bookmark: _Toc31199700][bookmark: _Toc54901149]Lead Entity
	Partners
	Project Number
	Project Name
	Project Description
	Project Type
	Project Status
	Estimated Completion Date
	TN Reduction (lbs/yr)
	TP Reduction (lbs/yr)
	Project Zone
	Acres Treated
	Cost Estimate
	Cost Annual O&M
	Funding Source
	Funding Amount
	DEP Contract Agreement Number

	FDACS
	N/A
	FDACS-02
	Credit for Changes in Land Use
	Credit for changes in land use. Project canceled in 2020 since land use changes were incorporated into the load estimation tool (LET).
	Land Use Change
	Canceled
	N/A
	N/A
	N/A
	B
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A

	FDACS
	Agricultural Producers
	FDACS-04
	BMP Implementation and Verification
	Enrollment and verification of BMPs by agricultural producers. Acres treated based on FDACS OAWP July 2020 Enrollment and FSAID VII. Reductions based on SWIL Model-LET.
	Agricultural BMPs
	Ongoing
	N/A
	33.24878
	6.02843
	B
	35.47696
	TBD
	TBD
	FDACS
	TBD
	N/A

	FDACS
	Not provided
	FDACS-06
	FDACS Cost Share Projects
	Cost-share projects paid for by FDACS. Acres treated based on FDACS OAWP July 2020 Enrollment. Reductions based on SWIL Model-LET.
	Agricultural BMPs
	Ongoing
	N/A
	0.084929
	0.563334
	B
	TBD
	TBD
	TBD
	FDACS
	TBD
	N/A

	SJRWMD
	DEP/ FIND/ Brevard County/ City of Melbourne
	SJRWMD-01
	Eau Gallie River Muck Dredging
	Dredging commenced in January 2017 and was completed in 2019. Approximately 633,000 cubic yards of muck were removed, reducing nitrogen and phosphorus from the legacy loads in this tributary. 
	Muck Removal/ Restoration Dredging
	Completed
	2019
	TBD
	TBD
	B
	N/A
	23750000
	Not provided
	Ad Valorem/ DEP/ FIND/ Brevard County/ City of Melbourne
	Not provided
	27974

	Brevard County
	Not provided
	BC-008
	Twin Lakes North
	Construction of a bafffle box.
	Baffle Boxes- First Generation
	Completed
	2014
	0.323739
	0.209861
	B
	7.7
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Brevard County
	Not provided
	BC-009
	Twin Lakes South
	Construction of a bafffle box.
	Baffle Boxes- First Generation
	Completed
	2014
	0.36242
	0.23567
	B
	8.5
	20082
	Not provided
	Not provided
	Not provided
	N/A

	Brevard County
	DEP
	BC-010
	Lucas Place 640 Baffle Box
	Construction of a bafffle box. Baffle box was replaced by a second generation baffle box and is credited in BC-33.
	Baffle Boxes- First Generation
	Canceled
	2003
	N/A
	N/A
	B
	5.2
	36835
	1000
	DEP/ County
	Not provided
	S0620

	Brevard County
	DEP
	BC-011
	Rockledge Drive 2055
	Construction of a bafffle box.
	Baffle Boxes- First Generation
	Completed
	2008
	0.109712
	0.075499
	B
	2.4
	61094
	1000
	DEP
	Not provided
	S0620

	Brevard County
	Not provided
	BC-012
	Rockledge and Riverwoods Baffle Box
	Construction of a bafffle box. Baffle box was replaced by a second generation baffle box and is credited in BC-38.
	Baffle Boxes- First Generation
	Canceled
	2000
	N/A
	N/A
	B
	3.8
	47686
	1000
	Not provided
	Not provided
	N/A

	Brevard County
	DEP
	BC-013
	Anchor Lane
	Construction of a bafffle box.
	Baffle Boxes- First Generation
	Completed
	2000
	1.358613
	0.918662
	B
	29.4
	49560
	1000
	DEP
	Not provided
	S0620

	Brevard County
	Not provided
	BC-014
	Kelmore Baffle Box
	Construction of a bafffle box.
	Baffle Boxes- First Generation
	Completed
	2003
	5.475097
	3.771069
	B
	9.7
	21817
	1000
	Not provided
	Not provided
	N/A

	Brevard County
	DEP
	BC-015
	Puesta Del Sol 735 Baffle Box
	Construction of a bafffle box.
	Baffle Boxes- First Generation
	Completed
	2003
	0.105045
	0.07101
	B
	2.2
	24953
	1000
	DEP
	Not provided
	S0620

	Brevard County
	SJRWMD
	BC-016
	Tequesta Harbor Baffle Box
	Construction of a bafffle box.
	Baffle Boxes- First Generation
	Completed
	2009
	0.639115
	0.431646
	B
	13.1
	27582
	1000
	Not provided
	Not provided
	N/A

	Brevard County
	NRCS
	BC-017
	Broadway Boulevard Pond
	Constructon of a detention pond to treat runoff.
	Wet Detention Pond
	Completed
	2000
	304.1263
	95.3932
	B
	85.7
	553169
	14972.5
	Not provided
	Not provided
	N/A

	Brevard County
	Not provided
	BC-018
	Fairglen Elementary School Pond
	Constructon of a detention pond to treat runoff.
	Wet Detention Pond
	Completed
	2003
	214.5747
	56.9956
	B
	80.2
	730869
	Not provided
	Not provided
	Not provided
	N/A

	Brevard County
	DEP
	BC-019
	Lake George
	Constructon of a detention pond to treat runoff.
	Wet Detention Pond
	Completed
	2010
	1409.133
	441.5093
	B
	719
	347255
	17750
	DEP
	Not provided
	LP8952

	Brevard County
	Not provided
	BC-020
	Merritt Island Courthouse Pond
	Constructon of a detention pond to treat runoff.
	Wet Detention Pond
	Completed
	2003
	4.69317
	0.616847
	B
	7
	95584
	Not provided
	Not provided
	Not provided
	N/A

	Brevard County
	Not provided
	BC-021
	Parkway Drive Phase 2 Pond
	Constructon of a detention pond to treat runoff.
	Wet Detention Pond
	Completed
	2004
	7148.169
	1920.565
	B
	1796.9
	1817720
	Not provided
	Not provided
	Not provided
	N/A

	Brevard County
	Not provided
	BC-022
	Street Sweeping
	Monthly Street Sweeping 786 curb lane miles.
	Street Sweeping
	Ongoing
	N/A
	636
	408
	B
	N/A
	106665
	Not provided
	Not provided
	Not provided
	N/A

	Brevard County
	Not provided
	BC-023
	Education Efforts
	FYN; landscape, irrigation, fertilizer, and pet waste ordinances; PSAs; pamphlets; website, Illicit Discharge Program.
	Education Efforts
	Ongoing
	N/A
	8391.96
	1244.76
	B
	N/A
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Brevard County
	DEP
	BC-024
	Pine Island Phase I and II
	Two Wet Detention Ponds (80-acres & 23 acres) with Gravity Flow and Pump Station.
	Wet Detention Pond
	Completed
	2015
	13153.59
	3504.234
	B
	6232.9
	4131255
	34705
	DEP TMDL/ EPA 319
	DEP TDML/ EPA 319 - $1,677,079
	G0288/ G0344

	Brevard County
	N/A
	BC-025
	Merritt Island Airport
	N/A
	Wet Detention Pond
	Canceled
	N/A
	1.860414
	0.422764
	B
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A

	Brevard County
	DEP
	BC-026
	Pines Industrial
	Construction of a pond to treat runoff where no treatment was provided.
	Wet Detention Pond
	Underway
	2020
	TBD
	TBD
	B
	71
	822000
	TBD
	DEP
	Not provided
	NF003

	Brevard County
	DEP
	BC-027
	Johnson Junior High
	Discharge regulation, phosphorus reduction, and denitrification. Biosorption activated media added.
	Floating Islands/ Managed Aquatic Plant Systems (MAPS)
	Completed
	2017
	1416.869
	200.4724
	B
	133.4
	499416.4
	Not provided
	DEP
	DEP - $489,200
	G0430

	Brevard County
	DEP
	BC-028
	Florida Boulevard
	Installation of floating vegetative islands for Nutrient uptake.
	Floating Islands/ Managed Aquatic Plant Systems (MAPS)
	Completed
	2014
	57.20182
	5.019217
	B
	88.4
	40772
	18295
	DEP
	Not provided
	G0430

	Brevard County
	DEP
	BC-029
	Fairglen Elementary
	Installation of floating vegetative islands for Nutrient uptake.
	Floating Islands/ Managed Aquatic Plant Systems (MAPS)
	Completed
	2017
	37.81732
	3.123288
	B
	80.2
	34996
	15703
	DEP
	Not provided
	G0430

	Brevard County
	DEP
	BC-030
	Port St. John B
	Installation of floating vegetative islands for Nutrient uptake.
	Floating Islands/ Managed Aquatic Plant Systems (MAPS)
	Completed
	Prior to 2013
	57.05205
	8.353006
	B
	57.9
	16308
	7315
	DEP
	Not provided
	G0430

	Brevard County
	DEP
	BC-031
	Wickham Park North
	Installation of floating vegetative islands for Nutrient uptake.
	Floating Islands/ Managed Aquatic Plant Systems (MAPS)
	Completed
	2017
	TBD
	TBD
	B
	1796.9
	75428
	24175
	DEP
	Not provided
	G0430

	Brevard County
	DEP
	BC-032
	West Avenue 6600
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	2017
	98.12982
	11.50099
	B
	50.7
	15000
	2140
	DEP
	DEP - $275,000
	S0648

	Brevard County
	DEP
	BC-033
	Lucas Place
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	Prior to 2013
	9.394442
	1.160118
	B
	2.7
	12507
	2140
	DEP
	DEP - $275,000
	S0648

	Brevard County
	DEP
	BC-034
	Indian River Isles
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	Prior to 2013
	68.21853
	7.315461
	B
	7.3
	30844
	2140
	DEP
	DEP - $275,000
	S0648

	Brevard County
	DEP
	BC-035
	Granada Street 1030 East
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	Prior to 2013
	145.8459
	17.21973
	B
	38.6
	15000
	2140
	DEP
	DEP - $275,000
	S0648

	Brevard County
	DEP
	BC-036
	Haverhill Avenue
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	Prior to 2013
	89.00115
	10.50584
	B
	47.5
	35857
	2140
	DEP
	DEP - $275,000
	S0648

	Brevard County
	DEP
	BC-037
	Manth Avenue
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	Prior to 2013
	125.6019
	15.11945
	B
	69.1
	12507
	2140
	DEP
	DEP - $275,000
	S0648

	Brevard County
	Not provided
	BC-038
	Rockledge and Riverwoods Boulevard Rockledge
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	Prior to 2013
	5.981847
	0.702575
	B
	3.8
	15000
	2140
	Not provided
	Not provided
	N/A

	Brevard County
	DEP
	BC-039
	Alamanda Indian Harbour Beach
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	Prior to 2013
	5.075029
	0.606811
	B
	2.8
	12507
	2140
	DEP
	DEP - $275,000
	S0648

	Brevard County
	DEP
	BC-040
	River Shore 1848 Indialantic
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	Prior to 2013
	4.87445
	0.582884
	B
	2.7
	31751
	2140
	DEP
	DEP - $275,000
	S0648

	Brevard County
	DEP
	BC-041
	River Shore 1925 Indialantic
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	Prior to 2013
	34.66021
	4.452528
	B
	7.4
	12507
	2140
	DEP
	DEP - $275,000
	S0648

	Brevard County
	DEP
	BC-042
	Cedar Lane Indialantic
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	Prior to 2013
	6.65755
	0.797401
	B
	3.8
	12507
	2140
	DEP
	DEP - $275,000
	S0648

	Brevard County
	DEP
	BC-043
	Riverview 9856 Indialantic
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	Prior to 2013
	TBD
	TBD
	B
	5.7
	15000
	2140
	DEP
	DEP - $275,000
	S0648

	Brevard County
	DEP
	BC-044
	Riverview 9864 Indialantic
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	Prior to 2013
	TBD
	TBD
	B
	98.5
	15000
	2140
	DEP
	DEP - $275,000
	S0648

	Brevard County
	DEP
	BC-045
	Oak Ridge Indialantic
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	Prior to 2013
	219.2554
	25.80792
	B
	126.5
	15000
	2140
	DEP
	DEP - $275,000
	S0648

	Brevard County
	SOIRL
	BC-046
	Kingsmill-Aurora Phase 2
	Expansion of a Wet Detention Pond and adding Denitrifcation to pond slope.
	Wet Detention Pond
	Planned
	2022
	3354.058
	915.9812
	B
	1220.4
	1600000
	1000
	SOIRL
	TBD
	N/A

	Brevard County
	N/A
	BC-047
	Sediment Trap, Grated Inlet Basket, Inlet Weir Cleaning
	Annual maintenance, removing captured debris from structures.
	BMP Cleanout
	Ongoing
	Prior to 2013
	TBD
	TBD
	B
	N/A
	392105
	250000
	N/A
	N/A
	N/A

	Brevard County
	DEP
	BC-048
	Merritt Ridge 3A
	Alum pond.
	Floating Islands/ Managed Aquatic Plant Systems (MAPS)
	Completed
	Prior to 2013
	3.81868
	0.566291
	B
	32.1
	100362
	41817.5
	DEP/ County
	Not provided
	G0430

	Brevard County
	DEP
	BC-049
	Lake George
	Construction of a regional wet detention pond. Wet pond credited in BC-19.
	Floating Islands/ Managed Aquatic Plant Systems (MAPS)
	Completed
	2017
	282.2497
	27.2907
	B
	719
	51200
	Not provided
	DEP/ County
	Not provided
	LP852

	Brevard County
	Not provided
	BC-050
	Wickham Park
	The provided treatment volume is .17 ac-It.
	Stormwater Reuse
	Completed
	2010
	TBD
	TBD
	B
	Not provided
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Brevard County
	Not provided
	BC-051
	Ellington Park
	Construction of a wet detention pond.
	Stormwater Reuse
	Completed
	2005
	532.4965
	76.27736
	B
	Not provided
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Brevard County
	Not provided
	BC-052
	Rockledge Barton Park Reuse
	Barton Park Pond was constructed by Rockledge. Brevard Parks withdraws water for irrigation for Rockledge Park.
	Stormwater Reuse
	Completed
	2009
	274.8434
	38.51213
	B
	Not provided
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Brevard County
	Not provided
	BC-053
	Florida Boulevard Pond
	Construction of a wet detention pond.
	Wet Detention Pond
	Completed
	2002
	175.6096
	29.96473
	B
	88.4
	350384
	Not provided
	Not provided
	Not provided
	N/A

	Brevard County
	DEP
	BC-054
	McGiver South
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	2013
	5.188995
	0.5991
	B
	2.8
	12507
	2140
	DEP
	DEP - $275,000
	S0648

	Brevard County
	DEP
	BC-055
	651 Franklyn
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	2013
	24.96365
	2.985472
	B
	13.7
	12507
	2140
	DEP
	DEP - $275,000
	S0648

	Brevard County
	Not provided
	BC-056
	Fountainhead
	Removing vegetation from a wet detention pond.
	Aquatic Vegetation Harvesting
	Completed
	2014
	401
	64.7
	B
	125.458
	39274
	Not provided
	Not provided
	Not provided
	N/A

	Brevard County
	DEP
	BC-057
	Fiske
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	2014
	138.0553
	16.15228
	B
	126.2
	12507
	2140
	DEP
	DEP - $275,000
	S0648

	Brevard County
	DEP
	BC-061
	Port St. John C
	Installation of vegetative floating island into an exiting detention pond.
	Floating Islands/ Managed Aquatic Plant Systems (MAPS)
	Completed
	2016
	18.56176
	2.720649
	B
	19.98812
	14062
	3070.5
	DEP/County
	Not provided
	G0430

	Brevard County
	DEP
	BC-062
	Shoreview Circle
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	2015
	5.707652
	0.682577
	B
	Not provided
	11270
	2140
	DEP
	DEP - $275,000
	S0648

	Brevard County
	DEP
	BC-063
	Granada West
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	2015
	15.10811
	1.809408
	B
	Not provided
	11220
	2140
	DEP
	DEP - $275,000
	S0649

	Brevard County
	DEP
	BC-064
	Shoreview Lane
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	2015
	11.62614
	1.389388
	B
	Not provided
	24543.44
	2140
	DEP
	DEP - $275,000
	S0650

	Brevard County
	DEP
	BC-065
	Sunset Park North
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen.
	Baffle Boxes- Second Generation
	Completed
	2015
	42.15312
	5.038728
	B
	Not provided
	11170
	2140
	DEP
	DEP - $275,000
	S0651

	Brevard County
	DEP
	BC-066
	Oak Street
	Upgrading a 1st Generation to a 2nd generation baffle box by adding the nutrient separating screen. Project accounted for in CIRL-BC-02 and is outside the NIRL boundary.
	Baffle Boxes- Second Generation
	Canceled
	2015
	N/A
	N/A
	B
	Not provided
	10895
	2140
	DEP
	DEP - $275,000
	S0652

	Brevard County
	DEP
	BC-067
	Fountainhead Advanced Denitrification
	Phosphorus reduction & denitrification.
	Denitrification Walls
	Underway
	2020
	TBD
	TBD
	B
	234.65
	381000
	Not provided
	DEP
	Not provided
	LP05115

	Brevard County
	DEP
	BC-069
	Multiple Ditch Outfall Denitrification D4 (replace by individual Basin #s/names)
	Providing base flow/grondwater treatment in open drainage basins.
	Biosorption Activated Media (BAM)
	Planned
	2019
	TBD
	TBD
	B
	Not provided
	2140000
	Not provided
	DEP
	Not provided
	LP0511A

	Brevard County
	Not provided
	BC-070
	Otter Creek Basin D4
	Providing base flow/grondwater treatment in open drainage basins.
	Biosorption Activated Media (BAM)
	Planned
	2019
	TBD
	TBD
	B
	Not provided
	130000
	Not provided
	Not provided
	Not provided
	N/A

	Brevard County
	SJRWMD
	BC-071
	Suntree In-Channel Denitrification D4
	Providing base flow/grondwater treatment in open drainage basins.
	Biosorption Activated Media (BAM)
	Planned
	2018
	TBD
	TBD
	B
	Not provided
	71000
	Not provided
	SJRWMD
	Not provided
	N/A

	Brevard County
	DEP
	BC-072
	Multiple Ditch Outfall Denitrification D5 (replace by individual Basin#s/names)
	Providing base flow/grondwater treatment in open drainage basins.
	Biosorption Activated Media (BAM)
	Underway
	2019
	TBD
	TBD
	B
	Not provided
	100000
	Not provided
	DEP
	DEP - $100,000
	LP0511A

	Brevard County
	SOIRL
	BC-073
	EauGallie Area Muck Dredging
	Not provided.
	Muck Removal/Restoration Dredging
	Completed
	2017
	TBD
	TBD
	B
	Not provided
	26250000
	N/A
	SOIRL
	SOIRL - $26,250,000
	N/A

	Brevard County
	Not provided
	BC-077
	Merritt Ridge 2B D2
	Not provided.
	Grass Swales without Swale Blocks or Raised Culverts
	Completed
	2016
	3.072829
	0.452165
	B
	2
	45000
	Not provided
	Not provided
	Not provided
	N/A

	Brevard County
	Not provided
	BC-078
	Merritt Ridge 2E D2
	Wet detention pond construction.
	Wet Detention Pond
	Planned
	TBD
	289.5378
	73.04627
	B
	Not provided
	720000
	Not provided
	Not provided
	Not provided
	N/A

	Brevard County
	N/A
	BC-080
	Wickham Park Solar Bee
	Installing a mixer to reduce the amount of algae and cyanobacteria on an existing pond.
	BMP Treatment Train
	Planned
	TBD
	TBD
	TBD
	B
	TBD
	TBD
	TBD
	TBD
	TBD
	N/A

	Brevard County
	All Cities
	BC-081a
	Education Efforts
	Fertilizer video, rain barrel workshops, Facebook page, bus wrap, and billboard.
	Education Efforts
	Ongoing
	N/A
	N/A
	N/A
	B
	N/A
	Not provided
	TBD
	SOIRL
	Not provided
	N/A

	Brevard County
	N/A
	BC-088
	Septic Removal - NIRL -MIRA
	SOIRL-44.
	OSTDS Phase Out
	Underway
	2020
	TBD
	N/A
	B
	Not provided
	2130852
	Not provided
	SOIRL
	SOIRL - $2,130,852
	N/A

	Brevard County
	N/A
	BC-093
	N. Wickham Road Upflow Filter - BB#1298
	Upflow filter with Biosorption Activated Media installed within existing detention pond system to remove nitrogen from baseflow.
	Biosorption Activated Media (BAM)
	Underway
	2019
	TBD
	TBD
	B
	170
	125000
	2500
	Legislative Funding
	Legislative Funding - $35,000
	LP0511A

	Brevard County
	SOIRL/ Brevard Zoo
	BC-100
	Bomalaski Oyster Bar
	Construct 100 linear foot oyster reef.
	Creating/ Enhancing Oyster Reefs
	Completed
	2018
	N/A
	N/A
	B
	Not provided
	8900
	Not provided
	SOIRL
	SOIRL - $8,900
	N/A

	Brevard County
	SOIRL/ MRC
	BC-101a
	Grass Clippings Campaign Phase 1
	Not provided.
	Enhanced Public Education
	Ongoing
	2019
	N/A
	N/A
	B
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A

	Brevard County
	SOIRL
	BC-102a
	Education Efforts
	Fertilizer, grass clippings, and septic system maintenance.
	Enhanced Public Education
	Ongoing
	N/A
	N/A
	N/A
	B
	Not provided
	N/A
	N/A
	N/A
	N/A
	N/A

	Brevard County
	SOIRL/ SJRWMD
	BC-108
	MIRA Phase 1 Septic to Sewer
	Connect approximately 11 properties to a central sewer system.
	OSTDS Phase Out
	Completed
	2017
	TBD
	N/A
	B
	N/A
	320000
	Not provided
	SOIRL/ SJWMD
	Not provided
	N/A

	Brevard County
	N/A
	BC-109
	Denitrifcation Basin - 1329
	Upflow filter through a BAM media to treat baseflow.
	Biosorption Activated Media (BAM)
	Underway
	2020
	TBD
	TBD
	B
	Not provided
	155113
	Not provided
	LF/ SOIRL
	70000
	LP0511A

	City of Rockledge
	SOIRL
	BC-79
	Breeze Swept Septic to Sewer
	Hood up to sewer - SOIRL-01.
	Wastewater Service Area Expansion
	Completed
	2017
	TBD
	TBD
	B
	Not provided
	3400000
	Not provided
	City/ SOIRL
	880530
	N/A

	City of Cocoa
	SOIRL
	BC-82
	Stormwater Project - NIRL - Cocoa - Church St Type II Baffle Box
	SOIRL-14. See CC-17.
	Baffle Boxes- Second Generation
	Completed
	2018
	TBD
	TBD
	B
	75.2033
	233455
	Not provided
	DEP TMDL
	DEP TMDL - $20,856
	NF025

	City of Melbourne
	SOIRL
	BC-86
	Stormwater Project - NIRL - Melbourne - Cliff Creek Baffle Box
	SOIRL-34.
	Baffle Boxes- Second Generation
	Underway
	2019
	TBD
	TBD
	B
	515.41
	347781
	Not provided
	SOIRL/ City
	347781
	N/A

	City of Melbourne
	SOIRL
	BC-87
	Stormwater Project - NIRL - Melbourne - Thrush Dr Baffle Box
	SOIRL-35.
	Baffle Boxes- Second Generation
	Planned
	2019
	TBD
	TBD
	B
	422.9518
	322200
	Not provided
	SOIRL/ City
	322200
	N/A

	City of Melbourne
	SOIRL
	BC-90
	Stewart Rd Dry Retrofit
	Stormwater Project - CIRL - Melbourne, SOIRL-39.
	Dry Detention Pond
	Planned
	2020
	TBD
	TBD
	B
	Not provided
	18344
	Not provided
	SOIRL/ City
	18344
	N/A

	City of Cocoa
	SJRWMD
	CC-01
	Bracco Pond B
	SOIRL-01.
	Wet Detention Pond
	Completed
	2014
	1608.641
	491.0925
	B
	630.168
	35000
	12000
	City/ SJRWMD
	City - $250,000/ SJRWMD - $250,000
	N/A

	City of Cocoa
	SJRWMD
	CC-02
	Bracco Expansion Area
	Provide the community with a park along the ponds.
	Wet Detention Pond
	Completed
	2014
	103.7369
	28.34129
	B
	880.6833
	570762
	5000
	City/ SJRWMD
	City - $262,500/ SJRWMD - $262,500
	N/A

	City of Cocoa
	EPA/ SJRWMD
	CC-03
	Cocoa Village Park
	Subsurface detention storage that is part of a redevelopment project of the Cocoa Village Park and Riverwalk Esplanade areas.
	Dry Detention Pond
	Completed
	2018
	13.81442
	1.829297
	B
	13.5
	330000
	35000
	City/ SJRWMD
	City - $1,250,000/ SJRWMD - $1,250,000
	WM736

	City of Cocoa
	Rockledge/ SOIRL
	CC-04
	Morris Pond
	Joint project with the City of Rockledge to accommodate previously untreated runoff.
	Wet Detention Pond
	Completed
	2014
	59.60025
	16.45238
	B
	16.2
	247480
	N/A
	City of Rockledge
	N/A
	N/A

	City of Cocoa
	N/A
	CC-05
	North Brevard Avenue Stormwater Treatment Facility
	Hydrodynamic separators that remove sediment, trap debris and separate floating oils from runoff.
	Hydrodynamic Separators
	Completed
	2014
	N/A
	1.82407
	B
	11.3
	N/A
	N/A
	City of Titusville
	N/A
	N/A

	City of Cocoa
	SJRWMD
	CC-06
	North Fiske Stormwater Retention Facility
	Wet detention pond to reduce the discharge of stormwater runoff into surface waters in the state by complete on-site storage.
	100% On-site Retention
	Completed
	2014
	16.28465
	2.158203
	B
	33.9
	330000
	5000
	City
	City - $250,000/ SJRWMD - $250,000
	N/A

	City of Cocoa
	N/A
	CC-07
	Suntree Baffle Box #1 on 2116 IRD
	Capture previously untreated runoff.
	Baffle Boxes- Second Generation
	Completed
	2014
	10.96489
	1.333427
	B
	5.9
	80000
	3500
	City
	City - $40,000
	N/A

	City of Cocoa
	N/A
	CC-08
	Street Sweeping
	Pavement cleaning by sweeping, vacuum, or cleaning.
	Street Sweeping
	Ongoing
	N/A
	405
	260
	B
	N/A
	80000
	100000
	City
	N/A
	N/A

	City of Cocoa
	N/A
	CC-09
	Bracco Supplemental Water Supply
	Joint project with the WWTP to provide reclaimed water.
	WWTF Diversion to Reuse
	Completed
	2014
	1102.896
	107.7542
	B
	N/A
	1200000
	N/A
	City
	City - $250,000
	N/A

	City of Cocoa
	Community Development Block Grant (CDBG)
	CC-10
	Diamond Square Stormwater Improvements
	Retrofit existing storm sewer in Dimond Square, including the construction of a wet detention pond.
	Wet Detention Pond
	Completed
	2011
	41.03529
	4.216735
	B
	98.69961
	210000
	2500
	City
	City - $450,000
	N/A

	City of Cocoa
	N/A
	CC-11
	Education Efforts
	Fertilizer ordinance.
	Education Efforts
	Ongoing
	N/A
	636.615
	92.575
	B
	N/A
	N/A
	N/A
	City
	N/A
	N/A

	City of Cocoa
	Space Coast Transportation Planning Organization (SCTPO)/ FDOT
	CC-12
	Peachtree St. Reconstruction
	Roadway and stormwater improvements.
	Stormwater System Rehabilitation
	Completed
	2016
	N/A
	N/A
	B
	3
	1700000
	N/A
	City/ FDOT
	City - $161,250/ FDOT - $1,387,500
	N/A

	City of Cocoa
	N/A
	CC-13
	Cocoa Riverfront Park
	Amphitheatre and stormwater improvements. Same as Project Number CC-03 where information is captured. Recommend removing from list.
	Stormwater System Rehabilitation
	Completed
	2016
	N/A
	N/A
	B
	12
	162000
	N/A
	City
	N/A
	N/A

	City of Cocoa
	N/A
	CC-14
	Control Gate
	Flood control gate installed at Bracco pond outfall.
	Control Structure
	Completed
	2016
	TBD
	TBD
	B
	N/A
	Not provided
	N/A
	City
	City - $50,000
	N/A

	City of Cocoa
	SCTPO/ FDOT
	CC-15
	Florida Avenue Improvements
	Infiltration through pervious pavers and then ultimately to the AT&T pond.
	BMP Treatment Train
	Completed
	2017
	TBD
	TBD
	B
	6.9
	3344222
	1500
	City/ FDOT
	City - $2,587,000/ FDOT - $913,000
	N/A

	City of Cocoa
	SJRWMD
	CC-16
	AT&T Detention Pond Retrofit
	Incoming inlets will have 2nd generation baffle boxes.
	BMP Treatment Train
	Completed
	2017
	391.2669
	53.90877
	B
	75.09657
	297877
	1500
	City/ SJRWMD
	City - $199,578/ SJRWMD - $98,299
	N/A

	City of Cocoa
	SJRWMD/ SOIRL
	CC-17
	Church Street Baffle Box
	The goal of this project is to capture and treat stormwater that flows untreated and directly into the Indian River Lagoon.
	Baffle Boxes- Second Generation with Media
	Completed
	2018
	323.0418
	41.54147
	B
	75
	173620
	1500
	City/ SJRWMD/ SOIRL
	City - $116,326/ SJRWMD - $50,000/ SOIRL - $20,000
	N/A

	City of Cocoa
	N/A
	CC-18
	John Garren Street Realignment & Parking
	Roadway and stormwater improvements.
	BMP Treatment Train
	Canceled
	N/A
	N/A
	N/A
	B
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A

	City of Cocoa
	N/A
	CC-19
	Brevard Ave. Bioretention and Tree Preservation
	Roadway and stormwater improvements.
	BMP Treatment Train
	Canceled
	N/A
	N/A
	N/A
	B
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A

	City of Cocoa
	TBD
	CC-20
	U.S. 1 and Forrest Ave. Stormwater Treatment Facility
	Develop a dry detention stormwater facility adjacent to U.S. 1.
	Dry Detention Pond
	Underway
	2021
	TBD
	TBD
	B
	16.39
	TBD
	TBD
	City
	TBD
	N/A

	City of Cocoa
	SJRWMD
	CC-21
	Broadmoor Acres and Fiske Blvd. Drainage Improvements
	Roadway and stormwater improvements.
	Stormwater System Rehabilitation
	Planned
	2020
	N/A
	N/A
	B
	7
	TBD
	TBD
	City/ SJRWMD
	TBD
	TBD

	City of Cocoa
	TBD
	CC-22
	Cocoa Waterfront Stormwater Study
	Stormwater Study for the Cocoa waterfront.
	Study
	Completed
	2019
	N/A
	N/A
	B
	N/A
	TBD
	N/A
	City
	N/A
	N/A

	City of Cocoa
	Brevard County
	CC-23
	Septic to Sewer Indian River Drive
	Design and Install new sewer along Indian River to provide sewer service and remove septic tank use.
	OSTDS Phase Out
	Underway
	2021
	TBD
	TBD
	B
	N/A
	3000000
	N/A
	City/SOIRL Tax
	N/A
	N/A

	City of Cocoa
	N/A
	CC-24
	Annual Sewer Inspection
	Annual sewer inspection and maintenance.
	Sanitary Sewer Inspections
	Ongoing
	N/A
	N/A
	N/A
	B
	N/A
	N/A
	335000
	City
	N/A
	N/A

	City of Cocoa
	N/A
	CC-25
	Diamond Square Stormwater PS Feasibility Study
	PS study for pumping stormwater across US 1 to Church Street baffle box.
	Study
	Underway
	2020
	N/A
	N/A
	B
	N/A
	26620
	N/A
	City
	N/A
	N/A

	FDOT District 5
	N/A
	FDOT-04
	70010-3517-01 French Drains
	Missing from Model. French Drain system along State Road 5 from University Boulevard to Aurora Road. Project canceled. Start date prior to 2000. BMP is accounted for in new model.
	BMP Missing from Model
	Canceled
	Prior to 2013
	N/A
	N/A
	B
	21.3
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-05
	70100-3544-01 French Drains
	Missing from Model. Add lanes East of H. Humphrey Bridge to Sykes Creek Parkway. Project canceled. Start date prior to 2000. BMP is accounted for in new model.
	BMP Missing from Model
	Canceled
	Prior to 2013
	N/A
	N/A
	B
	7
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-06
	70020-3501-01 Pond 1
	Missing from Model. State Road 5 -Add lanes and reconstruct from Aurora Road to Post Road.
	Wet Detention Pond
	Completed
	2004
	0.034169
	0.005201
	B
	17.1
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-07
	70020-3501-02A Pond 2A
	Missing from Model. State Road 5 -Add lanes and reconstruct from Aurora Road to Post Road.
	Wet Detention Pond
	Completed
	2004
	0
	0
	B
	12.6
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-08
	70020-3501-02B Pond 2B
	Missing from Model. State Road 5 -Add lanes and reconstruct from Aurora Road to Post Road.
	Wet Detention Pond
	Completed
	2004
	0
	0
	B
	4.8
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-09
	70020-3501-03 Pond 3
	Missing from Model. State Road 5 -Add lanes and reconstruct from Aurora Road to Post Road.
	Wet Detention Pond
	Completed
	2004
	0.180339
	0.030943
	B
	8.4
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-10
	70020-3501-04 Pond 4
	Missing from Model. State Road 5 -Add lanes and reconstruct from Aurora Road to Post Road.
	Dry Detention Pond
	Completed
	2004
	0.005296
	0.000722
	B
	7.9
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-11
	70020-3549-01 Pond 1
	Missing from Model. State Road 5 - Add lanes and reconstruct from Post Road to State Road 404.
	Wet Detention Pond
	Completed
	2005
	0.206761
	0.046868
	B
	9.9
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-12
	70020-3549-02 Pond 2
	Missing from Model. State Road 5 - Add lanes and reconstruct from Post Road to State Road 404.
	Wet Detention Pond
	Completed
	2005
	0.731734
	0.217515
	B
	18.9
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-13
	70020-3549-03 Pond 3
	Missing from Model. State Road 5 - Add lanes and reconstruct from Post Road to State Road 404.
	Wet Detention Pond
	Completed
	2005
	0
	0
	B
	11.2
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-14
	70020-3549-04 Pond 4
	Missing from Model. State Road 5 - Add lanes and reconstruct from Post Road to State Road 404.
	Wet Detention Pond
	Completed
	2005
	0.666256
	0.268816
	B
	3.4
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-15
	70020-3549-05 Pond 5
	Missing from Model. State Road 5 - Add lanes and reconstruct from Post Road to State Road 404.
	Wet Detention Pond
	Completed
	2005
	0.064628
	0.014893
	B
	3.4
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-16
	 70140-3514-01 Pond A
	Missing from Model. State Road 3 - Replace Christa McAuliffe Bridge.
	BMP Missing from Model
	Completed
	Prior to 2013
	1.317169
	0.298326
	B
	1.5
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-17
	 70140-3514-02 Pond B
	Missing from Model. State Road 3 - Replace Christa McAuliffe Bridge.
	BMP Missing from Model
	Completed
	Prior to 2013
	0.045317
	0.007279
	B
	5.9
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-18
	70120-3518-01 Pond 7
	Missing from Model. State Road 518 at State Road 513. Project canceled. Start date prior to 2000. BMP is accounted for in new model.
	BMP Missing from Model
	Canceled
	Prior to 2013
	N/A
	N/A
	B
	9.9
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-19
	70008-3505-01 Pond 1
	Missing from Model. From south of State Road 518 (Eau Gallie Causeway) to Banana River Drive. Project canceled. Start date prior to 2000. BMP is accounted for in new model.
	BMP Missing from Model
	Canceled
	Prior to 2013
	N/A
	N/A
	B
	2.3
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-20
	Education Efforts
	IDDE training, stormwater brochures, NDPES flyer.
	Education Efforts
	Ongoing
	N/A
	79.21
	10.59
	B
	N/A
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-21
	Street Sweeping
	Street sweeping.
	Street Sweeping
	Ongoing
	N/A
	466
	254
	B
	N/A
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	FDOT District 5
	N/A
	FDOT-22
	Fertilizer Cessation
	Elimination of fertilizer use along the rights-of-way.
	Fertilizer Cessation
	Completed
	2005
	2785
	426
	B
	N/A
	Not provided
	Not provided
	Florida Legislature
	Not provided
	N/A

	Kennedy Space Center
	Not provided
	KSC-11
	Landscape Fertilizer Reduction
	Fertilizer use reduced from 60 tons/year in 2000 to 20 tons/year in 2010; formula changed from rapid nitrogen release 16-4-8 to slow nitrogen release, phosphate-free 15-0-15.
	Fertilizer Reduction
	Completed
	Prior to 2013
	312
	44.2
	B
	N/A
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Kennedy Space Center
	Not provided
	KSC-12
	Citrus Grove Termination Jerome Road West
	Grove lease termination resulted in abandonment of previously fertilized areas. Accounted for in 2020 BMAP update.
	Land Use Change
	Canceled
	2010
	N/A
	N/A
	B
	N/A
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Kennedy Space Center
	N/A
	KSC-13
	KARS II Racquetball Court M6-0328A
	Demolition of facility resulted in loss of impervious area and change of land use.
	Land Use Change
	Completed
	2010
	TBD
	TBD
	B
	0.1
	N/A
	N/A
	N/A
	N/A
	N/A

	Kennedy Space Center
	N/A
	KSC-14
	Visitor Center Storage Building M6-0503
	Demolition of facility resulted in loss of impervious area and change of land use.
	Land Use Change
	Completed
	2010
	TBD
	TBD
	B
	0.1
	N/A
	N/A
	N/A
	N/A
	N/A

	Kennedy Space Center
	Not provided
	KSC-15
	Causeway Wetland Mitigation
	Missing from Model. Existing permitted stormwater treatment pond.
	Wet Detention Pond
	Completed
	2014
	22.29577
	4.904328
	B
	12.6
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Kennedy Space Center
	Not provided
	KSC-16
	Visitors Complex/ NASA Badging Center
	Missing from Model. Existing permitted stormwater treatment pond.
	Wet Detention Pond
	Completed
	2014
	228.457
	47.51404
	B
	131.7
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Kennedy Space Center
	Not provided
	KSC-17
	NASA Parkway West
	Missing from Model. Ditch along south side of NASA Parkway West, ends before the lagoon.
	Grass Swales without Swale Blocks or Raised Culverts
	Completed
	2014
	175.3956
	32.40774
	B
	109.4268
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Kennedy Space Center
	N/A
	KSC-19
	Demolition of Facility M5-1546
	Demolition of facility resulted in loss of impervious area and change of land use.
	Land Use Change
	Completed
	2014
	TBD
	TBD
	B
	5
	N/A
	N/A
	N/A
	N/A
	N/A

	City of Melbourne
	N/A
	MEL-01
	Fee and Apollo Drainage Improvements
	No treatment is provided within the existing development; complete a water quality addition.
	Wet Detention Pond
	Completed
	2010
	17.05262
	23.97905
	B
	43.6
	525161
	Not provided
	City
	Not provided
	N/A

	City of Melbourne
	N/A
	MEL-02
	Dove Street Pond
	No treatment is provided within the existing development; complete a water quality addition.
	Wet Detention Pond
	Completed
	2003
	39.24446
	10.43259
	B
	14.9
	156164
	Not provided
	City
	Not provided
	N/A

	City of Melbourne
	N/A
	MEL-03
	Charles Drive Pipe Replacement
	Replaced failing stormwater pipe and created wet detention pond; little to no treatment is provided within existing developments.
	Wet Detention Pond
	Completed
	2010
	149.5285
	89.87712
	B
	143.3
	462644
	Not provided
	City
	Not provided
	N/A

	City of Melbourne
	N/A
	MEL-04
	Wickham Park Pond
	Ponds along with piping upgrades help eliminate flooding within the area along with treatment.
	Wet Detention Pond
	Completed
	2004
	4180.671
	1111.084
	B
	1796.9
	250000
	Not provided
	City
	City - $250,000
	N/A

	City of Melbourne
	N/A
	MEL-05
	Babcock Street Realignment
	Additional treatment was provided for the adjacent drainage basins.
	On-line Retention BMPs
	Completed
	2005
	133.9586
	18.87824
	B
	42.3
	1757186
	Not provided
	City
	Not provided
	N/A

	City of Melbourne
	N/A
	MEL-06
	Garfield Street Ponds - Lot 12 (North)
	Two small dry detention ponds within an existing subdivision (with MEL-7).
	Dry Detention Pond
	Canceled
	N/A
	N/A
	N/A
	B
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A

	City of Melbourne
	N/A
	MEL-07
	Garfield Street Ponds - Lot 24 (South)
	Two small dry detention ponds within an existing subdivision (with MEL-6).
	Dry Detention Pond
	Canceled
	N/A
	N/A
	N/A
	B
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A

	City of Melbourne
	N/A
	MEL-08
	Education Efforts
	FYN, Irrigation, fertilizer, pet waste management, and landscaping ordinances; pamphlets, presentations, website, Illicit Discharge Program.
	Education Efforts
	Ongoing
	N/A
	4667.46
	685.2
	B
	N/A
	Not provided
	Not provided
	City
	Not provided
	N/A

	City of Melbourne
	N/A
	MEL-09
	Street Sweeping
	Street sweeping in the basin and debris removal.
	Street Sweeping
	Ongoing
	N/A
	701
	378
	B
	N/A
	N/A
	162500
	City
	Not provided
	N/A

	City of Melbourne
	DEP
	MEL-10
	Autumn Woods
	Construction of a wet detention pond for water quality treatment.
	Wet Detention Pond
	Completed
	2016
	0
	0
	B
	56.90956
	879220
	Not provided
	City/ DEP
	Not provided
	LP05094

	City of Melbourne
	N/A
	MEL-11
	Participation in FYN
	Future participation in FYN Program. Credited in MEL-08.
	Education Efforts
	Canceled
	N/A
	N/A
	N/A
	B
	N/A
	Not provided
	Not provided
	City
	Not provided
	N/A

	City of Melbourne
	DEP
	MEL-12
	South Croton Baffle Box
	Dry retention and baffle box.
	BMP Treatment Train
	Completed
	2017
	TBD
	TBD
	B
	14.8
	487296
	Not provided
	City/ DEP
	191100
	LP05092

	City of Melbourne
	DEP
	MEL-13
	Bell Street Baffle Box
	Construction of a new baffle box.
	Baffle Boxes- Second Generation with Media
	Completed
	2017
	994.6079
	171.8716
	B
	127.2
	300000
	Not provided
	City/ DEP
	517050
	LP05093

	City of Melbourne
	N/A
	MEL-14
	Paradise Baffle Box
	Retrofit existing baffle box to upgrade to second generation.
	Baffle Boxes- Second Generation with Media
	Completed
	2016
	TBD
	TBD
	B
	125.6
	19000
	Not provided
	City
	City - $19,000
	N/A

	City of Melbourne
	DEP
	MEL-15
	Garfield North Baffle Box
	Construction of a new baffle box.
	Baffle Boxes- Second Generation with Media
	Completed
	2017
	501.2342
	80.29042
	B
	67
	350000
	Not provided
	City/ DEP
	Not provided
	LP05093

	City of Melbourne
	DEP
	MEL-16
	Garfield South Baffle Box
	Construction of a new baffle box.
	Baffle Boxes- Second Generation with Media
	Completed
	2017
	92.08779
	14.67222
	B
	11.8
	150000
	Not provided
	City/ DEP
	Not provided
	LP05093

	City of Melbourne
	DEP
	MEL-17
	Sherwood Stormwater Quality Project
	Construction of a new wet detention pond for a subdivision without any treatment.
	Wet Detention Pond
	Underway
	2020
	TBD
	TBD
	B
	246.1714
	2168800
	Not provided
	City/ DEP
	400000
	NS013

	City of Melbourne
	SJRWMD
	MEL-18
	Croton Road (Lime) Baffle Box
	Installation of baffle box.
	Baffle Boxes- Second Generation with Media
	Completed
	2016
	98.05499
	16.87653
	B
	70
	260660
	Not provided
	City/ SJRWMD
	72752
	Not provided

	City of Melbourne
	N/A
	MEL-19
	Young Street Existing Baffle Box Upgrade
	Upgrade existing 1st generation baffle boxes to 2nd generation baffle boxes with BAM.
	Baffle Boxes- Second Generation with Media
	Completed
	2016
	TBD
	TBD
	B
	7.04
	20000
	Not provided
	City
	City - $20,000
	N/A

	City of Melbourne
	SOIRL
	MEL-20
	Thrush Drive Baffle Box
	Baffle Box - 2nd generation with media filter.
	Baffle Boxes- Second Generation with Media
	Underway
	TBD
	TBD
	TBD
	B
	422
	450000
	Not provided
	City/ SOIRL
	322200
	N/A

	City of Melbourne
	SOIRL
	MEL-21
	Cliff Creek Baffle Box
	Baffle Box - 2nd generation with media filter.
	Baffle Boxes- Second Generation with Media
	Underway
	TBD
	TBD
	TBD
	B
	515
	450000
	Not provided
	City/ SOIRL
	347781
	N/A

	City of Melbourne
	SOIRL
	MEL-22
	Riverside Drive Septic to Sewer Conversion
	Providing for 12 lots to be converted to municipal sewer.
	Wastewater Service Area Expansion
	Underway
	TBD
	TBD
	TBD
	B
	TBD
	215000
	Not provided
	City/ SOIRL
	265960
	N/A

	City of Melbourne
	SOIRL
	MEL-23
	Leewood Forest Wetland and Baffle Box
	The proposed project consists of construction a wetland treatment area and baffle box to provide stormwater quality treatment.
	Constructed Wetland Treatment
	Planned
	TBD
	TBD
	TBD
	B
	149.5
	2590000
	Not provided
	City/ SOIRL
	TBD
	N/A

	City of Melbourne
	N/A
	MEL-24
	South Sarno Drainage Improvements
	Retrofit existing ditch system to include dry detention shelves.
	Dry Detention Pond
	Completed
	2015
	1238.746
	173.3101
	B
	1475
	2227000
	Not provided
	City
	City - $2,227,000
	N/A

	City of Melbourne
	N/A
	MEL-25
	Sarno Road Turn Lane
	Dry detention above needs for turn lane construction.
	Dry Detention Pond
	Completed
	2018
	7.201077
	1.035737
	B
	6.79
	560000
	Not provided
	City
	City - $560,000
	N/A

	City of Melbourne
	SOIRL
	MEL-26
	Apollo/GA Baffle Box
	2nd generation baffle box with BAM.
	Baffle Boxes- Second Generation with Media
	Planned
	2019
	TBD
	TBD
	B
	854
	825000
	Not provided
	City/ SOIRL
	297522
	N/A

	City of Melbourne
	SOIRL
	MEL-27
	Stewart Road WQ Project
	Installation of BAM filter box on existing culvert.
	Biosorption Activated Media (BAM)
	Planned
	2020
	TBD
	TBD
	B
	36
	435000
	Not provided
	City/ SOIRL
	18344
	N/A

	City of Melbourne
	SOIRL
	MEL-28
	Cherry Street Baffle Box
	2nd generation baffle box with BAM.
	Baffle Boxes- Second Generation with Media
	Underway
	2020
	1017.391
	161.0921
	B
	1307
	550000
	Not provided
	City/ SOIRL
	92120
	N/A

	City of Melbourne
	SOIRL
	MEL-29
	Spring Creek Baffle Box
	2nd generation baffle box with BAM.
	Baffle Boxes- Second Generation with Media
	Underway
	2020
	812.9534
	123.1028
	B
	110
	450000
	Not provided
	City/ SOIRL
	99358
	N/A

	City of Melbourne
	SOIRL
	MEL-30
	Brevard County Partnership Projects
	Project approved by the SOIRL Project Plan not built by the City of Melbourne.
	BMP Treatment Train
	Underway
	TBD
	TBD
	TBD
	B
	TBD
	TBD
	N/A
	SOIRL
	TBD
	N/A

	City of Melbourne
	SOIRL/ SRF Loan
	MEL-31
	Grant Street Water Reclamation Facility Improvements
	Improvements include rehabilitation of major treatment elements and structures of facility.
	WWTF Nutrient Reduction
	Planned
	TBD
	TBD
	TBD
	B
	TBD
	10038000
	Not provided
	City/ SOIRL/ SRF
	5415600
	N/A

	City of Melbourne
	TBD
	MEL-32
	Dove Street Pond Retrofit
	Retrofting of existing pond to enhance treatment potential.
	BMP Treatment Train
	Planned
	TBD
	TBD
	TBD
	B
	TBD
	TBD
	Not provided
	TBD
	TBD
	N/A

	City of Melbourne
	TBD
	MEL-33
	Melbourne Cemetery Baffle Box
	2nd generation baffle box with BAM.
	Baffle Boxes- Second Generation with Media
	Planned
	TBD
	TBD
	TBD
	B
	TBD
	TBD
	Not provided
	TBD
	TBD
	N/A

	City of Melbourne
	TBD
	MEL-34
	Funeral Home Baffle Box
	2nd generation baffle box with BAM.
	Baffle Boxes- Second Generation with Media
	Planned
	TBD
	TBD
	TBD
	B
	TBD
	TBD
	Not provided
	TBD
	TBD
	N/A

	City of Melbourne
	TBD
	MEL-35
	Melbourne High Baffle Box
	2nd generation baffle box with BAM.
	Baffle Boxes- Second Generation with Media
	Planned
	TBD
	TBD
	TBD
	B
	TBD
	TBD
	Not provided
	TBD
	TBD
	N/A

	Town of Palm Shores
	Not provided
	PS-01
	Education Efforts
	Fertilizer and landscaping ordinances, pamphlets, and presentations.
	Education Efforts
	Ongoing
	N/A
	28.86
	4.14
	B
	N/A
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	City of Rockledge
	SOIRL
	ROCK-01
	Orange Avenue Baffle Box
	The second generation (nutrient separating) baffle box includes a wire mesh box that captures vegetative debris, litter, and other materials from settling in the water in the bottom of the box, thereby preventing leaching of the nutrients.
	Baffle Boxes- Second Generation
	Completed
	2009
	18.66393
	2.32657
	B
	10.4
	8600
	2555
	Not provided
	Not provided
	N/A

	City of Rockledge
	SOIRL
	ROCK-02
	Barton Avenue Baffle Box
	The second generation (nutrient separating) baffle box includes a wire mesh box that captures vegetative debris, litter, and other materials from settling in the water in the bottom of the box, thereby preventing leaching of the nutrients.
	Baffle Boxes- Second Generation
	Completed
	2009
	50.74786
	6.624264
	B
	27.1
	9350
	2555
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-03
	Hardee Circle Baffle Box
	The second generation (nutrient separating) baffle box includes a wire mesh box that captures vegetative debris, litter, and other materials from settling in the water in the bottom of the box, thereby preventing leaching of the nutrients.
	Baffle Boxes- Second Generation
	Completed
	2009
	26.37994
	3.156715
	B
	14.59948
	43420
	2555
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-04
	Rockledge Avenue Baffle Box
	The second generation (nutrient separating) baffle box includes a wire mesh box that captures vegetative debris, litter, and other materials from settling in the water in the bottom of the box, thereby preventing leaching of the nutrients.
	Baffle Boxes- Second Generation
	Completed
	2004
	69.96821
	8.45365
	B
	40.97382
	21448
	3682
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-05
	Bougainvillea Drive Baffle Box
	The second generation (nutrient separating) baffle box includes a wire mesh box that captures vegetative debris, litter, and other materials from settling in the water in the bottom of the box, thereby preventing leaching of the nutrients.
	Baffle Boxes- Second Generation
	Completed
	2000
	58.02128
	6.704771
	B
	35.73918
	29495
	2566
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-06
	Park Avenue Baffle Box
	The second generation (nutrient separating) baffle box includes a wire mesh box that captures vegetative debris, litter, and other materials from settling in the water in the bottom of the box, thereby preventing leaching of the nutrients.
	Baffle Boxes- Second Generation
	Completed
	2007
	23.47041
	2.769965
	B
	13.18246
	52529
	2555
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-07
	Little John Lane Baffle Box
	The second generation (nutrient separating) baffle box includes a wire mesh box that captures vegetative debris, litter, and other materials from settling in the water in the bottom of the box, thereby preventing leaching of the nutrients.
	Baffle Boxes- Second Generation
	Completed
	2004
	21.59321
	2.562747
	B
	11.86976
	60000
	2555
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-08
	Fernwood Drive Baffle Box
	The second generation (nutrient separating) baffle box includes a wire mesh box that captures vegetative debris, litter, and other materials from settling in the water in the bottom of the box, thereby preventing leaching of the nutrients.
	Baffle Boxes- Second Generation
	Completed
	Prior to 2013
	23.37143
	2.850717
	B
	12.8809
	55750
	Not provided
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-09
	Valencia Drive Baffle Box
	The second generation (nutrient separating) baffle box includes a wire mesh box that captures vegetative debris, litter, and other materials from settling in the water in the bottom of the box, thereby preventing leaching of the nutrients.
	Baffle Boxes- Second Generation
	Completed
	2008
	41.62701
	4.966122
	B
	22.8785
	58960
	2555
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-10
	Knollwood Baffle Box
	The second generation (nutrient separating) baffle box includes a wire mesh box that captures vegetative debris, litter, and other materials from settling in the water in the bottom of the box, thereby preventing leaching of the nutrients.
	Baffle Boxes- Second Generation
	Completed
	2002
	44.15473
	5.279585
	B
	24.3
	68248
	3682
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-11
	Sutton Street Baffle Box
	The second generation (nutrient separating) baffle box includes a wire mesh box that captures vegetative debris, litter, and other materials from settling in the water in the bottom of the box, thereby preventing leaching of the nutrients.
	Baffle Boxes- Second Generation
	Completed
	2011
	14.99895
	1.943021
	B
	8
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-12
	River Groves Baffle Box
	The second generation (nutrient separating) baffle box includes a wire mesh box that captures vegetative debris, litter, and other materials from settling in the water in the bottom of the box, thereby preventing leaching of the nutrients.
	Baffle Boxes- Second Generation
	Completed
	2011
	13.12516
	1.568483
	B
	7.4
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-13
	Summer Place Baffle Box
	The second generation (nutrient separating) baffle box includes a wire mesh box that captures vegetative debris, litter, and other materials from settling in the water in the bottom of the box, thereby preventing leaching of the nutrients.
	Baffle Boxes- Second Generation
	Completed
	2011
	17.1487
	2.021108
	B
	9.8
	35000
	Not provided
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-14
	Sweet Street Swale
	Swales are designed to infiltrate a defined quantity of runoff (the treatment volume) through the permeable soils of the swale floor and side slopes into the shallow ground water aquifer immediately following a storm event.
	Grass Swales without Swale Blocks or Raised Culverts
	Completed
	2011
	27.78534
	4.103821
	B
	8
	10000
	Not provided
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-15
	Community Park of Rockledge Regional Facility Phase 1
	"Wet detention" means the collection and temporary storage of stormwater in a permanently wet impoundment in such a manner as to provide for treatment through physical, chemical, and biological processes with subsequent gradual release of the stormwater.
	Wet Detention Pond
	Completed
	2004
	13.50891
	1.689118
	B
	25.6
	50000
	23974
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-16
	Pineland Park Unit Three
	"Wet detention" means the collection and temporary storage of stormwater in a permanently wet impoundment in such a manner as to provide for treatment through physical, chemical, and biological processes with subsequent gradual release of the stormwater.
	Wet Detention Pond
	Completed
	2009
	0.450827
	0
	B
	54.3
	100000
	6234
	Not provided
	Not provided
	N/A

	City of Rockledge
	DEP
	ROCK-17
	Barton Park Regional Detention System
	"Wet detention" means the collection and temporary storage of stormwater in a permanently wet impoundment in such a manner as to provide for treatment through physical, chemical, and biological processes with subsequent gradual release of the stormwater.
	Wet Detention Pond
	Completed
	2010
	2597.514
	670.0999
	B
	757
	2600000
	40000
	DEP
	Not provided
	S0538

	City of Rockledge
	Not provided
	ROCK-18
	Florida Avenue Stormwater Facility
	"Wet detention" means the collection and temporary storage of stormwater in a permanently wet impoundment in such a manner as to provide for treatment through physical, chemical, and biological processes with subsequent gradual release of the stormwater.
	Wet Detention Pond
	Completed
	2010
	37.69719
	18.37597
	B
	25.2
	435000
	40950
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-19
	Police Department Pond
	"Wet detention" means the collection and temporary storage of stormwater in a permanently wet impoundment in such a manner as to provide for treatment through physical, chemical, and biological processes with subsequent gradual release of the stormwater.
	Wet Detention Pond
	Completed
	2010
	12.72484
	2.517782
	B
	39.1
	350000
	7035
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-20
	Huntington Lakes I
	"Wet detention" means the collection and temporary storage of stormwater in a permanently wet impoundment in such a manner as to provide for treatment through physical, chemical, and biological processes with subsequent gradual release of the stormwater.
	Wet Detention Pond
	Completed
	2014
	15.40124
	3.901349
	B
	36.9
	950000
	Not provided
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-21
	Street Sweeping
	Pavement cleaning by sweeping, vacuum, or washing.
	Street Sweeping
	Ongoing
	N/A
	794
	337
	B
	N/A
	Not provided
	54000
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-22
	Treatment Missing from Model
	Wet detention ponds – missing from model. Project canceled after model update.
	BMP Missing from Model
	Canceled
	Prior to 2013
	N/A
	N/A
	B
	383.2
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-23
	Education Efforts
	Irrigation, fertilizer, pet waste management, and landscaping ordinances; pamphlets, presentations, website, illicit discharge program. Video "Know Your Waterways".
	Education Efforts
	Ongoing
	N/A
	1660.14
	238.92
	B
	N/A
	7385
	0
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-24
	Huntington Lakes II
	Project provides treatment to some of the basin that leads into ROCK-17.
	Wet Detention Pond
	Completed
	2016
	298.4588
	34.24327
	B
	133.5
	900000
	15000
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-25
	Aquatic Harvesting
	Data is collected by location in yards; determining method to convert to dry weight.
	Aquatic Vegetation Harvesting
	Completed
	2015
	TBD
	TBD
	B
	N/A
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-26
	Breeze Swept Septic Phase-out
	Estimates will be calculated using the latest version of ArcNLET for the septic tank phase out.
	Wastewater Service Area Expansion
	Completed
	2017
	TBD
	TBD
	B
	39.6
	3700000
	20000
	DEP, SJRWMD, 1/2 cent Lagoon Tax
	2580000
	N/A

	City of Rockledge
	Not provided
	ROCK-27
	River Ridge Non Discharge
	Nondisharge dry retention basin.
	100% On-site Retention
	Completed
	2015
	304.8869
	44.00242
	B
	35.25983
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-28
	Southwest Gus Hipp Conveyance
	Add BAM for denitrification to major canal in the city.
	BMP Treatment Train
	Underway
	2019
	TBD
	TBD
	B
	TBD
	17000
	Not provided
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-29
	Gus Hipp Pond
	Conversion of borrow pit to a wet detention pond.
	Wet Detention Pond
	Planned
	TBD
	TBD
	TBD
	B
	TBD
	335000
	Not provided
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-30
	Public Works Pond 1
	Enlarge current retention area.
	Dry Detention Pond
	Completed
	2017
	5.042222
	0.705844
	B
	5.687929
	5000
	600
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-31
	Public Works Pond 2
	Enlarge current retention area.
	Dry Detention Pond
	Completed
	2017
	6.510994
	0.878181
	B
	6.96163
	10000
	600
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-32
	School Triangle Pond
	Create dry detention pond on city-owned land.
	Dry Detention Pond
	Completed
	2017
	1.023658
	0.144694
	B
	1.219959
	20300
	1000
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-33
	Barton Park Irrigation
	Use wet pond (Barton Lake) for irrigation.
	Stormwater Reuse
	Planned
	TBD
	TBD
	TBD
	B
	TBD
	TBD
	TBD
	TBD
	TBD
	N/A

	City of Rockledge
	Not provided
	ROCK-34
	Winchester Cove Non Discharge
	Nondisharge dry retention basin.
	100% On-site Retention
	Completed
	2015
	17.94158
	2.638036
	B
	1.9
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-35
	Florida Ave and Dixie Lane Swale
	Grass swale with blocks or culverts.
	Grass swales with swale blocks or raised culverts
	Completed
	2018
	94.89466
	12.96
	B
	9.6
	5000
	Not provided
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-36
	WWTP EQ Basin Nutrient Uptake
	Modification of WWTP Process.
	WWTF Upgrade
	Planned
	TBD
	TBD
	TBD
	B
	TBD
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-37
	WWTP Biosolids
	Modification of WWTP Process.
	WWTF Upgrade
	Planned
	TBD
	TBD
	TBD
	B
	TBD
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	City of Rockledge
	Not provided
	ROCK-38
	Rockled Indian River Dr
	Septic to Sewer.
	Wastewater Service Area Expansion
	Planned
	TBD
	TBD
	TBD
	B
	TBD
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Town of Indialantic
	Not provided
	TI-01
	Swales North of U.S. 192 Causeway
	Swales provide treatment as a part of TI-02 and all reductions are accounted for below.
	Grass Swales without Swale Blocks or Raised Culverts
	Completed
	2001
	N/A
	N/A
	B
	29.2
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Town of Indialantic
	Not provided
	TI-02
	100% On-Site Retention
	Not provided.
	100% On-site Retention
	Completed
	2001
	1280.45
	190.0857
	B
	3.5
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	Town of Indialantic
	Not provided
	TI-03
	Education Efforts
	Pamphlet, website, and fertilizer ordinance.
	Education Efforts
	Ongoing
	N/A
	64.92
	9.76
	B
	N/A
	Not provided
	Not provided
	Not provided
	Not provided
	N/A

	City of Titusville
	N/A
	TV-09
	Education Efforts
	Irrigation, fertilizer, pet waste management, and landscaping ordinances; pamphlets, presentations, website, illicit discharge program.
	Education Efforts
	Ongoing
	N/A
	313.56
	42.18
	B
	N/A
	N/A
	5000
	City
	N/A
	N/A

	City of Titusville
	N/A
	TV-10
	Street Sweeping
	Approximately 205,725 lbs of debris removed from North B during the reporting period.
	Street Sweeping
	Ongoing
	N/A
	116
	74
	B
	N/A
	188120
	63106
	City
	Not provided
	N/A

	Brevard County
	DEP
	BC-068
	Multiple Ditch Outfall Denitrification D1
	Providing base flow/grondwater treatment in open drainage basins.
	Biosorption Activated Media (BAM)
	Canceled
	2019
	N/A
	N/A
	N/A
	N/A
	900000
	N/A
	Florida Legislature/ Brevard County
	900600
	LP0511A

	Brevard County
	DEP
	BC-068a
	Multiple Ditch Outfall Denitrification D1
	Providing base flow/grondwater treatment in open drainage basins.
	Biosorption Activated Media (BAM)
	Canceled
	2019
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	DEP
	Not provided
	LP0511A

	Brevard County
	SOIRL
	BC-091
	Kingsmill Aurora Phase II
	Construction of 5 ac pond with weirs, drop structures, etc. Duplicate with BC-46.
	Wet Detention Pond
	Canceled
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A
	N/A





[bookmark: _Toc58684919][bookmark: _Toc58592579]Compliance and Adaptive Management
[bookmark: _Toc31199749][bookmark: _Hlk30962484][bookmark: _Toc58684920][bookmark: _Toc58592580] Future Growth
[bookmark: _Hlk56792929]To ensure that this BMAP effort can achieve and ultimately maintain the goal of meeting TMDL requirements, the overall restoration strategy must include actions and planning for future growth and development. Any new development would likely fall into two general source categories: (1) urban and (2) agricultural. Nutrient impacts from new development will be addressed through a variety of mechanisms as well as other provisions of Florida law.
While the majority of the restoration projects and programs listed in this BMAP address current loading, the need to plan and implement sound management strategies to address additional population growth in the BMAP area must be considered. DEP has included in this BMAP specific elements to address all current and future WWTF effluent, septic systems, and stormwater sources. Broader laws—such as local land development regulations, comprehensive plans, ordinances, incentives, Environmental Resource Permit requirements, and consumptive use permit requirements—all provide additional mechanisms and avenues for protecting water resources and reducing the impact of new development and other land use changes as they occur. As more information becomes available, the modeling efforts used for determining loading to the lagoon will continue to be refined.
The recommendations presented in Chapter 2 should be considered by local governments during master planning and land use decision-making efforts. It should also be noted that any additional loading, such as from land use changes from low to high density, or any increase in intensity of use (that may include additional nutrient loadings), will be evaluated during future BMAP review efforts. If an increase in loading has occurred, additional restoration actions will be required to remediate impacts. DEP recommends that all local governments revise their planning and land use ordinance(s) to adequately address all future growth, and consider limitations on growth in sensitive areas, such as lands with a direct hydrologic connection to impaired waterbodies, wetland areas, or coastal areas.
[bookmark: _Toc31199750][bookmark: _Ref55407078][bookmark: _Toc58684921][bookmark: _Ref55412805][bookmark: _Toc58592581] Compliance
[bookmark: _Toc58684922][bookmark: _Toc58592582]TMDL Compliance
The intent of the TMDLs is to recover the deeper water seagrass habitats with the biological response of the seagrass being the most important factor in evaluating the success of achieving TMDL targets. To assess progress for the IRL Basin towards the median seagrass depth limit target, a two-step process was used in the A and B Project Zones. For the 2013 BMAP, DEP conducted this two-step evaluation using seagrass data from 2003, 2005, 2006, 2007, and 2009, which were the latest datasets available at the time of the analysis. For the NIRL, Project Zones A and B were not compliant, and stakeholders in both zones were assigned detailed allocations in the first BMAP iteration.
Since the 2013 BMAP, further evaluations of the seagrass depth limits in the NIRL have been conducted to reassess whether the NIRL project zones continued to be compliant. Table 23 and Table 24 list the results of both steps of these evaluations since 2013, including the number of years that passed Step 2 of the evaluation. In 2020, the evaluation was conducted using the 2013, 2015, 2017, and 2019 seagrass mapping data, which were the latest datasets available at that time. Figure  15 and Figure 16 show the results of both steps of the 2020 evaluation for Project Zones A and B, respectively. Neither of the project zones were compliant. As indicated in the 2013 BMAP, DEP assigns detailed allocations in project zones where compliance is not maintained.
[bookmark: _Ref55408375][bookmark: _Toc58575568][bookmark: _Toc58576508][bookmark: _Toc58605358][bookmark: _Toc58513922][bookmark: _Toc58576511][bookmark: _Toc58576677][bookmark: _Toc58605298]Table 23. Summary of seagrass compliance results, Step 1
	[bookmark: _Hlk54946697]Step 1
	North A
	North B

	2007 - 2013
	Fail
	Fail

	2009 - 2015
	Fail
	Fail

	2011 - 2017
	Fail
	Fail

	2013 - 2019
	Fail
	Fail



[bookmark: _Ref55408376][bookmark: _Ref55414083][bookmark: _Toc58513923][bookmark: _Toc58576512][bookmark: _Toc58576678][bookmark: _Toc58605299][bookmark: _Hlk54946747]Table 24. Summary of seagrass compliance results, Step 2
[bookmark: _Hlk58592188]Note: Parentheses indicate number of years passing of those assesed for the compliance period of record
	Step 2
	North A
	North B

	2007 - 2013
	Fail 
(0 of 4)
	Fail 
(0 of 4)

	2009 - 2015
	Fail 
(0 of 4)
	Fail 
(0 of 4)

	2011 - 2017
	Fail 
(0 of 4)
	Fail 
(0 of 4)

	2013 - 2019
	Fail 
(0 of 4)
	Fail 
(0 of 4)
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[bookmark: _Ref55408417][bookmark: _Toc58514026][bookmark: _Toc58684156]Figure 15. NIRL Project Zone A seagrass evaluation results for Compliance Step 1 and Step 2
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[bookmark: _Ref55408418][bookmark: _Toc58514027][bookmark: _Toc58684157]Figure 16. NIRL Project Zone B seagrass evaluation results for Compliance Step 1 and Step 2

[bookmark: _Toc58684923][bookmark: _Toc58592583]BMAP Compliance 
In addition to IRL TMDL compliance and the measurement of seagrass deep edge recovery, there are other compliance elements related to the BMAP. DEP has set BMAP TN and TP reduction milestones for the years 2025 and 2030 to ensure that significant progress will be made in each five-year increment prior to the 2035 total reduction deadline. The percent reductions in the milestones apply to the total BMAP required reductions; so as various entities implement their projects, the overall milestones are also being met. Individual entities must achieve compliance by meeting their own required reductions by the 2035 deadline, as well as show progress towards the BMAP milestones by planning and implementing projects. 
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[bookmark: _Toc58592585][bookmark: _Toc58684925][bookmark: AppendixA][bookmark: AppendixA2][bookmark: _Toc21936367][bookmark: _Toc31199753]Appendices
[bookmark: _Toc58684926][bookmark: _Toc58592586]Appendix A. BMAP Projects Supporting Information
[bookmark: _Hlk498430569][bookmark: _Hlk498434034][bookmark: _Hlk483854253][bookmark: _Toc497741403][bookmark: _Toc497748504][bookmark: _Toc499899557]The project tables in this BMAP (Table 20 and Table 22) list the implementation status of the BMAP projects as of July 31, 2020. The tables list the TN and TP reductions in lbs/yr attributable to each individual project. These projects were submitted to DEP by responsible entities with the understanding that the projects and activities would be included in the BMAP, thus setting the expectation for each entity to implement the proposed projects and activities to achieve the assigned load reduction estimates in the specified time.
However, the list of projects is meant to be flexible enough to allow for changes that may occur over time. During the annual review of BMAP implementation efforts, project-specific information may be revised and updated, resulting in changes to the estimated reductions for those projects. The revisions may increase or decrease estimated reductions, and DEP will work with stakeholders to address revisions as they are identified.
The project status column is standardized into the following five categories:
Canceled: Project or activity that was planned but will no longer take place. This category includes the cessation of ongoing activities.
Completed: Project, activity, or task that is finished. This category includes fully implemented activities (i.e., ongoing activities) that must continue to maintain assigned credits indefinitely (such as street sweeping, BMP cleanout, catch basin cleanout, public education, fertilizer cessation/reduction, and vegetation harvesting).
Planned: Project or activity that is conceptual or proposed.
Underway: Project or activity that has commenced or initiated but is not completed and is not yet reducing nutrient loads from the treated area.
Ongoing: The lead entity is performing actions each year. This status is used when a project is typically nonstructural and continuous. Ongoing projects are not a continuation of a reduction for a structural project.
Prior to reporting project information, DEP contacts each lead entity to gather new information on projects and confirm previously reported information. The terms used throughout the project tables are defined as follows:
Not provided: Denotes that information was requested by DEP but was not provided by the lead entity.
TBD: To be determined. Denotes that information is not currently available but will be provided by the stakeholder when it is available.
N/A: Not applicable. Denotes that information for that category is not relevant to that project.
0: Zero. Denotes the numeric value for that category as zero.
[bookmark: _Toc483903011]The project tables are based on current information, and project details may be updated as further information becomes available.
This BMAP requires stakeholders to implement their projects to achieve reductions as soon as practicable. However, the full implementation of the BMAP will be a long-term process. While some of the projects and activities listed in the BMAP were recently completed or are currently ongoing, several projects require more time to design, secure funding, and construct. Unlike the existing and planned projects, these future projects are not yet considered commitments of the entities but rather are intended for future BMAP credit, pending the availability of funding and other resources.
Although BMAP implementation is a long-term process, the goal of this BMAP is to achieve the TMDLs by the 2035 milestone. It is understood that all waterbodies can respond differently to the implementation of reduced loadings to meet applicable water quality standards. Continued coordination and communication by the stakeholders will be essential to ensure that management strategies continue to meet the implementation milestones.

[bookmark: _Toc58684927][bookmark: _Toc58592587]Appendix B. North IRL Allocation Calculations
The first step in the allocation process was to establish the total TN and TP load, by segment group, from the SWIL Model. This is an important step because the watershed loads to each segment are based on the updated information and model refinements incorporated in the model. Table B-1 lists the TN and TP starting loads from the SWIL Model for each segment group and the associated acres of watershed in that segment.
[bookmark: _Ref58417168][bookmark: _Ref58501962][bookmark: _Toc58513924][bookmark: _Toc58745919][bookmark: _Toc58576679][bookmark: _Toc58605300]Table B-1. North IRL Segment Group starting loads from model
	Segment Group
	Area (Acres)
	TN Starting Load
(lbs/yr)
	TP Starting load
(lbs/yr)

	IR1-5
	135,169
	399,161
	46,021

	IR6-7
	40,022
	152,737
	20,424

	IR8-11
	37,291
	167,774
	23,971

	IR8-11, EauGallie
	4,608
	39,412
	5,808




[bookmark: _Ref58501980]The TMDLs for the IRL (Rule 62.304.520, F.A.C.) include a percent reduction from the starting load, by segment group, for TN and TP. In some cases, the segment groups represent one WBID, while other segment groups include multiple WBIDs. Table B-2 describes the TMDL rule percent reduction for each segment group and lists the WBIDs and project zone to which the segment group belongs.
[bookmark: _Ref58417207][bookmark: _Toc58576680][bookmark: _Toc58605301][bookmark: _Toc58513925][bookmark: _Toc58745920]Table B-2. North IRL BMAP Segment Group TMDL required reduction percentage
	WBID
	Project Zone
	Segment Group
	% TN Reduction
	% TP Reduction

	2963F & 2963E
	A
	IR1-5
	35
	47

	2963D & 3028
	B
	IR6-7
	36
	53

	2963B & 2963C
	B
	IR8-11
	36
	48

	3082
	B
	IR8-11, EauGallie
	51
	58




The second step in the allocation calculations was to apply the segment group TMDL percent reduction (Table B-2) for TN and TP to the starting load (Table B-1). Table B-3 lists the TN and TP reductions to meet the TMDL based on these calculations. The allowable load after the reductions are met is called the allocation. To calculate the TN allocation and the TP allocation in the table, the TN reduction or TP reduction is subtracted from the TN or TP starting load listed in Table B-1.
[bookmark: _Ref58417472][bookmark: _Toc58513926]

[bookmark: _Ref58502017][bookmark: _Toc58576681][bookmark: _Toc58605302][bookmark: _Toc58745921][bookmark: _Hlk58500011]Table B-3. North IRL Segment Group load reduction and allowable load (allocation) before adjustments
	Segment Group
	TN Reduction (lbs/yr)
	TN Allocation (lbs/yr)
	TP Reduction (lbs/yr)
	TP Allocation (lbs/yr)

	IR1-5
	139,706
	259,455
	21,630
	24,391

	IR6-7
	54,985
	97,751
	10,825
	9,599

	IR8-11
	60,399
	107,375
	11,506
	12,465

	IR8-11, EauGallie
	20,100
	19,312
	3,369
	2,439




Now that the total reductions are calculated with the TMDL percent reductions, a test is completed to ensure there are no requirements to make reductions from natural land uses. To test whether the calculated reductions would go beyond reductions for converted land uses (anthropogenic land uses), DEP calculated the weighted average load per acre of natural lands (natural load per acre) in each segment group. The natural load per acre values were calculated from loads associated with natural lands in the initial model output. Any land use adjustments that were later incorporated into the allocation process were not accounted for in the natural load per acre calculations. Table B-4 outlines the data that were used to calculate the natural load per acre for TN and TP. The acreage and the weighted average loading from only the natural lands were calculated from the SWIL Model, by segment group. Then the loading for TN and TP was divided by the acres of natural lands, respectively, to derive the natural load per acre and the values were rounded. These natural loads per acre were compared to the allowable loads per acre, as shown in Table B-5.
[bookmark: _Ref58424632][bookmark: _Ref58502082][bookmark: _Toc58513927][bookmark: _Toc58745922][bookmark: _Toc58576682][bookmark: _Toc58605303]Table B-4. North IRL allowable load per acre from model natural loading 
Lbs/ac/yr = Pounds per acre per year
	Segment Group
	Land Type
	Area (Acres)
	TN Natural Lands Load (lbs/yr)
	TP Natural Lands Load (lbs/yr)
	Natural TN Load 
(lbs/ac/yr)
	Natural TP Load 
(lbs/ac/yr)

	IR1-5
	Natural Lands
	113,157
	234,870
	22,061
	2.08
	0.19

	IR6-7
	Natural Lands
	26,352
	43,044
	4,380
	1.63
	0.17

	IR8-11
	Natural Lands
	19,700
	20,337
	2,527
	1.03
	0.13

	IR8-11, EauGallie
	Natural Lands
	438
	1,986
	248
	4.54
	0.57




DEP then calculated the allowable load per acre for each segment group. The allowable load per acre is the allocation load divided by the acres in the segment group. The allowable load is calculated for both TN and TP and compared to the weighted average load per acre of natural lands (natural load per acre) in that segment group. If the allowable load per acre is less than the natural load per acre, an adjustment is made. In Table B-5, the allowable load per acre for TN and TP are shown and "True" is entered if the allowable load per acre is less than the natural load per acre. When the test is "True" an adjustment is made for the TN reduction, TP reduction, or both. 
[bookmark: _Ref58420826][bookmark: _Toc58513928]

[bookmark: _Ref58502109][bookmark: _Toc58745923][bookmark: _Toc58576683][bookmark: _Toc58605304]Table B-5. North IRL allowable load per acre from the total allocation
	Segment Group
	Allowable TN Load Per Acre
	Natural TN Load (lbs/ac/yr)
	Is Allowable TN Load Per Acre (LPA) Less than Natural TN LPA?
	Allowable TP Load Per Acre
	Natural TP Load 
(lbs/ac/yr)
	Is Allowable TP LPA Less than Natural TP LPA?
	Result

	IR1-5
	1.92
	2.08
	TRUE
	0.18
	0.19
	TRUE
	Use adjustment for both

	IR6-7
	2.44
	1.63
	FALSE
	0.24
	0.17
	FALSE
	No adjustment for either

	IR8-11
	2.88
	1.03
	FALSE
	0.33
	0.13
	FALSE
	No adjustment for either

	IR8-11, EauGallie
	4.19
	4.54
	TRUE
	0.53
	0.57
	TRUE
	Use adjustment for both



When an adjustment was indicated, the reductions were then adjusted by taking the starting loads from Table B-1 and subtracting the adjusted allowable load and adjusting the reductions listed previously in Table B-3. Only those reductions noted as needing a adjustment (see Table B-5) were adjusted. A summary of the TN and TP reductions (adjusted, if appliable) and the TN and TP allocations are listed in Table B-6. 
[bookmark: _Ref58491240][bookmark: _Ref58502198][bookmark: _Toc58576684][bookmark: _Toc58605305][bookmark: _Toc58513929][bookmark: _Toc58745924]Table B-6. Adjusted North IRL Segment Group load reduction and allowable load (allocation)
	Segment Group
	Adjusted TN Reduction (lbs/yr)
	Adjusted TN Allocation (lbs/yr)
	Adjusted TP Reduction (lbs/yr)
	Adjusted TP Allocation (lbs/yr)

	IR1-5
	118,009
	281,152
	20,339
	25,682

	IR8-11, EauGallie
	18,492
	20,920
	3,181
	2,627




[bookmark: _Ref58427241][bookmark: _Toc58513931]After the reductions are calculated for each segment group, the relative starting load in the segment group for each stakeholder is used to assign their entity reductions. The natural lands are separated from each entity's area to assess their relative anthropogenic contributions, so that stakeholders would not be asked to reduce loads from natural lands in their jurisdiction. In Table B-7, Table B-8, Table B-9, and Table B-10, the natural lands are separated from the starting loads, and so only the anthropogenic loadings are included in the entity loads. 

[bookmark: _Ref58502641][bookmark: _Toc58745925][bookmark: _Toc58576513][bookmark: _Toc58576685][bookmark: _Toc58605306]Table B-7. North IRL Segment IR1-5 entity starting loads from model, natural lands separated
	Segment Group
	Entity
	TN Starting Load (lbs/yr)
	TP Starting load (lbs/yr)

	IR1-5
	Natural Lands
	235,399
	22,127

	IR1-5
	Agricultural Producers
	28,374
	4,278

	IR1-5
	Brevard County
	38,328
	5,842

	IR1-5
	City of Edgewater
	2,704
	361

	IR1-5
	City of Oak Hill
	371
	49

	IR1-5
	City of Titusville
	51,549
	7,561

	IR1-5
	FDOT District 5
	5,972
	766

	IR1-5
	Kennedy Space Center
	13,435
	1,728

	IR1-5
	Volusia County
	23,029
	3,309

	IR1-5 
	Total
	399,161
	46,021



[bookmark: _Ref58502647][bookmark: _Ref58439408][bookmark: _Toc58745926][bookmark: _Toc58576686][bookmark: _Toc58605307][bookmark: _Toc58513932]Table B-8. North IRL Segment IR6-7 entity starting loads from model, natural lands separated 
	Segment Group
	Entity
	TN Starting Load (lbs/yr)
	TP Starting load (lbs/yr)

	IR6-7
	Natural Lands
	43,012
	4,381

	IR6-7
	Agricultural Producers
	7,923
	1,218

	IR6-7
	Brevard County
	72,774
	10,872

	IR6-7
	City of Cocoa
	15,169
	2,219

	IR6-7
	City of Titusville
	5,226
	703

	IR6-7
	FDOT District 5
	3,796
	508

	IR6-7
	Kennedy Space Center
	4,836
	524

	IR6-7 
	Total
	152,737
	20,424



[bookmark: _Ref58439444][bookmark: _Ref58502658][bookmark: _Toc58745927][bookmark: _Toc58576687][bookmark: _Toc58605308][bookmark: _Toc58513933]Table B-9. North IRL Segment IR8-11 entity starting loads from model, natural lands separated 
	Segment Group
	Entity
	TN Starting Load (lbs/yr)
	TP Starting load (lbs/yr)

	IR8-11
	Natural Lands
	20,166
	2,505

	IR8-11
	Agricultural Producers
	1,723
	242

	IR8-11
	Brevard County
	60,227
	8,864

	IR8-11
	City of Cocoa
	3,020
	427

	IR8-11
	City of Melbourne
	47,884
	6,960

	IR8-11
	City of Rockledge
	27,669
	3,982

	IR8-11
	FDOT District 5
	3,539
	472

	IR8-11
	Town of Indialantic
	1,623
	244

	IR8-11
	Town of Palm Shores
	1,924
	276

	IR8-11 
	Total
	167,774
	23,971


[bookmark: _Ref58502660]
[bookmark: _Ref58439416][bookmark: _Toc58745928][bookmark: _Toc58576688][bookmark: _Toc58605309][bookmark: _Toc58513934]Table B-10. North IRL Segment IR8-11, EauGallie entity starting loads from model, natural lands separated 
	Segment Group
	Entity
	TN Starting Load (lbs/yr)
	TP Starting Load (lbs/yr)

	IR8-11, EauGallie
	Natural Lands
	1,976
	247

	IR8-11, EauGallie
	Agricultural Producers
	78
	12

	IR8-11, EauGallie
	Brevard County
	6,866
	1,010

	IR8-11, EauGallie
	City of Melbourne
	29,907
	4,460

	IR8-11, EauGallie
	FDOT District 5
	586
	79

	IR8-11, EauGallie 
	Total
	39,412
	5,808




After the natural lands were separated from the entity loading estimates based on the SWIL Model, the relative contribution of each entity to the total segment group anthropogenic load was calculated. Table B-11, Table B-12, Table B-13, and Table B-14 show the percent contribution within the segment group to anthropogenic TN and TP, respectively, by entity. The TN contribution percentage is calculated by dividing the entity anthropogenic TN load by the total anthropogenic TN segment load and then a similar calculation is performed for each entity's TP loads.
[bookmark: _Ref58427382][bookmark: _Ref58502880][bookmark: _Toc58745929][bookmark: _Toc58576689][bookmark: _Toc58605310][bookmark: _Toc58513935][bookmark: _Ref58502887][bookmark: _Hlk58500649]Table B-11. North IRL Segment IR1-5 entity anthropogenic starting loads from model, natural lands separated 
	Segment Group
	Entity
	Anthropogenic TN (lbs/yr)
	Anthropogenic TP (lbs/yr)
	% Contribution to Anthropogenic TN
	% Contribution to Anthropogenic TP

	IR1-5
	Natural Lands
	0
	0
	0.00%
	0.00%

	IR1-5
	Agricultural Producers
	28,374
	4,278
	17.33%
	17.90%

	IR1-5
	Brevard County
	38,328
	5,842
	23.40%
	24.45%

	IR1-5
	City of Edgewater
	2,704
	361
	1.65%
	1.51%

	IR1-5
	City of Oak Hill
	371
	49
	0.23%
	0.20%

	IR1-5
	City of Titusville
	51,549
	7,561
	31.48%
	31.65%

	IR1-5
	FDOT District 5
	5,972
	766
	3.65%
	3.21%

	IR1-5
	Kennedy Space Center
	13,435
	1,728
	8.20%
	7.23%

	IR1-5
	Volusia County
	23,029
	3,309
	14.06%
	13.85%

	IR1-5 
	Total
	163,762
	23,894
	100.00%
	100.00%






[bookmark: _Ref58503843][bookmark: _Ref58439562][bookmark: _Toc58745930][bookmark: _Toc58576690][bookmark: _Toc58605311][bookmark: _Toc58513936]Table B-12. North IRL Segment IR6-7 entity anthropogenic starting loads from model, natural lands separated 
	Segment Group
	Entity
	Anthropogenic TN (lbs/yr)
	Anthropogenic TP (lbs/yr)
	% Contribution to Anthropogenic TN
	% Contribution to Anthropogenic TP

	IR6-7
	Natural Lands
	0
	0
	0.00%
	0.00%

	IR6-7
	Agricultural Producers
	7,923
	1,218
	7.22%
	7.59%

	IR6-7
	Brevard County
	72,774
	10,872
	66.32%
	67.77%

	IR6-7
	City of Cocoa
	15,169
	2,219
	13.82%
	13.83%

	IR6-7
	City of Titusville
	5,226
	703
	4.76%
	4.38%

	IR6-7
	FDOT District 5
	3,796
	508
	3.46%
	3.17%

	IR6-7
	Kennedy Space Center
	4,836
	524
	4.41%
	3.26%

	IR6-7 
	Total
	109,725
	16,043
	100.00%
	100.00%




[bookmark: _Ref58503852][bookmark: _Ref58439565][bookmark: _Toc58745931][bookmark: _Toc58576691][bookmark: _Toc58605312][bookmark: _Toc58513937][bookmark: _Hlk58503328]Table B-13. North IRL Segment IR8-11 entity anthropogenic starting loads from model, natural lands separated 
	Segment Group
	Entity
	Anthropogenic TN (lbs/yr)
	Anthropogenic TP (lbs/yr)
	% Contribution to Anthropogenic TN
	% Contribution to Anthropogenic TP

	IR8-11
	Natural Lands
	0
	0
	0.00%
	0.00%

	IR8-11
	Agricultural Producers
	1,723
	242
	1.17%
	1.13%

	IR8-11
	Brevard County
	60,227
	8,864
	40.80%
	41.29%

	IR8-11
	City of Cocoa
	3,020
	427
	2.05%
	1.99%

	IR8-11
	City of Melbourne
	47,884
	6,960
	32.44%
	32.42%

	IR8-11
	City of Rockledge
	27,669
	3,982
	18.75%
	18.55%

	IR8-11
	FDOT District 5
	3,539
	472
	2.40%
	2.20%

	IR8-11
	Town of Indialantic
	1,623
	244
	1.10%
	1.14%

	IR8-11
	Town of Palm Shores
	1,924
	276
	1.30%
	1.29%

	IR8-11 
	Total
	147,608
	21,466
	100.00%
	100.00%



[bookmark: _Ref58503858]
[bookmark: _Ref58439567][bookmark: _Toc58745932][bookmark: _Toc58576692][bookmark: _Toc58605313][bookmark: _Toc58513938]Table B-14. North IRL Segment IR8-11, EauGallie entity anthropogenic starting loads from model, natural lands separated 
	Segment Group
	Entity
	Anthropogenic TN (lbs/yr)
	Anthropogenic TP (lbs/yr)
	% Contribution to Anthropogenic TN
	% Contribution to Anthropogenic TP

	IR8-11, EauGallie
	Natural Lands
	0
	0
	0.00%
	0.00%

	IR8-11, EauGallie
	Agricultural Producers
	78
	12
	0.21%
	0.22%

	IR8-11, EauGallie
	Brevard County
	6,866
	1,010
	18.34%
	18.16%

	IR8-11, EauGallie
	City of Melbourne
	29,907
	4,460
	79.89%
	80.20%

	IR8-11, EauGallie
	FDOT District 5
	586
	79
	1.56%
	1.43%

	IR8-11, EauGallie 
	Total
	37,436
	5,561
	100.00%
	100.00%




For the unadjusted Segment Groups IR6-7 and IR8-11, each entity's reduction was calculated by multiplying the total segment group starting load (Table B-1) by the segment group required reduction (Table B-3) and by the entity's percent contribution to anthropogenic loading, as defined in Table B-12 and Table B-13. The calculations for the entity reductions were performed separately for TN and TP. The entity TN and TP allowable loading (allocations) are then computed by subtracting the entity required reductions in Table B-15 and Table B-16 from the entity anthropogenic starting loads (Table B-12 and Table B-13).
[bookmark: _Ref58504228][bookmark: _Ref58439846][bookmark: _Toc58513939][bookmark: _Toc58745933][bookmark: _Toc58576693][bookmark: _Toc58605314]Table B-15. North IRL Segment IR6-7 entity reduction and allowable loading (allocation)
	Segment Group
	Entity
	Entity TN Reduction (lbs/yr)
	Entity TP Reduction (lbs/yr)
	Entity TN Allocation (lbs/yr)
	Entity TP Allocation (lbs/yr)

	IR6-7
	Natural Lands
	0
	0
	43,012
	4,381

	IR6-7
	Agricultural Producers
	3,971
	822
	3,953
	396

	IR6-7
	Brevard County
	36,468
	7,336
	36,305
	3,536

	IR6-7
	City of Cocoa
	7,602
	1,497
	7,568
	722

	IR6-7
	City of Titusville
	2,619
	474
	2,607
	229

	IR6-7
	FDOT District 5
	1,902
	343
	1,894
	165

	IR6-7
	Kennedy Space Center
	2,423
	353
	2,413
	170

	IR6-7 
	Total
	54,985
	10,825
	97,751
	9,599




[bookmark: _Ref58504230][bookmark: _Ref58439849][bookmark: _Toc58513940][bookmark: _Toc58745934][bookmark: _Toc58576694][bookmark: _Toc58605315]Table B-16. North IRL Segment IR8-11 entity reduction and allowable loading (allocation)
	Segment Group
	Entity
	Entity TN Reduction (lbs/yr)
	Entity TP Reduction (lbs/yr)
	Entity TN Allocation (lbs/yr)
	Entity TP Allocation (lbs/yr)

	IR8-11
	Natural Lands
	0
	0
	20,166
	2,505

	IR8-11
	Agricultural Producers
	705
	130
	1,018
	112

	IR8-11
	Brevard County
	24,644
	4,751
	35,583
	4,113

	IR8-11
	City of Cocoa
	1,236
	229
	1,784
	198

	IR8-11
	City of Melbourne
	19,593
	3,731
	28,290
	3,229

	IR8-11
	City of Rockledge
	11,322
	2,135
	16,348
	1,848

	IR8-11
	FDOT District 5
	1,448
	253
	2,091
	219

	IR8-11
	Town of Indialantic
	664
	131
	959
	113

	IR8-11
	Town of Palm Shores
	787
	148
	1,137
	128

	IR8-11 
	Total
	60,399
	11,506
	107,375
	12,465




For Segment Groups IR1-5 and IR8-11/EauGallie, the entity reductions and allowable loads were calculated differently to incorporate the natural load per acre adjustment. Here, the segment group allocation was calculated by multiplying the acres in the segment group (Table B-4) by the segment group natural load per acre (Table B-4). Next, the entity allocation was computed by multiplying the adjusted segment group allocation (Table 6) by the entity percent contribution to anthropogenic loading (Table B-11 and Table B-14). Once the entity allocation was known, then the entity reduction was calculated by subtracting the entity allocation from the entity starting load. The reductions and allocations are listed in Table B-17 and B-18.
[bookmark: _Ref58428264][bookmark: _Ref58504615][bookmark: _Toc58513941][bookmark: _Toc58745935][bookmark: _Toc58576697][bookmark: _Toc58605318]Table B-17. North IRL Segment IR1-5 entity reduction and allowable loading at natural load per acre adjustment (allocation)
	Segment Group
	Entity
	Natural LPA TN Reduction (lbs/yr)
	Natural LPA TP Reduction (lbs/yr)
	Natural LPA TN Allocation (lbs/yr)
	Natural LPA TP Allocation (lbs/yr)

	IR1-5
	Natural Lands
	0
	0
	235,399
	22,127

	IR1-5
	Agricultural Producers
	20,550
	3,522
	7,824
	757

	IR1-5
	Brevard County
	27,759
	4,809
	10,569
	1,033

	IR1-5
	City of Edgewater
	1,959
	297
	746
	64

	IR1-5
	City of Oak Hill
	269
	40
	102
	9

	IR1-5
	City of Titusville
	37,334
	6,224
	14,215
	1,337

	IR1-5
	FDOT District 5
	4,325
	631
	1,647
	135

	IR1-5
	Kennedy Space Center
	9,730
	1,422
	3,705
	305

	IR1-5
	Volusia County
	16,679
	2,724
	6,350
	585

	IR1-5 
	Total
	118,604
	19,669
	280,558
	26,352




[bookmark: _Ref58504638][bookmark: _Toc58513942][bookmark: _Toc58745936][bookmark: _Toc58576698][bookmark: _Toc58605319]Table B-18. North IRL Segment IR8-11, EauGallie entity reduction and allowable loading at natural load per acre adjustment (allocation)
	Segment Group
	Entity
	Natural LPA TN Reduction (lbs/yr)
	Natural LPA TP Reduction (lbs/yr)
	Natural LPA TN Allocation (lbs/yr)
	Natural LPA TP Allocation (lbs/yr)

	IR8-11, EauGallie
	Natural Lands
	0
	0
	1,976
	247

	IR8-11, EauGallie
	Agricultural Producers
	39
	7
	40
	5

	IR8-11, EauGallie
	Brevard County
	3,394
	580
	3,472
	430

	IR8-11, EauGallie
	City of Melbourne
	14,785
	2,561
	15,122
	1,899

	IR8-11, EauGallie
	FDOT District 5
	289
	46
	296
	34

	IR8-11, EauGallie 
	Total
	18,507
	3,194
	20,905
	2,615




As described above, the entity calculations were performed by segment group. Once these were complete, the information was summarized by entity. In Table B-19, the starting loads for each entity are totaled across all the segment groups in which they have a land area. Also listed are their relative percentage of anthropogenic load for TN and TP, respectively, in the BMAP area. 
One stakeholder contributes less than 0.30 % of both the TN and TP loading from the watershed to the NIRL. The contribution to the overall nutrient loading from these stakeholders is low enough that reductions from these areas would have essentially no impact on the required reductions for the BMAP during this phase of implementation; therefore, this entity is currently considered a low priority for implementing reductions. Low-priority entities will be evaluated in future phases of BMAP implementation, as their contributions may change over time. The stakeholder meeting the requirements for low priority is highlighted in grey.
[bookmark: _Ref58504671][bookmark: _Ref58443871][bookmark: _Toc58513943][bookmark: _Toc58745937][bookmark: _Toc58576701][bookmark: _Toc58605322]Table B-19. North IRL starting loads
	Entity
	Starting TN Load (lbs/yr)
	Anthropogenic % TN in BMAP
	Starting TP Load (lbs/yr)
	Anthropogenic % TP in BMAP

	Agricultural Producers
	38,099
	8.31%
	5,750
	8.59%

	Brevard County
	178,194
	38.86%
	26,588
	39.70%

	City of Cocoa
	18,189
	3.97%
	2,645
	3.95%

	City of Edgewater
	2,704
	0.59%
	361
	0.54%

	City of Melbourne
	77,791
	16.97%
	11,420
	17.05%

	City of Rockledge
	27,669
	6.03%
	3,982
	5.95%

	City of Titusville
	56,775
	12.38%
	8,264
	12.34%

	FDOT District 5
	13,893
	3.03%
	1,825
	2.73%

	Kennedy Space Center
	18,271
	3.98%
	2,251
	3.36%

	Town of Indialantic
	1,623
	0.35%
	244
	0.36%

	Town of Palm Shores
	1,924
	0.42%
	276
	0.41%

	Volusia County
	23,029
	5.02%
	3,309
	4.94%

	City of Oak Hill
	371
	0.08%
	49
	0.07%

	Total of Allocated Entities
	458,532
	100.00%
	66,964
	100.00%

	Natural Lands
	300,552
	N/A
	29,259
	N/A

	Total of BMAP
	759,084
	N/A
	96,224
	N/A




Table B-20 and Table B-21 breakdown the TN and TP reductions for each entity by project zone and in total for the BMAP area.
[bookmark: _Ref58504693][bookmark: _Ref58492241][bookmark: _Toc58513944][bookmark: _Toc58745938][bookmark: _Toc58576702][bookmark: _Toc58605323]Table B-20. North IRL entity TN reductions by project zone
*Indicates a project zone with a segment group adjustment
	Entity
	Project Zone A
	Project Zone B
	Total

	Brevard County
	27,759
	64,506
	92,265

	City of Melbourne
	0
	34,378
	34,378

	City of Titusville
	37,334
	2,619
	39,953

	Agricultural Producers
	20,550
	4,714
	25,264

	City of Rockledge
	0
	11,322
	11,322

	Volusia County
	16,679
	0
	16,679

	Kennedy Space Center
	9,730
	2,423
	12,153

	City of Cocoa
	0
	8,837
	8,837

	FDOT District 5
	4,325
	3,640
	7,965

	City of Edgewater
	1,959
	0
	1,959

	Town of Palm Shores
	0
	787
	787

	Town of Indialantic
	0
	664
	664

	City of Oak Hill
	269
	0
	N/A

	Total
	118,604*
	133,891*
	252,226



[bookmark: _Ref58504695][bookmark: _Ref58444001][bookmark: _Toc58513945][bookmark: _Toc58745939][bookmark: _Toc58576703][bookmark: _Toc58605324]Table B-21. North IRL entity TP reductions by project zone
*Indicates a project zone with a segment group adjustment
	Entity
	Project Zone A
	Project Zone B
	Total

	Brevard County
	4,809
	12,667
	17,476

	City of Melbourne
	0
	6,292
	6,292

	City of Titusville
	6,224
	474
	6,698

	Agricultural Producers
	3,522
	958
	4,480

	City of Rockledge
	0
	2,135
	2,135

	Volusia County
	2,724
	0
	2,724

	Kennedy Space Center
	1,422
	353
	1,775

	City of Cocoa
	0
	1,726
	1,726

	FDOT District 5
	631
	641
	1,272

	City of Edgewater
	297
	0
	297

	Town of Palm Shores
	0
	148
	148

	Town of Indialantic
	0
	131
	131

	City of Oak Hill
	40
	0
	0

	Total
	19,669*
	25,524*
	45,154






[bookmark: APPB][bookmark: AppendixB][bookmark: _Ref519686823][bookmark: _Ref519686828][bookmark: _Toc21936368][bookmark: _Toc31199754][bookmark: _Toc58684928][bookmark: _Toc58592588][bookmark: _Hlk22197974][bookmark: _Hlk25102745]Appendix C. Agricultural Enrollment and Reductions
[bookmark: _Toc31199755](Language in this appendix was provided by FDACS.)
All agricultural nonpoint sources in the North Indian River Lagoon BMAP area are statutorily required either to implement FDACS-adopted BMPs or to conduct water quality monitoring prescribed by DEP or the applicable water management district. Under Paragraph 403.067(7)(c), F.S., the proper implementation of FDACS-adopted, DEP-verified BMPs, in accordance with FDACS rules, provides a presumption of compliance with state water quality standards for the pollutants addressed by the BMPs.
FDACS Role in BMP Implementation and Follow-up
[bookmark: _Hlk55404921][bookmark: _Hlk55404948]When DEP adopts a BMAP that includes agriculture, it is the agricultural landowner's responsibility to enroll in the FDACS BMP Program and implement all applicable FDACS-adopted BMPs to help achieve load reductions. To date, FDACS OAWP has adopted BMP manuals by rule[footnoteRef:1] for cow/calf, citrus, vegetable and agronomic crops, nurseries, equine, sod, dairy, poultry, and specialty fruit and nut operations. All OAWP BMP manuals are periodically revised, updated, and subsequently reviewed and preliminarily verified by DEP before re-adoption. OAWP intends to update BMP manuals every five years. [1:  https://www.fdacs.gov/Agriculture-Industry/Water/Agricultural-Best-Management-Practices] 

To enroll in the FDACS BMP Program, landowners must meet with an OAWP representative to determine the BMPs that are applicable to their operation. The landowner must submit an NOI to implement the BMPs on the checklist from the applicable BMP manual to an OAWP representative. Because many agricultural operations are diverse and are engaged in the production of multiple commodities, a landowner may sign multiple NOIs for a single parcel.
[bookmark: _Hlk55405034][bookmark: _Hlk55405055]FDACS is required to conduct implementation verification site visits every two years to verify that landowners are implementing BMPs identified in their NOIs. BMP verification site visits are conducted to verify that all BMPs are being implemented properly, to review nutrient and irrigation management records, and to collect records FDACS is required to retain. In addition, FDACS verifies that cost-share items are being appropriately utilized. Procedures used to verify the implementation of agricultural BMPs are outlined in Rule 5M-1.008, F.A.C. Producers not implementing BMPs according to the process outlined in Title 5M-1, F.A.C., are referred to DEP for enforcement action after attempts at remedial action are exhausted.
[bookmark: _Hlk22650826][bookmark: _Hlk57986781]Section 403.067, F.S., requires that, where water quality problems persist despite the proper implementation of adopted agricultural BMPs, FDACS must reevaluate the practices, in consultation with DEP, and modify them if necessary. Continuing water quality problems will be detected through the monitoring component of the BMAP and other DEP, and SJRWMD activities. If a reevaluation of the BMPs is needed, FDACS will also include SJRWMD and other partners in the process pursuant to Subsection 403.067(7), F.S.
Adopted BMAP Agricultural Land Use and Enrollment
Land use data are helpful as a starting point for estimating agricultural acreage, determining agricultural nonpoint source loads, and developing strategies to reduce those loads in a BMAP area, but there are inherent limitations in the available data. The time of year when land use data are collected (through aerial photography) affects the accuracy of photo interpretation. Flights are often scheduled during the winter months because of better weather conditions and reduced leaf canopies. While these are favorable conditions for capturing aerial imagery, they make photo interpretation for determining agricultural land use more difficult. Agricultural lands are often fallow in the winter months and can lead to inappropriate analysis of the photo imagery.
There is also a significant variation in the frequency with which various sources of data are collected and compiled, and older data are less likely to capture the frequent changes that often typify agricultural land use. In addition, it is not always apparent that an agricultural activity is being conducted on the land. Consequently, DEP relies on local stakeholder knowledge and coordination with FDACS to verify agricultural acreage and BMP implementation.
[bookmark: _Hlk27249678]FDACS uses the FSAID Geodatabase to estimate agricultural acreages statewide. FSAID is derived from water management district land use data, and is refined using county property appraiser data, OAWP BMP enrollment data, U.S. Department of Agriculture data for agriculture, such as the Cropland Data Layer and Census of Agriculture, FDACS Division of Plant Industry citrus data, water management district water use and permitting data, as well as field verification performed by USGS, the water management districts, and OAWP. Ongoing mapping and ground-truthing efforts of the FSAID dataset provide the best available data on the status of agricultural lands in Florida. 
[bookmark: _Hlk27249796]In terms of NOIs, enrolled acreage fluctuates when parcels are sold, when leases end or change hands, or when production areas downsize or production ceases, among other reasons. OAWP BMP enrollments are delineated in GIS using county property appraiser parcels. Nonproduction areas such as forest, roads, urban structures, and water features are often included within the parcel boundaries. Conversely, agricultural lands in the FSAID only include areas identified as agriculture. To estimate the agricultural acres enrolled in the BMP Program, OAWP overlays FSAID and BMP enrollment data within GIS to calculate the acres of agricultural land in an enrolled parcel.
[bookmark: _Hlk30337524]To address the greatest resource concerns, OAWP utilizes a phased approach based on commodity type and agricultural acreages, while ensuring that all entities identified as agriculture will be notified. Table C-1 lists the agricultural acreage based on FSAID VII that is enrolled in the North Indian River Lagoon BMAP area.
Table C-2 shows the agricultural acreage enrolled in the North Indian River Lagoon BMAP area by project zone. Table C-3 through Table C-5 show the agricultural land use acreage enrolled in the BMP Program by commodity. Figure C-1 shows the parcels enrolled in the BMP Program by commodity in the North Indian River Lagoon BMAP area; however, compliance with Section 403.067, F.S. is based on the NOIs and site visits described in Section 2.3.1.
[bookmark: _Ref55486008][bookmark: _Ref56192342][bookmark: _Toc58513946][bookmark: _Toc58745940][bookmark: _Toc58576514][bookmark: _Toc58576704][bookmark: _Toc58605325]Table C-1. Agricultural land use acreage enrolled summary in the BMP Program in the NIRL BMAP area as of July 2020
	Category
	Acres

	FSAID VII agricultural acres in the BMAP area
	7,256

	Total agricultural acres enrolled
	401

	% of FSAID VII agricultural acres enrolled
	6%



[bookmark: _Ref55486054][bookmark: _Ref56192353][bookmark: _Toc58513947][bookmark: _Toc58576515][bookmark: _Toc58576705][bookmark: _Toc58745941][bookmark: _Toc58605326]Table C-2. Agricultural land use acreage enrolled in the BMP Program in the NIRL BMAP area by project zone
	Project Zone
	Total Agricultural Acres
	Agricultural Acres Enrolled
	% of Agricultural Acreage Enrolled

	A
	5,683
	327
	6

	B
	1,573
	74
	5

	Total
	7,256
	401
	6


[bookmark: _Toc31199888]
[bookmark: _Ref55486090][bookmark: _Ref56192364][bookmark: _Toc58513948][bookmark: _Toc58745942][bookmark: _Toc58576516][bookmark: _Toc58576706][bookmark: _Toc58605327]Table C-3. Agricultural land use acreage enrolled in the NIRL BMAP area by BMP Program
	Related OAWP BMP Programs
	Agricultural Acres Enrolled

	Citrus
	280

	Cow/Calf
	114

	Fruit/Nut
	6

	Nursery
	1

	Total
	401


[bookmark: _Toc24623809][bookmark: _Toc31199889]
[bookmark: _Toc58513949][bookmark: _Toc58745943][bookmark: _Toc58576517][bookmark: _Toc58576707][bookmark: _Toc58605328]Table C-4. Agricultural land use acreage enrolled in the BMP Program in Project Zone A
	Related OAWP BMP Programs
	Agricultural Acres Enrolled

	Citrus
	213

	Cow/Calf
	114

	Total
	327



[bookmark: _Ref55486223][bookmark: _Toc58513950][bookmark: _Toc58576518][bookmark: _Toc58576708]

[bookmark: _Toc58745944][bookmark: _Toc58605329]Table C-5. Agricultural land use acreage enrolled in the BMP Program in Project Zone B
	Related OAWP BMP Programs
	Agricultural Acres Enrolled

	Citrus
	67

	Fruit/Nut
	6

	Nursery
	1

	Total
	74



[bookmark: _Toc58605361]
[image: ]
[bookmark: _Ref55486370][bookmark: _Ref56192416][bookmark: _Toc58514028][bookmark: _Toc58684158][bookmark: _Toc58575617]Figure C-1. BMP enrollment in the North Indian River Lagoon BMAP area as of July 2020


Unenrolled Agricultural Acreage
As of July 2020, 6 % of the agricultural acres in the North Indian River Lagoon BMAP area are enrolled in FDACS' BMP Program and are implementing practices designed to improve water quality. FDACS continues to increase enrollment in all BMAPs to meet the BMAP goal of enrolling 100% of the enrollable agricultural acres in the BMP Program. To achieve that goal, land use analyses are conducted to ensure that areas containing commercial agricultural land uses are prioritized. Lands classified as agriculture where the ability to implement agricultural BMPs under the BMP Program is limited, such as smaller rural homesteads, receive lower priority for enrollment.
General Considerations
Although land use data have been used as the basis for prioritizing FDACS enrollment efforts, many land use issues not captured by these databases affect FDACS enrollment efforts. Many areas within the North Indian River Lagoon BMAP boundaries experience rapid land use changes, especially at the urban/rural boundary. Agricultural lands are regularly converted to residential, industrial, commercial, or multiuse properties, but still appear in various databases as pasture or other rural lands. While these lands are likely to be developed in the near future, the agricultural land use classifications require these properties to comply with the BMP enrollment requirements.
[bookmark: _Hlk55405633]Additionally, the counties' methods of classifying small acreages as agricultural lands can affect the BMP enrollment process. Along with these changes, there are also large agricultural parcels being subdivided but remaining classified as "agriculture." These rural homesteads—also called residential agriculture, rural residential, rural estates, equine communities, ranchettes, and other descriptive names for homes with some acreage and agricultural zoning—present a particular challenge for FDACS The current BMP manuals and the measures they contain target commercial agricultural production practices and, in many cases, cannot be scaled down to appropriately enroll activities on these smaller, non-commercial agricultural properties. The increasing number of these smaller parcels with noncommercial agricultural activity represents a growing component of unenrolled acreage. It will be necessary to develop a suite of options to apply to these properties or develop a new classification that may subject these types of areas to other requirements to ensure their nutrient loading contribution is being appropriately identified and reduced. 
Further, thousands of acres of open land, scrubland, unimproved pasture, and grazing land exist without a readily identifiable agricultural production activity that will fit within the framework of existing FDACS BMP manuals. Also, these types of parcels are usually controlled by many different individuals. It will be necessary to develop a suite of options to apply to these properties or develop a new classification that may subject these types of areas to alternative methods to ensure their nutrient loading contribution is being appropriately identified and reduced.
Another challenging area includes those agricultural lands that are inactive or fallow—i.e., lands that, on the day the FDACS representative visits, display no enrollable agricultural activity. These lands may be part of a rotation implemented by a landowner, scheduled for development, listed for sale, etc. The land use information FDACS receives is consistently improving the classification of these areas, but policy options remain limited in scope to ensure the implementation of practices aimed at reducing nutrient inputs from these areas.
Characterization of Unenrolled Agricultural Lands
To characterize unenrolled agricultural acres, OAWP identified FSAID VII features outside the BMP enrollment areas and overlaid these features with property appraiser parcels within GIS. OAWP then identified the number of parcels that encompass the unenrolled agricultural lands and the number of agricultural acres present within the parcels. The parcel owner information, other parcel details, and aerial imagery were used identify parcels that are unlikely to contain agricultural activity. As previously mentioned, OAWP BMP enrollments are initially delineated based on county property appraiser parcel data, even if the entire parcel is not agriculture, to allow BMPs to be tied to the specific parcels where agricultural activities are occurring. FSAID agricultural lands are delineated based on land use features identified as agriculture and represent a more refined analysis of those areas actually in agricultural production.
Because of differences in the spatial geometries between the OAWP BMP enrollment, FSAID, and property appraiser parcels, when they are combined or compared, the boundaries often do not align precisely, creating "slivers." Slivers are not enrollable because they are an artifact of the geospatial analysis and do not represent lands with active agricultural practices. For example, a sliver can represent the area between the boundary of a parcel and the beginning of a road, canal, easement, etc. A sliver can also represent a small portion of an FSAID feature outside the BMP enrollment areas that is slightly overlapped by a property appraiser parcel. Slivers are often associated with previously enrolled agricultural operations but because of the delineation differences, these slivers are not captured within the enrolled parcel during geoprocessing. When characterizing unenrolled agricultural lands, slivers are excluded. Figure C-2 shows an example of a sliver created when performing geospatial analysis.
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[bookmark: _Ref55486396][bookmark: _Ref56192497][bookmark: _Toc31199780][bookmark: _Toc58514029][bookmark: _Toc58683286][bookmark: _Toc58684159][bookmark: _Toc58575618][bookmark: _Toc58605362][bookmark: _Toc27135008]Figure C-2. GIS example of a sliver 


Large areas that are identified as agricultural land use but are unlikely to have enrollable agricultural activities include lands owned by the state (Board of Trustees of the Internal Improvement Trust Fund) and water management districts (SJRWMD). It is possible that these lands, in whole or in part, may be leased to other entities that conduct agricultural activities, but such leasing is infrequent. If leasing occurs, the leasing entity will be required to enroll in the BMP Program. Ongoing coordination between FDACS, DEP Division of State Lands, and SJRWMD is needed to ensure that any public lands that are leased for the purposes of agricultural activities are required to implement and enroll in FDACS BMP Program as a condition of the lease.
Other smaller parcels that have been identified as nonagricultural but have features that cause them to be identified as agricultural lands in various databases, include those lands associated with utilities, telecommunication companies, churches, FDOT rights-of-way, and airports. The Florida Department of Revenue (DOR) uses code numbers 70 through 98 to identify these types of lands.
Those agricultural lands that have been identified as "fallow," "former [ag]," and "abandoned," as well as brushland/scrubland/open land, comprise 49 % of the total unenrolled agricultural acres in the North Indian River Lagoon BMAP area. These acres are still classified as agricultural land for the purposes of the BMAP nutrient load assessment. There are a variety of potential options to account for these lands, such as enrollment as "temporarily inactive" operations—particularly those that were previously enrolled and are planned to resume production. Another option may be to note the inactive acres at the time of a field visit and perform periodic reassessment on a cyclical basis. The possibility for DEP and FDACS to calculate nutrient reduction credits or adjust nutrient loading rates may also provide opportunities to present more accurate estimates and establish priorities.
Another factor considered in the prioritization of BMP enrollment is the number of agricultural acres on the parcel. Analyzing the number of agricultural acreages on the parcel and commodity type can give an idea of the efforts that are needed to enroll these areas in FDACS' BMP Program and also identify the areas most in need of enrollment. Figure C-3 summarizes the agricultural acres distributed by agricultural acreage found on each parcel.
[bookmark: _Hlk55405878]Further analysis was done to characterize the parcels based on agricultural acreage and land use type. For graphing purposes, land use distribution is displayed in two charts, one showing the land use for parcels containing 50 acres of agriculture or greater (Figure C-4) and a second for parcels containing less than 50 acres of agriculture (Figure C-5). Of the 5,176 acres of land identified as having potential agricultural fallow land comprises 46 % of this acreage.


[bookmark: _Toc27135009][bookmark: _Toc31199781][image: ]
[bookmark: _Ref55486431][bookmark: _Ref56192512][bookmark: _Toc58514030][bookmark: _Toc58683287][bookmark: _Toc58684160][bookmark: _Toc58575619][bookmark: _Toc58605363]Figure C-3. Distribution of agricultural acreage on parcels with potential agricultural activity, NIRL BMAP area
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[bookmark: _Ref55486443][bookmark: _Ref56192523][bookmark: _Toc27135010][bookmark: _Toc31199782][bookmark: _Toc58514031][bookmark: _Toc58683288][bookmark: _Toc58684161][bookmark: _Toc58575620][bookmark: _Toc58605364]Figure C-4. Agricultural land uses on parcels with 50 acres of agriculture and greater, NIRL BMAP area
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[bookmark: _Ref55486454][bookmark: _Ref56192536][bookmark: _Toc27135011][bookmark: _Toc31199783][bookmark: _Toc58514032][bookmark: _Toc58683289][bookmark: _Toc58684162][bookmark: _Toc58575621][bookmark: _Toc58605365]Figure C-5. Agricultural land uses on parcels with less than 50 acres of agriculture, NIRL BMAP area


Table C-6 lists the total acreage associated with the identified slivers and the lands that are not likely to have enrollable agricultural activities, along with the remaining total of unenrolled agricultural acres in the BMAP area. Figure C-6 and Figure C-7 summarize the unenrolled agricultural acres in the North Indian River Lagoon BMAP area by acres of agriculture within the parcels. However, they do not include acreages or parcels associated with slivers or lands that are not likely to have enrollable agricultural activities.
[bookmark: _Ref55486550][bookmark: _Ref56192308][bookmark: _Toc58513951][bookmark: _Toc58745945][bookmark: _Toc58576521][bookmark: _Toc58576711][bookmark: _Toc58605332][bookmark: _Hlk53741417]Table C-6. Summary of unenrolled agricultural land use acreage in the NIRL BMAP area
Note: Because of geometric variations between shapefiles used in the unenrolled agricultural lands analysis performed by OAWP, the unenrolled agricultural acres differ from subtraction of the FSAID VII Agricultural Acres in the BMAP and the Total Agricultural Acres Enrolled referenced in Table C-1.
	Category
	Acres

	Unenrolled agricultural acres
	6,855

	Acres identified within slivers of unenrolled agricultural areas
	164

	Lands without enrollable agricultural activity (e.g., tribal lands, residential development, and parcels with DOR use codes 70-98)
	1,515

	Total lands with potentially enrollable agricultural activities
	5,176
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[bookmark: _Ref55486574][bookmark: _Ref56192558][bookmark: _Toc27135012][bookmark: _Toc31199784][bookmark: _Toc58514033][bookmark: _Toc58683290][bookmark: _Toc58684163][bookmark: _Toc58575622][bookmark: _Toc58605366][bookmark: _Hlk54020949]Figure C-6. Number of parcels with 50 acres of agriculture and greater, NIRL BMAP area
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[bookmark: _Ref55486584][bookmark: _Ref56192565][bookmark: _Toc27135013][bookmark: _Toc31199785][bookmark: _Toc58514034][bookmark: _Toc58575623][bookmark: _Toc58605367]Figure C-7. Number of parcels with less than 50 acres of agriculture, NIRL BMAP area


[bookmark: _Hlk29549295]Unenrolled agriculture characterization information for each individual project zone, including the distribution of agricultural acres within each parcel and land use type, is presented in Figure C-8 through Figure C-11. 
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[bookmark: _Ref55486680][bookmark: _Ref56192588][bookmark: _Toc58514035][bookmark: _Toc58575624][bookmark: _Toc58605368]Figure C-8. Distribution of agricultural acreage on parcels with potential agricultural activity, Project Zone A
[bookmark: _Toc29558154][image: ]
[bookmark: _Toc58514036][bookmark: _Toc58575625][bookmark: _Toc58605369]Figure C-9. Land use type and distribution of agricultural acreage, Project Zone A
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[bookmark: _Toc58514037][bookmark: _Toc58575626][bookmark: _Toc58605370]Figure C-10. Distribution of agricultural acreage on parcels with potential agricultural activity, Project Zone B
[bookmark: _Toc29558158][image: ]
[bookmark: _Ref55488561][bookmark: _Toc58514038][bookmark: _Toc58575627][bookmark: _Toc58605371]Figure C-11. Land use type and distribution of agricultural acreage by parcel size, Project Zone B

Future Efforts
[bookmark: _Hlk55406473]To address resource concerns, FDACS continues enhancing coordination with producers, agencies and stakeholders to increase enrollment in the BMP Program. OAWP is sending correspondence to agricultural land owners within BMAP s that are not currently enrolled in the BMP Program to increase enrollment rates and verify land uses where additional focus may be required to achieve resource protection. This effort is utilizing a phased approach and targeting priority land uses and then using the amount of agricultural acreage for the remaining unenrolled lands, while ensuring that all entities identified as agriculture will be notified. Additionally, OAWP continues to coordinate with industry groups and outreach partners to educate and inform agricultural producers about the BMP Program.
Additional Factors Related to Agricultural Lands and Measuring Progress
Legacy loading can present an additional challenge to measuring progress in many of areas of Florida with adopted BMAPs. Based on research, initial verification by DEP, and long-term trends in water quality in the BMAP area, it is expected that current efforts, such as BMP implementation, will continue to provide improvements in overall water quality despite the impacts from legacy loads. 
While the implementation of BMPs will improve the water quality in the basin, it is not reasonable to assume that BMP implementation alone can overcome the issues of legacy loads, conversion to more urban environments, and the effects of intense weather events. BMP implementation is one of several complex and integrated components in managing the water resources of a watershed. Additional regional projects, precisely located and operated, may be needed to achieve the TMDLs for the North Indian River Lagoon basin.
Collaboration between DEP, the water management districts, and other state agencies, as well as local governments, federal partners, and agricultural producers, is critical in identifying projects and programs, as well as locating funding opportunities to achieve allocations provided for under this BMAP. To improve water quality while retaining the benefits agricultural production provides to local communities, wildlife enhancement, and the preservation of natural areas requires a commitment from all stakeholders to implementing protective measures in a way that maintain the viability of agricultural operations.
Recommended Updates to Land Use
BMAP loads and allocations, as well as water supply projections, are based primarily on land use data. Maintaining the most accurate agricultural land use dataset is critical to planning and policy decisions. Although crop changes, technology advances, and land ownership/lessee changes related to agricultural operations create dynamic environments and difficulties in estimating impacts from specific operations, FDACS and DEP continue to coordinate and develop ways to improve accuracy.
DEP and OAWP recognize that land use–related issues that consistently occur during BMAP development and/or updates. One of these issues is the differentiation between what is classified as an agricultural land use in the TMDL or BMAP model and that is no longer an agricultural land use by the time this BMAP is adopted or an update occurs.
OAWP has developed a methodology to identify agricultural land use changes to make adjustments in subsequent models and reports. Using GIS, OAWP compared the SWIL Model land use with the latest FSAID land use and BMP enrollment data. OAWP identified areas classified as agriculture by the BMAP modeled land use that do not overlap with the latest FSAID or BMP enrollment data.
OAWP reviewed the output of this overlay analysis by using county appraiser data and aerial imagery to determine if the nonoverlapping areas were still in production. OAWP identified 1,725 acres, classified as agriculture in the SWIL land use, that are now other land use types such as residential, industrial, or commercial (see Table C-7). DEP evaluated the land use changes identified by OAWP and apportioned the associated acres and loads to the appropriate entities after a discussion with each entity.
Often the analyses show changes that have occurred more rapidly than any land use data can capture, such as the transition to residential development. The land use changes are provided to DEP as a GIS shapefile with a description of the information in the county property appraiser database and aerial imagery reflected for the refinement of the acreage and loading allocated to agriculture in a BMAP area.
[bookmark: _Ref55488049][bookmark: _Ref56192270][bookmark: _Toc58513952][bookmark: _Toc58745946][bookmark: _Toc58576522][bookmark: _Toc58576712][bookmark: _Toc58605333]Table C-7. Agricultural land use change by project zone
	Project Zone
	Acres

	A
	637

	B
	1,088

	Total
	1,725




[bookmark: _Hlk27237105]In addition to identifying land use changes in the BMAP area modeled land use, OAWP regularly reviews FSAID data, at times daily or weekly, as it performs other job functions. Any edits or changes are reviewed and considered for inclusion in the next iteration of the FSAID.
Potential Site-Specific Nutrient Management Measures in Addition to BMPs
Beyond enrolling producers in the BMP Program and verifying implementation, OAWP will also work with producers to identify a suite of agricultural projects and research agricultural technologies that could be implemented on properties where they are deemed technically feasible and if funding is made available. FDACS executes contracts with soil and water conservation districts and other partners to administer cost-share funds and provide technical and administrative support for these districts and other partners. Cost-share funding is being used to implement higher level BMPs, innovative technologies, and regional projects to provide the next added increment of improving and protecting water quality. 
[bookmark: _Toc31199899]Table C-8 identifies the agricultural technologies that received cost-share assistance in the North Indian River Lagoon BMAP area and the associated nutrient reductions based on the 2016 Soil and Water Engineering Technology (SWET) report. Using the nutrient reductions from the report, OAWP developed a methodology to estimate nutrient reductions for NOIs that have received cost-share funding. The NOI boundary, based on property appraiser parcel data, was considered the area treated by the cost-shared agricultural technology or project. For parcels with more than one cost-share project, OAWP identified the order of treatment to determine the reductions for the multiple projects and created a workbook that provided the cost-share agricultural technologies and the formulas to estimate the nutrient reductions.
[bookmark: _Ref55488104]

[bookmark: _Ref56192248][bookmark: _Toc58513953][bookmark: _Toc58745947][bookmark: _Toc58576523][bookmark: _Toc58576713][bookmark: _Toc58605334]Table C-8. Cost-share project types and associated nutrient reductions recommended by OAWP
1 Reductions for this measure are not incorporated as part of this exercise
2 Reductions for this measure are from Table 5. Estimated Edge of Farm Nutrient Load Reductions for the FDACS Okeechobee BMP Program in the 2016 SWET Report (Bottcher 2016) and is represented in pounds per year per unit (each project is 1 unit)
	Project Types
	TN Reductions
(%)
	TP Reductions
(%)

	Chemigation/fertigation
	20
	20

	Fence
	10
	10

	Irrigation improvements, automation
	20
	20

	Precision agriculture technology
	30
	10

	Weather station1
	20
	5

	Well, pipeline, trough, pond, heavy use protection2
	50
	50




[bookmark: AppendixC][bookmark: _Toc58684929][bookmark: _Toc58592589]Appendix D. Seagrass Analysis
PROCESS TO CONDUCT THE SEAGRASS DEPTH LIMIT COMPLIANCE EVALUATION
The goal of the IRL Basin TMDLs is to recover the deeper seagrass habitats. The seagrass response is the most important factor in evaluating the success of the nutrient TMDLs. Even if the relationship among nutrient loads and seagrass recovery is not as predicted by the regression model, the load reduction requirements themselves will not determine TMDL success. The assessment of success is based on whether the seagrass grows at sufficient depths. 
The TMDL seagrass depth limit targets are based on a union coverage of the seagrass mapping data from 1943, 1986, 1989, 1992, 1994, 1996, and 1999. The SJRWMD created this union coverage when it set pollutant load reduction goals for the IRL Basin. The TMDL targets are not based on the full restoration of seagrass depths represented by this union coverage; instead, they were set at 90% of the full restoration estimate. These targets allow for seagrass growth almost to the depths previously seen in the lagoon, while accounting for the fact that changes have been made to the lagoon system that may limit seagrass growth in some areas, such as dredged areas similar to the Intracoastal Waterway. 
Compliance with the TMDL seagrass depth limit targets is assessed on a project zone scale using the latest four consecutive data sets of seagrass mapping data. For the assessment years to be compliant with the TMDL seagrass depth limit targets, the data must meet the requirements of a two-step evaluation process. 
The first step is a comparison of the TMDL union coverage cumulative frequency distribution curve with the assessment years' union cumulative frequency distribution curve. The cumulative distribution curves show what percentage of the seagrass deep edge is located at different depths. To be compliant, at least 50 % of the assessment years' curve, including the median, must be on or to the right of the TMDL curve. 
The second step in the evaluation process is a comparison of the TMDL union coverage median value with each assessment year's median value. To be compliant in the second step, at least three of the four assessment year medians must be equal to or greater than the TMDL median. If the seagrass data from the four assessment years are compliant with both steps of the test, the project zone is achieving the TMDL depth limit target. 
A series of GIS steps must be conducted to obtain the data necessary to complete the two-step evaluation process. These steps are as follows:
Start with the seagrass GIS shapefiles for the four latest assessment years and edit these files to include only Categories 9113 and 9116, which represent seagrass. Other categories in the GIS shapefiles represent algae cover, which should not be included in this assessment. The seagrass shapefiles only represent the location of the seagrass beds.
Use the dissolve function in GIS to create the union file of the assessment years. This union file results in a coverage of where seagrass beds were located during all four assessment years. 
Transform the polygons to a polyline in the assessment years' union file. This polyline represents the edges of the seagrass beds. 
Draw a 15.8-m buffer around the seagrass polyline that is 7.9 m inside and 7.9 m outside the seagrass bed. The bathymetry layer was created by the SJRWMD in 1996, and the bathymetry was measured every 15.2 m. The 15.8-m buffer around the seagrass polyline ensures that 1 bathymetry point will be captured in the GIS analysis.
Intersect the updated bathymetry shapefile with the seagrass coverage file that was transformed into a polyline. This intersection correlates the depth data with the seagrass locations so that depths along the seagrass bed edge can be determined. 
Intersect the deep edge file to each project zone (BRL A, BRL B, North A, North B, Central A, Central SEB, and Central B). 
Use the select by location function to identify and note points within dredged areas. The dredged areas are removed from this coverage because seagrass is not expected to grow in areas that have been dredged.
Identify and note points that fall below 0.3 m and above 3.5 m from the coverage. This step is needed because seagrass growing at depths less than 0.3 m are likely not light-limited, and seagrass are not expected to grow at depths greater than 3.5 meters. 
Identify and note points from the intersections of holes or bare areas, which do not represent the deep edge of the seagrass bed.
These steps are also followed separately for each assessment year so that the median value can be calculated. 
The final points that represent the seagrass deep edge boundary for the assessment years' union coverage are then exported from GIS into Excel to conduct the two-step evaluation. The depth points are sorted from highest to lowest, and the count of the number of points at each depth is determined. The cumulative count is determined by taking the count for the shallowest depth and adding it to the count for the next shallowest point until the counts for all the depths are added together to yield the total number of depth points. The cumulative count at each depth is divided by the total points to determine the percentage of the seagrass points at each depth. These points are then plotted as a curve on a graph for comparison with the TMDL cumulative distribution curve. For the Step 2 evaluation, the median depth point is calculated for each assessment year using Excel. These medians are then compared with the TMDL median to determine compliance. 
The maps in Figure D-1 and Figure D-2 include the locations of ground truthing conducted before and during aerial surveys. Additionally, the transect locations where SJRWMD conducts seasonal monitoring are shown. For more information on how SJRWMD and partners conduct seagrass surveys, SJRWMD's SOP is referenced in Chapter 5. 
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[bookmark: _Ref55484861][bookmark: _Ref56185515][bookmark: _Toc58514039][bookmark: _Toc58575632][bookmark: _Toc58576524][bookmark: _Toc58605376]Figure D-1. Map of the seagrass transects in NIRL A
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Spatial lterative Watershed Loading (SWIL) Model-Load Estimation
Tool(LET)
Allocation Calculations, AUgUSt 2020
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