Dear Mr. Livingston:  

I have been reading through the Draft and noted the following edits. 

p. 172, 
d. Round to 44 (Instead of 49)
e. From Appendix D, using the table for Zone 2 (not 1), for a DCIA of 18.76% (not 40%) and a non-DCIA curve number of 44 (not 49), the            retention depth is about 0.53 (not 1.12) inches of runoff...
The retention volume = 90 (not 3) * about 0.53 (not 1.12)* 1ft/12in = ?

p. 173, 
e.  The TN loading rate for Group 1 = 0.00064 (not 0.00769)  This effects the equations further down. 

p. 175, g.  The TN loading of should be 29.7 (not 35.3)

p. 177,
Table 22.3-1 Dry Retention Treatment Effectiveness for parallel BMP's.  In the Basin TP Load (pounds) column every value seems to be incorrect.  For example, the first row for Basin No. 1 should be 0.853 (not 1.88).  Also all the Retention Basin Volume values seem to be incorrect.  For example, the first row for Basin No. 1 should be 0.24 (not 1.00).  In the notes under the same table in note 4, the equation should be:

TP load discharged = basin TP load * (1 - retention basin efficiency)

p. 184, 
very top of page should reference Figure 13-2 (not 13-4).
Half way down page Appendix F (not E)
i.  Appendix F  (Not E).

This is as far as I was able to get this week.  I'm not sure how much time next week I will have to continue reviewing the design examples.  I would appreciate any comments back to help clarify the examples especially if my comments are in error.  I look forward to hearing from you. 
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