Middle Trout River Basin
Total Maximum Daily Load (TMDL) Required Load Reductions
January 13, 2011

	Source
	Total Nitrogen (lbs/yr)
	Total Phosphorus (lbs/yr)

	Urban Loads
	
	

	Middle Trout – Septic Tanks
	2,650.00
	1,104.00

	Middle Trout – Urban and Built-up 
	5,875.65
	795.99

	Upper Trout – Urban
	792.95
	94.31

	Gulley Branch – Urban 
	1,217.00
	153.82

	Total Urban Load
	10,535.60
	2,148.12

	Required Percent Reduction
	30%
	70%

	Urban Required Reduction
	3,160.68
	1,503.68

	
	
	

	Agriculture Loads
	
	

	Middle Trout – Agriculture  
	5,023.78
	703.51

	Upper Trout – Agriculture 
	2,000.27
	274.64

	Gulley Branch – Agriculture 
	752.23
	101.65

	Total Agriculture Load
	7,776.28
	1,079.80

	Required Percent Reduction
	30%
	70%

	Agriculture Required Reduction
	2,332.88
	755.86

	
	
	

	Undeveloped Area Loads
	
	

	Middle Trout – Forest/Wetland/Water/Open Lands 
	30,829.13
	1,244.33

	Upper Trout – Forest/Wetland/Water 
	6,079.69
	246.43

	Gulley Branch – Forest/Wetland/Water 
	2,726.70
	112.91

	Total Undeveloped Area Load
	39,635.52
	1,603.67

	Required Percent Reduction
	0%
	0%

	Undeveloped Area Required Reduction
	0.00
	0.00
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