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Meeting Summary:

1. Verified List of impaired waters was adopted by Secretarial Order on May 27.  Lake Jesup, Crane Strand, Crane Strand Drain, and Long Branch are listed as impaired waters, with TMDLs due by September 30, 2005.

2. Troy Keller has developed TN and TP targets for Lake Jesup.  Currently, numbers are under review, but will be available for next meeting.

3. Modeling Issues

· Status of modeling. Basin is set up hydraulically.  Refinements are needed to identify hotspot locations and sub-basins. 

· What is role of lake’s sediment?  Coarse analysis performed by DEP concluded that watershed loading was comparable in magnitude to output loading from Lake Jesup to St. Johns River.  More discussion at September meeting.   Question: Did DEP account for resuspension in calculations?  No, on an annual time frame, there is net deposition to the sediment.  How will resuspension affect TMDL model?   It is thought that effects of resuspension are short time period phenomena, while the TMDL is annualized. 

· Landuse. DEP will evaluate the change in landuse between the 1995/96 and 1999/2000 time periods.  Still need to identify areas of rapidly changing landuse that may need more detailed delineation.

· Suggested addition of Forest as a landuse category.

· Background landuse loadings.  DEP is interpreting historic aerial photos to estimate the ratio of wetland and upland forest to be used for estimating background landuse loadings. DEP has photos from Seminole County, but we still need 1938 photos from Orange County.

· Water quality evaluation period 1990-2000, or later date if needed.

· Loads from sewer line breaks/overflows and septic tanks.  Don’t know how much loading is contributed by sewer line breaks and overflows. Septic tanks are treated as a negative BMP.  Still need estimate of number and location of septic tanks. Septic tanks included as negative BMP.

· BMPs.  Seminole County has GIS coverage of BMPs. Orange County has an inventory of BMPs available.  Are there other BMPs that have not been included in existing GIS coverage? Need event mean concentration data. DEP is looking for water removal efficiencies for BMPs.  Watershed attenuation of loadings will be modeled by GIS coverage of BMPs.

· Bank seepage.  Contribution of surficial aquifer to lake loadings. DEP will model baseflow for Lake Jesup.  Still need ground water quality data. 

· Sediment Delivery Ratio.  Some natural attenuation of sediment loads by waterbodies may occur in basin.  Long lake chains in Howell Creek sub-basin may remove sediment and any associated nutrient.

4. New water quality projects or activities that could influence TMDL model:

· City of Sanford WWTP discharge directed to reuse.

· Oviedo has completed future landuse build out map.

· Sweetwater Creek stormwater treatment project

· Cameron Ranch Ditch stormwater project

5. 
Funds for Lake Jesup dredging are not in state budget.  Permit is temporarily shelfed with incomplete status.  Friends of Lake Jesup are assisting in the search for a new spoil disposal site. 

Action Steps 

1. Next meeting is scheduled for September 22 at Lake Sylvan Park. Start time is 9:00 AM.

2. Joe Walter, with PBSJ, is coordinating the collection and preparation of data for DEP.  Please contact Joe with information at jhwalter@pbsj.com. DEP maintains an FTP site at ftp.dep.state.fl.us/pub/water/incoming/Lake_Jesup_TMDL to assist with data transfers.  

3. Need ground water quality data, both surficial aquifer and spring data. Also need spring discharge data. SJRWMD is forwarding a report on springs to DEP.  DEP’s Ground Water Assessment Section is coordinating the collection of ground water data and will contact USGS and SJRWMD. Any other reports or contacts please forward to DEP.  

4. Rainfall data from SJRWMD.  SJRWMD needs sub-basin delineations from DEP to download data from their system.

5. Danielle Gephardt, CDM, will forward southeastern database of EMC values to DEP.

6. Need discharge data and gauging station locations.

