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Basin Management Action Plan for Implementation of Fecal Coliform and Dissolved Oxygen Total Maximum Daily Loads in Long Branch (WBID 3030), Orange County, Florida

The Long Branch Basin Management Action Plan (BMAP) addresses fecal coliform and dissolved oxygen (DO) impairments in Long Branch, a stream in northeastern Orange County, Florida (WBID 3030).  Long Branch was verified as impaired for elevated fecal coliform counts and low dissolved oxygen.  Total Maximum Daily Loads (TMDLs) were adopted for these parameters in 2005.  The BMAP focuses on a common-sense approach to identify pollutant sources and reduce their impacts.  The BMAP documents the management actions that have been or will be undertaken by Orange County, as the entire Long Branch watershed is located within the unincorporated County.  

The BMAP should be considered a working document.  The plan provides documentation of stakeholder commitments, primarily Orange County, to continue source identification and implement appropriate management actions to address elevated coliforms and low dissolved oxygen in Long Branch.  The plan is discussed in further detail in the following sections. 

Despite additional water testing and field investigations completed by the County as part of BMAP development, the sources of fecal coliform and nutrient loadings are not entirely clear, nor what percentage are man-induced versus naturally occurring.  The results strongly indicate that the major sources of the bacteria are from non-human sources (i.e. wildlife).  However, the data does not completely rule out human sources.  The seasonally low stream flow in Long Branch and technical and scientific limitations with field investigations and coliform sampling and analysis make it very difficult to conclude with 100 percent confidence that there are no human sources.  
Orange County has committed to further activities to help identify and isolate the pollutant sources contributing to current water impairments.  Additionally, despite any direct evidence that human sources are a major contributor of bacteria pollutants to Long Branch, the County has committed to or is implementing specific management actions address existing and future development.  These actions will protect water quality from pollutants, including fecal coliform bacteria, in stormwater runoff from new and existing development in the Long Branch basin. However, until a human-source of fecal coliform bacteria is identified, no new management actions to reduce pollutant loads from human-sources are being proposed.  
Looking toward the future, the County will monitor any changes in land use within the basin and will take water samples annually to monitor fecal coliform levels in Long Branch over the next five years.  The Florida Department of Environmental Protection (DEP) will reassess the basin as part of the Watershed Management Basin Rotation Cycle to determine the status of TMDL implementation.  As part of the 2009 reassessment the Basin Working Group will determine the appropriate actions based on the findings from ongoing or planned source identification studies and any changes in land use or water quality. 
A.1  Background

The Long Branch BMAP has been developed as part of DEP’s TMDL Program (authorized by the Florida Watershed Restoration Act [FWRA] [Section 403.067, Florida Statutes [F.S.]).  DEP implements the act using a watershed management approach that includes a five-year rotating basin cycle.  Each year of the cycle represents a different activity for the waters within a given basin group, as follows:  Initial Basin Assessment, Strategic Monitoring, Data Analysis and TMDL Development, Basin Management Action Plan Development; and Basin Management Action Plan Implementation.  At the end of each five-year, five-phase cycle, a new cycle begins for each group of basins in which additional waters may be identified for TMDL establishment and implementation. 

The Long Branch watershed is located within the Middle St. Johns Basin.  Long Branch is a tributary to the Big Econlockhatchee River and is located in east central Orange County as shown on Figure A-1.  The watershed is generally bounded on the west by the Big Econlockhatchee River, to the south by the Wedgefield Subdivision, and to the east and north by State Road 50.  The area of the WBID is entirely within unincorporated Orange County and comprises approximately 4,511 acres, including a small portion of the unincorporated Town of Bithlo.  Long Branch is located within the jurisdiction of the St. Johns River Water Management District (SJRWMD), DEP Central District, and Department of Transportation (DOT) District 5.

Land use in the study area is dominated by agriculture, forest, open land, and wetlands.  Combined, these account for more than 78 percent of the watershed.  There are a number of publicly owned lands within the study area.  Both the County and the SJRWMD own a number of parcels within the study area that are part of Long Branch Park, Hal Scott Preserve, regulatory easements and conservation easements.  With a total area of approximately 1,520 acres, 34 percent of the watershed is in public ownership or management.  Beyond the dominance of conservation land, the other significant feature in the watershed is the Orlando SpeedWorld facility.  

Long Branch consists of a northern tributary that drains the southeastern portion of Bithlo, a southern tributary that drains conservation area, and the main stem, flanked primarily by wetlands.  Streamflow in this system is intermittent, and there is typically only flow immediately after a storm event.  Times of no flow or stagnant water in Long Branch are common.  A summary of water quality conditions can be found in Figure A-2 (fecal coliforms) and Figure A-3 (dissolved oxygen).  Water quality samples taken near the SpeedWorld facility have shown highly variable results, but conditions in this portion of the watershed appear to correlate with rainfall.
A.2  Total Maximum Daily Loads

TMDLs are water quality targets for waterbodies that DEP has identified as impaired for specific pollutants (such as total phosphorus [TP], total nitrogen [TN], and others).  TMDLs, which DEP adopts by rule, establish the maximum amount of specific pollutants that a waterbody can assimilate while maintaining water quality standards.  Long Branch is designated as a Class III water in accordance with Rule 62-302, Florida Administrative Code (F.A.C.), meaning that it must have suitable water quality for recreational use and for the propagation and maintenance of a healthy, well-balanced population of fish and wildlife.  

To establish the TMDLs, DEP assessed Long Branch, the pollutant(s) contributing to the impairment, and the amount of the pollutant(s) entering the waterbody during a specified period.  DEP then determined the level of pollutant(s) that Long Branch could receive while maintaining its designated use (the TMDL), and calculated the corresponding pollutant reduction needed to achieve the TMDL.  
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Figure A-1: Location of the Long Branch Watershed
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Figure A-2: Summary of Fecal Coliform Data for Long Branch
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Figure A-3: Summary of Dissolved Oxygen Data for Long Branch

In 2005, DEP adopted TMDLs to address elevated fecal coliforms and low dissolved oxygen in Long Branch.  Table A-1 lists the TMDLs for these waterbodies.  Long Branch was also verified as impaired for total coliforms and iron.  However, between TMDL adoption and BMAP development, total coliforms were removed from the Florida water quality standards and an iron evaluation indicated that this impairment was naturally caused.  Thus, this BMAP addresses only the fecal coliform and dissolved oxygen impairments.

In the Long Branch dissolved oxygen TMDL, three different causative pollutants were found:  biochemical oxygen demand (BOD) in the tributaries, TP in the tributaries, and TN in the main stem.  Thus, the dissolved oxygen TMDL is expressed in terms of these three parameters.

Table A-1: Long Branch TMDLs
	Parameter
	TMDL
	Allocation

	
	
	Orange County Permitted Municipal Stormwater

(percent reduction)
	Other Nonpoint

(percent reduction)

	Fecal Coliform
	4.64 x 1010 counts/day
	32%
	32%

	BOD (tributaries)
	14.96 tons/year
	10%
	10%

	TP (tributaries)
	0.74 tons/year
	30%
	30%

	TN (main stem)
	5.20 tons/year
	17%
	17%


A.3  BMAP Process

Stakeholder involvement is essential to develop, gain support for, and secure commitments to implement the BMAP.  Because of the location of the Long Branch watershed, the vast majority of this BMAP was developed by Orange County, CDM, Inc., (under contract with Orange County), and DEP.  The County’s participation included staff from the Environmental Protection Division, Stormwater Management Division, and the Health Department.  Staff from the Florida Department of Agriculture and Consumer Services (DACS) were also involved.  

A public meeting to review, discuss, and comment on the BMAP was held on <INSERT DATE>.  The Orange County Commission was briefed on <INSERT DATE>.  During that same meeting the County approved a resolution in support of Long Branch BMAP implementation (see Figure A-4).
<INSERT>
Figure A-4: Orange County Resolution in Support of the Long Branch BMAP

A.3.1  Allocations

The TMDL provides a basis for allocating acceptable loads among all of the known pollutant sources in a watershed, so that appropriate control measures can be implemented and water quality standards achieved.  An adopted TMDL is expressed as the sum of all point source load allocations, nonpoint source load allocations, and an implicit or explicit margin of safety, which takes into account any uncertainty concerning the relationship between effluent limitations and water quality.

Under the FWRA (Subsection 403.067[7], F.S.), the TMDL allocation may be an “initial” pollutant allocation of allowable pollutant loads among point and nonpoint sources.  In such cases, the “detailed” allocation to specific point sources and specific categories of nonpoint sources must be established in the BMAP.  Under the FWRA, the “detailed” allocation to specific point sources and specific categories of nonpoint sources may be established in the BMAP.  Both initial and detailed allocations must be determined based on a number of factors listed in the FWRA, including cost-benefit, technical and environmental feasibility, implementation timeframes, and others.  Detailed allocations are most appropriate in basins with multiple point sources, detailed source identification, and sufficient data to support division of the initial TMDL allocations.
With only one permitted source is present in the watershed (Orange County MS4), there was no need to divide the initial TMDL allocation beyond “permitted nonpoint” [wasteload allocation (WLA)] and “non-permitted nonpoint” [load allocation (LA)].  Thus, detailed allocations were not developed for this BMAP.  The following factors also contributed to this decision:

· Source identification efforts resulted in qualitative information.  Thus, no information was available to calculate detailed allocations for the nutrient parameters related to the DO impairment.

· Coliform counts in the natural environment are notoriously variable.  Given the unknowns about coliform behavior in Long Branch specifically (e.g. potential for regrowth in the sediment, frequency of extremely low flow, effect of sampling day selection relative to flow), division of the coliform allocation was illogical.
A.3.2  Management Actions

This section provides information on the type of management actions being implemented to address Long Branch impairments.  The majority of management actions in this BMAP are being implemented by Orange County.  Long Branch management actions can be split into two groups:  broad-based and basin-specific.  Broad-based actions are those programs and activities that are implemented in a wider geographic area beyond the Long Branch watershed, such as the MS4 program and Environmental Resource Permitting (ERP).  Basin-specific management actions are primarily focused on source identification.  Table A-2 lists the Long Branch BMAP management actions.  

The Orange County Health Department (OCHD), Orange County Environmental Protection Department (OCEPD), and DEP worked closely together to evaluate coliform sources.  Despite additional water testing and follow-up investigations it is not entirely clear what the sources of fecal coliform loadings are and what percentage are man-induced versus naturally occurring.  The results strongly indicate that the major sources of the bacteria are from non-human sources; that is from wildlife.  However, the data does not completely rule out human sources.  The seasonally low stream flow in Long Branch and technical and scientific limitations with field investigations and coliform sampling and analysis make it very difficult to conclude with 100 percent confidence that there are no human sources.  However, the preponderance of data points to non-human sources as the major contributor.  These non-human sources are considered uncontrollable and therefore no management actions are proposed to reduce fecal coliform inputs from non-human sources within the Long Branch basin. 
Until a human-source of fecal coliform bacteria is identified, no new management actions to reduce pollutant loads from human-sources are being proposed.  However, as shown in Table A-2, Orange County has committed to further activities to help identify and isolate the pollutant sources contributing to current water impairments.  Additionally, despite any direct evidence that human sources are a major contributor of bacteria pollutants to Long Branch, management actions that address impacts from future development are included in this BMAP.  These actions will protect water quality from pollutants, including fecal coliform bacteria, in stormwater runoff from new and existing development in the Long Branch basin. 

Table A-2: Management Action Summary
	Management Action
	Description
	Timeline
	Responsible Party
	Related to County MS4 Permit

	Broad-Based Management Actions

	MS4 Permit Implementation
	Orange County is a Phase I MS4 (Permit No. FLS000011) responsible for developing and implementing a stormwater management program that reduces pollutants in stormwater to the maximum extent practicable.  This involves a broad range of activities from public education through erosion control, stormwater system and facility inspections, and system inventories.
	Ongoing
	Orange County EPD
	FLS000011

	Public Education and Outreach
	To help citizens develop a commitment to the environment’s health and well being, the County conducts two types of public outreach efforts: those intended to change behavior and those intended to inform the public about water resources.  These efforts include implementation of the Florida Yards and Neighborhoods Program, brochures, public presentations, school programs, Earth Day activities, and other outreach efforts.
	Ongoing
	Orange County (multiple departments)
	FLS000011

	Econlockhatchee River Protection Program
	Orange County has established special criteria for development within the Big Econlockhatchee River Basin, which are defined in Chapter 15 of the County’s Code of Ordinances. Within this basin, Orange County regulations require pollution abatement, recharge where possible, and flood protection.
	Ongoing
	Orange County EPD
	Not Applicable

	Parks Total Phosphorus Removal
	Fertilizer use on County park property is limited to 0 percent phosphorus, with 3 percent allowed if needed on regular turf, and a nitrogen application rate of less than 0.5 lbs per 1000 square feet.  Repeat applications within seven days are considered one application.  Phosphorus may be used selectively on plants that have high phosphorus needs, but this will be limited to small amounts and in localized areas.  The use of fertilizers, pesticides, and herbicides within 10 feet of shorelines and applying weed controls directly instead of broadcast applications of dry material are prohibited.  These restrictions apply to Bithlo and Long Branch Parks.
	Ongoing
	Orange County EPD and Parks and Recreation Division
	Not Applicable

	Lawn Maintenance Best Management Practices
	This program under development will educate lawn care workers on what happens to yard wastes that enter the stormwater and surface water system, and explain why it is important to reduce pollutants to surface waters by protecting the stormwater system.  The program is proposed to start with required training for all lawn care contractors who work for Orange County, and then, in conjunction with the Orange County Occupational License Office, to include the certification of all lawn care-related business owners.   
	Program under development; initiation anticipated in <INSERT YEAR>
	Orange County and Private Lawn Maintenance Companies
	Not Applicable

	Pollution Abatement Swale Design Criteria
	The County is currently researching the possibility of developing more specific criteria for the design, construction and maintenance of environmental berms and swales on properties abutting lakes and streams.  The County has identified specific deficiencies in the current code that require modification.  These modifications would apply to new development and redevelopment.
	Program under development; adoption anticipated in <INSERT YEAR>
	Orange County (stormwater? EPD?)
	Not Applicable

	Environmental Resource Permitting
	Activities that exceed SJRWMD permitting thresholds must be authorized by an Environmental Resource Permit from the District, which incorporates both stormwater treatment and mitigation of any wetland impacts.  
	Ongoing
	SJRWMD
	Not Applicable

	Agricultural Best Management Practices
	DACS develops, adopts, and implements agricultural Best Management Practices (BMPs) to reduce water quality impacts from agricultural discharges and enhance water conservation. A statewide BMP manual for cow/calf operations is under development.  Upon adoption, DACS will work with private landowners to implement the provisions of this BMP manual on their property.
	Program ongoing; Adoption of cow/calf BMP manual expected early 2008
	DACS and Private Landowners
	Not Applicable

	Basin-Specific Management Actions

	Hydrologic Measurements
	Flow meters will be installed at locations on both the north and south tributaries.  The County will also install a rainfall gage in the basin.  Data measured using these tools will provide a better understanding of the flow regimes in the Long Branch system.  Water quality data collected during future events can then also be correlated to flow and rainfall amounts.  
	Begin in 2008
	Orange County EPD
	Not Applicable

	Baseflow Analysis
	A baseflow separation analysis will be performed to more accurately determine the local influence that groundwater may have on the Long Branch system.
	Subsequent to flow meter installation
	Orange County EPD
	Not Applicable

	Sanitary Survey
	A detailed sanitary survey will be performed to determine what role septic systems play in the fecal coliform loading.  To help with prioritization, the County will first survey those properties constructed prior to 1984 which may not meet the current setback requirements and/or have the highest probability of failure.
	Begin in 2008
	Orange County Health Department and EPD
	Not Applicable

	Optical Brightener Testing
	Fluorometric detection of optical brighteners is a methodology used for detecting anthropogenic pollution in aquatic environments.  Pending equipment availability, the County will use this device to determine the presence of optical brightener dyes in the Long Branch system.  
	2008

(pending equipment availability)
	Orange County EPD
	Not Applicable


A.3.3  Management of Loadings from Future Growth
<INSERT; PENDING DEP’S ANALYSIS>
A.3.4  Cost of BMAP Implementation

<INSERT; PENDING INFO FROM COUNTY>
A.4  Monitoring Program

As part of the BMAP, stakeholders designed a strategy for monitoring water quality and measuring pollutant loads.  This strategy builds on the County’s existing water quality monitoring resources.  The strategy addresses monitoring parameters, quality assurance/ quality control (QA/QC), data management, and data evaluation to measure progress in achieving the TMDLs, while allowing for evaluation and feedback that better refine the monitoring strategy and provide information to better define how to achieve the TMDLs.  The specific objectives of this monitoring strategy are as follows

· Determine if positive trends in water quality conditions are being observed;

· Improve our ability to evaluate water quality conditions by enhancing flow measurements;

· Continue to improve source identification efforts; and

· Provide sufficient data to support the development of future management actions.

Information provided by the monitoring network will be useful in evaluating the cost-effectiveness of load reduction strategies, modifying existing and selecting future load reduction strategies, coordinating agency/group monitoring efforts to reduce duplication and conserve resources, and increasing the understanding of the relationship between pollutant loads and waterbody response.

The County intends to monitor basic water quality parameters and flow at critical points in the watershed.  These points were selected to facilitate ongoing source identification efforts.  Data collected by the network are maintained by DEP in a central database available to the public, and must meet QA requirements set by DEP.  Additional interagency data comparisons and QA checks will be conducted as practical. 

Observations of water quality conditions and trends will be discussed between the County, DEP, and other interested parties on a regular basis.  A more complete analysis of trends in the progress made toward achieving designated use will be made on a five-year basis, corresponding with DEP’s watershed management cycle.
A.5  Anticipated Outcomes

Since the adoption of the TMDL for Long Branch, Orange County has put forth significant effort to identify and isolate the source(s) contributing to both the DO and fecal coliform impairment.  To date, the County has been unsuccessful in identifying exact sources due to lack of flow in the Long Branch system as well as inconclusive sampling results.  Therefore, the BMAP will address further investigation of the sources of pollution and it is anticipated that BMAP implementation will achieve the following results:
· Identify and isolate sources of anthropogenic pollutants, if any, and develop management strategies to curb or eliminate these loads; 

· Identify those areas where the impairment may be attributed to natural background conditions (i.e., blackwater system, wildlife, etc.); 

· Enhanced understanding of Long Branch hydrology, water quality, and pollutant sources; and,

· Enhanced public awareness of pollutant sources, impacts, and management actions.

At this point, the activities outlined above are all qualitative.  As exact pollutant sources have not yet been identified, there are no data available to quantify anticipated nutrient loading reductions associated with BMAP activities as is typically done for other watersheds.  The following benefits are expected to result from the monitoring strategy proposed herein:
· Establish a long enough period of record for water quality data such that trends can be analyzed.

· Determine the relationship, if any, between water quality and the hydrologic data to be collected.

· Gain a better understanding of the relationships between the effect that nutrients have on DO, if any, in the Long Branch system.







