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Distributed for April 20, 2012 BMAP BWG Meeting
Wekiva BMAP Monitoring Plan Objectives:

Primary Objective: Long Term Trend Analysis 
Track inputs and concentration trends in TN and TP loads through groundwater , surface water, and MS4 sampling.

Secondary Objective: Source Assessment
Identify areas within the springshed/watershed with high loadings of nutrients to surface water and groundwater to better focus management efforts 

Sampling Parameters

	CORE PARAMETERS 
	SUPPLEMENTAL PARAMETERS 

	Total phosphorus (as P) 
	Total suspended solids (TSS) 

	Orthophosphate as P 
	Biochemical oxygen demand (BOD) 

	Nitrate/nitrite as N 
	Saturated Oxygen

	Total Kjeldahl nitrogen (TKN) 
	Color

	Chlorophyll-a (corrected)
	

	Dissolved oxygen (DO) 
	

	Temperature 
	

	Specific conductance 
	

	pH - field 
	



Monitoring Stations

	CORE (REQUIRED) STATIONS 
	SUPPLEMENTAL STATIONS

	All ambient ground water stations 
	All ground water monitoring stations associated with wastewater treatment plants 

	All surface water stations monitored at least monthly. 
	All other regularly sampled (e.g., quarterly, 3 times/ year, semi-annually, annually) ambient surface water or spring monitoring station



Additional Reference materials for the meeting
· Two (1) map of ambient ground water stations 
· Two (2) maps of the ground water monitoring stations associated with wastewater treatment plants (northern and southern portions of the basin)
· Two (2) maps of the surface water stations (northern and southern portions of the basin)
· List of monitoring stations.
