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Introduction
The information provided in Figures 1 through 7 in this appendix is intended to supplement the data summaries provided in Chapter 8B. Section 373.4595(3)(a)2.a., Florida Statutes, requires the evaluation of all available existing water quality data concerning total phosphorus (TP) in the Lake Okeechobee Watershed (LOW). Surface water quality monitoring networks have been in place in the LOW since the early 1980s. The purpose of the networks has been to collect ambient data for the long term and track changes in water quality over time within the watershed. 
[bookmark: _Hlk520788120]The South Florida Water Management District (SFWMD or District) currently has monitoring networks that include sampling locations at two hydrologic levels within the LOW: Level 1, subwatershed and drainage basin level (basin monitoring sites for which flow and TP concentration data are collected and TP load is calculated), and Level 2, subbasin level (upstream ambient/tributary sites). The locations of the Level 1 sites are shown in figures within this appendix for reference only, while the Level 1 data can be found in Table 8B-3 of Chapter 8B of this volume. The Level 2 tributary sites in the figures indicate locations where grab samples are collected during flow conditions for analysis of TP concentrations. Definitions of project codes in figures can be found in the Acronyms, Abbreviations, and Units of Measurements for the 2019 South Florida Environmental Report. 
[bookmark: _GoBack]This appendix presents TP data results for Water Year 2018 (WY2018; May 1, 2017–April 30, 2018) for the six subwatersheds north of Lake Okeechobee: Fisheating Creek, Indian Prairie, Lake Istokpoga, Upper Kissimmee, Lower Kissimmee, and Taylor Creek/Nubbin Slough basins S-191 and S‑154/S-154C. TP concentrations presented in Figures 1 through 7 are not flow-weighted because flow measurements are not available at most sites. TP concentrations ranges are grouped for reference in all figures. Box-and-whisker plots for each upstream monitoring site show the WY2018 average TP concentration compared to the distribution of TP concentrations for the most recent 10-year (WY2008–WY2017) period. 	Comment by Davis, Sara C.: Should this be in parentheses?
[bookmark: _Hlk520717146]In WY2016, 20 sites[footnoteRef:2] were temporarily suspended and monitoring was discontinued; the timeline for reinstating those sites is unknown. Also in WY2016, the sampling frequency at the majority of the upstream ambient/tributary sites was temporarily reduced from biweekly to monthly. SFWMD will continue an analysis to determine the impact of the frequency reduction and consider the findings in future monitoring optimization efforts.   [2:  The suspended sites included AJ33243122, AL11263113, AL24263113, AL34263113, CL19273123, CO35253112, HL08283014, BM15313111, IC35313112, KR23313113, KR32343214, LM29373514, TC09373513, AR21343013, RD01322813, HP09383151, HP27383124, HP36383112, IP29383313, and SD10373111.] 

[image: \\ad.sfwmd.gov\dfsroot\data\err_gis\projects\EVG\sfer\2019\png\Vol1_Appx8B-1\UpperK_TPAvg_WY2018_cm1.png]
Figure 1a. Upper Kissimmee Subwatershed upstream tributary average TP concentrations for WY2018. (Note: µg/L – micrograms per liter.)

	Upper Kissimmee
	WY2018
	Number of Samples per Water Yeara

	
	Number of Samples
	TP Concentration (µg/L)
	

	Map ID
	Site
	
	Avg
	Min
	Max
	2008
	2009
	2010
	2011
	2012
	2013
	2014
	2015
	2016
	2017

	1
	ABOGGN
	8
	61
	24
	197
	-
	-
	4
	12
	12
	12
	11
	11
	9
	4

	2
	BNSHINGLE
	10
	77
	35
	172
	9
	12
	10
	12
	10
	11
	11
	11
	10
	3

	3
	BS-59 (S59)
	7
	47
	16
	196
	3
	6
	8
	3
	9
	3
	8
	10
	5
	3

	4
	CL06283111 (S63A)
	4
	63
	29
	83
	-
	-
	-
	-
	13
	19
	15
	17
	11
	6

	5
	CL06283112
	2
	70
	56
	84
	-
	-
	-
	-
	-
	-
	-
	3
	-
	1

	6
	CL18273011 (S61)
	9
	48
	29
	64
	-
	-
	-
	-
	19
	11
	16
	23
	11
	6

	7
	CREEDYBR
	7
	106
	40
	184
	7
	10
	7
	8
	6
	7
	5
	9
	9
	3

	8
	DLMARNCR
	20b
	65
	26
	158
	-
	-
	-
	-
	-
	19
	26
	25
	19
	10

	9
	DLONDNCR
	10b
	79
	44
	154
	-
	-
	-
	-
	-
	5
	9
	16
	14
	6

	10
	EC-37
	21b
	78
	41
	173
	-
	-
	-
	-
	-
	-
	1
	19
	15
	8

	11
	ET05253114
	9
	40
	34
	56
	14
	10
	11
	5
	4
	10
	10
	17
	8
	11

	12
	ET06253113
	9
	173
	40
	979
	21
	19
	15
	20
	20
	23
	26
	24
	20
	9

	13
	GENTRYDTCH
	12b
	116
	24
	270
	-
	-
	-
	-
	-
	13
	7
	18
	18
	3

	14
	KUB009
	7b
	95
	44
	175
	-
	-
	-
	-
	-
	12
	8
	6
	19
	6

	15
	LG32263124 (S60)
	5
	23
	15
	29
	-
	-
	-
	-
	9
	7
	11
	16
	8
	5

	16
	LJACKDSCH
	8b
	98
	43
	158
	-
	-
	-
	-
	-
	16
	16
	19
	15
	5

	17
	LT32263013
	7
	92
	52
	171
	12
	15
	14
	11
	7
	3
	7
	7
	6
	2

	18
	MJ01253123
	5
	20
	17
	22
	-
	-
	-
	-
	7
	8
	8
	16
	7
	5

	19
	ML22303313
	7
	1551
	789
	2948
	-
	-
	-
	-
	-
	-
	-
	8
	11
	3

	20
	PA10313112
	10
	188
	41
	965
	12
	14
	17
	18
	14
	12
	11
	13
	11
	7

	21
	ROMCUT
	18b
	73
	38
	159
	-
	-
	-
	2
	2
	-
	-
	1
	-
	1


[bookmark: _Hlk523916859][bookmark: _Hlk520717211]a. During WY2016, the sampling frequency of the majority of the upstream ambient/tributary sites was reduced from biweekly to monthly because of SFWMD resource constraints.
b. These sites are visited biweekly, which may have resulted in a higher number of samples at the site.
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Figure 1b. Upper Kissimmee Subwatershed upstream tributary average TP concentrations for WY2018 and sample count for the previous 10-year period. (Note: µg/L -micrograms per liter, Avg – average, ID – Identification, Max – maximum, and Min – minimum.)
DRAFT	8B-8	10/26/201810/1/2018	
DRAFT	8B-16           	   10/26/201810/1/2018	
[image: ]
[image: ]
[bookmark: _Hlk520718312]Figure 1c. Box-and-whisker plot of WY2018 average TP concentration compared to the TP concentration distribution for the previous 10-year period for the upstream monitoring sites in the Upper Kissimmee Subwatershed.
[image: \\ad.sfwmd.gov\dfsroot\data\err_gis\projects\EVG\sfer\2019\png\Vol1_Appx8B-1\LowerK_TPAvg_WY2018_cm1.png]
Figure 2a. Lower Kissimmee Subwatershed upstream tributary average TP concentrations for WY2018. 

	Lower Kissimmee
	WY2018
	Number of Samples per Water Yeara

	
	Number of Samples
	TP Concentration (µg/L)
	

	Map ID
	Site
	
	Avg
	Min
	Max
	2008
	2009
	2010
	2011
	2012
	2013
	2014
	2015
	2016
	2017

	1
	02272676 (KREA 06)
	5b
	411
	114
	751
	-
	10
	29
	10
	7
	14
	11
	16
	15
	5

	2
	BB16313214
	3
	185
	131
	250
	11
	7
	13
	8
	6
	5
	1
	3
	-
	4

	3
	CY05353444
	8
	232
	48
	1040
	23
	24
	22
	22
	24
	25
	17
	21
	16
	4

	4
	CY06363411
	4
	471
	285
	683
	7
	6
	16
	5
	5
	11
	7
	11
	8
	1

	5
	CY17353413 (KREA 43A)
	4
	4100
	3159
	4790
	10
	7
	11
	7
	4
	10
	3
	1
	3
	2

	6
	KR05373311 (KREA 10D)
	9
	621
	148
	1707
	14
	13
	19
	18
	3
	7
	12
	7
	3
	1

	7
	KR24353114
	4
	266
	97
	524
	10
	10
	17
	12
	8
	11
	15
	18
	13
	6

	8
	KR29353334 (KREA 08)
	2
	720
	114
	1326
	3
	10
	11
	9
	3
	5
	9
	5
	5
	1

	9
	KR30353214
	5
	191
	67
	612
	25
	13
	15
	12
	-
	3
	2
	1
	1
	3

	10
	KR30353312 (KREA 07)
	1
	386
	386
	386
	3
	5
	13
	10
	4
	9
	2
	6
	-
	2

	11
	KR36363312 (KREA 16)
	4
	416
	156
	820
	10
	14
	19
	10
	2
	5
	5
	5
	3
	2

	12
	KREA 01
	4
	302
	181
	585
	11
	10
	12
	12
	11
	10
	12
	13
	8
	5

	13
	KREA 04
	7
	312
	103
	661
	9
	7
	11
	6
	10
	13
	13
	15
	15
	4

	14
	KREA 14
	6
	390
	67
	713
	6
	9
	4
	5
	8
	17
	16
	23
	15
	-

	15
	KREA 17A
	9
	405
	141
	762
	8
	14
	15
	12
	11
	14
	18
	19
	17
	7

	16
	KREA 22
	9
	125
	52
	350
	10
	8
	17
	22
	17
	14
	17
	22
	17
	5

	17
	KREA 23
	6
	65
	46
	83
	13
	9
	13
	11
	9
	17
	20
	23
	19
	6

	18
	KREA 41A
	2
	1822
	1703
	1942
	3
	5
	9
	9
	2
	10
	12
	13
	6
	2

	19
	OK09353212
	9
	211
	89
	361
	9
	19
	14
	10
	8
	8
	15
	22
	14
	7

	20
	S65A
	26
	79
	41
	176
	17
	23
	26
	23
	23
	26
	25
	27
	20
	13

	21
	S65D
	17
	192
	65
	541
	15
	31
	24
	22
	26
	24
	25
	26
	19
	6


a. During WY2016, the sampling frequency of the majority of the upstream ambient/tributary sites was reduced from biweekly to monthly because of SFWMD resource constraints.
b. This site is visited biweekly, which may have resulted in a higher number of samples at the site.
Figure 2b. Lower Kissimmee Subwatershed upstream tributary average TP concentrations for WY2018 and sample count for the previous 10-year period. 
(Note: Alias name of site is in parenthesis.)
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Figure 2c. Box-and-whisker plot of WY2018 average TP concentration compared to the TP concentration distribution for the previous 10-year period for the upstream monitoring sites in the Lower Kissimmee Subwatershed.
[image: \\ad.sfwmd.gov\dfsroot\data\err_gis\projects\EVG\sfer\2019\png\Vol1_Appx8B-1\TCNS_S154_S154C_TPAvg_WY2018_cm1.png]
Figure 3a. Taylor Creek/Nubbin Slough Subwatershed, S-154 and S‑154C Basins upstream tributary average TP concentrations for WY2018.
	S154 & S154C
	WY2018
	Number of Samples per Water Yeara

	
	Number of Samples
	TP Concentration (µg/L)
	

	Map ID
	Site
	
	Avg
	Min
	Max
	2008
	2009
	2010
	2011
	2012
	2013
	2014
	2015
	2016
	2017

	1
	KR16373414
	7
	686
	107
	1700
	24
	23
	23
	21
	12
	16
	12
	10
	10
	4

	2
	KR17373513 (KREA 29)
	7
	437
	115
	1147
	24
	25
	24
	22
	18
	16
	14
	13
	8
	2

	3
	KREA 20
	6
	832
	450
	1272
	2
	5
	1
	5
	4
	8
	8
	13
	7
	2

	4
	KREA 25
	5
	971
	671
	1299
	-
	5
	1
	7
	2
	4
	7
	-
	-
	1

	5
	KREA 28
	5
	854
	406
	1197
	-
	11
	7
	5
	4
	9
	9
	7
	12
	5

	6
	KREA 30A
	3
	628
	334
	806
	2
	4
	2
	2
	1
	4
	5
	2
	1
	1

	7
	TS26363411 (KREA 32)
	1
	710
	710
	710
	17
	20
	18
	19
	3
	5
	5
	4
	2
	1

	8
	TS36363411 (KREA 49)
	1
	3577
	3577
	3577
	16
	10
	9
	17
	5
	4
	5
	6
	3
	1

	9
	KR20373413
	3
	347
	239
	555
	8
	10
	10
	7
	4
	2
	4
	9
	4
	2


a. During WY2016, the sampling frequency of the majority of the upstream ambient/tributary sites was reduced from biweekly to monthly because of SFWMD resource constraints. 
Figure 3b. Taylor Creek/Nubbin Slough Subwatershed, S-154 and S‑154C Basins upstream tributary average TP concentrations for WY2018 and sample count for the previous 10-year period. (Note: Alias name of site is in parenthesis.)
[image: ]
Figure 3c. Box-and-whisker plot of WY2018 average TP concentration compared to the TP concentration distribution for the previous 10-year period for the upstream monitoring sites in the Taylor Creek/Nubbin Slough Subwatershed, S-154 and S‑154C Basins.

 [image: \\ad.sfwmd.gov\dfsroot\data\err_gis\projects\EVG\sfer\2019\png\Vol1_Appx8B-1\TCNS_S191_TPAvg_WY2018_cm1.png]
Figure 4a. Taylor Creek/Nubbin Slough Subwatershed, S-191 Basin upstream tributary average TP concentrations for WY2018. 
(Note: STA – Stormwater Treatment Area.)

	S191
	WY2018
	Number of Samples per Water Yeara 

	
	Number of Samples
	TP Concentration (µg/L)
	

	Map ID
	Site
	
	Avg
	Min
	Max
	2008
	2009
	2010
	2011
	2012
	2013
	2014
	2015
	2016
	2017

	1
	02275197
	7b
	523
	190
	1341
	-
	13
	28
	5
	8
	15
	18
	17
	16
	5

	2
	LB29353513 (TCNS 265)
	9
	783
	230
	3198
	13
	15
	18
	17
	16
	20
	12
	10
	11
	6

	3
	MS05373613 (TCNS 263)
	5
	1882
	856
	3120
	5
	15
	10
	21
	8
	5
	2
	1
	2
	1

	4
	MS08373611 (TCNS 262)
	9
	890
	111
	3005
	16
	18
	19
	16
	2
	13
	8
	11
	3
	5

	5
	MS08373614 (TCNS 277)
	3
	1839
	1174
	2579
	13
	11
	12
	6
	3
	5
	2
	2
	2
	1

	6
	OT29353514 (TCNS 243)
	4
	288
	143
	403
	7
	8
	14
	5
	2
	2
	14
	21
	9
	3

	7
	OT32353511 (TCNS 210)
	7
	716
	245
	1320
	6
	11
	14
	9
	5
	8
	8
	9
	10
	3

	8
	OT34353513 (TCNS 211)
	4
	725
	147
	2207
	19
	18
	19
	17
	6
	7
	8
	10
	8
	4

	9
	TC03373511
	5
	571
	200
	1102
	4
	3
	4
	3
	4
	7
	6
	10
	9
	4

	10
	TC27353413
	6
	356
	256
	444
	1
	2
	2
	1
	7
	7
	6
	10
	7
	1

	11
	TCNS 201
	8
	293
	123
	608
	7
	5
	9
	3
	6
	3
	6
	8
	7
	2

	12
	TCNS 204
	7
	788
	303
	1277
	8
	9
	11
	9
	13
	13
	13
	12
	11
	6

	13
	TCNS 207
	6
	381
	164
	646
	15
	9
	12
	4
	7
	16
	13
	7
	11
	6

	14
	TCNS 209
	7
	459
	131
	1108
	4
	14
	8
	5
	13
	13
	8
	7
	5
	3

	15
	TCNS 213
	6
	434
	211
	639
	20
	16
	16
	18
	21
	23
	10
	16
	15
	6

	16
	TCNS 214
	4
	856
	600
	1018
	22
	16
	10
	11
	3
	12
	13
	16
	14
	8

	17
	TCNS 217
	10
	262
	114
	541
	21
	15
	18
	23
	20
	22
	23
	25
	19
	8

	18
	TCNS 220
	7
	582
	215
	1249
	4
	9
	12
	8
	12
	11
	12
	18
	8
	5

	19
	TCNS 222
	5
	617
	189
	1085
	9
	12
	18
	14
	18
	18
	16
	23
	17
	9

	20
	TCNS 228
	3
	1063
	894
	1239
	7
	4
	6
	1
	3
	7
	4
	6
	4
	1

	21
	TCNS 230
	3
	821
	537
	995
	2
	3
	2
	-
	3
	4
	5
	3
	2
	3

	22
	TCNS 233
	3
	975
	651
	1158
	12
	6
	7
	1
	6
	8
	11
	8
	5
	4

	23
	TCNS 249
	3
	442
	91
	640
	5
	5
	10
	4
	1
	6
	4
	18
	9
	3


a. During WY2016, the sampling frequency of the majority of the upstream ambient/tributary sites was reduced from biweekly to monthly because of SFWMD resource constraints.
b. This site is visited biweekly, which may have resulted in a higher number of samples at the site.
Figure 4b. Taylor Creek/Nubbin Slough Subwatershed, S-191 Basin upstream tributary average TP concentrations for WY2018 and sample count for the previous 10-year period. (Note: Alias name of site is in parenthesis.)
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Figure 4c. Box-and-whisker plot of WY2018 average TP concentration compared to the TP concentration distribution for the previous 10-year period for the upstream monitoring sites in the Taylor Creek/Nubbin Slough Subwatershed, S-191 Basin.
[image: \\ad.sfwmd.gov\dfsroot\data\err_gis\projects\EVG\sfer\2019\png\Vol1_Appx8B-1\LkIstokpoga_TPAvg_WY2018_cm1.png]
Figure 5a. Lake Istokpoga Subwatershed upstream tributary average TP concentrations for WY2018.
	Lake Istokpoga
	WY2018
	Number of Samples by Water Yeara

	
	Number of Samples
	TP Concentration (µg/L)
	

	Map ID
	Site
	
	Avg
	Min
	Max
	2008
	2009
	2010
	2011
	2012
	2013
	2014
	2015
	2016
	2017

	1
	02270500
	47b
	153
	70
	559
	-
	17
	33
	12
	25
	45
	47
	52
	51
	44

	2
	AB27343014
	10
	170
	48
	343
	23
	25
	21
	24
	19
	20
	19
	21
	17
	8

	3
	AR06333013
	11
	99
	54
	146
	22
	23
	21
	24
	23
	26
	26
	25
	19
	12

	4
	AR18343012
	11
	142
	56
	384
	23
	25
	21
	21
	18
	14
	15
	20
	16
	9

	5
	BN03332911
	12
	577
	130
	886
	25
	26
	25
	25
	23
	25
	26
	26
	19
	12

	6
	BN08332912
	12
	1276
	131
	3774
	18
	20
	22
	24
	19
	16
	23
	19
	14
	11

	7
	LI02362923
	12
	67
	49
	117
	-
	-
	-
	-
	22
	26
	26
	27
	20
	10

	8
	LV14322813
	7
	255
	144
	306
	1
	4
	12
	21
	8
	11
	12
	21
	10
	4

	9
	PL01382911
	8
	1207
	945
	1707
	13
	20
	23
	24
	24
	19
	21
	22
	18
	7

	10
	RD08322913
	13
	119
	49
	194
	26
	26
	26
	25
	26
	25
	26
	26
	19
	12


a. During WY2016, the sampling frequency of the majority of the upstream ambient/tributary sites was reduced from biweekly to monthly because of SFWMD resource constraints.
b. This site has an autosampler and is visited weekly for servicing, which resulted in the higher number of samples at the site. However, data in this table only represent grab samples.
Figure 5b. Lake Istokpoga Subwatershed upstream tributary average TP concentrations for WY2018 and sample count for the previous 10-year period.
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Figure 5c. Box-and-whisker plot of WY2018 average TP concentration compared to the TP concentration distribution for the previous 10-year period for the upstream monitoring sites in the Lake Istokpoga Subwatershed. 

[image: \\ad.sfwmd.gov\dfsroot\data\err_gis\projects\EVG\sfer\2019\png\Vol1_Appx8B-1\IndianPrairie_TPAvg_WY2018_cm1.png]
Figure 6a. Indian Prairie Subwatershed upstream tributary average TP concentrations for WY2018.

	Indian Prairie
	WY2018
	Number of Samples per Water Yeara

	
	Number of Samples
	TP Concentration (µg/L)
	

	Map ID
	Site
	
	Avg
	Min
	Max
	2008
	2009
	2010
	2011
	2012
	2013
	2014
	2015
	2016
	2017

	1
	02273230
	4b
	372
	215
	604
	-
	3
	8
	2
	6
	14
	12
	15
	14
	7

	2
	HP06393242 (S70)
	7
	254
	75
	588
	11
	-
	-
	-
	12
	20
	16
	14
	14
	9

	3
	HP11373132 (S82)
	2
	88
	60
	116
	12
	4
	4
	7
	17
	16
	12
	10
	8
	2

	4
	HP15373112
	4
	731
	505
	975
	5
	20
	16
	21
	9
	12
	8
	5
	9
	3

	5
	HP22373112
	5
	399
	329
	465
	13
	18
	21
	13
	10
	14
	11
	9
	9
	3

	6
	HP23373111
	-
	-
	-
	-
	8
	4
	4
	3
	2
	4
	4
	10
	4
	2

	7
	HP24373013
	3
	1426
	1071
	1945
	17
	19
	14
	4
	5
	10
	14
	10
	4
	1

	8
	HP25373013
	10
	221
	118
	554
	26
	26
	26
	25
	25
	26
	24
	24
	20
	8

	9
	HP34373124
	1
	2204
	2204
	2204
	4
	12
	7
	7
	4
	8
	7
	2
	1
	-

	10
	HP35373113
	-
	-
	-
	-
	3
	4
	5
	3
	3
	6
	1
	3
	1
	-

	11
	HP36373013
	-
	-
	-
	-
	15
	24
	25
	16
	1
	6
	9
	4
	4
	-

	12
	IP09383232 (S75)
	6
	375
	111
	1114
	4
	-
	-
	-
	17
	18
	16
	12
	13
	7

	13
	IP24383214
	1
	470
	470
	470
	13
	5
	9
	2
	5
	2
	5
	6
	-
	-

	14
	SD28373312
	3
	418
	334
	492
	13
	13
	16
	18
	7
	2
	7
	5
	3
	1

	15
	SD33373314
	2
	519
	472
	566
	25
	23
	16
	13
	10
	6
	8
	6
	1
	1

	16
	SD34373313
	2
	1065
	72
	2058
	7
	2
	6
	2
	2
	1
	4
	7
	2
	-


a. During WY2016, the sampling frequency of the majority of the upstream ambient/tributary sites was reduced from biweekly to monthly because of SFWMD resource constraints.
b. This site is visited biweekly, which may have resulted in a higher number of samples at the site.
Figure 6b. Indian Prairie Subwatershed upstream tributary average TP concentrations for WY2018 and sample count for the previous 10-year period.
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Figure 6c. Box-and-whisker plot of WY2018 average TP concentration compared to the TP concentration distribution for the previous 10-year period for the upstream monitoring sites in the Indian Prairie Subwatershed.
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Figure 7a. Fisheating Creek Subwatershed upstream tributary average TP concentrations for WY2018.

	Fisheating Creek
	WY2018
	Number of Samples per Water Yeara

	
	Number of Samples
	TP Concentration (µg/L)
	

	Map ID
	Site
	
	Avg
	Min
	Max
	2008
	2009
	2010
	2011
	2012
	2013
	2014
	2015
	2016
	2017

	1
	02255600
	6b
	223
	158
	325
	-
	11
	24
	5
	4
	13
	11
	12
	14
	3

	2
	02256500
	5b
	288
	224
	353
	-
	13
	30
	9
	5
	3
	9
	8
	10
	5

	3
	BH04392912
	4
	393
	238
	664
	22
	18
	19
	20
	12
	10
	11
	17
	17
	5

	4
	BH32382914
	-
	-
	-
	-
	11
	9
	12
	12
	4
	3
	7
	3
	8
	-

	5
	FE03382911
	7
	1090
	913
	1440
	2
	2
	2
	2
	1
	4
	2
	8
	9
	1

	6
	FE20393013
	2
	489
	427
	550
	22
	18
	18
	20
	24
	7
	10
	4
	6
	1

	7
	FE21392913
	3
	328
	264
	431
	26
	26
	26
	17
	8
	10
	10
	8
	9
	3

	8
	FE21392914
	-
	-
	-
	-
	10
	10
	21
	12
	7
	4
	8
	4
	11
	1

	9
	FE26362812
	9
	245
	173
	319
	20
	22
	23
	14
	6
	11
	17
	21
	18
	5

	10
	FE32372814
	4
	163
	84
	349
	23
	16
	22
	16
	8
	5
	11
	4
	7
	2

	11
	GA09393011
	9
	325
	207
	452
	27
	26
	25
	21
	23
	20
	21
	15
	11
	9

	12
	GG05403011
	2
	859
	723
	995
	10
	11
	18
	10
	4
	3
	8
	5
	7
	2

	13
	PB24392912
	7
	577
	330
	1220
	21
	19
	18
	21
	23
	23
	24
	24
	18
	9


a. During WY2016, the sampling frequency of the majority of the upstream ambient/tributary sites was reduced from biweekly to monthly because of SFWMD resource constraints.
b. These sites are visited biweekly, which may have resulted in a higher number of samples at the site.
Figure 7b. Fisheating Creek Subwatershed upstream tributary average TP concentrations for WY2018 and sample count for the previous 10-year period.
[image: ]
Figure 7c. Box-and-whisker plot of WY2018 average TP concentration compared to the TP concentration distribution for the previous 10-year period for the upstream monitoring sites in the Fisheating Creek Subwatershed.
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