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Introduction
According to our study plan under the Memorandum of Understanding between the Department of Environmental Protection (DEP) and the Department of Health (DOH), DEP would provide quarterly reports on the monitoring activities and results for the experimental lined drainfield at 1914 Orchard Drive in Apopka, Florida.  This reports serves as the first quarterly report of those events and findings, which is a compilation from the first 5 months of the system’s operation.
This project began with the construction of a new lined drainfield underlain by reactive media layer composed of hardwood mulch.  A monitoring well was installed on July 6, 2016 to a depth of 39 feet.  Construction of the new lined drainfield occurred the week of July 18, 2016, and it began receiving septic tank effluent from the private citizen’s residence July 29, 2016.  Two diversion valves were installed in-line between the septic tank and the drainfield distribution header to divert flow from the old drainfield, and allow the experimental drainfield to begin receiving effluent.  At the time of construction, 6 horizontal monitoring wellpoints were installed on top of the liner and below the four rows of infiltrators, and 3 piezometers were installed with their screen intervals resting on top of the liner.  On July 27-28, 2016, 6 deep suction lysimeters, 7 shallow lysimeters, and a flow meter were installed.  Figures 1 and 2 show the layout of the drainfield and locations of the lysimeters, monitoring wells and piezometers.  The monitoring stations are described in Table 1.  
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Table 1.  Summary of information on monitoring stations included in study.
	Station Identifier
	Description
	Monitoring Objective

	STE-1
	Septic tank effluent from riser installed over septic tank inspection port
	Measure “input” constituent concentrations before effluent goes to the drainfield

	L1S through L6S
	Shallow lysimeters installed at 6 locations adjacent to the infiltrator rows; bottom of lysimeters 0.5 ft above mulch layer 
	Monitor pore water quality between the drainfield and the reactive media layer (intermediate level of treatment) to evaluate nitrogen concentration and nitrification  

	L7S
	Shallow lysimeter installed below the distribution header
	Monitor for leakage of effluent from header

	M1 through M6
	Horizontal well points on top of liner at 6 locations 
	Monitor water quality within saturated portion of mulch layer

	L1D through L6D
	Deep lysimeters installed along outside edge of liner; bottom of lysimeters 1 foot below edge of liner
	Monitor pore water quality in soil at edges of liner where water collected on liner discharges

	MW1
	Monitoring well near edge of the drainfield
	Measure ground water quality and ground water levels near edge of the drainfield

	P1 through P3
	Piezometers installed inside lined area, below the drainfield and above the reactive media layer 
	Measure presence of and depth to water to assess mounding above the saturated zone on liner and evaluate gradient toward liner edges 

	Flow
	Flow meter installed at supply well
	Measure flow to the septic system from the household


[image: Apopka_ImageryMap]Figure 1.  Aerial photograph with monitoring station sampling points
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Figure 2. Plan view of monitoring device locations at experimental drainfield.
Monitoring Results
Water quality samples have been collected from the effluent, lysimeters, and monitoring wells on 5 occasions.  These samples were analyzed by the DEP central laboratory.  Table 2 presents the laboratory results to date for the major parameters of interest.  The parameters include chloride (Cl), ammonium (NH4), total Kjeldahl nitrogen (TKN), nitrate+nitrite-nitrogen (NO3+NO2), and total phosphorous (TP).  
Table 2.  Monitoring results for key parameters, Wekiva experimental lined drainfield study
	Station
	Sample Date
	Cl (mg/L)
	NH4 (mg/L)
	TKN (mg/L)
	Org N (mg/L)
	NO3+NO2 (mg/L)
	TN (mg/L)
	TP (mg/L)

	STE1 
	09/14/16
	99
	64
	80
	16.00
	BDL
	80
	8.4

	 
	10/12/16
	70
	42
	45
	3.00
	BDL
	45
	5.2

	 
	11/09/16
	83
	53
	60
	7.00
	BDL
	60
	7.5

	 
	12/08/16
	75
	57
	65
	8.00
	BDL
	65
	7.3

	
	01/18/17
	79
	53
	61
	8.00
	BDL
	61
	6.9

	MW1
	09/14/16
	31
	0.008
	2.60
	2.59
	3.6
	6
	92

	 
	10/12/16
	39
	0.16
	120
	119.84
	11.0
	131
	490

	 
	11/09/16
	29
	0.80
	64
	63.20
	3.5
	68
	200

	 
	12/08/16
	26
	0.28
	63
	62.72
	2.9
	66
	200

	
	01/18/17
	27
	0.049
	27
	26.95
	3.1
	30
	200

	L1S
	09/14/16
	 
	 
	 
	 
	 
	 
	 

	 
	10/12/16
	 
	 
	 
	 
	 
	 
	 

	 
	11/09/16
	77
	34
	33
	BDL
	6.1
	39
	4.7

	 
	12/08/16
	 
	 
	 
	 
	 
	 
	 

	
	01/18/17
	82
	18
	18
	0
	11
	29
	3.2

	L1D
	09/14/16
	 
	 
	 
	 
	 
	 
	 

	 
	10/12/16
	29
	12
	14.0
	2.0
	BDL
	14
	29

	 
	11/09/16
	73
	0.46
	4.7
	4.24
	41
	46
	0.1

	 
	12/08/16
	 
	 
	 
	 
	 
	 
	 

	
	01/18/16
	71
	0.36
	1.7
	1.34
	11
	13
	0.04

	M1
	09/14/16
	100
	51
	57
	6.0
	BDL
	57
	2.8

	 
	10/12/16
	67
	43
	47
	4.0
	0.078
	47
	3.6

	 
	11/09/16
	77
	42
	46
	4.0
	BDL
	46
	6.7

	 
	12/08/16
	73
	19
	22
	3.0
	0.014
	22
	3.1

	
	01/18/17
	86
	4.9
	8
	3.0
	BDL
	8
	2.8

	L2S
	09/14/16
	 
	 
	 
	 
	 
	 
	 

	 
	10/12/16
	16
	0.12
	1.9
	1.78
	2.0
	4
	0.14

	
	11/09/16
	 
	0.036
	2.6
	2.56
	29
	32
	0.11

	 L2S
	12/08/16
	 
	 
	 
	 
	 
	 
	 

	
	01/18/17
	
	0.035
	2.5
	2.47
	23
	26
	0.13

	L2D
	09/14/16
	 
	 
	 
	 
	 
	 
	 

	 
	10/12/16
	38
	4.30
	6.9
	2.60
	4.2
	11
	0.19

	 
	11/09/16
	69
	0.55
	2.3
	1.75
	22
	24
	0.13

	 
	12/08/16
	 
	 
	 
	 
	 
	 
	 

	
	01/18/17
	62
	0.14
	1.6
	1.46
	19
	21
	0.06

	M2
	09/14/16
	100
	51
	61
	10.0
	BDL
	61
	2.5

	 
	10/12/16
	62
	38
	43
	5.0
	BDL
	43
	2.5

	 
	11/09/16
	75
	43
	45
	2.0
	0.066
	45
	4.5

	 
	12/08/16
	72
	31
	34
	3.0
	0.011
	34
	2.6

	
	01/18/17
	87
	26
	27
	1.0
	BDL
	27
	3.3

	L3S
	09/14/16
	 
	 
	 
	 
	 
	 
	 

	 
	10/12/16
	54
	0.067
	1.6
	1.53
	1.3
	3
	0.10

	 
	11/09/16
	27
	0.10
	2.4
	2.30
	11.0
	13
	0.10

	 
	12/08/16
	 
	 
	 
	 
	 
	 
	 

	
	01/18/17
	46
	0.11
	2.1
	1.99
	7.7
	10
	0.12

	L3D
	09/14/16
	110
	0.012
	3.9
	3.89
	4.20
	8
	0.43

	 
	10/12/16
	28
	0.076
	2.4
	2.32
	0.89
	3
	0.86

	 
	11/09/16
	30
	0.044
	2.7
	2.66
	7.70
	10
	0.26

	 
	12/08/16
	 
	 
	 
	 
	 
	 
	 

	
	01/18/17
	59
	0.053
	2.0
	1.95
	7.6
	10
	0.16

	M3
	09/14/16
	91
	18
	50
	32.0
	0.015
	50
	34

	 
	10/12/16
	58
	19
	31
	12.0
	BDL
	31
	8.4

	 
	11/09/16
	71
	16
	23
	7.0
	BDL
	23
	2.0

	 
	12/08/16
	69
	9
	16
	7.0
	BDL
	16
	1.6

	
	01/18/17
	74
	3
	9
	5.7
	BDL
	9
	2.1

	L4S
	09/14/16
	79
	0.022
	3.2
	3.18
	8.50
	12
	0.14

	 
	10/12/16
	85
	0.078
	2.5
	2.42
	0.73
	3
	0.10

	 
	11/09/16
	24
	0.023
	3.0
	2.98
	5.40
	8
	0.10

	 
	12/08/16
	 
	 
	 
	 
	 
	 
	 

	
	01/18/17
	73
	1.1
	2.7
	1.60
	9.90
	13
	0.13

	L4D
	09/14/16
	 
	 
	 
	 
	 
	 
	 

	 
	10/12/16
	54
	8.5
	13
	4.50
	BDL
	13
	0.27

	 
	110/9/16
	53
	6.3
	11
	4.70
	0.017
	11
	0.06

	 
	12/08/16
	 
	 
	 
	 
	 
	 
	 

	
	01/18/17
	61
	0.76
	2.3
	1.54
	2.60
	5
	0.02

	M4
	09/14/16
	96
	19
	64
	45.0
	0.047
	64
	54

	 
	10/12/16
	62
	13
	28
	15.0
	BDL
	28
	9.1

	 
	11/09/16
	73
	15
	21
	6.0
	BDL
	21
	2.2

	M4
	12/08/16
	72
	9.6
	17
	7.40
	BDL
	17
	0.8

	
	01/18/17
	72
	1.5
	9
	7.10
	BDL
	9
	1.7

	L5S
	09/14/16
	25
	0.062
	2.9
	2.84
	0.31
	3
	0.23

	 
	10/12/16
	6
	0.061
	1.8
	1.74
	0.60
	2
	0.12

	 
	11/09/16
	9
	0.063
	2.1
	2.04
	5.50
	8
	0.06

	 
	12/08/16
	 
	 
	 
	 
	 
	 
	 

	
	01/18/17
	48
	0.12
	1.0
	0.88
	0.40
	1
	0.03

	L5D
	09/14/16
	43
	0.16
	3.0
	2.84
	1.10
	4
	0.13

	 
	10/12/16
	14
	0.65
	2.9
	2.25
	BDL
	3
	0.17

	
	11/09/16
	30
	2.20
	4.5
	2.30
	0.56
	5
	0.04

	 
	12/08/16
	 
	 
	 
	 
	 
	 
	 

	
	01/18/17
	45
	0.2
	1.4
	1.23
	0.79
	2
	0.03

	M5
	09/14/16
	89
	7.5
	40
	32.50
	0.018
	40
	60

	 
	10/12/16
	52
	1.4
	24
	22.60
	BDL
	24
	10

	 
	11/09/16
	43
	0.6
	16
	15.39
	BDL
	16
	8.3

	
	12/08/16
	64
	2.2
	11
	8.80
	BDL
	11
	6.9

	
	01/18/17
	63
	0.3
	8
	7.45
	BDL
	8
	2.7

	L6S
	09/14/16
	16
	0.21
	2.50
	2.29
	0.022
	3
	0.31

	 
	10/12/16
	9
	0.18
	2.00
	1.82
	BDL
	2
	0.12

	 
	11/09/16
	13
	0.610
	2.80
	2.19
	BDL
	3
	0.06

	 
	12/08/16
	 
	 
	 
	 
	 
	 
	 

	
	01/18/17
	44
	0.33
	1.50
	1.17
	BDL
	1.5
	0.03

	L6D
	09/14/16
	 
	 
	 
	 
	 
	 
	 

	 
	10/12/16
	86
	16
	31
	15.00
	BDL
	31
	31

	 
	11/09/16
	62
	22
	27
	5.0
	BDL
	27
	20

	 
	12/08/16
	 
	 
	 
	 
	 
	 
	 

	
	01/18/17
	66
	17
	20
	3.00
	BDL
	20
	6.7

	M6
	09/14/16
	98
	6.9
	38
	31.10
	0.018
	38
	49

	 
	10/12/16
	54
	4.4
	28
	23.60
	BDL
	28
	14

	 
	11/09/16
	52
	2.8
	21
	18.20
	BDL
	21
	12

	 
	12/08/16
	68
	2.0
	11
	9.0
	BDL
	11
	8.6

	
	01/18/17
	68
	0.3
	10
	9.2
	BDL
	10
	2.9

	L7S
	09/14/16
	 
	 
	 
	 
	 
	 
	 

	 
	10/12/16
	43
	22
	18
	BDL
	0.510
	19
	0.51

	 
	11/09/16
	68
	10
	13
	3.0
	0.036
	13
	0.83

	
	12/08/16
	
	
	
	
	
	
	

	 
	01/18/17
	81 
	2.4
	3.2
	0.80
	34
	37
	1.5


Notes:  STE=septic tank effluent sample; L= lysimeter sample; MW=monitoring well sample; M=horizontal well sample
BDL=below detection limit, reported concentrations are in milligrams per liter, empty field indicates insufficient sample volume available for analysis

Water level and flow measurements were also taken.  Depths to water were measured in the 3 piezometers and the monitoring well, and flow was recorded from the flow meter during each site visit. These results are provided in Tables 3 and 4.  

Table 3.  Water levels, Wekiva experimental lined drainfield study
	Station
	Date
	Depth to Water (ft.)
	Height of Water Above Bottom of Liner (ft.)

	MW1
	09/13/16
	29.05
	N/A

	P1
	09/13/16
	5.47
	0.48

	P2
	09/13/16
	5.27
	0.48

	P3
	09/13/16
	5.22
	0.47

	
	
	
	

	MW1
	10/12/16
	27.90
	N/A

	P1
	10/12/16
	5.40
	0.55

	P2
	10/12/16
	5.30
	0.45

	P3
	10/12/16
	5.35
	0.34

	MW1
	11/09/16
	26.75
	N/A

	P1
	11/09/16
	5.55
	0.40

	P2
	11/09/16
	5.40
	0.35

	P3
	11/09/16
	5.35
	0.34

	MW1
	12/08/16
	27.90
	N/A

	P1
	12/08/16
	5.55
	0.40

	P2
	12/08/16
	5.45
	0.30

	[bookmark: _GoBack]P3
	12/08/16
	5.45
	0.24


Notes:  Elevations are relative to septic tank outlet bottom, assigned Elevation
of 100.0 feet. MW1=monitoring well, P=piezometer, N/A=not applicable


Table 4.  Flow measurements, Wekiva experimental lined drainfield study
	Date
	Meter Reading (gal.)
	Daily Average (gal.)
	Comments

	7/28/2016
	300
	~
	Commence flow measurements to drainfield

	9/13/2016
	1700
	30
	Homeowner on vacation

	10/12/2016
	2400
	23
	Homeowner on vacation

	11/9/2016
	32700
	1082
	Irrigation of newly installed sod

	12/8/2016
	42500
	327
	Normal irrigation use

	1/17/2017
	54100
	290
	Normal irrigation use


Note: Average daily flow includes irrigation and is based on flow since date of previous measurement

Results to Date
Operation of the experimental drainfield has proceeded since July 29, 2016.  The data collected during this period allow us to make the following observations:  
· Effluent concentrations have been variable, possibly due to intermittent use while the residents took vacations.  Except for one occasion, TN values were within a typical range for septic tank effluent.
· Recovery of water from suction lysimeters was poor, due in part to the dry season and in part to the uneven distribution of infiltrating water within the drainfield.
· Shallow lysimeter (L1S) data indicate that there is very uneven distribution of infiltrating effluent and incomplete nitrification is occurring.  The results from L1S may indicate that infiltrating effluent pools near the distribution header.  However, at other shallow lysimeter locations, high nitrate data indicate that nitrification appears to be occurring and nitrogen is being reduced in the upper layer.
· The chloride and nitrogen data from the horizontal wellpoints below the mulch layer seem to indicate that effluent is infiltrating into the mulch layer.  Ammonia detections, particularly at two locations closest to the header (M1 and M2), could be consistent with the results at shallow lysimeter L1S.  It is also possible that ammonia is being generated from conversion of organic nitrogen leached from the wood mulch.  High organic nitrogen concentrations that were detected in the horizontal well points could only be from the mulch.  Phosphorus appears to also be coming from the mulch based on a comparison of the effluent and horizontal wellpoint data.
· The data from deep lysimeters installed along the edge of the liner appear to reflect water quality influence by residence within the liner.  TN concentrations in all but one instance have been significantly lower than the effluent concentration.  Nitrogen in some samples is a mixture of organic and ammonia nitrogen forms and in some samples, it is in the form of nitrate.  It appears that these represent water quality influence by the effluent as well as the mulch material.
· The monitor well adjacent to the drainfield is a small-diameter (3/4-inch diameter) micro-well that was installed by the DEP-owned direct push rig.  Depth to groundwater at this site is almost 30 feet, so purging and sampling with a suction lift pump is not possible, and this well must be purged and sampled using a method that results in a turbid sample.  Sample turbidity is biasing the quality results for phosphorus and possibly TKN/organic nitrogen results.  In subsequent sampling trips, samples from the well will be filtered and a new monitoring well may be installed at a later date.
· Water levels in the piezometers indicate that water is pooling within the lined area and some of the wood mulch layer is saturated.  
· When the flow meter was installed, it was understood that it was being installed at a point where flow to the irrigation system would not be included.  However, it was determined later that irrigation flow is also being measured.  High water use measured during some months reflects irrigation of new sod during the dry season (Table 4).  DEP is currently working with the homeowner on a way to estimate irrigation use each month so that irrigation can then be subtracted from total flow. 

Next Steps
DEP staff will continue monthly sample collection and measurements of flow and water levels in the piezometers and monitoring well.  After three additional months of monitoring data are collected and analyzed, the second quarterly report will be submitted.  DEP believes that more time is needed to achieve stabilization of the mulch layer and equalization of flow within the drainfield.  Any decisions on modifications to the monitoring or treatment systems must be based on a more consistent data set.
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