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Introduction
According to our study plan under the Memorandum of Understanding between the Department of Environmental Protection (DEP) and the Department of Health (DOH), DEP would provide quarterly reports on the monitoring activities and results for the experimental lined drainfield at 1914 Orchard Drive in Apopka, Florida.  This report serves as the second quarterly report of those events and findings, which is a compilation from the first 8 months of the system’s operation.
This project began with the construction of a new lined drainfield underlain by reactive media layer composed of hardwood mulch.  A monitoring well was installed on July 6, 2016 to a depth of 39 feet.  Construction of the new lined drainfield occurred the week of July 18, 2016, and it began receiving septic tank effluent from the private citizen’s residence July 29, 2016.  Two diversion valves were installed in-line between the septic tank and the drainfield distribution header to divert flow from the old drainfield, and allow the experimental drainfield to begin receiving effluent.  At the time of construction, 6 horizontal monitoring well points were installed on top of the liner and below the four rows of infiltrators, and 3 piezometers were installed with their screen intervals resting on top of the liner.  On July 27-28, 2016, 6 deep suction lysimeters, 7 shallow lysimeters, and a flow meter were installed.  Figures 1 and 2 show the layout of the drainfield and locations of the lysimeters, monitoring wells, and piezometers.  The monitoring stations are described in Table 1.  
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Table 1.  Summary of information on monitoring stations included in study.
	Station Identifier
	Description
	Monitoring Objective

	STE-1
	Septic tank effluent from riser installed over septic tank inspection port
	Measure “input” constituent concentrations before effluent goes to the drainfield

	L1S through L6S
	Shallow lysimeters installed at 6 locations adjacent to the infiltrator rows; bottom of lysimeters 0.5 ft. above mulch layer 
	Monitor pore water quality between the drainfield and the reactive media layer (intermediate level of treatment) to evaluate nitrogen concentration and nitrification  

	L7S
	Shallow lysimeter installed below the distribution header
	Monitor for leakage of effluent from header

	M1 through M6
	Horizontal well points on top of liner at 6 locations 
	Monitor water quality within saturated portion of mulch layer

	L1D through L6D
	Deep lysimeters installed along outside edge of liner; bottom of lysimeters 1 foot below edge of liner
	Monitor pore water quality in soil at edges of liner where water collected on liner discharges

	MW1
	Monitoring well near edge of the drainfield
	Measure ground water quality and ground water levels near edge of the drainfield

	P1 through P3
	Piezometers installed inside lined area, below the drainfield and above the reactive media layer 
	Measure presence of and depth to water to assess mounding above the saturated zone on liner and evaluate gradient toward liner edges 

	Flow
	Flow meter installed at supply well
	Measure flow to the septic system from the household


[image: Apopka_ImageryMap]Figure 1.  Aerial photograph with monitoring station sampling points
[image: ]
Figure 2. Plan view of monitoring device locations at experimental drainfield.
Monitoring Results
Water quality samples have been collected from the effluent, lysimeters, and monitoring wells on 8 occasions.  These samples were analyzed by the DEP central laboratory.  Table 2 presents the laboratory results to date for the major parameters of interest.  The parameters include chloride (Cl), ammonium (NH4), total Kjeldahl nitrogen (TKN), nitrate+nitrite-nitrogen (NO3+NO2), and total phosphorous (TP).  Trend plots for chloride, TN, and TP in water samples from the monitoring devices are provided in Figures 3 through 11.  The findings are discussed in a following section of this report.

Table 2.  Monitoring results for key parameters, Wekiva experimental lined drainfield study
	Station
	Sample Date
	Cl (mg/L)
	NH4 (mg/L)
	TKN (mg/L)
	Org N (mg/L)
	NO3+NO2 (mg/L)
	TN (mg/L)
	TP (mg/L)

	STE1 
	9/14/16
	99
	64
	80
	16
	BDL
	80
	8.4

	
	10/12/16
	70
	42
	45
	3
	BDL
	45
	5.2

	
	11/9/16
	83
	53
	60
	7
	BDL
	60
	7.5

	
	12/8/16
	75
	57
	65
	8
	BDL
	65
	7.3

	
	1/18/17
	79
	53
	61
	8
	BDL
	61
	6.9

	
	2/23/17
	79
	28
	40
	12
	BDL
	40
	4.9

	
	3/23/17
	79
	63
	79
	16
	BDL
	79
	9.6

	
	4/19/17
	59
	45
	53
	8
	BDL
	53
	0.1

	L1S
	9/14/16
	100
	51
	57
	6.00
	BDL
	57
	2.8

	
	10/12/16
	
	
	
	
	
	
	

	
	11/9/16
	77
	34
	33
	BDL
	6.1
	39
	4.7

	
	12/8/16
	
	
	
	
	
	
	

	
	1/18/17
	82
	18
	18
	0
	11
	29
	3.2

	
	2/23/17
	70
	0.79
	2.2
	1
	26
	28
	3.4

	
	3/23/17
	73
	0.25
	1.3
	1
	57
	58
	1.3

	
	4/19/17
	53
	0.94
	1.7
	1
	18
	20
	0.2

	L2S
	9/14/16
	
	
	
	
	
	
	

	
	10/12/16
	16
	0.12
	1.9
	1.78
	2
	4
	0.14

	
	11/9/16
	
	0.036
	2.6
	2.56
	29
	32
	0.11

	
	12/8/16
	
	
	
	
	
	
	

	
	1/18/17
	
	0.035
	2.5
	2.47
	23
	26
	0.13

	
	2/23/17
	48
	0.035
	1.7
	1.67
	42
	44
	0.09
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	3/23/17
	38
	0.066
	2.3
	2.23
	23
	25
	0.07

	
	4/19/17
	44
	BDL
	1.6
	1.60
	34
	36
	0.05

	L3S
	9/14/16
	
	
	
	
	
	
	

	
	10/12/16
	54
	0.067
	1.6
	1.53
	1.3
	3
	0.10

	
	11/9/16
	27
	0.10
	2.4
	2.30
	11
	13
	0.10

	
	12/8/16
	
	
	
	
	
	
	

	
	1/18/17
	46
	0.11
	2.1
	1.99
	7.7
	10
	0.12

	
	2/23/17
	54
	0.073
	2.0
	1.93
	11
	13
	0.13

	
	3/23/17
	68
	0.027
	2.1
	2.07
	21
	23
	0.073

	
	4/19/17
	45
	0.028
	2.1
	2.07
	38
	40
	0.079

	L4S
	9/14/16
	79
	0.022
	3.2
	3.18
	8.50
	12
	0.14

	
	10/12/16
	85
	0.078
	2.5
	2.42
	0.73
	3
	0.10

	
	11/9/16
	24
	0.023
	3.0
	2.98
	5.40
	8
	0.10

	
	12/8/16
	
	
	
	
	
	
	

	
	1/18/17
	73
	1.1
	2.7
	1.60
	9.9
	13
	0.13

	
	2/23/17
	77
	8.7
	11.0
	2.30
	2.7
	14
	0.16

	
	3/23/17
	85
	0.9
	2.7
	1.82
	17
	20
	0.12

	
	4/19/17
	
	0.2
	1.9
	1.74
	9
	11
	0.13

	L5S
	9/14/16
	25
	0.062
	2.9
	2.84
	0.31
	3
	0.23

	
	10/12/16
	6
	0.061
	1.8
	1.74
	0.60
	2
	0.12

	
	11/9/16
	9
	0.063
	2.1
	2.04
	5.50
	8
	0.06

	
	12/8/16
	
	
	
	
	
	
	

	
	1/18/17
	48
	0.12
	1.0
	0.88
	0.40
	1
	0.03

	
	2/23/17
	52
	0.09
	0.8
	0.66
	0.75
	2
	0.02

	
	3/23/17
	88
	0.03
	1.1
	1.07
	8.20
	9
	0.01

	
	4/19/17
	37
	0.07
	1.1
	1.03
	3
	4
	BDL

	L6S
	9/14/16
	16
	0.21
	2.50
	2.29
	0.022
	3
	0.31

	
	10/12/16
	9
	0.18
	2.00
	1.82
	BDL
	2
	0.12

	
	11/9/16
	13
	0.61
	2.80
	2.19
	BDL
	3
	0.06

	
	12/8/16
	
	
	
	
	
	
	

	
	1/18/17
	44
	0.33
	1.50
	1.17
	BDL
	2
	0.03

	
	2/23/17
	45
	0.65
	2.00
	1.35
	0.03
	2
	0.03

	
	3/23/17
	98
	0.98
	2.50
	1.52
	0.13
	3
	0.03

	
	4/19/17
	
	
	
	
	
	
	

	L7S
	9/14/16
	
	
	
	
	
	
	

	
	10/12/16
	43
	22
	18
	BDL
	0.510
	19
	0.51

	
	11/9/16
	68
	10
	13
	3.00
	0.036
	13
	0.83

	
	12/8/16
	
	
	
	
	
	
	

	
	1/18/17
	81
	2.4
	3.2
	0.80
	34
	37
	1.5

	
	2/23/17
	74
	32
	34
	2.00
	33
	67
	4.0

	
	3/23/17
	80
	0.6
	2
	1.30
	40
	42
	1.4

	
	4/19/17
	63
	0.8
	3
	1.92
	22
	25
	3.5

	M1
	9/14/16
	100
	51
	57
	6
	BDL
	57
	2.8

	
	10/12/16
	67
	43
	47
	4
	0.078
	47
	3.6

	
	11/9/16
	77
	42
	46
	4
	BDL
	46
	6.7

	
	12/8/16
	73
	19
	22
	3
	0.014
	22
	3.1

	
	1/18/17
	86
	4.9
	8
	3
	BDL
	8
	2.8

	
	2/23/17
	77
	33
	36
	3
	BDL
	36
	5.6

	
	3/23/17
	83
	26
	28
	2
	0.010
	28
	4.0

	
	4/19/17
	64
	14
	15
	1
	0.013
	15
	4.8

	M2
	9/14/16
	100
	51
	61
	10
	BDL
	61
	2.5

	
	10/12/16
	62
	38
	43
	5
	BDL
	43
	2.5

	
	11/9/16
	75
	43
	45
	2
	0.066
	45
	4.5

	
	12/8/16
	72
	31
	34
	3
	0.011
	34
	2.6

	
	1/18/17
	87
	26
	27
	1
	BDL
	27
	3.3

	
	2/23/17
	74
	29
	32
	3
	BDL
	32
	4.8

	
	3/23/17
	88
	23
	29
	6
	BDL
	29
	4.2

	
	4/19/17
	64
	17
	20
	3
	BDL
	20
	4.7

	M3
	9/14/16
	91
	18
	50
	32.0
	0.015
	50
	34

	
	10/12/16
	58
	19
	31
	12.0
	BDL
	31
	8.4

	
	11/9/16
	71
	16
	23
	7.0
	BDL
	23
	2.0

	
	12/8/16
	69
	9
	16
	7.0
	BDL
	16
	1.6

	
	1/18/17
	74
	3
	9
	5.7
	BDL
	9
	2.1

	
	2/23/17
	73
	20
	26
	6.0
	0.052
	26
	1.4

	
	3/23/17
	80
	21
	26
	5.0
	BDL
	26
	2.5

	
	4/19/17
	61
	22
	26
	4.0
	0.014
	26
	1.9

	M4
	9/14/16
	96
	19
	64
	45.00
	0.047
	64
	54

	
	10/12/16
	62
	13
	28
	15.00
	BDL
	28
	9.1

	
	11/9/16
	73
	15
	21
	6.00
	BDL
	21
	2.2

	
	12/8/16
	72
	9.6
	17
	7.40
	BDL
	17
	0.8

	
	1/18/17
	72
	1.5
	9
	7.10
	BDL
	9
	1.7

	
	2/23/17
	73
	16
	24
	8.00
	BDL
	24
	1.6

	
	3/23/17
	83
	19
	28
	9.00
	BDL
	28
	1.1

	
	4/19/17
	63
	16
	20
	4.00
	BDL
	20
	1.3

	M5
	9/14/16
	89
	7.5
	40
	32.50
	0.018
	40
	60

	
	10/12/16
	52
	1.4
	24
	22.60
	BDL
	24
	10

	
	11/9/16
	43
	0.6
	16
	15.39
	BDL
	16
	8.3

	
	12/8/16
	64
	2.2
	11
	8.80
	BDL
	11
	6.9

	
	1/18/17
	63
	0.3
	8
	7.45
	BDL
	8
	2.7

	
	2/23/17
	65
	1.8
	9
	7.60
	BDL
	9
	1.9

	
	3/23/17
	76
	0.6
	6
	5.34
	0.021
	6
	1.2

	
	4/19/17
	
	
	
	
	
	
	

	M6
	9/14/16
	98
	6.9
	38
	31.10
	0.018
	38
	49

	
	10/12/16
	54
	4.4
	28
	23.60
	BDL
	28
	14

	
	11/9/16
	52
	2.8
	21
	18.20
	BDL
	21
	12

	
	12/8/16
	68
	2.0
	11
	9.0
	BDL
	11
	8.6

	
	1/18/17
	68
	0.3
	10
	9.2
	BDL
	10
	2.9

	
	2/23/17
	67
	0.4
	6
	5.3
	BDL
	6
	1.5

	
	3/23/17
	80
	0.5
	6
	5.3
	0.150
	6
	1.1

	
	4/19/17
	74
	0.2
	7
	6.5
	BDL
	7
	1.0

	L1D
	9/14/16
	
	
	
	
	
	
	

	
	10/12/16
	29
	12
	14
	2.00
	BDL
	14
	29

	
	11/9/16
	73
	0.46
	4.7
	4.24
	41
	46
	0.1

	
	12/8/16
	
	
	
	
	
	
	

	
	1/18/17
	71
	0.36
	1.7
	1.34
	11
	13
	0.04

	
	2/23/17
	68
	0.03
	0.9
	0.82
	19
	20
	0.03

	
	3/23/17
	76
	0.01
	0.9
	0.89
	18
	19
	0.02

	
	4/19/17
	60
	0.01
	1.1
	1.09
	21
	22
	0.02

	L2D
	9/14/16
	
	
	
	
	
	
	

	
	10/12/16
	38
	4.30
	6.9
	2.60
	4.2
	11
	0.19

	
	11/9/16
	69
	0.55
	2.3
	1.75
	22
	24
	0.13

	
	12/8/16
	
	
	
	
	
	
	

	
	1/18/17
	62
	0.14
	1.6
	1.46
	19
	21
	0.06

	
	2/23/17
	65
	0.43
	2.2
	1.77
	21
	23
	0.06

	
	3/23/17
	72
	0.01
	1.6
	1.59
	26
	28
	0.05

	
	4/19/17
	55
	BDL
	1.3
	1.30
	27
	28
	0.04

	L3D
	9/14/16
	110
	0.012
	3.9
	3.89
	4.20
	8
	0.43

	
	10/12/16
	28
	0.076
	2.4
	2.32
	0.89
	3
	0.86

	
	11/9/16
	30
	0.044
	2.7
	2.66
	7.70
	10
	0.26

	
	12/8/16
	
	
	
	
	
	
	

	
	1/18/17
	59
	0.053
	2.0
	1.95
	7.6
	10
	0.16

	
	2/23/17
	54
	0.026
	1.5
	1.47
	12
	14
	0.14

	
	3/23/17
	58
	0.018
	2.0
	1.98
	13
	15
	0.15

	
	4/19/17
	55
	0.005
	2.3
	2.30
	20
	22
	0.13

	L4D
	9/14/16
	
	
	
	
	
	
	

	
	10/12/16
	54
	8.5
	13
	4.50
	BDL
	13
	0.27

	
	11/9/16
	53
	6.3
	11
	4.70
	0.017
	11
	0.06

	
	12/8/16
	
	
	
	
	
	
	

	
	1/18/17
	61
	0.76
	2.3
	1.54
	2.60
	5
	0.02

	
	2/23/17
	67
	0.73
	2.1
	1.37
	2.40
	5
	0.02

	
	3/23/17
	81
	0.21
	1.7
	1.49
	4.70
	6
	0.01

	
	4/19/17
	61
	0.23
	1.7
	1.47
	14
	16
	0.01

	L5D
	9/14/16
	43
	0.16
	3.0
	2.84
	1.10
	4
	0.13

	
	10/12/16
	14
	0.65
	2.9
	2.25
	BDL
	3
	0.17

	
	11/9/16
	30
	2.20
	4.5
	2.30
	0.56
	5
	0.04

	
	12/8/16
	
	
	
	
	
	
	

	
	1/18/17
	45
	0.2
	1.4
	1.23
	0.79
	2
	0.03

	
	2/23/17
	49
	0.04
	1.1
	1.06
	1.50
	3
	0.02

	
	3/23/17
	53
	0.02
	1.2
	1.18
	3.10
	4
	0.01

	
	4/19/17
	45
	0.01
	1.2
	1.19
	2.00
	3
	0.01

	L6D
	9/14/16
	
	
	
	
	
	
	

	
	10/12/16
	86
	16
	31
	15.00
	BDL
	31
	31

	
	11/9/16
	62
	22
	27
	5.00
	BDL
	27
	20

	
	12/8/16
	
	
	
	
	
	
	

	
	1/18/17
	66
	17
	20
	3.00
	BDL
	20
	6.7

	
	2/23/17
	64
	0.081
	10
	9.92
	0.93
	11
	3.8

	
	3/23/17
	78
	3.4
	5.4
	2.00
	3.5
	9
	2.4

	
	4/19/17
	76
	0.38
	5
	4.62
	0.055
	5
	4.5

	MW1
	9/14/16
	31
	0.008
	2.60
	2.59
	3.6
	6
	92

	
	10/12/16
	39
	0.16
	120
	119.84
	11.0
	131
	490

	
	11/9/16
	29
	0.80
	64
	63.20
	3.5
	68
	200

	
	12/8/16
	26
	0.28
	63
	62.72
	2.9
	66
	200

	
	1/18/17
	27
	0.049
	27
	26.95
	3.1
	30
	200

	
	2/23/17
	26
	0.009
	0.19
	0.18
	4.2
	4
	0.29

	
	3/23/17
	32
	0.009
	0.32
	0.31
	3.9
	4
	0.01

	
	4/19/17
	32
	0.008
	0.32
	0.31
	3.9
	4
	0.01


Notes:  STE=septic tank effluent sample; L= lysimeter sample; MW=monitoring well sample; M=horizontal 
well sample; BDL=below detection limit.  Reported concentrations are in milligrams per liter, empty field 
indicates insufficient sample volume available for analysis.





Figure 3.  Shallow Lysimeters – Chloride mg/L


Figure 4.  Shallow Lysimeters – Total Nitrogen mg/L


Figure 5.  Shallow Lysimeters – Total Phosphorous mg/L


Figure 6.  Horizontal Monitoring Wells – Chloride mg/L

[bookmark: _Hlk481494767]Figure 7.  Horizontal Monitoring Wells – Total Nitrogen mg/L


Figure 8.  Horizontal Monitoring Wells – Total Phosphorous mg/L


Figure 9.  Deep Lysimeters – Chloride mg/L


Figure 10.  Deep Lysimeters – Total Nitrogen mg/L


Figure 11.  Deep Lysimeters – Total Phosphorous mg/L

Water level and flow measurements were also measured.  Depths to water were measured in the 3 piezometers and the monitoring well, and flow was recorded from the flow meter during each site visit. These results are provided in Tables 3 and 4.  

Table 3.  Water levels, Wekiva experimental lined drainfield study
	Station
	Date
	Depth to Water (ft.)
	Height of Water Above Bottom of Liner (ft.)

	P1
	9/13/16
	5.47
	0.53

	
	10/12/16
	5.40
	0.60

	
	11/9/16
	5.55
	0.45

	
	12/8/16
	5.55
	0.45

	
	1/17/17
	5.31
	0.69

	
	2/23/17
	N/A
	N/A

	
	3/23/17
	N/A
	N/A

	
	4/19/17
	N/A
	N/A

	P2
	9/13/16
	5.27
	0.53

	
	10/12/16
	5.30
	0.50

	
	11/9/16
	5.40
	0.40

	
	12/8/16
	5.45
	0.35

	
	1/17/17
	5.22
	0.58

	
	2/23/17
	N/A
	N/A

	
	3/23/17
	N/A
	N/A

	
	4/19/17
	5.13
	0.67

	P3
	9/13/16
	5.22
	0.48

	
	10/12/16
	5.35
	0.35

	
	11/9/16
	5.35
	0.35

	
	12/8/16
	5.45
	0.25

	P3
	1/17/17
	5.26
	0.44

	
	2/23/17
	N/A
	N/A

	
	3/23/17
	N/A
	N/A

	
	4/19/17
	N/A
	N/A

	MW1
	9/13/16
	29.05
	N/A

	
	10/12/16
	27.90
	N/A

	
	11/9/16
	26.75
	N/A

	MW1
	12/8/16
	27.90
	N/A

	
	1/17/17
	28.92
	N/A

	
	2/23/17
	29.50
	N/A

	
	3/23/17
	29.70
	N/A

	
	4/19/17
	30.25
	N/A


Notes:  Elevations are relative to septic tank outlet bottom, assigned Elevation
of 100.0 feet. MW1=monitoring well, P=piezometer, N/A=not available
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	Date
	Meter Reading (gal.)
	Daily Average (gal.)
	Comments

	7/28/2016
	300
	~
	Commence flow measurements to drainfield

	9/13/2016
	1700
	30
	Homeowner on vacation

	10/12/2016
	2400
	23
	Homeowner on vacation

	11/9/2016
	32700
	1082
	Irrigation of newly installed sod

	12/8/2016
	42500
	327
	Normal irrigation use

	1/17/2017
	54100
	290
	Normal irrigation use

	2/23/17
	64400
	271
	Normal irrigation use

	3/23/17
	71400
	250
	Normal irrigation use

	4/19/17
	81600
	378
	Normal irrigation use


Note: Average daily flow includes irrigation and is based on flow since date of previous measurement
	
Results to Date
Operation of the experimental drainfield has proceeded since July 29, 2016.  The data collected during this period allow us to make the following observations:  
· Effluent concentrations have been variable, possibly due to intermittent use while the residents took vacations.  Except for one occasion, TN values were within a typical range for septic tank effluent.  The average STE concentration of TN is 60 mg/L over the monitoring period to date.  Average chloride and TP concentrations are 78 and 6.1 mg/L, respectively, over the same period.
· Recovery of water from suction lysimeters was poor, due in part to the dry season and in part to the uneven distribution of infiltrating water within the drainfield.
· More recent data from the shallow lysimeters (L1S, L 2S, L3S, L4S) indicate more even flow between drainfield lines and complete nitrification within the drainfield and shallow soil.  Most of the infiltration occurs in the upstream half of drainfield, based on a comparison of results from lysimeters closest to header and those at the middle of the drainfield.  Data from lysimeters L5S and L6S seem to indicate greater influence from rainfall and irrigation water and less influence from infiltrating effluent.
· The more recent data from the shallow lysimeter below the header area (L7S) show similar concentrations to those beneath the drainfield and do not indicate leakage at the header.  
· The higher concentrations of chloride and ammonia from the horizontal wellpoints below the mulch layer closest to the header (M1 and M2) seem to indicate that effluent is infiltrating into the mulch layer and that anaerobic conditions prevail.  It is likely that some ammonia is being produced through decomposition of organic nitrogen in the mulch.  Higher organic nitrogen concentrations and lower concentrations of ammonia in the horizontal wells further away from the header (M3, M4, M5, and M6), which are comparably different from the detections in M1 and M2 may suggest that the infiltrating effluent stimulates biological activity.  It will be interesting to monitor these changes as the study continues.  
· Phosphorus release from the mulch, based on a comparison of the effluent and horizontal well point data, appears to have diminished, although it appears from some sites that the mulch continues to release some phosphorus.  Phosphorus values from the most recent sampling event appear to be anomalously low at several sites, including the STE. This anomaly is being investigated.
· The data from deep lysimeters installed along the edge of the liner appear to STEr influence, nitrification of the ammonia within the saturated zone, and some apparent denitrification.  TN concentrations (as nitrate) in the deep lysimeters collecting pore water outside and below the edge of the liner are lower than those detected in the horizontal wells and generally lower than those in nearby shallow lysimeters.  Again, most of the ones closest to the header have higher concentrations of chloride and nitrogen, reflective of influence by the infiltrating effluent, and ones further away reflect the background influences of infiltrating rainwater and irrigation water.  Over the monitoring period to date, average TN concentrations in the deep lysimeters that are most influenced by the STE (L1D, L2D, and L3D) range from 62 to 84 % lower than the average STE concentration.
· The monitor well adjacent to the drainfield is a small-diameter (3/4-inch diameter) micro-well that was installed by the DEP-owned direct push rig.  Depth to groundwater at this site is almost 30 feet, so purging and sampling with a suction lift pump is not possible, and this well must be purged and sampled using a method that results in a turbid sample.  Sample turbidity causes bias in the quality results for phosphorus and TKN/organic nitrogen.  Starting with the February 2017 sampling event, samples from the well have been filtered immediately after sample collection, and filtration of the suspended material appears to provide more representative phosphorous and nitrogen concentrations.  
· Water levels in the piezometers indicate that water is pooling within the lined area and some of the wood mulch layer is saturated.  Thickness of saturated mulch has varied, generally greater in the area closest to the header.  Samplers have had difficulties in getting depth-to-water measurements on some dates due to the small diameter of the piezometers.  In future installations, larger diameter piezometers should be installed.  
· When the flow meter was installed, it was understood that it was being installed at a point where flow to the irrigation system would not be included.  However, it was determined later that irrigation flow is also being measured.  High water use measured during some months reflects irrigation of new sod during the dry season.  Readings in Table 4 represent flow to the house as well as the irrigation system.   





Next Steps
DEP staff will continue monthly sample collection and measurements of flow and water levels in the piezometers and monitoring well.  After three additional months of monitoring data are collected and analyzed, the third quarterly report will be submitted.  Through continued monitoring, we anticipate additional stabilization of water quality within the mulch layer and equalization of flow within the drainfield.  Any future decisions on modifications to the monitoring or treatment systems will be made after a larger set of data are collected.




Shallow Lysimeters - Chloride mg/L

L-1S	42627	42655	42683	42753	42789	42817	42844	100	77	82	70	73	53	L-2S	42627	42655	42683	42753	42789	42817	42844	16	48	38	44	L-3S	42627	42655	42683	42753	42789	42817	42844	54	27	46	54	68	45	L-4S	42627	42655	42683	42753	42789	42817	42844	79	85	24	73	77	85	L-5S	42627	42655	42683	42753	42789	42817	42844	25	6.1	8.9	48	52	88	37	L-6S	42627	42655	42683	42753	42789	42817	42844	16	8.8000000000000007	13	44	45	98	L-7S	42627	42655	42683	42753	42789	42817	42844	43	68	81	74	80	63	STE1	42627	42655	42683	42753	42789	42817	42844	99	70	83	79	79	79	59	



Shallow Lysimeters - Total Nitrogen mg/L

L-1S	42627	42655	42683	42753	42789	42817	42844	57	39	29	28	58	20	L-2S	42627	42655	42683	42753	42789	42817	42844	4	32	26	44	25	36	L-3S	42627	42655	42683	42753	42789	42817	42844	3	13	10	13	23	40	L-4S	42627	42655	42683	42753	42789	42817	42844	12	3	8	13	14	20	11	L-5S	42627	42655	42683	42753	42789	42817	42844	3	2	8	1	2	9	4	L-6S	42627	42655	42683	42753	42789	42817	42844	3	2	3	1.5	2	3	L-7S	42627	42655	42683	42753	42789	42817	42844	19	13	37	67	42	25	STE1	42627	42655	42683	42753	42789	42817	42844	80	45	60	61	40	79	53	



Shallow Lysimeters - Total Phosphorous mg/L

L-1S	42627	42655	42683	42753	42789	42817	42844	2.8	4.7	3.2	3.4	1.3	0.2	L-2S	42627	42655	42683	42753	42789	42817	42844	0.14000000000000001	0.11	0.13	8.5999999999999993E-2	7.0000000000000007E-2	0.05	L-3S	42627	42655	42683	42753	42789	42817	42844	0.1	0.1	0.12	0.13	7.2999999999999995E-2	7.9000000000000001E-2	L-4S	42627	42655	42683	42753	42789	42817	42844	0.14000000000000001	9.9000000000000005E-2	9.6000000000000002E-2	0.13	0.16	0.12	0.13	L-5S	42627	42655	42683	42753	42789	42817	42844	0.23	0.12	5.6000000000000001E-2	2.5999999999999999E-2	1.4999999999999999E-2	0.01	0	L-6S	42627	42655	42683	42753	42789	42817	42844	0.31	0.12	6.0999999999999999E-2	0.03	2.5000000000000001E-2	2.9000000000000001E-2	L-7S	42627	42655	42683	42753	42789	42817	42844	0.51	0.83	1.5	4	1.4	3.5	STE1	42627	42655	42683	42753	42789	42817	42844	8.4	5.2	7.5	6.9	4.9000000000000004	9.6	0.1	



Horizontal Monitoring Wells - Chloride mg/L

M1	42627	42655	42683	42712	42753	42789	42817	42844	100	67	77	73	86	77	83	64	M2	42627	42655	42683	42712	42753	42789	42817	42844	100	62	75	72	87	74	88	64	M3	42627	42655	42683	42712	42753	42789	42817	42844	91	58	71	69	74	73	80	61	M4	42627	42655	42683	42712	42753	42789	42817	42844	96	62	73	72	72	73	83	63	M5	42627	42655	42683	42712	42753	42789	42817	42844	89	52	43	64	63	65	76	M6	42627	42655	42683	42712	42753	42789	42817	42844	98	54	52	68	68	67	80	74	STE1	42627	42655	42683	42712	42753	42789	42817	42844	99	70	83	75	79	79	79	59	



Horizontal Monitoring Wells - Total Nitrogen mg/L

M1	42627	42655	42683	42712	42753	42789	42817	42844	57	47	46	22	8	36	28	15	M2	42627	42655	42683	42712	42753	42789	42817	42844	61	43	45	34	27	32	29	20	M3	42627	42655	42683	42712	42753	42789	42817	42844	50	31	23	16	9	26	26	26	M4	42627	42655	42683	42712	42753	42789	42817	42844	64	28	21	17	9	24	28	20	M5	42627	42655	42683	42712	42753	42789	42817	42844	40	24	16	11	8	9	6	M6	42627	42655	42683	42712	42753	42789	42817	42844	38	28	21	11	10	6	6	7	STE1	42627	42655	42683	42712	42753	42789	42817	42844	80	45	60	65	61	40	79	53	



Horizontal Monitoring Wells - Total Phosphorous mg/L

M1	42627	42655	42683	42712	42753	42789	42817	42844	2.8	3.6	6.7	3.1	2.8	5.6	4	4.8	M2	42627	42655	42683	42712	42753	42789	42817	42844	2.5	2.5	4.5	2.6	3.3	4.8	4.2	4.7	M3	42627	42655	42683	42712	42753	42789	42817	42844	34	8.4	2	1.6	2.1	1.4	2.5	1.9	M4	42627	42655	42683	42712	42753	42789	42817	42844	54	9.1	2.2000000000000002	0.81	1.7	1.6	1.1000000000000001	1.3	M5	42627	42655	42683	42712	42753	42789	42817	42844	60	10	8.3000000000000007	6.9	2.7	1.9	1.2	M6	42627	42655	42683	42712	42753	42789	42817	42844	49	14	12	8.6	2.9	1.5	1.1000000000000001	1	STE1	42627	42655	42683	42712	42753	42789	42817	42844	8.4	5.2	7.5	7.3	6.9	4.9000000000000004	9.6	0.1	



Deep Lysimeters - Chloride mg/L

L-1D	42627	42655	42683	42753	42789	42817	42844	29	73	71	68	76	60	L-2D	42627	42655	42683	42753	42789	42817	42844	38	69	62	65	72	55	L-3D	42627	42655	42683	42753	42789	42817	42844	110	28	30	59	54	58	55	L-4D	42627	42655	42683	42753	42789	42817	42844	54	53	61	67	81	61	L-5D	42627	42655	42683	42753	42789	42817	42844	43	14	30	45	49	53	45	L-6D	42627	42655	42683	42753	42789	42817	42844	86	62	66	64	78	76	STE1	42627	42655	42683	42753	42789	42817	42844	99	70	83	79	79	79	59	



Deep Lysimeters - Total Nitrogen mg/L

L-1D	42627	42655	42683	42753	42789	42817	42844	14	46	13	20	19	22	L-2D	42627	42655	42683	42753	42789	42817	42844	11	24	21	23	28	28	L-3D	42627	42655	42683	42753	42789	42817	42844	8	3	10	10	14	15	22	L-4D	42627	42655	42683	42753	42789	42817	42844	13	11	5	5	6	16	L-5D	42627	42655	42683	42753	42789	42817	42844	4	3	5	2	3	4	3	L-6D	42627	42655	42683	42753	42789	42817	42844	31	27	20	11	9	5	STE1	42627	42655	42683	42753	42789	42817	42844	80	45	60	61	40	79	53	



Deep Lysimeters - Total Phosphorous mg/L

L-1D	42627	42655	42683	42753	42789	42817	42844	29	7.0000000000000007E-2	4.2000000000000003E-2	2.5999999999999999E-2	2.1999999999999999E-2	0.02	L-2D	42627	42655	42683	42753	42789	42817	42844	0.19	0.13	6.4000000000000001E-2	5.6000000000000001E-2	4.5999999999999999E-2	0.04	L-3D	42627	42655	42683	42753	42789	42817	42844	0.43	0.86	0.26	0.16	0.14000000000000001	0.15	0.13	L-4D	42627	42655	42683	42753	42789	42817	42844	0.27	5.8000000000000003E-2	2.1999999999999999E-2	1.7999999999999999E-2	1.2999999999999999E-2	0.01	L-5D	42627	42655	42683	42753	42789	42817	42844	0.13	0.17	3.7999999999999999E-2	2.5000000000000001E-2	1.7999999999999999E-2	1.0999999999999999E-2	0.01	L-6D	42627	42655	42683	42753	42789	42817	42844	31	20	6.7	3.8	2.4	4.5	STE1	42627	42655	42683	42753	42789	42817	42844	8.4	5.2	7.5	6.9	4.9000000000000004	9.6	0.1	
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