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	Type of Entity
	Name

	Responsible Stakeholders
	City of Brooksville
Hernando County
Pasco County
Agricultural producers
Golf courses

	Responsible Agencies
	Florida Department of Agriculture and Consumer Services
Florida Department of Environmental Protection
Florida Department of Health
Southwest Florida Water Management District

	Other Interested Stakeholders
	Citizens
City of Weeki Wachee
Florida Farm Bureau
Florida Onsite Wastewater Association
Florida Springs Institute
Hernando Beach Government Affairs Committee
Hernando County Task Force
Hernando Environmental Land Protectors (HELP)
Save the Manatee Club



See Appendix A for links to important sources referenced in this document. For additional information on the watershed management approach in the Weeki Wachee Basin, contact:
Terry Hansen, P.G., Basin Coordinator
Florida Department of Environmental Protection
Water Quality Restoration Program, Watershed Planning and Coordination Section
2600 Blair Stone Road, Mail Station 3565
Tallahassee, FL 32399-2400
Email: terry.hansen@dep.state.fl.us
Phone: (850) 245–8561
Fax: (850) 245–8434
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Executive Summary
Weeki Wachee Basin
The Florida Springs and Aquifer Protection Act (Chapter 373, Part VIII, Florida Statutes [F.S.]), provides for the protection and restoration of Outstanding Florida Springs (OFS), which comprise 24 first magnitude springs, 6 additional named springs, and their associated spring runs. The Florida Department of Environmental Protection (DEP) has assessed water quality in each OFS, and has determined that 24 of the 30 OFS are impaired for the nitrate form of nitrogen. The Weeki Wachee Spring Group is one of the impaired first magnitude OFS.
[bookmark: _Hlk491168664]The Weeki Wachee Basin Management Action Plan (BMAP) area (Figure ES-1) consists of 200,474 acres located in southern Hernando County, including a portion of the City of Brooksville, and northern Pasco County. The BMAP area contains the Weeki Wachee Spring Group which is composed of a single, large main spring and numerous smaller springs spread over an area of nearly five square miles. Weeki Wachee Spring is the primary source of the Weeki Wachee River and the largest spring (by discharge) in the group. The BMAP area also contains Magnolia-Aripeka Springs Group; Mud Spring, Salt Spring, Wilderness Spring (collectively referred to as the "Wilderness-Mud-Salt Springs Group"); and Jenkins Creek Spring which are located within the Weeki Wachee riverine system Outstanding Florida Water (OFW) boundaries. 

Weeki Wachee Priority Focus Area (PFA)
The PFA (see Appendix C) comprises 90,415 acres and includes a region in the western part of the springshed for Weeki Wachee Spring. The PFA represents the area in the basin where the aquifer is most vulnerable to inputs and where there are the most connections between groundwater and the springs. 










[bookmark: _Toc512092347][bookmark: _Toc512092691][bookmark: _Toc514421536]Figure ES-1[image: ]. Weeki Wachee BMAP and PFA boundaries
[bookmark: _Ref439623235][bookmark: _Toc445717773]
Nitrogen Source Identification, Required Reductions, and Options to Achieve Reductions
DEP adopted nutrient total maximum daily loads (TMDLs) for Weeki Wachee Spring and Weeki Wachee River in 2014. The TMDLs established monthly average nitrate targets of 0.28 milligrams per liter (mg/L) for Weeki Wachee Spring and 0.20 mg/L for Weeki Wachee River. DEP adopted nitrate targets of 0.23 mg/L for Magnolia-Aripeka Springs Group; Wilderness-Mud-Salt Springs Group; and Jenkins Creek Spring through adoption of TMDLs in 2016.
Onsite sewage treatment and disposal systems (OSTDS) represent 30 % of the nitrogen loading to groundwater, agriculture (including farm fertilizer [FF] and livestock waste [LW]) 27 %, and urban turfgrass fertilizer (UTF) 22 % of the total loading to groundwater based on the DEP analysis conducted using the Nitrogen Source Inventory Loading Tool (NSILT). 
The total load reduction required to meet the TMDLs at the vents is 195,200 pounds of nitrogen per year (lb-N/yr). To measure progress towards achieving the necessary load reduction, DEP is establishing the following milestones:
· 58,560 lb-N/yr (30 %) within 5 years. 
· 97,600 lb-N/yr (50 %) within 10 years. 
· 39,040 lb-N/yr (20 %) within 15 years.
· Total of 195,200 lb-N/yr within 20 years.
The policies and submitted projects included within this BMAP are estimated to achieve a reduction of 384,857 to 498,088 lb-N/yr. The BMAP is designed to achieve 80 % of the effort within 10 years of adoption and 100 % within 15 years. Projects and strategies are designed to achieve nitrogen reductions at Weeki Wachee, but are expected to provide benefits to all springs vents within the springshed/contributing area. DEP will evaluate progress towards these milestones and will report to the Governor and Florida Legislature. DEP will adjust management strategies to ensure the target concentrations are achieved. This may include expanding the area to which the OSTDS remediation policies apply; any such change, however, would be incorporated into an updated BMAP through a formal adoption process.
There are currently 58 projects to improve water quality (see Appendix B), of which 27 projects have estimated load reductions. Included are owner-implemented best management practices (BMPs) for FF, LW, sports turfgrass (STF); wastewater treatment facility (WWTF) upgrades; projects to reduce UTF application; and OSTDS conversions to sewer.
Restoration Approaches
[bookmark: _Hlk506197773]New OSTDS – Upon BMAP adoption, the OSTDS remediation plan prohibits new systems on lots of less than 1 acre within the PFAs, unless the system includes enhanced treatment of nitrogen as defined by the OSTDS remediation plan, or unless the OSTDS permit applicant demonstrates that sewer connections will be available within 5 years. Local governments and utilities are encouraged to develop master wastewater treatment feasibility plans to identify specific areas to be sewered within 20 years of BMAP adoption. The OSTDS remediation plan is incorporated as Appendix D.
Existing OSTDS – Upon completion of the feasibility plan, rulemaking, and funding milestones included in the OSTDS remediation plan, but no later than five years after BMAP adoption, modification or repair permits issued by FDOH for all OSTDS within the PFA on all lot sizes will require enhanced treatment of nitrogen, unless sewer connections will be available based on a BMAP-listed project. All OSTDS subject to the policy must include enhanced treatment of nitrogen no later than 20 years after BMAP adoption.
WWTFs − The effluent standards listed in Table ES-1 will apply to all new and existing WWTFs in the BMAP area (inside and outside the PFA).
[bookmark: _Toc505866866][bookmark: _Toc512092348][bookmark: _Toc512092900][bookmark: _Toc514421067]Table ES-1. WWTF effluent standards
[bookmark: _Hlk490739434]gpd = Gallons per day
	
95% of the Permitted Capacity (gpd)
	Nitrogen Concentration Limits for Rapid Infiltration Basins (RIBs) and Absorption Fields (mg/L)
	Nitrogen Concentration Limits for All Other Land Disposal Methods, Including Reuse (mg/L)

	Greater than 100,000
	3
	3

	20,000 to 100,000
	3
	6

	Less than 20,000
	6
	6


· UTF – UTF sources can receive up to 6 % credit for the DEP-approved suite of public education and source control ordinances. Entities have the option to collect and provide monitoring data to quantify reduction credits for additional measures.
· STF – STF sources include golf courses and other sporting facilities. Golf courses can receive up to 10 % credit for implementing the Golf Course BMP Manual. Other sports fields can receive up to 6 % credit for managing their fertilizer applications to minimize transport to groundwater.
· FF – All FF sources are required to implement best management practices (BMPs) or perform monitoring to demonstrate compliance with the TMDL. A 15 % reduction to groundwater is estimated for owner-implemented BMPs. Additional credits could be achieved through better documentation of reductions achieved through BMP implementation or implementation of additional agricultural projects or practices, such as precision irrigation, soil moisture probes, controlled release fertilizer, and cover crops.
· LW – All LW sources are required to implement BMPs or perform monitoring. A 10 % reduction to groundwater is estimated for owner-implemented BMPs. Additional credits could be achieved through additional projects and practices if data are available.
[bookmark: _Hlk486490351]


[bookmark: _Toc159826191][bookmark: _Toc159831621]

1. [bookmark: _Toc475022059][bookmark: _Toc514419733]: Background
[bookmark: _Toc514419734]Legislation
[bookmark: _Toc475022061]Chapter 373, Part VIII, Florida Statutes (F.S.), created the Florida Springs and Aquifer Protection Act to provide for the protection and restoration of Outstanding Florida Springs (OFS), which comprise 24 first magnitude springs, 6 additional named springs, and their associated spring runs. The Florida Department of Environmental Protection (DEP) has assessed water quality in each OFS, and has determined that 24 of the 30 OFS are impaired for the nitrate form of nitrogen. The Weeki Wachee Spring Group is one of the impaired first magnitude OFS.
Development of the basin management action plan (BMAP) to meet the new requirements of the Florida Springs and Aquifer Protection Act for the Weeki Wachee Basin was initiated in 2016.
[bookmark: _Toc514419735][bookmark: _Toc475022062]Water Quality Standards and Total Maximum Daily Loads (TMDLs)
A TMDL represents the maximum amount of a given pollutant that a waterbody can assimilate and still meet water quality criteria. The waters of the Weeki Wachee Spring Group, Magnolia-Aripeka Springs Group, Wilderness-Mud-Salt Springs Group, and Jenkins Creek Spring that are addressed in this BMAP are Class III waterbodies with a designated use of recreation, propagation, and the maintenance of a healthy, well-balanced population of fish and wildlife. These waters are impaired by nitrate nitrogen, which in excess has been demonstrated to adversely affect flora or fauna through the excessive growth of algae. Excessive algal growth results in ecological imbalances in springs and rivers and can produce human health problems, foul beaches, inhibit navigation, and reduce the aesthetic value of the resources.
DEP adopted nutrient TMDLs for the Weeki Wachee Spring Group in 2014 (see Table 1). The TMDLs established a target of an annual average of 0.28 milligrams per liter (mg/L) of nitrate for Weeki Wachee Spring and 0.20 mg/L for Weeki Wachee River. The period of record for water quality data for the TMDLs was January 2004 through December 2012. DEP adopted nutrient TMDLs for the Magnolia-Aripeka Springs Group, Wilderness-Mud-Salt Springs Group, and Jenkins Creek Spring in 2016 (see Table 1). The TMDLs established a target of an annual average of 0.23 mg/L of nitrate. The period of record for the water quality data for the TMDLs was January 2004 through December 2014.
[bookmark: _Toc505866867][bookmark: _Toc512092909]

[bookmark: _Toc514421079]Table 1. Restoration targets for Weeki Wachee Spring Group, Magnolia-Aripeka Springs Group, Wilderness-Mud-Salt Springs Group, and Jenkins Creek Spring
	Waterbody or Spring Name
	Waterbody Identification (WBID) Number
	Parameter
	TMDL
(mg/L)

	Weeki Wachee Spring 
	1382B
	Nitrate, annual average
	0.28

	Weeki Wachee River
	1382F
	Nitrate, annual average
	0.20

	Magnolia-Aripeka Springs Group
	1391B
	Nitrate, annual average
	0.23

	Wilderness-Mud-Salt Springs Group
	1382G
	Nitrate, annual average
	0.23

	Jenkins Creek Spring
	1389
	Nitrate, annual average
	0.23



[bookmark: _Toc514419736]BMAP Requirements
[bookmark: _Ref488245493]Section 403.067(7), F.S., provides DEP with the statutory authority for the BMAP Program. A BMAP is a comprehensive set of strategies to achieve the required pollutant load reductions. In addition to this authority, the Florida Springs and Aquifer Protection Act (Part VIII of Chapter 373, F.S.) describes additional requirements for 30 springs. BMAP Area
[bookmark: _Ref488219833]The BMAP area (Figure 1) comprises 200,474 acres located in southern Hernando County, including a portion of the City of Brooksville, and northern Pasco County. The BMAP area contains the Weeki Wachee Spring Group which is composed of a single, large main spring and numerous smaller springs spread over an area of nearly five square miles. Weeki Wachee Spring is the primary source of the Weeki Wachee River and the largest spring (by discharge) in the group. The BMAP area also contains Magnolia-Aripeka Springs Group; Mud Spring, Salt Spring, Wilderness Spring (collectively referred to as the "Wilderness-Mud-Salt Springs Group"); and Jenkins Creek Spring which are located within the Weeki Wachee riverine system Outstanding Florida Water (OFW) boundaries.  
This area includes the surface water basin as well as the groundwater contributing areas for the springs (or springsheds). Springsheds for the OFS were delineated or reviewed by Southwest Florida Water Management District (SWFWMD) with input from the Florida Geological Survey (FGS). A springshed is the area of land that contributes water to a spring or group of springs, mainly via groundwater flow. 
[bookmark: _Toc514419737]PFA
In compliance with the Florida Springs and Aquifer Protection Act, this BMAP delineates a PFA, defined as the area(s) of a basin where the Floridan aquifer is generally most vulnerable to pollutant inputs and where there is a known connectivity between groundwater pathways and an OFS. The PFA provides a guide for focusing restoration strategies where science suggests these efforts will most benefit the springs. The document describing the delineation process for the PFA is on the DEP website. The link to the PFA document is provided in Appendix C.
Description
Nitrogen sources are more likely to influence groundwater quality under certain conditions. For example, where soils are sandy and well drained, less nitrogen is converted to gas and released into the atmosphere or taken up by plants, compared with other soil types. Therefore, local soil types play a role in how much nitrogen travels from the land surface to groundwater in a specific springshed. Also, the underlying geologic material influences the vulnerability of the underlying aquifers and the rate of lateral movement within the Floridan aquifer toward the springs. These conditions, and others, were considered in the delineation of the PFA (see Appendix C). 
Following BMAP adoption, DEP will ensure that the GIS files associated with the PFA boundary are available to the public on the DEP Map Direct webpage. 
[image: ]
[bookmark: _Ref489865682][bookmark: _Toc512092349][bookmark: _Toc512092704][bookmark: _Toc514421543]Figure 1. Weeki Wachee BMAP, springshed, and PFA boundaries
Additional Requirements  
In accordance with Section 373.811, F.S., the following activities are prohibited in the PFA: 
· New domestic wastewater disposal facilities, including rapid infiltration basins (RIBs), with permitted capacities of 100,000 gpd or more, except for those facilities that meet an advanced wastewater treatment (AWT) standard of no more than 3 mg/L total nitrogen (TN) on an annual permitted basis.
· [bookmark: _Hlk512515711]New OSTDS on lots of less than one acre inside the PFAs unless additional nitrogen treatment is provided, as specified in the OSTDS remediation plan (see Appendix D for details).
· New facilities for the disposal of hazardous waste.
· The land application of Class A or Class B domestic wastewater biosolids not in accordance with a DEP-approved nutrient management plan establishing the rate at which all biosolids, soil amendments, and sources of nutrients at the land application site can be applied to the land for crop production, while minimizing the amount of pollutants and nutrients discharged to groundwater or waters of the state.
· New agricultural operations that do not implement BMPs, measures necessary to achieve pollution reduction levels established by DEP, or groundwater monitoring plans approved by a WMD, or DEP.
Biosolids and Septage Application Practices
[bookmark: _Hlk497979941]In the PFA, the aquifer contributing to the springs is highly vulnerable to contamination by nitrogen sources and soils have a high to moderate tendency to leach applied nitrogen. DEP previously documented elevated nitrate concentrations in groundwater beneath septage application zones in spring areas. To assure that nitrogen losses to groundwater are minimized from permitted application of biosolids and septage in the PFA, the following requirements apply to newly-permitted application sites and existing application sites upon permit renewal.
[bookmark: _Hlk497914585][bookmark: _Hlk497913357]All permitted biosolids application sites that are agricultural operations must be enrolled in the Florida Department of Agriculture and Consumer Services (FDACS) BMP Program or be within an agricultural operation enrolled in the FDACS BMP Program for the applicable crop type.  Implementation of applicable BMPs will be verified by FDACS in accordance with Chapter 5M-1, Florida Administrative Code (F.A.C.). Permitted biosolids application sites that are new agricultural operations must also comply with Subsection 373.811(5), F.S.  Biosolids application sites must be certified as viable agricultural operations by an acknowledged agricultural professional such as an agricultural consultant or agricultural extension agent. Effective nutrient management practices must be ongoing at the application zones in the permit. Plant uptake and harvesting are vital components of the nutrient management plan to remove nitrogen and prevent it from leaching to groundwater. If DEP determines that the site is not a viable agricultural site implementing a nutrient management plan, corrective action will be required.
Groundwater monitoring for nitrate is required for all biosolids and septage land application sites in the PFA to assure compliance with nutrient management objectives in this BMAP. However, groundwater monitoring is not required if the site nutrient management plan limits biosolids application rates to TN with no adjustment for available nitrogen normally allowed by subsections 62-640.500(5) and (6), F.A.C. (e.g. for a recommended fertilizer rate of 160 pounds of nitrogen per acre, only 160 pounds of TN per acre shall be applied).  For septage application, groundwater monitoring is not required if the site nutrient management plan limits application rates to 30,000 gallons per acre for sites accepting mixtures of septage and grease (food establishment sludge) or to 40,000 gallons per acre for sites accepting septage without grease. The permit renewal application will include a trend analysis for nitrate in groundwater monitoring wells during the previous permit cycle, and an evaluation of the potential for the facility to cause or contribute to exceedance of the TMDL. 
Changes are proposed to the upcoming FDACS Cattle BMP Manual revision that will likely impact biosolid application. This will necessitate coordination between FDACS and DEP permitting staff. 
[bookmark: _Toc514419738]Other Scientific and Historical Information
In preparing this BMAP, DEP collected and evaluated credible scientific information on the effect of nutrients, particularly forms of nitrogen, on springs and springs systems. Some of the information collected is specific to the Weeki Wachee Basin, while other references provide information on related knowledge for restoring springs, such as nitrogen-reducing technologies, the treatment performance of OSTDS, and runoff following fertilizer applications. 
[bookmark: _Toc514419739]Stakeholder Involvement
Stakeholder involvement is critical to develop, gain support for, and secure commitments in a BMAP. The BMAP process engages stakeholders and promotes coordination and collaboration to address the pollutant load reductions necessary to achieve the TMDLs. DEP invites stakeholders to participate in the BMAP development process and encourages public participation and consensus to the greatest practicable extent. Table A-1 identifies the stakeholders who participated in the development of this BMAP.
During the development of the Weeki Wachee BMAP, DEP held a series of meetings involving stakeholders and the general public. The purpose of these meetings was to consult with stakeholders to gather information, evaluate the best available science, develop an OSTDS remediation plan (including a public education plan), define management strategies and milestones, and establish monitoring requirements. All of the meetings were open to the public and noticed in the Florida Administrative Register (F.A.R.). Additionally, a public meeting on the current draft BMAP was held on January 17, 2018, and was noticed in the F.A.R. and in local newspapers.
Upon BMAP adoption, DEP intends to facilitate annual meetings with stakeholders to review progress towards achieving the TMDLs.
[bookmark: _Toc514419740]Description of BMPs Adopted by Rule
Table 2 identifies the adopted BMPs and BMP manuals relevant to this BMAP.
[bookmark: _Toc505866868][bookmark: _Toc512092910][bookmark: _Toc514421080]Table 2. BMPs and BMP manuals adopted by rule as of June 2017
	Agency
	F.A.C. Chapter
	Chapter Title

	FDACS Office of Agricultural Water Policy (OAWP)
	5M-6
	Florida Container Nursery BMP Guide

	FDACS OAWP
	5M-8
	BMPs for Florida Vegetable and Agronomic Crops

	FDACS OAWP
	5M-9
	BMPs for Florida Sod

	FDACS OAWP
	5M-11
	BMPs for Florida Cow/Calf Operations

	FDACS OAWP
	5M-12
	Conservation Plans for Specified Agricultural Operations

	FDACS OAWP
	5M-13
	BMPs for Florida Specialty Fruit and Nut Crop Operations

	FDACS OAWP
	5M-14
	BMPs for Florida Equine Operations

	FDACS OAWP
	5M-16
	BMPs for Florida Citrus

	FDACS OAWP
	5M-17
	BMPs for Florida Dairies

	FDACS OAWP
	5M-18
	Florida Agriculture Wildlife BMPs

	FDACS OAWP
	5M-19
	BMPs for Florida Poultry

	FDACS Division of Agricultural Environmental Services
	5E-1
	Fertilizer

	FDACS Division of Aquaculture
	5L-3
	Aquaculture BMPs

	FDACS Florida Forest Service
	5I-6
	BMPs for Silviculture

	FDACS Florida Forest Service
	5I-8
	Florida Forestry Wildlife BMPs for State Imperiled Species

	SWFWMD
	40D-26
	Facilitating Agricultural Resource Management Systems (FARMS) Program

	DEP
	62-330
	Environmental Resource Permitting
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[bookmark: _Toc445731340][bookmark: _Toc445732100][bookmark: _Ref445748928][bookmark: _Toc475022063]
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[bookmark: _Toc514419741]: Implementation to Achieve TMDLs
[bookmark: _Toc514419742]Allocation of Pollutant Loads
[bookmark: _GoBack]DEP collected and evaluated credible scientific information on the effect of nutrients, particularly forms of nitrogen, on Weeki Wachee Spring.
Nutrients in the Springs and Spring Systems
[bookmark: _Toc445716598][bookmark: _Toc445717650][bookmark: _Toc445717695][bookmark: _Toc445717746][bookmark: _Toc445731344][bookmark: _Toc445732104][bookmark: _Toc408412577][bookmark: _Toc408412601][bookmark: _Toc475022066]DEP developed the Nitrogen Source Inventory Loading Tool (NSILT) to provide information on the major sources of nitrogen in the groundwater contributing area and spring contributing area for the OFS. In addition, this tool is used to estimate nitrogen loads to groundwater from these sources in the spring contributing area. The NSILT is a GIS- and spreadsheet-based tool that provides spatial estimates of the relative contribution of nitrogen from major nitrogen sources and accounts for the transport pathways and processes affecting the various forms of nitrogen as they move from the land surface through the soil and geologic strata.
The first major factor to be considered in estimating the loading to groundwater in the NSILT is the attenuation of nitrogen as it moves from its source through the environment, before it reaches the Upper Floridan aquifer (UFA). Biological and chemical processes that occur as part of the nitrogen cycle, as well as hydrogeological processes, control the movement of nitrogen from the land surface to groundwater. Many of these processes attenuate (impede or remove) the amount of nitrogen transported to groundwater. An understanding of how water moves through the subsurface and the processes that transform the different forms of nitrogen is essential for estimating nitrogen loading to groundwater from various sources.
A second major factor to consider in estimating the loading to groundwater is the geological features in the springshed and the related recharge rate to the aquifer. Water movement between the shallow groundwater (surficial aquifer, where present) and the deeper aquifer (UFA) is slowed by a low permeability layer of clay, silt, and fine sand that retards the vertical movement of infiltrating water from the surface. The UFA occurs in limestone that can be prone to dissolving and, over geologic time, the development of numerous karst features (sinkholes, caves, and conduits). These features allow water from the land surface to move directly and relatively rapidly into the aquifer and in some areas for groundwater in the aquifer to move rapidly to the springs.
Potential recharge rates from the surface to the UFA are affected by variations in the geologic materials and the presence of karst features. DEP estimated the recharge rate ranges and grouped them into three rate categories, which were applied to the NSILT:
· Low recharge (Less than 3 inches per year [in/yr]).
· Medium recharge (3 to 10 in/yr).
· High recharge (10 in/yr or greater). 
In the NSILT, DEP applies different attenuation factors to different types of sources, so that various biological, chemical, and hydrogeological effects can be estimated. The attenuation that is applied means that the amount of nitrogen leaving a source (such as a livestock operation or a just-fertilized yard), reduces the amount of nitrogen predicted to reach the aquifer. In the NSILT, the average attenuation rates range from 90 % (for atmospheric deposition) to 25 % (for wastewater disposal in a RIB). Using these examples, only 10 % of nitrogen from atmospheric deposition is expected to reach the aquifer, while 75 % of nitrogen from a RIB is expected to reach groundwater, because the remainder is attenuated by various chemical and biological processes.
Phosphorus is naturally abundant in the geologic material underlying much of Florida and is often present in high concentrations in surface water and groundwater. Monitoring and evaluation of phosphorus and influences on the springs continues as the nitrate TMDLs are implemented.
Estimated Nitrogen Loads
Table 3 lists the estimated nitrogen loads to groundwater by source. Note that urban stormwater loads are included in UTF estimates, while agricultural stormwater loads are included in FF and LW loading estimates. Nitrogen loading to surface water will be reduced through the activities and strategies for the sources identified in this chapter for groundwater loading.
[bookmark: _Ref488220979][bookmark: _Toc505866869][bookmark: _Toc512092911][bookmark: _Toc514421081]Table 3. Estimated nitrogen load to groundwater by source in the BMAP area
	Nitrogen Source 
	Total Nitrogen Load to Groundwater 
(lb-N/yr) 
	% Contribution 

	OSTDS
	282,875
	30

	UTF
	209,833
	22

	Atmospheric Deposition
	93,208
	10

	FF
	163,935
	17

	STF
	53,841
	6

	LW
	91,347
	10

	WWTF
	45,105
	5

	Total
	940,144
	100



Assumptions and Considerations
The NSILT estimates are based on the following assumptions and considerations: 
NSILT Nitrogen Inputs – The methods used to calculate nitrogen inputs for each pollutant source were based on a detailed synthesis of information, including direct water quality measurements, census data, surveys, WWTF permits, published scientific studies and reports, and information obtained in meetings with agricultural producers. For some pollutant source categories, the nitrogen inputs were calculated using assumptions and extrapolations. As a result, these estimated inputs could be subject to further refinement if more detailed information becomes available.
OSTDS Load Contribution – A per capita contribution to an OSTDS of 9.012 lb-N/year was used to calculate loading from OSTDS. The average household contribution was estimated based on 2010 U.S. Census Bureau data on average number of people per household by county (2.41 in Hernando County and 2.45 in Pasco County) within the area and additional information on the amount of time spent away from home by the school-age population and labor force (adjusted to an effective persons per household rate of 2.08 in Hernando County and 2.07 in Pasco County). 
[bookmark: _Hlk479840066]Nitrogen Attenuation Factors – To estimate the amount of nitrogen loading to the aquifer, DEP applied two nitrogen attenuation factors. Biological and chemical processes that occur as part of the nitrogen cycle, as well as hydrogeological processes, control the movement of nitrogen from the land surface to groundwater. Biochemical attenuation accounts for biochemical processes that convert or transform the different forms of nitrogen, while hydrogeological attenuation accounts for spatial variations that affect the rate of water infiltrating through geological media to recharge the UFA. Given the relatively large range of literature-reported values of biochemical nitrogen attenuation for each source category, DEP used an average biochemical attenuation factor for each source based on land use practices and hydrogeological conditions in the contributing areas. 
Other assumptions and considerations for BMAP implementation include the following:
· Unquantified Project Benefits – Nitrogen reductions for some of the projects and activities listed in this BMAP cannot currently be quantified. However, because of their positive impact, it is assumed that these actions will help reduce pollutant loads, and estimated loading reductions may be determined at a later date and assigned to these activities. 
· [bookmark: _Hlk481068187][bookmark: _Hlk490054235]Atmospheric Deposition – Atmospheric sources of nitrogen are local, national, and international.  Atmospheric sources are generally of low nitrogen concentration compared with other sources and are further diminished through additional biological and chemical processes before they reach groundwater. Atmospheric deposition sources and trends will be reevaluated periodically.
OSTDS Inventory and Loading Calculations – The total number of OSTDS in the basin is estimated based on local information and Florida Department of Health (FDOH) data. Future BMAPs and the associated OSTDS loading calculations may be adjusted based on improved data on the number and location of existing septic systems, and may include additional OSTDS installed since BMAP adoption.
PFA – The PFA provides a guide for focusing strategies where science suggests efforts will best benefit the springs. The PFA boundary may be adjusted in the future if additional relevant information becomes available. 
Project Collection Period – The BMAP project collection period is limited to projects after a certain date, based on the data used to calculate the reductions needed. Reductions from older projects are already accounted for in the baseline loading. Projects completed in the springshed after January 1, 2013, were considered for inclusion in this BMAP.
Legacy Sources – Historical land uses or management practices in the basin may still be affecting the nitrate concentration of the springs. The movement of water from the land surface through the soil column to the UFA and through the UFA to the spring system varies both spatially and temporally and is influenced by local soil and aquifer conditions. As a result, there may be a lag between when nitrogen input to the UFA occurs and ultimately when that load arrives at the Weeki Wachee Spring Group. The impact of this delay is not fully known.
Implementation Schedule – BMAP implementation is intended to be a 20-year process. This plan defines nitrogen reduction milestones for 5-year (30 %), 10-year (50 %), and 15-year (20 %) implementation, so that the TMDLs will be met no later than the 20-year goal (see Section 2.1.6 for further details). Further, the total reductions and the project credits may be adjusted under the adaptive management approach used for the BMAP. This approach requires regular follow-up to ensure that management strategies are carried out and that their incremental effects are assessed. The process acknowledges that there is some uncertainty associated with the outcomes of proposed management strategies and the estimated response in nitrogen concentration at the springs. As more information is gathered and progress towards each 5-year milestone is reviewed, additional management strategies to achieve the TMDLs will be developed or existing strategies refined to better address the sources of nitrogen loading. 
Changes in Spring Flows – The role of this BMAP is specifically to promote the implementation of projects that reduce nitrogen load to groundwater while the minimum flows and levels (MFLs) established for specific springs address water flows and levels. To maximize efforts between the two programs, spring protection projects should provide both water quality and quantity benefits.
Loading by Source
[bookmark: _Ref460401342][bookmark: _Ref460401356][bookmark: _Toc475022071][bookmark: _Toc422152962][bookmark: _Ref366663958][bookmark: _Ref329608521]Based on the NSILT results, the pie chart in Figure 2 depicts the estimated percentage of nitrogen loading to groundwater by source in the springshed. Septic systems represent 30 % of the total nitrogen loading to groundwater, agriculture 27 %, and UTF 22 % of the total loading. Stormwater loading to groundwater is incorporated into the various source categories.
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[bookmark: _Ref488394953][bookmark: _Toc479941188][bookmark: _Toc512092350][bookmark: _Toc512092705][bookmark: _Toc514421544]Figure 2. Loading to groundwater by source in the Weeki Wachee Springshed
Loading Allocation
[bookmark: _Hlk481067152]The nitrogen source reductions are based on the measured nitrate concentrations and flows at the vent, along with the TMDL target nitrate concentration. Table 4 lists the measured nitrate (as nitrogen) loads at the spring vents compared with the TMDL loading based on a target nitrate concentration of 0.28 mg/L. The difference between the spring vent loading and the TMDL loading calculations is the required reduction to meet the TMDLs. The total load that is required to be reduced in the basin is being allocated to the entire basin.
[bookmark: _Ref488221441][bookmark: _Toc505866870][bookmark: _Toc512092912][bookmark: _Hlk501465271]


[bookmark: _Toc514421082]Table 4. Total reduction required to meet the TMDLs
	[bookmark: _Hlk501465098]Description
	Nitrogen Loads (lb-N/yr)
	Notes Regarding Data Used 

	Total Load at Spring Vents
	289,000
	Upper 95% confidence interval - nitrate data and flow data from 2000 to 2017 (170 cubic feet per second [cfs])

	TMDL Load
	93,800
	TMDL target is 0.28 mg/L and using the same flow data from 2000 to 2017

	Required Reduction
	195,200
	



[bookmark: _Ref488221047]Description of 5-, 10-, and 15-year Milestones/Reduction Schedule
The overall load reduction targets are 30 % of the total within 5 years; 80 % of the total within 10 years; and 100 % of the total within 15 years. DEP will evaluate progress towards these milestones and will report to the Governor and Florida Legislature. DEP will adjust management strategies to ensure the target concentrations are achieved. This may include expanding the area to which the OSTDS remediation policies apply; any such change, however, would be incorporated into an updated BMAP through a formal adoption process.
Table 5 identifies the estimated nitrogen reductions needed, by milestone. Progress will be tracked yearly and adjustments made as needed. At the five-year milestone, progress will be assessed and load reductions adjusted as necessary. Entities have flexibility in the types and locations of projects as long as they achieve the overall required load reductions. The monitoring of existing groundwater and springs sampling locations is essential. Section 2.3 describes detailed source reduction strategies.
[bookmark: _Ref488221490][bookmark: _Toc505866871][bookmark: _Toc512092913][bookmark: _Toc514421083]Table 5. Nitrogen reduction schedule (lb-N/yr)
	5-Year Milestone
(30% of Total)
	10-Year Milestone
(50% of Total)
	15-Year Milestone
(20% of Total)
	Total Nitrogen Reduction
(100%)

	58,560
	97,600
	39,040
	195,200


[bookmark: _Toc480372118][bookmark: _Ref488221526][bookmark: _Toc514419743][bookmark: _Ref289163884]Prioritization of Management Strategies
[bookmark: _Hlk500320005]The management strategies listed in Appendix B, Appendix E, and Appendix F are ranked with a priority of high, medium, or low. In 2016, the Florida Legislature amended the Watershed Restoration Act (Section 403.067, F.S.), creating additional requirements for all new or revised BMAPs. BMAPs must now include planning-level details for each listed project, along with their priority ranking. 
Project status was selected as the most appropriate indicator of a project’s priority ranking. Projects with a "completed" status were assigned a low priority. Projects classified as "underway" were assigned a medium priority because some resources have been allocated to these projects, but some work still needs to be completed. High priority was assigned to projects listed as "planned" as well as certain "completed" projects that are ongoing each year (any project with one of these project types: "street sweeping," "catch basin inserts/inlet filter cleanout,"  "public education efforts," "fertilizer cessation," "fertilizer reduction," or "aquatic vegetation harvesting"), and select projects that are elevated because substantial, subsequent project(s) are reliant on their completion.
[bookmark: _Toc514419744]Load Reduction Strategy 
The total load reduction to groundwater needed to meet the TMDL is 195,200 lb-N/yr. Based on the totals of all the credits from BMAP actions and policies, the range of total reductions to groundwater is between 384,857 - 498,088 lb-N/yr (see Table 6).
To achieve reductions outside the scope of the policies listed, additional project options are available to local entities but have not been planned. Other efforts could be pursued to further reduce the nitrogen load to groundwater in the basin. 
[bookmark: _Toc514421084][bookmark: _Hlk491178190]Table 6. Summary of potential credits for the Weeki Wachee BMAP to meet the TMDLs
Note: No reductions are estimated for atmospheric deposition sources
	Nitrogen Source
	Credits to Load to Groundwater (lb-N/yr)
	Description

	OSTDS
	195,668 - 285,977
	 Credits are based on lots of all sizes inside the PFA being remediated by either enhancing onsite system or connecting to sewer. An estimated 27,538 lb-N/yr have been provided as OSTDS remediation projects which may be on these lots or in the larger BMAP area. Any projects outside the PFA would add additional reductions to the estimates listed.

	UTF
	12,590
	DEP approved credits (6%) for public education activities as well as credits identified for stakeholder stormwater projects.

	STF
	5,342
	6% BMP credit for sports fields and 10% BMP credit for golf courses on STF load to groundwater, assuming 100% BMP implementation on golf courses and sports fields.

	FF
	24,590
	15% BMP credit on FF load to groundwater, assuming 100% owner-implemented BMPs on all fertilized lands.

	LW
	9,135
	10% BMP credit on LW load to groundwater, assuming 100% owner-implemented BMPs at all livestock facilities.

	WWTF
	33,058
	Achieved by BMAP WWTF policy if BMAP-wide (achieving 3 or 6 mg/L).

	WWTF - Decommission
	46,171
	Hernando County Spring Hill WRF Decommissioning Project (Project HC-20).

	WWTF – Biological Application
	53,272
	Pasco County Crews Lake Restoration Project (Project PC-02).

	Total Credits from BMAP Policies and Submitted Projects
	379,826 - 470,134
	

	Advanced Ag BMPs
	5,032 – 27,954
	Pursue additional practices over next 20 years. 


	Total Credits
	384,857 - 498,088
	Estimated load reduction to meet TMDL is 195,200 lb-N/yr.



[bookmark: _Toc514419745]OSTDS Management Strategies
Overall there are currently around 35,000 OSTDS in the PFA, based on FDOH estimates. This BMAP lists 5 specific projects (Appendix B) that reduce nitrogen loading from existing OSTDS on variably sized parcels by a total of 27,538 lb-N/yr. Figure 3 shows the locations of all OSTDS in the BMAP area. 
[bookmark: _Hlk512518617][bookmark: _Hlk512519325]In addition to the 5 listed projects, DEP assessed the overall OSTDS loading compared with other nitrogen sources in the PFA, as well as the relative loading in the wide BMAP area. Based on these assessments, DEP has determined that for the Weeki Wachee BMAP area, OSTDS contribute 30 % pollutant loading in the springshed area and approximately 44 % of the nitrogen loading in the PFA. Cumulatively, nitrogen loading from OSTDS within this springshed result in the significant degradation of groundwater that impacts the Weeki Wachee BMAP area. Therefore, the comprehensive remediation of OSTDS, consistent with the requirements of this BMAP, is necessary to prevent associated groundwater and surface water contamination so that the TMDLs can ultimately be achieved and so that increases in nitrogen loads from future growth are limited. The OSTDS remediation plan is incorporated as Appendix D.
[image: ]
[bookmark: _Ref488396361][bookmark: _Toc512092351][bookmark: _Toc512092706][bookmark: _Toc514421545]Figure 3. Locations of OSTDS in the Weeki Wachee BMAP area
[bookmark: _Hlk514257578]In addition to the actions outlined in the OSTDS remediation plan (incorporated into this BMAP as Appendix D), remedial efforts on existing conventional OSTDS could achieve nitrogen reductions. Table 7 summarizes the nitrogen inputs, attenuation and recharge factors, and loads to groundwater for a conventional OSTDS. The conventional OSTDS nitrogen input is based on a per capita contribution of 9.012 lb-N/yr. This value is multiplied by the estimated number of people using the system and additional information on the amount of time spent away from home by the school-age population and labor force (2.08 effective persons per household on average in counties within the BMAP). Percent reductions for enhanced or replaced systems are applied to the conventional OSTDS nitrogen groundwater loads to valuate possible improvements to groundwater. Enhanced OSTDS can achieve an estimated 65 % improvement in the load to groundwater compared to a conventional system. OSTDS replaced by sewer reduce the conventional nitrogen inputs by an estimated 95 %, assuming a sewer connection to a WWTF meeting AWT levels.
The results show an estimated nitrogen reduction (i.e., credit) of 5.5 in high recharge areas, 3.0 in medium recharge areas, and 0.6 in low recharge areas for each enhanced OSTDS and an estimated nitrogen reduction of 8.0 in high recharge areas, 4.5 in medium recharge areas, and 0.9 in low recharge areas for each replaced OSTDS. Estimated costs for retrofitting (onsite treatment improvements) or removing (sewering) OSTDS range from $10,000 to $20,000 per system, which would be anticipated to be offset somewhat by cost-share from state funds. These costs can be refined as projects are completed and detailed cost data are available.
[bookmark: _Toc514421085]Table 7. Estimated individual OSTDS improvements to groundwater  
	Recharge Category
	Conventional OSTDS Load To Groundwater (lb-N/yr/OSTDS)
	Reduction To Groundwater 
(lb-N/yr/OSTDS)

	
	
	Enhanced OSTDS 
	Replaced OSTDS

	Nitrogen Input 
	19
	‒
	‒

	Attenuation (0.5)
	9.4
	‒
	‒

	Low Recharge (0.1)
	0.9
	0.6
	0.9

	Medium Recharge (0.5)
	4.7
	3.0
	4.5

	High Recharge (0.9)
	8.4
	5.5
	8.0


[bookmark: _Toc490754468][bookmark: _Toc514419746]UTF Management Strategies
UTF consists of fertilizers applied to the turfgrass typically found in residential and urban areas (including residential lawns and public green spaces). It is applied by either the homeowner or a lawn service company on residential properties, while on nonresidential properties they may be applied by contractors or maintenance staff. 
Fertilizer Ordinance Adoption
As required by the Florida Legislature, as described in Subsection 373.807(2), F.S., local governments with jurisdictional boundaries that include an OFS or any part of a springshed or delineated PFA of an OFS, are required to develop, enact, and implement a fertilizer ordinance by July 1, 2017. The statutes require any ordinance to be based, at a minimum, on the DEP model ordinance for Florida-friendly fertilizer use on urban landscapes. 
Prioritized Management Strategies and Milestones
Based on the fertilizer ordinances and public education activities in place at the time of BMAP adoption, the associated credits for UTF reductions to groundwater are 4,090 lb-N/yr (see Table 8). Additional environmental benefits could be credited if the counties and municipalities implement other public education efforts and source control ordinances, as described below.
Local stormwater projects that treat urban runoff, including nitrogen from urban fertilizer are also in place (see Appendix B) for a total estimated reduction to groundwater of 1,140 lb-N/yr.
[bookmark: _Toc505866872][bookmark: _Toc512092914][bookmark: _Toc514421086]Table 8. Current project credits to reduce UTF loading to groundwater
	Project Category
	Project Credits (lb-N/yr) Based on Management Actions in Appendix B

	Fertilizer Ordinances and Public Education Activities
	4,090

	Stormwater Improvements
	1,140

	Total Project Credits
	5,230


Since there is uncertainty about the data used in the NSILT to calculate the UTF loading to groundwater, DEP will work toward collecting better data by documenting reductions with the stakeholders. Also, DEP will work with stakeholders to develop additional measures to reduce fertilizer application.
The anticipated reduction from UTF sources is currently limited to 6 % of the estimated load to groundwater. This reduction can be achieved through a 6 % total credit if each local government has an applicable fertilizer ordinance, landscape ordinance, irrigation ordinance, and pet waste ordinance; carries out public education activities; and implements the Florida Yards and Neighborhood (FYN) Program (see Table 9). 
If all the local governments implement the full suite of public education measures, a 12,590 lb-N/yr reduction can be achieved. Currently, local government public education credits total 4,090 lb-N/yr. Thus, an additional 8,500 lb-N/yr reduction could be achieved through public education and source control efforts.






[bookmark: _Toc514421087]Table 9. Maximum UTF load reductions based on existing public education credit policies
	Urban Turfgrass Source Control Measures
	Credit Based on Estimated Load to Groundwater 
(%)
	Possible Nitrogen Credits (lb-N/yr)

	Fertilizer Ordinance
	0.5
	1,049

	Pet Waste Ordinance
	0.5
	1,049

	Landscape Ordinance
	0.5
	1,049

	Irrigation Ordinance
	0.5
	1,049

	FYN Program
	3.0
	6,295

	Public Education Program
	1.0
	2,098

	Total Possible Credits
	6.00
	12,590



[bookmark: _Toc514419747]STF Management Strategies
Sports turfgrass areas fall into two main categories that are evaluated separately: golf courses and sporting facilities (such as baseball, football, soccer, and other fields). There are 14 golf courses covering 1,723 acres in the BMAP area that are the main source of the load to groundwater in this source category. The majority of the golf course acreage is located in high recharge areas (1,703 acres. Sporting facilities account for 88 acres in the BMAP area and are all located in high recharge areas. 
Prioritized Management Strategies and Milestones
DEP will work with sports field managers and golf course superintendents to ensure relevant BMP implementation and to estimate reductions associated with these efforts. To improve the golf course loading estimate over a literature-based approach, DEP will also confer with golf course superintendents to identify the actual rate of fertilizer application to update the estimate of the golf course load to groundwater. Golf courses are expected to implement the BMPs described in the DEP BMP manual, Best Management Practices for the Enhancement of Environmental Quality on Florida Golf Courses for an estimated 10 % reduction in loads to groundwater.
Managers of sports fields can assist by reducing fertilizer use, using products that reduce leaching, and more efficiently irrigating sports turf. The estimated credit for better management of nongolf sports turfgrass is 6 % of the starting load to groundwater. Based on these approaches, the initial estimates of reductions from STF sources is 5,342 lb-N/yr, as listed in Table 10. 
[bookmark: _Toc505866873][bookmark: _Toc512092915]




[bookmark: _Toc514421088]Table 10. Maximum load reductions from STF improvements based on existing credit policies
	STF Source Control Measures
	Credit Based on Estimated Load to Groundwater (%)
	Possible Nitrogen Credits (lb-N/yr)

	Golf Course BMP Implementation
	10
	5,280

	Sports Fields BMPs
	6
	62

	Total Possible Credits
	
	5,342


[bookmark: _Ref488222106][bookmark: _Toc514419748]Agricultural Sources Management Strategies
Based on the data provided by FDACS, there are 45,701 acres of agricultural land in the BMAP area:  4,738 acres are identified as crop fertilizer lands, 9,391 acres as livestock lands, and 31,572 acres are identified as both crop fertilizer lands and livestock lands.
FF Loading
Nitrogen in agricultural fertilizer is applied at varying rates, depending on the crop and individual farm practices. The NSILT estimated total nitrogen load to groundwater from FF is 163,935 lb-N/year, or 17 % of the total nitrogen load to groundwater in the BMAP area.
LW
Agricultural practices specific to this livestock management were obtained through meetings with University of Florida Institute of Food and Agricultural Sciences (UF-IFAS) extension staff, FDACS field representatives, agricultural producers, and stakeholders. The NSILT estimated total nitrogen load to groundwater from LW is 91,347 lb-N/year, or 10 % of the total nitrogen load to groundwater in the BMAP area.
Prioritized Management Strategies and Milestones
Subsection 403.067, F.S., requires agricultural nonpoint sources in a BMAP either to implement the applicable FDACS-adopted BMPs, which provides a presumption of compliance with water quality standards, or conduct water quality monitoring prescribed by DEP or SWFWMD that demonstrates compliance with water quality standards. 
Within BMAP areas, the Florida Springs and Aquifer Protection Act, Subsection 373.811(5), F.S., requires that any new agricultural operations must implement one of the following: applicable BMPs, measures necessary to achieve pollution reduction levels established by DEP, or a WMD- or DEP-approved groundwater monitoring plan. Failure to do so may result in enforcement action by DEP.
FDACS will work with applicable producers within the BMAP area to ensure enrollment and, within the first five-year period, verify implementation of BMPs.  In addition, FDACS will undertake projects such as precision irrigation, soil moisture probes, and cover crop planting, contingent on the availability of funds for cost-share. As of December 31, 2017, there are Notices of Intent (NOIs) to implement BMPs covering 15,349 acres in the Weeki Wachee BMAP area. No producers are conducting water quality monitoring in lieu of implementing BMPs at this time. Appendix B lists project information. Appendix G provides detailed information on BMPs and agricultural practices in the BMAP area. 
[bookmark: _Hlk490054521]With crop-specific BMP enrollment or monitoring for FF areas, an estimated 24,590 lb-N/yr reduction to groundwater can be achieved by owner-implemented crop-specific BMPs, based on an average reduction of 15 % in the nitrogen load to groundwater. While DEP has listed larger percentage reductions in nitrogen from agricultural BMPs in estimating benefits to surface waters, the best data available indicate a 15 % reduction in the load to groundwater, where owner-implemented BMPs are in place. This number could increase as more data are collected on the impact of BMPs to groundwater.
For livestock operations, owner-implemented BMPs are expected to achieve a reduction of 9,135 lb-N/yr, using an estimated 10 % reduction in the load to groundwater from owner-implemented BMPs at livestock operations. 
Summarizing the reductions discussed above, the total reduction from BMP implementation of all agricultural sources is 33,725 lb-N/yr.  
Additional Agricultural Reduction Options
Further reductions can be achieved through implementing additional agricultural projects or practices, including land acquisition and conservation easements. SWFWMD is implementing projects to encourage low input agriculture and water quality improvement technologies. Examples of these projects include providing incentives for producers to transition to less intensive cropping systems, changing land use to fallow or native landscape, or changing the type of cropping system. Other reductions associated with the implementation and modification of BMPs may be realized through ongoing studies and data collection. Basin-specific studies are underway to evaluate and demonstrate the effectiveness of BMPs on a site-specific basis. 
Additional reductions may also be achieved through implementing additional agricultural projects and practices. Table 11 lists these projects and practices with their estimated load reductions, based on existing crop types. FDACS supplied the acreages, load reductions associated with applicable practices, and estimated the costs of implementation. 








[bookmark: _Toc514421089]Table 11. Estimated reductions for additional agricultural projects or practices
	Action
	Acreage
	Reduction Credit for High Recharge Area
(lb-N/yr)
	Reduction Credit for Medium Recharge Area
(lb-N/yr)
	Cost

	Controlled Release Fertilizer
	1,382
	373
	2,073
	$24,870

	Cover Crops
	1,021
	827
	4,595
	$45,953

	Precision Fertilization
	2,617
	1,697
	9,427
	$306,148

	Precision Irrigation
	1,882
	120
	667
	$839,555

	Soil Moisture Probes
	3,006
	2,015
	11,192
	$210,000

	Total
	9,908
	
	
	$1,426,526


The projects and practices listed in Table 11 are a component of the reductions to groundwater that could be achieved through changes in practices (Table 12). For example, a 75 % reduction of fertilizer loss to groundwater on 25 % of the fertilized lands would result in an estimated reduction of 30,738 lb-N/yr. Note that these estimates are averaged over the entire basin, and the recharge characteristics of a specific site and the fertilization practices for specific crops may change the estimated reduction for specific acres with a conservation easement or change in fertilization.
[bookmark: _Toc514421090]Table 12. Calculations for additional load reductions to groundwater
	% of Fertilized Acres with a Change in Practice
	Amount of Fertilized Acres with a Change in Practice
	100%
Reduction in Load to Ground-water 
(lb-N/yr reduced)
	75% Reduction in Load to Ground-water
 (lb-N/yr reduced)
	50% Reduction in Load to Ground-water 
(lb-N/yr reduced)
	25% Reduction in Load to Ground-water 
(lb-N/yr reduced)
	10% Reduction in Load to Ground-water 
(lb-N/yr reduced)

	100
	36,111
	163,935
	122,951
	81,968
	40,984
	16,394

	75
	27,083
	122,951
	92,213
	61,476
	30,738
	12,295

	50
	18,056
	81,968
	61,476
	40,984
	20,492
	8,197

	25
	9,028
	40,984
	30,738
	20,492
	10,246
	4,098

	10
	3,611
	16,394
	12,295
	8,197
	4,098
	1,639


Additional reductions in agricultural loading may be achievable based on the results of ongoing research. Current research areas include increased reductions associated with BMP implementation, up to a 30 % reduction for fertilized crops, the installation of nitrate recovery wells and bioreactors, and increased reductions associated with widespread rotational production and cover crop planting.
Beyond enrolling producers in the FDACS BMP Program and verifying implementation, FDACS will work with DEP to improve the data used to estimate agricultural land uses in the springshed. FDACS will also work with producers to implement a suite of agricultural projects and research agricultural technologies on properties where they are deemed technically feasible and if funding is made available. The acreages provided by FDACS are preliminary estimates of the maximum acreages and will be evaluated and refined over time. As presented here, these projects are based on planning-level information. Actual implementation would require funding as well as more detailed designs based on specific information, such as actual applicable acreages and willing landowners.
[bookmark: _Toc514419749]WWTF Management Strategies
WWTFs receive and treat domestic wastewater. In the Weeki Wachee BMAP area, treated effluent containing nitrogen is discharged to sprayfields, RIBs, and percolation ponds, and is reused for irrigation water. The estimated nitrogen load from WWTFs is 45,105 lb-N/year. The discharge location (such as proximity to the spring, highly permeable soils, etc.) and level of wastewater treatment are important factors to consider when calculating loadings to groundwater. Additionally, addressing the nitrogen loading from OSTDS could increase the volume of effluent treated and disposed of by WWTFs.
Summary of Facilities
There are 23 domestic WWTFs located in the Weeki Wachee BMAP area, including 7 WWTFs permitted to discharge more than 100,000 gallons of treated effluent per day (or 0.1 million gallons per day [mgd]). Figure 4 shows the locations of WWTFs in the Weeki Wachee Basin with discharges greater than 0.1 mgd and those with discharges less than 0.1 mgd.
[image: ]
[bookmark: _Ref488221949][bookmark: _Toc512092352][bookmark: _Toc512092707][bookmark: _Toc514421546]Figure 4. Locations of WWTFs in the Weeki Wachee BMAP Area
[bookmark: _Ref488221585]Wastewater Management Standards and Reuse Management
The Florida Springs and Aquifer Protection Act prohibits new domestic wastewater disposal facilities in the PFA, including RIBs, with permitted capacities of 100,000 gpd or more, except for facilities that provide AWT that reduces total nitrogen in the effluent to 3 mg/L or lower, on an annual permitted basis. 
To provide regulatory consistency in the BMAP area and to further improve wastewater management to protect the Weeki Wachee Basin, DEP requires the nitrogen effluent limits listed below in any new or existing wastewater permit, unless the utility/entity can demonstrate reasonable assurance that the reuse or land application of effluent would not cause or contribute to an exceedance of the nitrate concentrations established by the Weeki Wachee Spring Group, Magnolia-Aripeka Springs Group, Wilderness-Mud-Salt Springs Group, and Jenkins Creek Spring TMDLs. To demonstrate reasonable assurance, the utility/entity shall provide relevant water quality data, physical circumstances, or other site-specific credible information needed to show their facility would not cause a nitrate concentration that would be greater than 0.28 mg/L at the Weeki Wachee spring vents and 0.23 mg/L at the Magnolia-Aripeka spring vents. This demonstration may include factors such as dilution, site-specific geological conditions, research/studies, including dye tracer tests, and groundwater transport modeling. Should DEP concur with the reasonable assurance demonstration request, the TN effluent requirements established here may be modified for the applicant or waived. 
The nitrogen effluent limits set forth in Table 13 will be applied as an annual average to all new and existing WWTFs with a DEP-permitted discharge. New effluent standards will take effect at the time of permit renewal or no later than five years after BMAP adoption, whichever is sooner.
[bookmark: _Toc505866874][bookmark: _Toc512092916][bookmark: _Toc514421091]Table 13. Wastewater effluent standards for the BMAP area
	
95% of the Permitted Capacity (gpd)
	TN Concentration Limits for RIBs and Absorption Fields (mg/L)
	TN Concentration Limits for All Other Land Disposal Methods, Including Reuse (mg/L)

	Greater than 100,000
	3
	3

	20,000 to 100,000
	3
	6

	Less than 20,000
	6
	6


Additionally, new or existing wastewater permits in the BMAP area must require at least quarterly sampling of the effluent discharge for TN and must report these sampling results in the discharge monitoring reports (DMRs) submitted to DEP. 
[bookmark: _Ref488221570]DEP encourages the reuse of treated wastewater for irrigation as a water conservation measure. The expansion of reuse water for irrigation can reduce reliance on the Floridan aquifer for water supply. The nitrogen load to groundwater from reuse water is expected to be reduced through these WWTF policies, as improvements in reuse water quality will both reduce loads from this source and limit future increases in loading from reuse because of higher treatment levels.
Prioritized Management Strategies and Milestones
Based on the current volumes of discharge and effluent concentrations, the estimated reductions to be achieved through the implementation of these revised wastewater standards are 33,058 lb-N/yr. Appendix B contains detailed information on projects that have been completed, are underway, or are planned to reduce nitrogen loading from WWTFs. 
Two WWTF projects identified in Appendix B, Hernando County's Decommissioning of the Spring Hill Water Reclamation Facility (WRF) (Project HC-20) and Pasco County's Crews Lake Natural Systems Restoration Project (Project PC-02), are estimated to achieve reductions of 46,171 lb-N/yr and 53,272 lb-N/yr, respectively.
[bookmark: _Ref488221078][bookmark: _Toc514419750]Atmospheric Deposition Management Strategies
Summary of Loading
Atmospheric deposition is largely a diffuse, albeit continual, source of nitrogen. Nitrogen species and other chemical constituents are measured in wet and dry deposition at discrete locations around the U.S. In 2014, Schwede and Lear developed a hybrid model for estimating the total atmospheric deposition of nitrogen and sulfur for the entire U.S., referred to as "TDEP." Deposition data from several monitoring networks—including the Clean Air Status and Trends Network (CASTNET), the National Atmospheric Deposition Program (NADP) Ammonia Monitoring Network, the Southeastern Aerosol Research and Characterization Network, and modeled data from the Community Multiscale Air Quality (CMAQ) Modeling System—are combined in a multistep process with National Trends Network (NTN) wet deposition values to model total deposition. The TDEP model run used for the NSILT included data from 2011 to 2013. 
Description of Approach
Atmospheric sources of nitrogen are local, national, and international. Atmospheric sources are generally of low nitrogen concentration compared with other sources and are further diminished through additional biological and chemical processes before they reach groundwater. Atmospheric deposition sources and trends will be re-evaluated periodically. 
[bookmark: _Toc514419751]Future Growth Management Strategies
Local land development regulations, comprehensive plans, ordinances, incentives, BMPs, environmental resource permit requirements, and consumptive use permit limits provide mechanisms for protecting water resources and reducing the impact of new development and other land use changes as they occur. They are the primary mechanisms available to address additional nitrogen loadings from urban and agricultural growth. Future agricultural operations will be subject to the same requirements as existing operations with regard to the implementation of FDACS-adopted BMPs (Section 2.7). 
The associated increased load from OSTDS to groundwater must also be addressed in addition to the current loads. Future development on lots less than one acre in the PFA must connect to central sewer, if available, or include nitrogen-reducing OSTDS as described in Appendix D. This BMAP recognizes local protections described in Appendix H as important components of the BMAP and encourages local governments to further strengthen local watershed protection frameworks. 
[bookmark: _Toc514419752]Protection of Surface Water and Groundwater Resources through Land Conservation
Maintaining land at lower intensity uses through land purchases or easements for conservation and recreational use is one strategy that can help reduce water quality impacts in the Weeki Wachee Basin. Table 14 identifies land conservation purchases in the BMAP area since 2012, which is the last year of the period of record used for developing the Weeki Wachee TMDLs. 
[bookmark: _Toc505866875][bookmark: _Toc512092917]





[bookmark: _Toc514421092]Table 14. Stakeholder conservation land purchases
TBD = To be determined
	
Lead Entity
	Name of Conservation Purchase
	Description
	Purchase Status
	Cost
	Acreage Acquired
	Year Acquired

	Pasco County
	Jumping Gully/Crews Lake Phase I
	Protect identified ecological corridor between Starkey Wilderness Park and Cross Bar Ranch.
	Completed
	$6,600,000
	1,600
	2015

	Pasco County
	Aripeka Heights
	Coastal Ecological Planning Unit
	Completed
	$2,400,000
	210
	2012

	Pasco County
	Jumping Gully/Crews Lake Phase II
	Protect identified ecological corridor between Starkey Wilderness Park and Cross Bar Ranch.
	Planned
	$1,100,000
	100
	2017

	Pasco County
	Connerton to Cross Bar
	Protect identified ecological corridor between Connerton and Cross Bar.
	Planned
	TBD
	800
	TBD

	Pasco County
	Coastal Ecological Planning Unit
	Conservation program to acquire land identified along the coast.
	Planned
	TBD
	TBD
	TBD

	Hernando County
	Norfleet Property
	Provide a greenway corridor connection from Hernando County to Pasco County that conserves habitat and listed species, buffers a spring run and coastal spring, minimizes flood hazards, and maintains natural stormwater treatment for Hammock Creek.
	Planned
	$250,000
	60
	TBD

	SWFWMD
	Boat Spring
	Protect the water resources of the Hammock Creek system, link existing SWFWMD ownerships, and enhance the natural systems of the Weeki Wachee Preserve
	Completed
	$1,370,000
	81
	2015


[bookmark: _Toc514419753]Commitment to Implementation
Successful BMAP implementation requires commitment, dedicated state funding, and follow-up. Stakeholders have expressed their intention to carry out the plan, monitor its effects, and continue to coordinate within and across jurisdictions to achieve nutrient reduction goals. As the TMDLs must be achieved within 20 years, DEP, FDACS, and SWFWMD will implement management actions with a portion of the annual $50 million state appropriations to reduce nitrogen in the Weeki Wachee Basin. 


[bookmark: _Ref296955766][bookmark: _Toc475022072][bookmark: _Toc514419754]
: Monitoring and Reporting
[bookmark: _Toc514419755]Methods for Evaluating Progress
[bookmark: _Toc408412586][bookmark: _Toc408412610][bookmark: _Toc475022074]DEP will work with stakeholders to track project implementation and organize the monitoring data collected each year. The project and monitoring information will be presented in an annual update. Stakeholders have agreed to meet annually after the adoption of the BMAP to follow up on plan implementation, share new information, and continue to coordinate on TMDL restoration related issues. The following activities may occur at annual meetings:
Implementation data and reporting:
Collect project implementation information from stakeholders, including FDACS agricultural BMP enrollment and FDOH-issued permits, and compare with the BMAP schedule.
Discuss the data collection process, including any concerns and possible improvements to the process.
Review the monitoring plan implementation, as detailed in Section 3.3.
Sharing new information:
Report on results from water quality monitoring and trend information.
Provide updates on new management strategies in the basin that will help reduce nutrient loading.
Identify and review new scientific developments on addressing nutrient loads and incorporate any new information into annual progress reports.
Coordinating on TMDL restoration-related issues:
Provide updates from DEP on the basin assessment cycle and activities related to any impairments, TMDLs, and BMAP.
Obtain reports from other basins where tools or other information may be applicable to the Weeki Wachee Spring Group, Magnolia-Aripeka Springs Group, Wilderness-Mud-Salt Springs Group, and Jenkins Creek Spring TMDLs.
[bookmark: _Toc514419756]Adaptive Management Measures
[bookmark: _Ref438641467][bookmark: _Toc419968101][bookmark: _Toc444867141]Adaptive management involves making adjustments in the BMAP when circumstances change or monitoring indicates the need for additional or more effective restoration strategies. Adaptive management measures may include the following: 
Implementing procedures to determine whether additional cooperative strategies are needed.
Using criteria/processes for determining whether and when plan components need revision because of changes in costs, project effectiveness, social effects, watershed conditions, or other factors.
Revising descriptions of stakeholders' roles during BMAP implementation and after BMAP completion.
Updating information on corrective actions (and any supporting documentation) being implemented as data are gathered to refine project implementation schedules and performance expectations.
Key components of adaptive management to share information and expertise are tracking plan implementation, monitoring water quality and pollutant loads, and holding periodic meetings. 
[bookmark: _Ref488242948][bookmark: _Toc514419757]Water Quality and Biological Monitoring
Objectives
Focused objectives are critical for a monitoring strategy to provide the information needed to evaluate implementation success. Since the BMAP implementation involves an iterative process, the monitoring efforts are related to primary and secondary objectives. The primary objectives focus on achieving water quality targets, while the secondary objectives focus on water quality parameters that can be used to provide information for future refinements of the BMAP. The monitoring strategy may be updated as necessary.
Primary objectives:
Measure the water quality and biological response in the impaired springs, river, and/or groundwater at the beginning of the BMAP period and during implementation.
Document nutrient trends in the Weeki Wachee Basin and associated springs and groundwater.
Focus BMP efforts by using water quality results combined with appropriate project information and land use in conjunction with statistical and spatial analysis tools.
Secondary objectives:
Identify areas where groundwater data and modeling might help in understanding the hydrodynamics of the system.
Confirm and refine nutrient removal efficiencies of agricultural and/or urban BMPs.
Identify and implement more effective nutrient reduction strategies.
Use nitrogen isotope and tracer sampling for evaluating nitrogen contributions from organic and inorganic sources.
Water Quality Parameters, Frequency, and Network
[bookmark: _Ref488243023][bookmark: _Hlk490732735]To achieve the objectives listed above, the monitoring strategy focuses on two types of indicators to track improvements in water quality: core and supplemental (Tables 15 and 16, respectively). The core indicators are directly related to the parameters causing impairment in the river or associated springs. Supplemental indicators are monitored primarily to support the interpretation of core water quality parameters. The monitoring network is established for a variety of purposes.
For this BMAP, nitrate is considered to be the key core parameter measured, to track progress in decreasing nitrogen concentrations in groundwater and the water flowing from the spring vent. The other parameters are considered supplementary parameters for the BMAP, as they build information about groundwater and the spring but are not direct measurements of impairment.
At a minimum, the core parameters will be tracked to determine the progress made towards meeting the TMDLs and/or achieving the numeric nutrient criteria (NNC). Resource responses to BMAP implementation may also be tracked. A significant amount of time may be needed to observe changes in water chemistry. 
[bookmark: _Toc505866882][bookmark: _Toc512092924][bookmark: _Toc514421093]Table 15. Core water quality indicators and field parameters
	Core Parameters

	Chloride

	Sulfate

	Potassium

	Ammonia as Nitrogen

	Total Kjeldahl Nitrogen

	Nitrate/Nitrite as Nitrogen


[bookmark: _Ref488243039]
[bookmark: _Toc505866883][bookmark: _Toc512092925][bookmark: _Toc514421094]Table 16. Supplemental water quality indicators and field parameters
	Supplemental Parameters

	Specific Conductance

	Dissolved Oxygen (DO)

	pH

	Temperature

	Total Suspended Solids (TSS)

	Nitrate and Oxygen Isotopes


[bookmark: _Ref488243068]
Initially, data from the ongoing sampling effort being conducted by SWFWMD will be used to meet the primary objectives. Surface water and groundwater monitoring network locations were selected to track changes in water quality and allow the annual evaluation of progress toward achieving the TMDL. Figure 5 shows the location of the river and spring stations currently being sampled that will be used for the BMAP monitoring in the Weeki Wachee Basin.
[image: ]
[bookmark: _Ref488243124][bookmark: _Toc512092353][bookmark: _Toc512092708][bookmark: _Toc514421547]Figure 5. Groundwater and surface water stations sampled in the Weeki Wachee Basin
Biological Monitoring
Biological resource responses represent improvements in the overall ecological health of the Weeki Wachee Basin (see Table 17).
[bookmark: _Toc514421095]Table 17. Anticipated resource responses from BMAP implementation
	Resource Responses

	Increase in Stream Condition Index (SCI) score

	Increase in Linear Vegetation Survey (LVS) score

	Increase in Rapid Periphyton Survey (RPS) score

	Increase in key fish populations



An RPS will be conducted to assess the abundance and variety of algae in the river. An LVS will be conducted to assess the types and density of vegetation present in the river and to identify the native versus non-native species. An SCI will be conducted to measure the number of different organisms present in the river. In addition, habitat assessments (HAs) will be conducted to assess the river conditions and habitat present to support the SCI evaluation. Water quality samples will also be collected with the biological monitoring.
Data Management and Assessment
As of June 30, 2017, water quality data in Florida are entered by the entity collecting the data into the Florida Watershed Information Network (WIN) Database, which has replaced the Florida Storage and Retrieval System (STORET). DEP pulls water quality data directly from WIN for impaired waters evaluations and TMDL development. Data providers are required to upload their data regularly, so the information can be used as part of the water quality assessment process and for annual reporting. Data providers should upload their data to WIN, upon completion of the appropriate quality assurance/quality control (QA/QC) checks. All data collected in the last quarter of the calendar year should be uploaded no later than April 1 of the following year.
Biological data are stored in the DEP Statewide Biological (SBIO) Database. Biological data collected by data providers should also be uploaded regularly, after the appropriate QA/QC checks. All biological data collected in the last quarter of the calendar year should be uploaded no later than April 1 of the following year.
The water quality will be analyzed during BMAP implementation to determine trends in water quality and the health of the biological community. A wide variety of statistical methods are available for the water quality trend analyses. The selection of an appropriate data analysis method depends on the frequency, spatial distribution, and period of record available from existing data. Specific statistical analyses were not identified during BMAP development. 
QA/QC
Stakeholders participating in the monitoring plan must collect water quality data in a manner consistent with Chapter 62-160, F.A.C., and the DEP standard operating procedures (SOPs) for QA/QC required by rule. The most current version of these procedures is available on the DEP website. For BMAP-related data analyses, entities should use National Environmental Laboratory Accreditation Conference (NELAC) National Environmental Laboratory Accreditation Program (NELAP)–certified laboratories or other labs that meet the certification and other requirements outlined in the SOPs.

[bookmark: _Toc514419758]Appendices
[bookmark: _Ref488219549][bookmark: _Ref488219550][bookmark: _Toc514419759]Appendix A. Important Links
The links below were correct at the time of document preparation. Over time, the locations may change and the links may no longer be accurate. None of these linked materials are adopted into this BMAP.
· DEP Website: http://www.floridadep.gov 
· [bookmark: _Hlk496864162]DEP Map Direct Webpage: https://ca.dep.state.fl.us/mapdirect/
· Searchable online version of PFA maps: https://www.floridadep.gov/pfamap
· Florida Statutes: http://www.leg.state.fl.us/statutes
· Florida Watershed Recovery Act (Section 403.067, F.S.)
· Florida Springs and Aquifer Protection Act (Part VIII of Chapter 373, F.S.)
· DEP Model Ordinances: http://fyn.ifas.ufl.edu/fert_ordinances.html 
· DEP Standard Operating Procedures for Water Quality Samples: https://floridadep.gov/dear/quality-assurance/content/dep-sops  
· NELAC NELAP: https://fldeploc.dep.state.fl.us/aams/index.asp 
· FDACS BMPs: https://www.freshfromflorida.com/Business-Services/Best-Management-Practices-BMPs/Agricultural-Best-Management-Practices 
· FDACS BMP and Field Staff Contacts: http://www.freshfromflorida.com/Divisions-Offices/Agricultural-Water-Policy
· Florida Administrative Code (Florida Rules): https://www.flrules.org/ 
·  SWFWMD 2017 Weeki Wachee River Surface Water Improvement and Management SWIM Plan: http://www.swfwmd.state.fl.us/files/database/calendar/Weeki_Wachee_GB_FINAL_SWIM_Plan_v2.pdf
· SWFWMD Springs: http://www.swfwmd.state.fl.us/springs/
· SWFWMD Social Research: http://www.swfwmd.state.fl.us/projects/social_research/ 
· UF-IFAS Research: http://research.ifas.ufl.edu/ 


[bookmark: _Toc514419760]Appendix B. Projects to Reduce Nitrogen Sources
Prioritization of Management Strategies
The management strategies in Table B-1 are ranked with a priority of high, medium, or low. In 2016, the Florida Legislature amended the Watershed Restoration Act (Section 403.067, F.S.), creating additional requirements for all new or revised BMAPs. BMAPs must now include planning-level details for each listed project, along with their priority ranking. 
Project status was selected as the most appropriate indicator of a project’s priority ranking based primarily on need for funding. Projects with a "completed" status were assigned a low priority. Projects classified as "underway" were assigned a medium priority because some resources have been allocated to these projects, but additional assistance may be needed for the project to be completed. High priority was assigned to projects listed with the project status "planned" as well as certain "completed" projects that are ongoing each year (any project with one of these project types: "street sweeping," "catch basin inserts/inlet filter cleanout,"  "public education efforts," "fertilizer cessation," "fertilizer reduction," or "aquatic vegetation harvesting"), and select projects that are elevated because substantial, subsequent project(s) are reliant on their completion.
Description of the Management Strategies 
Responsible entities submitted these management strategies to the department with the understanding that the strategies would be included in the BMAP, thus requiring each entity to implement the proposed strategies in a timely way and achieve the assigned load reduction estimates.  However, this list of strategies is meant to be flexible enough to allow for changes that may occur over time. Any change in listed management strategies, or the deadline to complete these actions, must first be approved by the department. Substituted strategies must result in equivalent or greater nutrient reductions than expected from the original strategies.
While the 20-year planning period for this BMAP is 2018 to 2038, projects completed since January 1, 2013, count toward the overall nitrogen reduction goals. 
Estimated nitrogen reductions are subject to refinement based on DEP verification and/or on adjustment to calculations based on loading to groundwater rather than surface water. Agriculture load reductions (FDACS-01 and FDACS-02) assume 100 % enrollment and verification. Projects with a designation of TBD (to be determined) denotes information is not currently available, but will be provided by the stakeholder when it is available. Projects with a designation of N/A (not applicable) indicates the information for that category is not relevant to that project. Projects with a designation of "Not Provided" denotes that information was requested by DEP but was not provided by the lead entity.


[bookmark: _Toc505866885][bookmark: _Toc512092927][bookmark: _Toc514421155]Table B-1. Stakeholder projects to reduce nitrogen sources
*Denotes project that is applicable in another Springs Coast BMAP. The dollar amount is the total project amount (not split among the BMAPs).
	Lead Entity
	Project Number
	Project Name
	Project Description
	Project Type
	Project
Status
	Start Date
	Estimated Completion Date
	Nitrogen Source Addressed by Project
	Estimated Nitrogen Load Reduction (lb-N/yr)
	Cost Estimate
	Funding Source
	Funding Amount

	City of Brooksville
	COB-01
	Public Education Activities
	Adopt fertilizer ordinance in 2017; website, public service announcements, brochures, etc.
	Public Education
	Underway
	2017
	2018
	UTF
	22
	TBD
	County
	TBD

	City of Brooksville
	COB-02
	Septic to Sewer Conversion
	Connect approximately 75 septic systems to central sewer system.
	Wastewater Service Area Expansion
	Planned
	2019
	2021
	OSTDS
	TBD
	$1,400,000
	City/DEP
	TBD

	City of Brooksville
	COB-03
	Septic to Sewer Conversion
	Connect approximately 300 septic systems to central sewer system.
	Wastewater Service Area Expansion
	Planned
	2027
	2030
	OSTDS
	TBD
	$6,000,000
	City/DEP/Other
	TBD

	City of Brooksville
	COB-04
	Reuse Water to Hernando Oaks Golf Course
	Connect Brooksville reclaim transmission line to Hernando Oaks Golf Course for irrigation purposes.
	Reuse Project
	Planned
	2018
	2019
	STF
	TBD
	$490,000
	DEP
	DEP: $490,000

	Hernando County
	HC-01
	Package Plant Connection Project
	Connect several private wastewater package plants to the county's central wastewater collection system.
	Wastewater System Upgrade
	Underway
	2016
	2019
	WWTF
	Not Provided
	$3,689,270
	County/ DEP
	DEP: $3,432,970 County: $256,300

	Hernando County
	HC-02
	Oakley Island Sewer Infrastruc-ture
	Design, permit, and construct a municipal sewer system to eliminate 15 septic systems and connect the county park to the sewer system.
	Wastewater Service Area Expansion
	Underway
	2016
	2019
	OSTDS
	338
	$578,760
	County/ DEP
	DEP: $491,160 County: $87,600

	Hernando County
	HC-03
	Septic to Sewer Conversion Study
	Quantified and studied the feasibility of converting approximately 30,000 septic systems within 19 districts to central sewer in the Spring Hill area.
	Study
	Completed
	2016
	2017
	OSTDS
	N/A
	$240,000
	Fish & Wildlife Foundation/County
	Foundation$138,000       County: $102,000

	Hernando County
	HC-04
	District A - Phase I Septic to Sewer Conversion
	Convert 450 septic systems to central sewer.
	Wastewater Service Area Expansion
	Planned
	2019
	2021
	OSTDS
	5,500
	$10,000,000
	County/ DEP
	TBD

	Hernando County
	HC-05
	District A - Phase II Septic to Sewer Conversion
	Convert 450 septic systems to central sewer.
	Wastewater Service Area Expansion
	Planned
	2021
	2023
	OSTDS
	5,500
	$10,000,000
	County/ DEP
	TBD

	Hernando County
	HC-06
	District B - Phase I Septic to Sewer Conversion
	Convert 650 septic systems to central sewer.
	Wastewater Service Area Expansion
	Planned
	2023
	2026
	OSTDS
	8,100
	$14,000,000
	County/ DEP
	TBD

	Hernando County
	HC-07
	District B - Phase II Septic to Sewer Conversion
	Convert 660 septic systems to central sewer.
	Wastewater Service Area Expansion
	Planned
	2025
	2027
	OSTDS
	8,100
	$14,000,000
	County/ DEP
	TBD

	Hernando County
	HC-08
	Pine Island Park Septic to Sewer Conversion
	Convert 90 septic systems to central sewer.
	Wastewater Service Area Expansion
	Planned
	2018
	2020
	OSTDS
	TBD
	$2,135,960
	County/ DEP
	TBD

	Hernando County
	HC-09
	Mary's Fish Camp Septic to Sewer Conversion
	Convert 25 recreation vehicle lot septic systems to central sewer.
	Wastewater Service Area Expansion
	Planned
	2020
	2021
	OSTDS
	TBD
	$717,800
	County/ DEP
	TBD

	Hernando County
	HC-10
	U.S. 19 Reclaimed Water Transmission - Phase I
	This is the first phase of a reclaimed water main loop around western Hernando County. The project will initially provide 1.7 MGD of reclaimed water to the Timber Pines Subdivision and Golf Course, with future utilization up to 4.5 MGD.
	Wastewater System Upgrade
	Underway
	2016
	2018
	WWTF
	Reduction included in HC-20
	$12,000,000
	DEP/ SWFWMD/ County
	DEP: $6,000,000  County: $3,000,000 SWFWMD $3,000,000

	Hernando County
	HC-11*
	Reclaimed Water Master Plan Revision
	Revision to current reclaimed water plan to identify future growth and needed interconnections. The increased use of reclaimed water will reduce fertilizer application.
	Study
	Underway
	2016
	2018
	UTF
	N/A
	$150,000
	County/ SWFWMD
	SWFWMD $75,000   County: $75,000

	Hernando County
	HC-12
	Public Education Activities
	Adopted fertilizer ordinance; pet waste ordinance; website, brochures, public service announcements, etc.
	Public Education
	Completed
	2013
	2013
	UTF
	3,772
	Not Provided
	County
	County: $20,000

	Hernando County
	HC-13
	Drainage Retention Area Retrofits
	Conceptual planning for the retrofitting of 10 drainage retention areas within two miles of the Weeki Wachee Spring using biosorption activated media. Construction should occur in 2020 depending on funding.
	Wet Detention Pond
	Planned
	2017
	2021
	UTF
	200
	$750,000
	County/ DEP/ SWFWMD
	Not Provided

	Hernando County
	HC-14
	BMAP Manager
	Proposed position to be filled by a high-level staff person to lead all aspects of BMAP implementation for Hernando County. This position will be responsible for intergovernmental coordination with agencies to fulfill BMAP requirements.
	Other
	Planned
	2017
	2031
	Other
	N/A
	$150,000
	TBD
	TBD

	Hernando County
	HC-15
	South Brooksville BMP 5 Dauson Stormwater Project
	Construction of a stormwater pond providing water quality treatment and flood storage for runoff from untreated existing urban area.
	Wet Detention Pond
	Completed
	2012
	2014
	UTF
	179
	$498,625
	County/ SWFWMD
	SWFWMD$175,000 County: $323,625

	Hernando County
	HC-16
	South Brooksville BMP 6 Josephine Street Stormwater Project
	Construction of a stormwater pond providing water quality treatment and flood storage for runoff from untreated existing urban area.
	Wet Detention Pond
	Underway
	2015
	2018
	UTF
	36
	$612,000
	County/ SWFWMD
	SWFWMD$175,000 County: $437,000

	Hernando County
	HC-17
	South Brooksville BMP 7 Russell Street Stormwater Project
	Construction of a stormwater pond providing water quality treatment and flood storage for runoff from untreated existing urban area.
	Wet Detention Pond
	Underway
	2015
	2017
	UTF
	80
	$1,115,612
	County/ SWFWMD
	SWFWMD $475,000 County: $640,612

	Hernando County
	HC-18
	Peck Sink Preserve Stormwater Management Facility
	Construction of stormwater treatment train providing water quality pretreatment of surface discharges to Peck Sink.
	BMP Treatment Train
	Completed
	2010
	2014
	UTF
	Not Provided
	$3,200,000
	County/ SWFWMD/ DEP/ USDA
	Not Provided

	Hernando County
	HC-19
	Decommis-sioning of the Berkeley Manor WTF
	Diverting wastewater flow to Airport WWTP that achieves better nitrogen removal and demolishing the Berkeley Manor WTF.
	Wastewater Treatment Facility Upgrade
	Underway
	2012
	2017
	WWTF
	Not Provided
	$1,100,000
	County
	County: $1,100,000

	Hernando County
	HC-20
	Decommis-sioning of the Spring Hill Water Reclamation Facility (WRF)
	Diverting wastewater flow to other county treatment facilities that achieve better nitrogen removal and demolishing the Spring Hill WRF.
	Wastewater Treatment Facility Upgrade
	Planned
	2019
	2020
	WWTF
	46,171
	$11,277,000
	County
	County: 11,277,000

	Hernando County
	HC-21
	Airport WWTP Upgrade
	Add filtration and expand capacity; allow public access reuse.
	Wastewater Treatment Facility Upgrade
	Planned
	2020
	2022
	WWTF
	TBD
	$35,000,000
	County/ DEP
	TBD

	Hernando County
	HC-22
	Rogers Park Low Impact Development (LID) Improve-ments
	Design, permit, and construct stormwater improvements at Rogers Park to reduce sediment, nutrient, and other contaminant loads to the Weeki Wachee River.
	Low Impact Develop-ment
	Underway
	2014
	2018
	UTF
	12
	$525,000
	SWFWMD/Hernando Co
	SWFWMD$225,000  Hernando Co.: $300,000

	Hernando County
	HC-23
	Street Sweeping
	Street sweeping of 46 miles of urban roadways
	Street Sweeping
	Underway
	Not Pro-vided
	Not Provided
	UTF
	320
	$8,000
	County
	County: $8,000/yr

	Hernando County
	HC-24
	Septic Drain Field Enhancement Rulemaking
	Coordinate with the Florida Department of Health (FDOH) on rulemaking and permitting process for septic system enhancements.
	Other
	Planned
	2017
	2020
	OSTDS
	N/A
	TBD
	TBD
	TBD

	Hernando County
	HC-25
	Weeki Wachee Prairie Watershed Management Plan
	Completion of watershed management plan that included a stormwater level of service analysis, surface water resource assessment, and BMP alternative analysis.
	Studies
	Underway
	2015
	2017
	Other
	N/A
	$227,500
	County/ SWFWMD
	SWFWMD$165,000 County: $62,500

	Hernando County
	HC-26
	Peck Sink Watershed Master Plan
	Comprehensive watershed master plan to remedy water quality issues associated with stormwater runoff entering the Floridan aquifer via the Peck Sink complex in Hernando County.
	Studies
	Completed
	2002
	2017
	Other
	N/A
	$297,410
	SWFWMD/Hernando Co
	SWFWMD$242,410  Hernando Co.: $55,000

	Hernando County
	HC-27
	Powell Sink Watershed Master Plan
	Comprehensive engineering analysis, water quality assessment, watershed model development, and conceptual BMP designs.
	Studies
	Completed
	2014
	2016
	Other
	N/A
	$150,000
	SWFWMD/Hernando Co
	SWFWMD $75,000  Hernando Co.: $75,000

	Hernando County
	HC-28
	Spring Hill Lakes Resource Assessment and BMP Plan
	Comprehensive engineering analysis, water quality assessment, watershed model development, and conceptual BMP designs.
	Studies
	Underway
	2015
	2017
	Other
	N/A
	$200,000
	SWFWMD/Hernando Co
	SWFWMD $100,000  Hernando Co.: $100,000

	Hernando County
	HC-29
	Squirrel Prairie Resource Assessment and BMP Plan
	Comprehensive engineering analysis, water quality assessment, watershed model development, and conceptual BMP designs.
	Studies
	Underway
	2015
	2017
	Other
	N/A
	$200,000
	SWFWMD/Hernando Co
	SWFWMD$100,000  Hernando Co.: $100,000

	Hernando County
	HC-30
	Oman/Indian Creek Resource Assessment and BMP Plan
	Comprehensive engineering analysis, water quality assessment, watershed model development, and conceptual BMP designs.
	Studies
	Completed
	2013
	2015
	Other
	N/A
	$100,000
	SWFWMD/Hernando Co
	SWFWMD$50,000  Hernando Co.: $50,000

	Hernando County
	HC-31
	Willow Sink Watershed Master Plan
	Comprehensive engineering analysis, water quality assessment, watershed model development, and conceptual BMP designs.
	Studies
	Completed
	2013
	2015
	Other
	N/A
	$150,000
	SWFWMD/Hernando Co
	SWFWMD$75,000  Hernando Co.: $75,000

	Hernando County
	HC-32
	Wiscon Watershed Master Plan
	Comprehensive engineering analysis, water quality assessment, watershed model development, and conceptual BMP designs.
	Studies
	Completed
	2014
	2016
	Other
	N/A
	$150,000
	SWFWMD/Hernando Co
	SWFWMD$75,000  Hernando Co.: $75,000

	Hernando County
	HC-33
	High Point Stormwater Improvement
	Construction of a stormwater pond providing water quality treatment and flood storage for runoff from untreated existing residential area.
	Wet Detention Pond
	Completed
	2013
	2014
	UTF
	20
	$175,000
	County
	County: $175,000

	Hernando County
	HC-34
	Coastal Way Shopping District Parking Lot Water Quality Retrofit
	Retrofit a water quality system with enhanced nitrogen removal technology that serves an existing commercial district discharging into Weeki Wachee springshed.
	Wet Detention Pond
	Planned
	TBD
	2021
	UTF
	73
	$350,000
	TBD
	TBD

	Hernando County
	HC-35
	Brentlawn Street Enhanced Treatment Stormwater Improve-ments
	Construction of treatment train with enhanced nitrogen removal technology to provide water quality pretreatment of groundwater discharges to Weeki Wachee springshed.
	BMP Treatment Train
	Planned
	TBD
	2022
	UTF
	19
	$160,000
	TBD
	TBD

	Hernando County
	HC-36
	Harper Street Enhanced Treatment Stormwater Improve-ments
	Construction of treatment train with enhanced nitrogen removal technology to provide water quality pretreatment of groundwater discharges to Weeki Wachee springshed.
	BMP Treatment Train
	Planned
	TBD
	2022
	UTF
	89
	$80,000
	TBD
	TBD

	Pasco County
	PC-01
	Central Pasco County Beneficial Water Reuse Project
	Design, permit, and construct a wetland infiltration system that uses excess reclaimed water quality polishing and groundwater recharge. Up to 5 MGD of surplus reclaimed water will be delivered to the site with up to 1.6 MGD expected to infiltrate into the Upper Floridan aquifer.
	Reuse Project
	Underway
	2015
	2021
	Other
	Not Provided
	$13,224,955
	SWFWMD/County
	Not Provided

	Pasco County
	PC-02
	Crews Lake Natural Systems Restoration Project
	Construction of infrastructure providing reclaimed water and restoring approximately 200 acres of wetlands in and adjacent to Crews Lake. Nutrient flows that are currently delivered to the RIB complex will be diverted to the Crews Lake site where biological process will remove nitrogen to background levels.
	Other
	Underway
	2017
	2021
	WWTF
	53,272
	$8,497,770
	DEP/ SWFWMD/ County
	DEP: $4,248,885 SWFWMD $2,124,442  County: $2,124,443

	Pasco County
	PC-03
	Street Sweeping
	This project includes street sweeping in 500,000 square feet in collector roads, located within the springsheds. Six sweeping events a year.
	Street Sweeping
	Planned
	2019
	2021
	UTF
	100
	$10,000
	Pasco County
	County: $10,000

	Pasco County
	PC-04
	Public Education Activities
	Adopted fertilizer ordinance; website, brochures, public service announcements, etc.
	Public Education
	Completed
	2013
	2014
	UTF
	296
	Not Provided
	Pasco County
	Not Provided

	Pasco County
	PC-05
	Pet Waste Ordinance
	Pasco County staff intend to present the Board of County Commissioners a pet waste ordinance for adoption.
	Public Education
	Planned
	2019
	2021
	UTF
	TBD
	TBD
	Pasco County
	TBD

	Pasco County
	PC-06
	Heritage Pines Reclaimed Water Service
	Provide reclaimed water to 1,300 homes for residential irrigation.
	Reuse Project
	Completed
	2013
	2016
	UTF
	Not Provided
	$1,266,600
	DEP/ SWFWMD/ County
	DEP: $300,000 SWFWMD $333,300    County: $633,300

	FDACS
	FDACS-01
	Agricultural BMPs - Farm Fertilizer
	Implementation of existing BMPs on applicable acreage. Up to 15 % reduction in load to groundwater.
	BMPs
	Underway
	Underway
	TBD
	FF
	24,590
	TBD
	TBD
	TBD

	FDACS
	FDACS-02
	Agricultural BMPs - Livestock Waste
	Implementation of existing BMPs on applicable acreage. Up to 10 % reduction in load to groundwater.
	BMPs
	Underway
	Underway
	TBD
	LW
	9,135
	TBD
	TBD
	TBD

	 SWFWMD
	SWF-01
	Weeki Wachee SWIM Plan
	Implementation and periodic review and update of the Weeki Wachee SWIM Plan.
	Study
	Completed
	2015
	2017
	Other
	N/A
	$200,000
	SWFWMD
	SWFWMD $200,000

	SWFWMD
	SWF-02
	Weeki Wachee River Canoe Launch and Parking Area
	Stabilization of soils at the ramp entrance and improvements to the parking area near the launch to reduce stormwater pollutants entering the Weeki Wachee River.
	Shoreline Stabili-zation
	Completed
	2012
	2017
	UTF
	12
	$350,000
	SWFWMD
	SWFWMD $350,000

	SWFWMD
	SWF-03*
	Facilitating Agricultural Resource Management Systems (FARMS) Program
	The FARMS Program is an agricultural BMP cost-share program to promote improved water quality in spring systems through approved precision nutrient application technologies.
	BMPs
	Underway
	Prior to 2012
	2021
	FF
	Not Provided
	$6,000,000
	SWFWMD
	SWFWMD $6,000,000

	SWFWMD
	SWF-04*
	Evaluation of Nitrogen Leaching from Reclaimed Water
	This project will determine typical nitrogen leaching rates from reclaimed water application to lawns, spray fields, and rapid infiltration basins. This information can be used to refine estimates of nitrogen loading to the aquifer and springs, and identify the best reclaimed water disposal methods to minimize nitrogen loading to groundwater.
	Studies
	Underway
	2014
	2018
	UTF
	N/A
	$294,000
	SWFWMD
	SWFWMD $294,000

	SWFWMD
	SWF-05*
	Springs Coast Wastewater Disposal Treatment Wetlands
	This project will assess areas to determine sites appropriate for construction of wetlands to treat WWTF effluent.
	Studies
	Underway
	2014
	2017
	WWTF
	N/A
	$400,000
	SWFWMD
	SWFWMD $400,000

	UF-IFAS
	IFAS-01*
	Development of Landscape Fertilizer BMPs
	The objective of this project is to verify the accuracy of the Florida Yards and Neighborhoods (FYN) and Florida Green Industries BMPs fertilizer recommendations.
	Studies
	Underway
	2012
	2018
	UTF
	N/A
	$274,429
	SWFWMD
	SWFWMD $274,429

	UF-IFAS
	IFAS-02*
	Composting at Animal Stock Facilities
	Evaluate the nutrient removal efficiency from composting animal waste. The project will compare nutrient leaching efficiency for manure stockpiling and composting facilities
	Studies
	Underway
	2016
	2018
	LW
	N/A
	$175,000
	SWFWMD
	SWFWMD $175,000

	Golf Courses
	GC-01
	Golf Course Reduction Credits
	6% BMP credit on golf course load to groundwater, assuming 100% BMP implementation by golf course owners.
	BMPs
	Planned
	TBD
	TBD
	STF
	5,280
	TBD
	TBD
	TBD

	Sports Fields
	SF-01
	Sports Field Reduction Credits
	10% BMP credit on sports field load to groundwater, assuming 100% BMP implementation by sports field owners.
	BMPs
	Planned
	TBD
	TBD
	STF
	62
	TBD
	TBD
	TBD

	Wastewater Utilities
	WU-01
	Wastewater Treatment Facility Reduction Credits
	Achieved by WWTF policy if implemented BMAP-wide, achieving 3 or 6 mg/L.
	Wastewater Treatment Facility Upgrade
	Planned
	TBD
	TBD
	WWTF
	33,058
	TBD
	TBD
	TBD






[bookmark: _Toc514419761]Appendix C. Weeki Wachee PFA Report
A PFA (Weeki Wachee Spring, October 2016) is defined as the area(s) of a basin where the Floridan aquifer is generally most vulnerable to pollutant inputs and where there is a known connectivity between groundwater pathways and an OFS. As required by the Florida Springs and Aquifer Protection Act, DEP delineated a PFA for the Weeki Wachee Spring Group. This PFA is adopted and incorporated by reference into this BMAP. Information on this and other springshed PFAs is available in report format at the following link:
http://publicfiles.dep.state.fl.us/DEAR/BMAP/Adopted%20BMAPs/Weeki%20Wachee/PFA%20and%20GIS%20Files/


[bookmark: _Toc514419762]Appendix D.  OSTDS Remediation Plan
The Florida Aquifer and Springs Protection Act specifies that if during the development of a BMAP for an OFS, DEP identifies OSTDS as contributors of at least 20 % of nonpoint source nitrogen pollution in a PFA or if DEP determines remediation is necessary to achieve the TMDLs, the BMAP shall include an OSTDS remediation plan. Based on the Weeki Wachee NSILT and GIS coverages, OSTDS contribute approximately 44 % pollutant loading in the PFA. Irrespective of the percent contribution from OSTDS, DEP has determined that an OSTDS remediation plan is necessary to achieve the TMDLs and to limit the increase in nitrogen loads from future growth.
D.1	Plan Elements
D.1.1 Permits for Installation of New OSTDS
Per statute, new OSTDS on lots of less than one acre are prohibited within PFAs, if the addition of the specific systems conflicts with an OSTDS remediation plan incorporated into an OFS BMAP (see Section 373.811(2), F.S.). This OSTDS remediation plan prohibits installation of new conventional systems on lots of less than one acre within the PFA, unless the OSTDS includes enhanced treatment of nitrogen or unless the OSTDS permit applicant demonstrates that sewer connections will be available within 5 years. Local governments and utilities are encouraged to develop master wastewater treatment feasibility plans to identify specific areas to be sewered within 20 years of BMAP adoption. To aid in implementation, the DEP Map Direct webpage includes a detailed downloadable springs PFA boundary shapefile. DEP also maintains on its website an interactive map of the PFA and BMAP boundaries; the map can be easily searched for specific street address locations.
FDOH permits the installation of new OSTDS pursuant to Chapter 64E-6, F.A.C., which includes not only systems installed on a property where one has not previously been installed, but also systems installed to replace illegal systems, systems installed in addition to existing systems, and other new systems. FDOH permitting requirements with respect to the definition of "new" or "less than one acre" will be followed for this remediation plan. For FDOH to issue a permit for a new OSTDS on a lot of less than one acre within a PFA, the system must include at least one of the following nitrogen reducing enhancements:
· Features allowed pursuant to FDOH rule, such as in-ground nitrogen-reducing biofilters (media layer systems).
· Features consistent with and identified in the FDOH Florida Onsite System Nitrogen Removal Strategy Studies report, such as in-tank nitrogen-reducing biofilters.
· Other FDOH-approved treatment systems capable of meeting or exceeding the NSF Standard 245 nitrogen removal rate before disposing the wastewater in the drain field, such as aerobic treatment units (ATU) and performance-based treatment systems (PBTS). For FDOH-approved treatment systems that meet NSF 245, but do not meet or exceed the minimum treatment level expected from the in-ground nitrogen-reducing biofilters, the drain fields, at minimum, shall be installed with a 24-inch separation between the bottom of the drain field and the seasonal high-water table.
D.1.2 Permits for Modification or Repair of Existing OSTDS
Per statute, the OSTDS remediation plan must provide loading reductions consistent with achieving the TMDL within 20 years of plan adoption (see Section 373.807(1)(b)8., F.S.). This plan therefore establishes the following remediation policy for existing systems, based on (a) the potential for reducing nitrogen loads by converting existing OSTDS to enhanced nitrogen removing systems or by connecting homes to central sewer, (b) the total amount of nitrogen load that must be reduced to achieve the TMDL, and (c) the relative contribution of nitrogen load from existing OSTDS. 
· Where does the remediation policy for existing systems apply? It applies to all existing OSTDS within the PFA on lots of all sizes.
· What is required by the remediation policy for existing systems? For FDOH to issue a modification or repair permit to an existing OSTDS in the area subject to the policy, the system must include at least one of the following nitrogen reduction enhancements, unless the OSTDS permit applicant demonstrates that sewer connections will be available within 5 years.
· Enhanced treatment of nitrogen means inclusion of features allowed pursuant to FDOH rules, such as in-ground nitrogen-reducing biofilters (media layer systems); features consistent with and identified in the FDOH Florida Onsite System Nitrogen Removal Strategy Studies report, such as in-tank nitrogen-reducing biofilters; or other FDOH-approved treatment systems capable of meeting or exceeding the NSF Standard 245 nitrogen removal rate before disposing the wastewater in the drain field, such as ATUs and PBTSs. For FDOH-approved treatment systems that meet NSF 245, but do not meet or exceed the minimum treatment level expected from the in-ground nitrogen-reducing biofilters, the drain fields, at minimum, shall be installed with a 24-inch separation between the bottom of the drain field and the seasonal high-water table.
· FDOH permitting requirements with respect to defining "modification," "repair," and lot size (i.e., acreage) will be followed for this remediation plan
· When is the remediation policy for existing systems effective? It begins following completion of the master wastewater treatment feasibility plans, rulemaking, and funding milestones included in Sections D.3 and D.4, but no later than five years after BMAP adoption.
D.1.3 Achieving Necessary Load Reductions
All conventional OSTDS in areas subject to the remediation policy for existing systems are required to adopt enhanced treatment of nitrogen no later than 20 years after BMAP adoption.
D.1.4 Other Plan Elements
Statutes also require that OSTDS remediation plans contain the following elements.
An evaluation of credible scientific information on the effect of nutrients, particularly forms of nitrogen, on springs and spring systems. (See Section D.2.)
Options for repair, upgrade, replacement, drain field modification, the addition of effective nitrogen-reducing features, connection to a central sewer system, or other action. (See Section D.3.)
A public education plan to provide area residents with reliable, understandable information about OSTDS and springs. (See Section D.4.)
Cost-effective and financially feasible projects necessary to reduce the nutrient impacts from OSTDS. (See Section 2 and Appendix B.)
A priority ranking for each project for funding contingent on appropriations in the General Appropriations Act. (See Section 2 and Appendix B.)
The Florida Springs and Aquifer Protection Act defines an OSTDS as a system that contains a standard subsurface, filled, or mound drain field system; an aerobic treatment unit; a graywater system tank; a laundry wastewater system tank; a septic tank; a grease interceptor; a pump tank; a solids or effluent pump; a waterless, incinerating, or organic waste–composting toilet; or a sanitary pit privy that is installed or proposed to be installed beyond the building sewer on land of the owner or on other land on which the owner has the legal right to install such a system. The term includes any item placed within, or intended to be used as a part of or in conjunction with, the system. The term does not include package sewage treatment facilities and other treatment works regulated under Chapter 403, F.S.
[bookmark: _Toc480372153]D.2	Collection and Evaluation of Credible Scientific Information
As discussed in Section 2, DEP developed the Weeki Wachee NSILT, a planning tool that provides estimates of nitrogen loading to groundwater based on best available scientific data at the time the tool is used for a particular geographic area. The NSILT results were peer-reviewed by SWFWMD, FDOH, and FDACS. Additional technical support information concerning the NSILT can be found in Appendix E.
DEP also consulted the Weeki Wachee River SWIM Plan adopted by SWFWMD in March 2017 for science-related OSTDS actions and projects. At a public meeting on August 23, 2016, DEP presented and obtained concurrence from stakeholders for actions and projects that include the following (lead entities are listed in parentheses):
Monitoring and research:
Improve understanding of the ecological responses to nutrient enrichment and reductions (DEP/SWFWMD/universities).
Maintain and expand water quality monitoring programs (SWFWMD/DEP).
Report annual status and trends (SWFWMD).
Evaluate new and emerging technologies (SWFWMD).
Research and develop advanced septic systems (FDOH/DEP/UF-IFAS).
Completed project:
Florida Onsite Sewage Nitrogen Reduction Strategies Study (FDOH).
Ongoing projects:
Quarterly springs water quality monitoring (SWFWMD).
Stream water quality monitoring (SWFWMD).
UFA nutrient modeling (SWFWMD).
Springs Initiative modeling (SWFWMD).
Project COAST (collect and analyze monthly surface water quality data at 50 fixed stations along the coasts of Hernando, Citrus, and Levy Counties) (SWFWMD/University of Florida).
U.S. Geological Survey (USGS) Groundwater Data Collection (USGS/SWFWMD).
USGS Surface Water Data Collection (USGS/SWFWMD).
Proposed projects:
Nutrient hot-spot loading identification (DEP/SWFWMD).
Groundwater quality monitoring for BMAP assessment (DEP/SWFWMD).
[bookmark: _Hlk490055322]DEP developed calculation methods to estimate nitrogen reductions associated with septic system enhancement and replacement projects, WWTF projects, golf course BMPs, other sports turfgrass BMPs, and urban turfgrass BMPs. 
[bookmark: _Toc480372154]D.3	Remediation Options
The NSILT estimates that OSTDS contribute approximately 44 % of the pollutant loading to groundwater in the PFA. Table D-1 lists the number of existing OSTDS in the PFA and the estimated nitrogen reductions associated with enhancement or connection to sewer. Figure D-1 shows the areas where OSTDS are located. 
[bookmark: _Toc505866886][bookmark: _Toc512092928][bookmark: _Toc514421172]Table D-1. Estimated reduction credits for additional OSTDS enhancement or sewer *
*Estimated reductions are for either enhancement or sewer per parcel classification. Reductions cannot be combined for the same parcel classification, but can be combined between the different classifications. For example, the sewer credit associated with parcels less than one acre in size can be combined with the sewer credit associated with parcels one acre or greater in size.
	Recharge Area
	OSTDS Parcels Less Than One Acre in PFAs 
	Credit for Enhancement (lb-N/yr)
	Credit for Sewer (lb-N/yr)
	OSTDS Parcels One Acre and Greater in PFAs 
	Credit for Enhancement (lb-N/yr))
	Credit for Sewer (lb-N/yr) 

	High
	29,840
	158,152
	229,768
	5,847
	30,989
	45,022

	Medium
	0
	0
	0
	0
	0
	0

	Total
	29,840
	158,152
	229,768
	5,847
	30,989
	45,022


As required by statute, this OSTDS remediation plan identifies remediation options for existing OSTDS, including repair, upgrade, replacement, drain field modification, the addition of effective nitrogen-reducing features, connection to a central sewer system, or other action. More simply, remediation options can be classified as enhancement or replacement. Enhancement options consist of systems identified in either existing FDOH rules or existing and ongoing FDOH studies, or systems not otherwise prohibited by FDOH. Examples of enhancements include in-ground nitrogen-reducing biofilters (media layer systems); in-tank nitrogen-reducing biofilters; and ATU or PBTS capable of meeting or exceeding the NSF Standard 245 nitrogen removal rate before disposing wastewater in the drain field.
Nitrogen impacts from new development could also be reduced through prohibiting new conventional OSTDS on all lot sizes, throughout the BMAP area.
DEP, FDOH, and local governments will develop programs to provide funding to homeowners and individuals to upgrade existing OSTDS by adding nutrient reducing features. The funding program will be designed to prioritize OSTDS where it is most economical and efficient to add nutrient reducing features (i.e., systems needing a permit for a repair or modification, within the PFA, and on lots of less than one acre). 
To facilitate incorporation of nitrogen reducing features at the time of a permit to repair or modify an existing OSTDS, FDOH will pursue regulatory solutions to accomplish the following objectives:
· Update OSTDS rule language regarding permits, variances, and waivers to include consideration of DEP-adopted OSTDS remediation plans. 
· Update OSTDS rules to allow installation of passive remediation systems, including systems featuring liners, nitrogen reducing material, or both underneath the drain field. 
[image: ]
[bookmark: _Toc479941193][bookmark: _Toc512092354][bookmark: _Toc514421609]Figure D-1. Locations of OSTDS in the PFA in the Weeki Wachee BMAP
[bookmark: _Toc480372156]D.4	Public Education Plan
DEP and FDOH will develop and disseminate educational material focused on homeowners and guidance for builders and septic system contractors. The materials will identify the need for advanced, nitrogen reducing OSTDS along with the requirements for installing nitrogen reducing technologies under this OSTDS remediation plan. DEP will coordinate with industry groups such as Florida Home Builders Association and FOWA.
DEP hosted a brainstorming session on July 19, 2016 to gather local input on the primary facets of a public education plan, including key audiences, the identification of major themes for communication/education, and the identification of misconceptions about septic systems.
Based on this discussion and one-on-one coordination with local governments and other stakeholders with interest in public education, prioritized target audiences, messaging, and materials/resources (see Table D-2) were presented at a public meeting. 
Step 1 – Understand the data and issues associated with OSTDS.
Step 2 – Identify existing and short-term activities to address the issues.
Step 3 – Undertake a pilot project outreach and social marketing campaign
Step 4 – Identify future actions for basin-wide implementation.
[bookmark: _Toc505866887][bookmark: _Toc512092929][bookmark: _Toc514421173]Table D-2. Prioritized target audiences, messaging, and materials/resources
	Audience
	Messaging
	Materials/Resources

	Schools
	Convey cost of doing nothing
	PSAs

	Residents
	Preserving our waterways
	SWFWMD springs education webpage

	Builders/realtors/developers/ community
	Conventional septic systems provide minimal nitrogen treatment; septic system enhancement is needed
	Social media




[bookmark: _Toc512092355][bookmark: _Toc514421174]Table D-3. Stakeholder educational activities to implement the OSTDS remediation plan

*Denotes activity that is applicable in all Springs Coast BMAPs. The dollar amount is the total project amount (not split among the BMAPs).
	Lead Entity
	Activity Number
	Activity Name
	Description of Activity
	Activity Status
	Partners
	Estimated Start Date
	Estimated Completion Date
	Cost Estimate
	Funding Source
	Funding Amount

	City of Brooksville
	COB-E-1
	Public Service Announcements (PSAs)
	Include FDOH PSAs in septic system utility bills twice per year.
	Planned
	N/A
	2018
	2018
	$5,000
	City
	$5,000

	City of Brooksville
	COB-E-2
	Think About Personal Pollution (TAPP) Program
	Transfer or deploy City of Tallahassee TAPP Program in Brooksville.
	Planned
	N/A
	2018
	2020
	$5,000
	City
	$5,000

	City of Brooksville
	COB-E-3
	City Website
	Post springs-related and OSTDS-related information on city website.
	Planned
	N/A
	2018
	2018
	$5,000
	City
	$5,000

	Hernando County
	HC-E-1
	OSTDS Enhancement Education Campaign
	Develop education campaign in conjunction with identified partners on OSTDS enhancement options.
	Planned
	Not Provided
	2018
	2021
	$50,000
	Not Provided
	Not Provided

	Hernando County
	HC-E-8
	Drain Field Enhancement Demonstration Project
	Implement drain field enhancement demonstration project on public property.
	Planned
	N/A
	2022
	2025
	$250,000
	Not Provided
	Not Provided

	Hernando County
	HC-E-10
	Training on Septic Drain Field Enhancements
	Conduct training for local government permitting staff on the availability and permitting process for septic system drain field enhancements.
	Planned
	N/A
	2022
	2022
	$1,000
	County
	$1,000

	UF-IFAS
	IFAS-E-1*
	OFS OSTDS Campaign, Phase 1
	Implement social marketing campaign that links septic systems to springs.
	Planned
	N/A
	2018
	2020
	$30,000
	TBD
	TBD

	UF-IFAS
	IFAS-E-2*
	OFS OSTDS Campaign, Phase 2
	Create on-line clearinghouse of fact sheets, videos, public service announcements, etc.
	Planned
	N/A
	2018
	2018
	$7,000
	TBD
	TBD

	UF-IFAS
	IFAS-E-3*
	OFS OSTDS Campaign, Phase 3
	Presentations to realtors and distribution of information kits for home buyers.
	Planned
	N/A
	2018
	2018
	$10,000
	TBD
	TBD

	UF-IFAS
	IFAS-E-4*
	OFS OSTDS Campaign, Phase 4
	Six to eight septic system workshops for elected officials.
	Planned
	N/A
	2018
	2019
	$5,000
	TBD
	TBD

	UF-IFAS
	IFAS-E-5*
	OFS OSTDS Campaign, Phase 5
	Homeowner workshops with field demonstrations.
	Planned
	N/A
	2018
	2020
	$25,000
	TBD
	TBD



[bookmark: _Toc514419763]Appendix E. Technical Support Information 
E.1	NSILT Data
An NSILT was completed on the Weeki Wachee Spring and River Contributing Area for the Weeki Wachee BMAP. This technical support information identifies the data sources relied upon during NSILT development and documents all the major assumptions used by DEP when applying the NSILT approach to the Weeki Wachee BMAP.
The general NSILT approach involves estimating the nitrogen load to the surface for various source categories based on land use. The NSILT subjects the surface loading to recharge and attenuation to derive the estimated load to groundwater at the top of the aquifer. The estimated load to groundwater determines the scope of reduction strategies needed in the BMAP for each source category. For additional information about the general NSILT approach, see any of the NSILT reports posted online at http://publicfiles.dep.state.fl.us/DEAR/NSILT. 
E.1.1	Source Category General Data Inputs
Hydrogeology and Aquifer Recharge
Information on recharge to the UFA is from a groundwater flow model that was developed in 2002 by the United States Geological Survey (USGS) based on well data from 1993-94. The raster-based model was smoothed and classified into three recharge categories, discharge, medium recharge, and high recharge.
Land Use
Land use information is from SWFWMD based on the 2011 Florida Land Use Cover and Forms Classification System (FLUCCS) and 2014 Hernando County and Pasco County property appraiser data.
E.1.2	Estimating Nitrogen Inputs to the Land Surface (NSILT Section 2.0)
Atmospheric Deposition
Atmospheric deposition information is derived from the TDEP hybrid model that inputs wet and dry monitoring network data for the U.S. and calculates an estimated TN deposition load (Schwede and Lear 2014). The data set is comprised of data from 2011 to 2013.
WWTFs
The average annual input of nitrogen to the land surface was estimated for each effluent land application site in the BMAP area using TN concentration and discharge volume data available in the DEP Wastewater Facility Regulation (WAFR) database. Smaller WWTFs are not always required to monitor and report TN effluent concentrations, and therefore may not have data available in the WAFR database. For these, DEP estimated TN concentrations based on nitrate-N (NO3-N) data (assuming the NO3-N concentration was 38.5 % of the TN, based on a 2009 cooperative study with the Water Reuse Foundation of 40 domestic WWTFs across the state). The range of years for which data were available varied with the individual WWTFs; however, the majority of the data were from 2013 to 2014.
OSTDS
The number of OSTDS was initially estimated from the 2009 FDOH model which was correlated with current property appraiser land use information (Hall and Clancy 2009). The results were corrected for parcels identified with more than one OSTDS and the proximity of sewer lines. After the NSILT was produced, FDOH released an updated OSTDS inventory for Hernando and Pasco Counties; the data sets were compared and minimal differences identified.
[bookmark: _Hlk513110985][bookmark: _Hlk513110991]The population served by the OSTDS was estimated using the 2010 U.S. Census Bureau data for Hernando and Pasco Counties. Data were used to estimate the effective population and OSTDS usage. The 2010 persons per household (adjusted for time spent away from home) for Hernando and Pasco Counties were 2.08 and 2.07, respectively.  Several literature sources have reported a per capita contribution of 9.012 lb-N/yr, and this value was multiplied by the number of people using septic tanks within the different regions of the BMAP area (U.S. Environmental Protection Agency [EPA] 2002; Toor et al. 2011; Viers et al. 2012).
UTF
The UTF application rate is estimated based on the results of a 2008 SWFWMD study (Martin 2008). The results provide input data on percent of the population that fertilize, the applicator (i.e., landscape professional versus homeowner), and application rates.
The type of property where fertilizer is applied is estimated for nonresidential and residential parcels. The acreage receiving fertilizer is estimated the same for both parcel types by using county property appraiser data and zoning data. Impervious and pervious land areas are determined for each parcel.
Fertilizer application on commercial and public green spaces was assumed to be performed by lawn service professionals or trained staff using application rates and frequencies similar to those recommended in the Green Industries BMP Manual (DEP 2010). Nonresidential parcels are assumed to be fertilized by a commercial service provider at a rate of 21.78 lb-N/acre (ac). Residential parcels are evaluated by estimating the percentage of the property fertilized and the probability of fertilization. For residential parcels, these factors are determined by utilizing property values (higher valued properties fertilize more often and in greater amounts) and parcel type (single-family residences fertilize more frequently than other residence types). 
STF
Sports turfgrass areas include golf courses and sporting facilities. DEP sent golf course mangers surveys to provide basic information on fertilizer application. Responses were received from 46 % of the managers and an input of 43 lb-N/ac/yr was used by DEP. The remaining 54 % was estimated using the statewide application rate of 141.1 lb-N/ac/yr (assuming 72 % of the course area is fertilized) (Sartain 2002; DEP 2007).
Sporting facilities were assessed based on property appraiser data and contacting the responsible entity to determine application rates. The fertilizer application rate for nonresidential parcels was used (21.78 lb-N/ac).
LW
Livestock operation practices are obtained through meetings with producers. For cow-calf operations, a stocking rate of 1 cow per 6 to 8 acres is used and the estimated quantity of pasture acreage is based on property appraiser data. For other livestock animals, populations are estimated from the U.S. Department of Agriculture (USDA) census of agriculture and SWFWMD land use coverage adjusted by percent of land use type in the BMAP area. The nitrogen waste factor for each animal type is based on published literature values (listed in NSILT) and subdivided into locations and recharge area.
FF
Agricultural fertilizer is applied at varying rates depending on crop type and farm practices. Estimated application rates are based on UF-IFAS recommendations, and types of crops likely grown are estimated from the county property appraiser database.
Estimated Nitrogen Inputs to Land Surface
The estimated input from each source category above is summed and a relative percent calculated.
E.1.3	Attenuation and Groundwater Loading 
The two types of attenuation that are evaluated are biochemical attenuation factors (BAFs) and hydrogeological attenuation (i.e., recharge).
BAFs and Uncertainty Factors
The BAFs used to account for the processes affecting the movement of nitrogen from each source category in the subsurface are based on literature review of studies in Florida and similar areas. The BAFs in Table E-1 are the result of this evaluation. The BAF is used to estimate what percent of the surface input could infiltrate to groundwater. For example, if 70 % of urban fertilizer is biologically attenuated, then the remaining 30 % could infiltrate to the groundwater.
The environmental attenuation of nitrogen from specific sources within the categories can vary substantially, both spatially and with depth in the subsurface, and will affect the amount of nitrogen leaching to groundwater and the relative contribution of nitrogen from each source category. The range in nitrogen attenuation can result from variability in soil properties, crop types, agricultural practices, nitrogen storage, volatilization of ammonia to the atmosphere, uptake by vegetation, denitrification, and other removal processes.
The potential range in nitrogen attenuation for each source is shown in Table E-1.

[bookmark: _Toc514421247]Table E-1. Range of environmental attenuation of nitrogen from a detailed literature review
	N Source Category
	Low-Level Attenuation (%)
	Attenuation Used 
for This Analysis (%)
	High-Level Attenuation (%)

	Atmospheric Deposition
	85
	90
	95

	WWTFs-RIBs
	10
	25
	40

	WWTFs-Sprayfields
	50
	60
	75

	WWTF-Reuse
	50
	75
	85

	Septic Systems
	40
	50
	75

	Livestock Operations
	80
	90
	95

	Farm Fertilizer
	50
	70
	85

	Urban Fertilizer
	50
	70
	85



Hydrogeological Attenuation (i.e., Recharge)
The recharge rate for the area where the surface input is calculated is based on the composite recharge map previously described. To account for variations in recharge rates to the UFA, non-attenuated nitrogen inputs in high rate recharge areas are multiplied by a weighting factor of 0.9, while nitrogen inputs are multiplied by a weighting factor of 0.5 for medium rate recharge areas and 0.1 for low. Groundwater discharge areas were not included in the calculations of nitrogen loads to the groundwater contributing area, as these areas do not contribute nitrogen to the aquifer.
Estimated Nitrogen Loads to Groundwater
The surface inputs by source category are adjusted by applying the BAFs for the appropriate source category and location-based recharge factors to estimate the load to groundwater by source category.
It is important to note that this load is estimated for the top of the aquifer. As the load interacts with the aquifer, additional factors likely modify it prior to discharge at the spring vents.
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[bookmark: _Toc514419764]Appendix F. Educational Activities to Implement the UTF Management Strategies
Prioritization of Management Strategies
The management strategies in Table F-1 are ranked with a priority of high, medium, or low. In 2016, the Florida Legislature amended the Watershed Restoration Act (Section 403.067, F.S.), creating additional requirements for all new or revised BMAPs. BMAPs must now include planning-level details for each listed project, along with their priority ranking. 
Project status was selected as the most appropriate indicator of a project’s priority ranking based primarily on need for funding. Projects with a "completed" status were assigned a low priority. Projects classified as "underway" were assigned a medium priority because some resources have been allocated to these projects, but additional assistance may be needed for the project to be completed. High priority was assigned to projects listed with the project status "planned" as well as certain "completed" projects that are ongoing each year (any project with one of these project types: "street sweeping," "catch basin inserts/inlet filter cleanout,"  "public education efforts," "fertilizer cessation," "fertilizer reduction," or "aquatic vegetation harvesting"), and select projects that are elevated because substantial, subsequent project(s) are reliant on their completion.


[bookmark: _Toc505866889][bookmark: _Toc512092358][bookmark: _Toc514421260]Table F-1.  Stakeholder educational activities to implement UTF management strategies   
*Denotes activity that is applicable in all Springs Coast BMAPs. The dollar amount is the total project amount (not split among the BMAPs).
	Lead Entity
	Activity Number
	Activity Name
	Description of Activity
	Activity Status
	Partners
	Estimated Start Date
	Estimated Completion Date
	Cost Estimate
	Funding Source
	Funding Amount

	City of Brooksville
	COB-E-4
	PSAs
	Include PSAs on fertilizer use on utility bills twice per year.
	Planned
	N/A
	2018
	2018
	$5,000
	City
	$5,000

	City of Brooksville
	COB-E-5
	City Website
	Post springs-related and fertilizer-related information on city website.
	Planned
	N/A
	2018
	2017
	$5,000
	City
	$5,000

	Hernando County
	HC-E-2
	Fertilizer Survey
	Mass mailing to single family residences with request to take on-line survey regarding fertilizer ordinance and activities.
	Completed
	N/A
	2016
	2017
	$16,844
	Fish & Wildlife Foundation/County
	Foundation: $14,511 County: $2,333

	Hernando County
	HC-E-3
	Water's Journey: Kass Circle to Weeki Wachee Springs
	Educate residents and business owners of the Kass Circle community on how stormwater runoff affects Weeki Wachee Springs.
	Underway
	N/A
	2018
	2018
	$2,250
	Not Provided
	Not Provided

	Hernando County
	HC-E-4
	Stormwater Nutrient Reduction Education
	Stormwater education per NPDES permit requirements.
	Underway
	N/A
	Prior to 2012
	2031
	$15,000/yr
	FDOT/County
	$15,000/yr

	Hernando County
	HC-E-5
	Hernando County Groundwater Guardians
	Annual public workshop on water quality and water resources.
	Planned
	N/A
	2018
	2021
	$2,000/yr
	County
	$2,000/yr

	Hernando County
	HC-E-6
	Fertilizer Ordinance Education
	Public education campaign on existing fertilizer ordinance.
	Underway
	UF-IFAS
	2012
	2021
	$30,000
	Not Provided
	Not Provided

	Hernando County
	HC-E-7
	Public Outreach on Fertilizer Use
	Outreach by county extension staff on the Florida-Friendly Landscaping Program.
	Planned
	UF-IFAS
	2018
	2021
	Not Provided
	Not Provided
	Not Provided

	Hernando County
	HC-E-9
	Update "Water's Journey" Public Education Campaign
	Potential multi-partner and multi-jurisdiction effort to update the existing "Water's Journey" campaign.
	Planned
	Not Provided
	2022
	2026
	$100,000
	Not Provided
	Not Provided

	Hernando County
	HC-E-11
	Training on Green Industries Best Management Practices
	Train professionals and master gardener volunteers on exemptions from the fertilizer ordinance.
	Underway
	UF-IFAS
	2013
	2021
	Not Provided
	Not Provided
	Not Provided

	Hernando County
	HC-E-12
	Expert Lawn Care and Landscaping Course
	Conduct classes to homeowners on a variety of topics including irrigation and fertilization.
	Underway
	UF-IFAS
	2016
	2021
	Not Provided
	Not Provided
	Not Provided

	Hernando County
	HC-E-13
	Social Media Awareness Campaign
	Education for residents on urban turfgrass fertilizer through a variety of social media platforms.
	Planned
	UF-IFAS
	2018
	2018
	$5,000
	Not Provided
	Not Provided

	Hernando County
	HC-E-14
	Hernando County Water Watch
	Citizen-science water quality program that would be part of a statewide coastal water watch program to complement LAKEWATCH.
	Planned
	Florida Sea Grant Program/UF-IFAS
	2018
	2031
	Not Provided
	Not Provided
	Not Provided

	Hernando County
	HC-E-15
	Florida Master Naturalist Program (FMNP) in Hernando County
	The mission of the FMNP is to promote awareness, understanding, and respect of Florida's natural world among Florida's citizens and visitors.
	Underway
	Florida Sea Grant Program/UF-IFAS
	2017
	2031
	$5,000
	Not Provided
	Not Provided

	Hernando County
	HC-E-16
	Florida-Friendly Landscaping Annual Workshop
	Conduct annual workshop for residents.
	Underway
	UF-IFAS
	2017
	2030
	$3,000
	County/DEP/SWFWMD
	$3,000

	Hernando County
	HC-E-17
	Community Event Education Booth
	Sponsor education booth at various community events that focus on fertilizer BMPs.
	Underway
	UF-IFAS
	2017
	2031
	$3,000
	County/DEP/SWFWMD
	$3,000

	Hernando County
	HC-E-18
	Springs Workshop
	Biannual workshop for local government leaders on springs protection and BMPs
	Underway
	UF-IFAS
	Prior to 2012
	2031
	$5,000
	County/DEP/SWFWMD
	$5,000

	Hernando County
	HC-E-19
	Direct Mail Fertilizer Education Brochures
	Insert in Hernando County Utility Department customer bill three times per year.
	Underway
	N/A
	Prior to 2012
	2031
	$9,500
	County/WRWSA
	$9,500

	Hernando County
	HC-E-20
	Presentations to Homeowner Associations (HOAs)
	On-site presentations to HOAs on BMPs.
	Underway
	UF-IFAS
	Prior to 2012
	2031
	$2,000
	County/WRWSA
	$2,000

	Pasco County
	PC-E-1
	Public Outreach
	Brochures and pamphlets
	Planned
	N/A
	2018
	2021
	$2,000
	County stormwater utility fund
	$2,000

	Pasco County
	PC-E-2
	Public Outreach
	PSAs on radio and TV
	Planned
	N/A
	2018
	2021
	$2,000
	County stormwater utility fund
	$2,000

	Pasco County
	PC-E-3
	Public Outreach
	Utility bill inserts
	Planned
	N/A
	2018
	2021
	$5,000
	County stormwater utility fund
	$5,000

	Pasco County
	PC-E-4
	Landscape Professionals
	Educate landscape industry professionals (i.e., Pasco Co. employees, Pasco Co. School Board employees) on athletic field and park turfgrass fertilization.
	Completed
	UF-IFAS
	2012
	Not Provided
	Not Provided
	University of Florida
	Not Provided

	Pasco County
	PC-E-5
	Florida-Friendly Training for Code Compliance Officers
	Train Pasco Co. code compliance officers in Florida-Friendly landscape principles, including proper fertilization.
	Planned
	UF-IFAS
	2018
	2021
	Not Provided
	Not Provided
	Not Provided

	SWFWMD
	SWF-E-2*
	Fertilizer Campaign
	Fertilizer campaign is in place with existing communication products produced by the District's Public Affairs Bureau.
	Underway
	Not Provided
	Not Provided
	Not Provided
	$10,000
	SWFWMD
	$10,000 (annual)

	UF-IFAS
	IFAS-E-6*
	Social Marketing Campaign
	Implement social marketing campaign to increase awareness of local fertilizer ordinances and to encourage good fertilizer practices.
	Planned
	Not Provided
	2018
	2020
	$30,000
	 Not Provided
	 Not Provided



[bookmark: _Toc514419765]Appendix G. FDACS BMPs
[bookmark: _Toc426464321]G.1	Implementation of Agricultural BMPs
Agricultural nonpoint sources in a BMAP area are required by state law (Subsection 403.067[7], F.S.) either to implement FDACS-adopted BMPs, which provides a presumption of compliance with water quality standards, or to conduct water quality monitoring prescribed by DEP or SWFWMD. Failure either to implement BMPs or conduct monitoring may result in enforcement action by DEP.  
Growers who implement BMPs may be eligible for cost-share funding from FDACS, SWFWMD, or others to partially defray the costs of implementation. Through OAWP, the Florida Forest Service, and the Division of Aquaculture, FDACS develops, adopts, and assists producers in implementing agricultural BMPs to improve water quality and water conservation.
FDACS identified potential land for enrollment in the FDACS BMP Program within the Weeki Wachee BMAP area using the Florida Statewide Agriculture Irrigation Demand (FSAID) IV geodatabase. 
Table G-1 summarizes the agricultural land use data in the Weeki Wachee BMAP area. Based on the FSAID IV geodatabase, the total agricultural lands within the BMAP area is 45,701 acres. Table G-2 summarizes the agricultural land by crop type that was estimated to be fertilized and the corresponding acreages. The primary fertilized agricultural land use in the BMAP area is Cropland and Pastureland which comprises 87 % of the fertilized land use. Table G-3 summarizes the agricultural lands with livestock. It is important to note that some of the agricultural lands include more than one agricultural practice.   
Figure G-1 shows the approximate location of the agricultural lands based on the FSAID IV geodatabase within the BMAP area.  
[bookmark: _Toc481069347][bookmark: _Toc505866890][bookmark: _Toc512092930][bookmark: _Toc514421452]Table G-1. Agricultural land use within the BMAP area
	Agricultural Nitrogen Loading Category
	Acres

	Crop Fertilizer Lands only
	4,738

	Livestock Lands only
	9,391

	Crop Fertilizer and Livestock Lands
	31,572

	Total
	45,701







[bookmark: _Toc505866891][bookmark: _Toc512092931][bookmark: _Toc514421453]Table G-2. Fertilized crop lands within the BMAP area
	Crop Type
	Application Rate (lbs/acre)
	Acres

	Blueberries
	100
	352

	Citrus
	600
	1,030

	Container Nursery
	90
	190

	Cropland and Pastureland
	30
	31,572

	Field Nursery
	90
	30

	Grains
	100
	174

	Grass/Pasture
	60
	8

	Hay
	480
	429

	Other Groves
	150
	2

	Pasture
	160
	123

	Peanuts
	0
	60

	Peppers Fall
	240
	44

	PeppersSpring_PeppersFall
	240
	83

	Small Veg
	150
	85

	Small Veg Spring
	150
	7

	SmallVegFall_SmallVegSpring
	150
	74

	Tomatoes Spring
	480
	661

	TomatoesFall_TomatoesSpring
	240
	7

	Tree Crops
	150
	1,318

	Tree Plantations
	0
	60

	Total
	-
	36,311



[bookmark: _Toc505866892][bookmark: _Toc512092932][bookmark: _Toc514421454]Table G-3. Livestock lands within the BMAP area
	Livestock Category
	Acres

	Cropland and Pastureland
	31,572

	Feeding Operations
	773

	Other Open Lands (Rural)
	5,632

	Specialty Farms
	2,986

	Total
	40,963



Agricultural land use data are critical for determining agricultural nonpoint source loads and developing strategies to reduce those loads in a BMAP area, but there are inherent limitations in the available data. The time of year when land use data are collected (through aerial photography) affects the accuracy of photo interpretation. Flights are often scheduled during the winter months due to weather conditions and reduced leaf canopies, and while these are favorable conditions for capturing aerial imagery, they make photo interpretation for determining agricultural land use more difficult (e.g., more agricultural lands are fallow in the winter months) and can result in inappropriate analysis of the photo imagery. There is also a significant variation in the frequency with which various sources of data are collected and compiled, and older data are less likely to capture the frequent changes that often typify agricultural land use. In addition, agricultural activity being conducted on the land is not always apparent. For example, acreage classified as improved pasture may be used for a cow-calf operation, consist of forage grass that is periodically harvested for hay, or simply be a fallow vegetable field awaiting planting. Finally, the classification method itself may be an issue. For example, property appraiser data assigns an agricultural land use designation to an entire parcel, although agricultural production may only be conducted on a portion of the parcel. Because of error in the collection and characterization of land use data and changes in land use over time, agricultural land use acreage estimates are subject to adjustment.


[image: ]
[bookmark: _Toc512092359][bookmark: _Toc514421630]Figure G-1. Agricultural lands in the BMAP area
[bookmark: _Toc391415063][bookmark: _Toc418789273][bookmark: _Toc426464322]G.2	Agricultural BMPs
BMPs are individual or combined practices determined through research, field-testing, and expert review to be effective and practicable means for improving water quality, considering economic and technological feasibility. FDACS has authority for establishing agricultural BMPs through the Florida Forest Service (Silviculture BMP Program), Division of Aquaculture (Aquaculture Certification Program), and OAWP (all other agricultural BMP programs).  As of February 2018, OAWP has adopted manuals for cow-calf, statewide citrus, vegetable and agronomic crops, nurseries, equine operations, specialty fruit and nut, sod, dairy, and poultry operations. Development is underway for a small farms manual, and adoption is expected in 2018. The sod and cow-calf manuals are currently under review and revision.
The OAWP BMPs fall into two categories: structural and management. Structural BMPs, e.g., water-control structures and fencing, involve the installation of structures or changes to the land and are usually costlier than management BMPs. Management BMPs, such as nutrient and irrigation management, comprise the majority of the practices and often are not readily observable. Nutrient management addresses fertilizer type, amount, placement, and application timing, and it includes practices such as soil and tissue testing, application methods, correct fertilizer formulations, and setbacks from water resources. Irrigation management consists of maintenance, scheduling, and other measures that improve the overall efficiency of irrigation systems. FDACS-funded mobile irrigation labs (MILs) are available to evaluate irrigation system efficiency and provide recommendations to producers to improve efficiency. The implementation of these recommendations results in billions of gallons of water saved throughout the state and helps reduce nutrient runoff and leaching.  
Table G-4 identifies key management and structural BMPs applicable to agricultural operations in the BMAP area. By definition, BMPs are developed to be technically and economically feasible. However, FDACS BMP manuals do contain some BMPs that may be affordable only with financial assistance through cost-share programs. The BMP checklists allow producers to indicate whether implementing a BMP requires financial assistance.
Information on the BMP manuals and field staff contact information can be obtained here:  http://www.freshfromflorida.com/Divisions-Offices/Agricultural-Water-Policy. Printed BMP manuals can be obtained by contacting OAWP field staff.





[bookmark: _Toc424132827][bookmark: _Toc481069350][bookmark: _Toc505866893][bookmark: _Toc512092933][bookmark: _Toc514421455]Table G-4. Key management and structural BMPs adopted by FDACS OAWP
	BMP Category
	BMP
	Description

	Nutrient Management (Right Source)
	Use of Correct Formulations
	Use of fertilizer formulations that are appropriate for the environmental conditions. Includes enhanced efficiency fertilizers, as warranted.

	Nutrient Management (Right Rate)
	Soil and Tissue Testing
Nutrient Budgeting
	Used to base fertilizer applications on plant needs and available nutrients in the soil; helps prevent the over application of fertilizer.
Consideration of all nutrient sources, such as commercial fertilizers, biosolids, legumes, manure, and nutrient-laden irrigation water to ensure that fertilization meets crop nutrient requirements.

	Nutrient Management (Right Placement)
	Precision Application of Nutrients
	Use of specialized equipment for precise placement of nutrients on targeted areas at specified rates; reduces total amount used and prevents stray applications.

	Nutrient Management (Right Timing)
	Split Fertilizer Applications
	Multiple applications timed with optimal growth stages; allows plants to assimilate nutrients more efficiently; reduces nutrient loss in leaching and runoff.

	Nutrient Management (Special Fertilization Practices)
	Special Fertilization Practices
	Commodity specific fertilization practices to address nuances on a case-by-case basis.

	Nutrient Management (Fertilizer Storage and Handling)
	Fertilizer Storage and Handling
	Proper location/storage of bulk fertilizer products to prevent nutrient loadings.
Use of appropriate dedicated or temporary mix/load areas located away from waterbodies to prevent nutrient loading.

	Irrigation and Water Table Management
	Irrigation Scheduling
	Planning when to irrigate to reduce water and nutrient losses, based on available soil moisture content, evapotranspiration levels, recent rainfall, and time of day.

	Irrigation and Water Table Management
	Irrigation System Maintenance
	Use of MILs to identify efficiency issues, maintenance, and incorporation of potential upgrades to irrigation system.

	Irrigation and Water Table Management
	Wellhead Protection
	Establishing safe practices around irrigation and drinking water wells.

	Water Resource Protection
	Buffers and Setbacks
	Fertilizer application setbacks from waterbodies (e.g., wetlands, watercourses, sinks, springs, etc.) and use of appropriate buffers around water resource features.

	Water Resource Protection
	Ditch Maintenance and Water Control Structures
	Use of rip rap, sediment traps, staging structures, and permanent vegetative bank cover to minimize erosion and transport of nutrient-laden sediments.

	Water Resource Protection
	Erosion Control
	Vegetated strips of land designed to reduce nutrients and sediments in surface water runoff from fields, pastures, and livestock high-intensity areas before it reaches downstream waterbodies.

	Livestock Management
	Manure Management
	Appropriate storage and disposal of animal waste.

	Livestock Management
	Water Requirements and Sources
	Use of upland livestock watering ponds and/or water troughs; minimizes manure deposition in waterbodies.

	Livestock Management
	Forage, Pasture and Grazing Management
	Movement of cattle to different grazing areas on a planned basis; prevents concentrated waste accumulations and denuding of pasture areas.  May involve fencing.
Also involves siting of cowpens, supplemental feed areas, etc., away from waterbodies to minimize nutrient loadings.

	Livestock Management
	Use Exclusion
	Used when stream banks have significant rill or gully erosion because of cattle trampling.

	Operations Management
	Fertilizer Storage
	Proper location/storage of bulk fertilizer products to prevent nutrient loadings.



[bookmark: _Toc391415064][bookmark: _Toc418789274][bookmark: _Toc426464323]G.3	BMP Enrollment
Figure G-2 shows the acres enrolled in the FDACS BMP Program in the Weeki Wachee BMAP area as of December 31, 2017. Table G-5 lists the acres enrolled in the FDACS BMP Program by manual and the number of NOIs associated with those acres. Given that the enrolled acres where BMPs are implemented can contain nonproduction acres (such as buildings, parking lots, and fallow acres), only the enrollment for the land classified as agriculture based on the FSAID IV geodatabase is included in the tables. 
As of December 31, 2017, NOIs cover 15,349 acres in the BMAP area. No producers are conducting water quality monitoring in lieu of implementing BMPs at this time.
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[bookmark: _Toc481069281][bookmark: _Toc512092360][bookmark: _Toc514421631]Figure G-2. BMP enrollment in the BMAP area as of December 31, 2017
[bookmark: _Toc505866894][bookmark: _Toc512092934][bookmark: _Toc514421456][bookmark: _Toc426464324][bookmark: _Toc481069351]Table G-5. Agricultural acreage and BMP enrollment in the BMAP area as of 
[bookmark: _Toc505866895][bookmark: _Toc512092935]December 31, 2017
N/A = Not applicable.
	Related FDACS BMP Programs
	NOI Acreage Enrolled
	Agricultural Land Use Acres within NOIs

	Cow/Calf Operations
	543
	502

	Nurseries
	13,307
	12,414

	Specialty Fruit and Nut
	205
	172

	Citrus
	210
	133

	Vegetable and Agronomic Crops
	1,065
	833

	Total
	15,349
	14,073



[bookmark: _Toc426464325]G.4	FDACS OAWP Role in BMP Implementation and Follow-Up

OAWP works with producers to submit NOIs to implement the BMPs applicable to their operations, provides technical assistance to growers, and distributes cost-share funding, as available, to eligible producers for selected practices. OAWP follows up with growers through site visits to evaluate the level of BMP implementation and record keeping, identify areas for improvement, if any, and discuss cost-share opportunities.
When DEP adopts a BMAP that includes agriculture, it is the agricultural producer’s responsibility to implement BMPs adopted by FDACS to help achieve load reductions. If land use acreage corrections and BMP implementation do not fully account for the current agricultural load reduction allocation, it may be necessary to develop and implement additional projects and practices that reduce nutrients from agricultural nonpoint sources. In that case, FDACS will work with DEP and SWFWMD to identify appropriate options for achieving further agricultural load reductions.
Section 403.067, F.S. requires that, where water quality problems are demonstrated despite the proper implementation of adopted agricultural BMPs, FDACS must re-evaluate the practices, in consultation with DEP, and modify them if necessary. Continuing water quality problems will be detected through the BMAP monitoring component and other DEP and SWFWMD activities. If a reevaluation of the BMPs is needed, FDACS will also include SWFWMD and other partners in the process.
G.5	OAWP Implementation Assurance Program
OAWP formally established its Implementation Assurance (IA) Program in 2005 in the Suwannee River Basin as part of the multi-agency/local stakeholder Suwannee River Partnership. In 2007, OAWP initiated the IA Program in the Lake Okeechobee Watershed and launched a standardized follow-up program for the remaining areas of the state in 2013, beginning with the Ridge Citrus and Indian River Citrus BMPs. Because of program-specific needs, the follow up process for each of these three components was different. In early 2014, OAWP began to streamline the IA Program to ensure consistency statewide and across commodities and BMP manuals. This effort resulted in a single IA site-visit form, which is currently used by OAWP staff.  
The current IA Program is based on interactions with producers during a site visit by OAWP staff. Site visits are conducted by OAWP field staff and technicians as workload allows. For the visits, field staff and technicians use a standard form (not BMP specific) developed in 2014. This form focuses on nutrient management, irrigation management, and water resource protection BMPs common to all of the BMPs that have been adopted by rule. The paper forms are submitted to OAWP staff and compiled into a spreadsheet, and the data are reported annually. From 2007 to 2015, OAWP conducted 1,936 site visits. However, it is difficult to compare data collected prior to the implementation of the recently developed single IA site visit form because of regional differences (e.g., different forms and information requested) in the administration of the IA Program.
Additional emphasis was given to verifying the implementation of BMPs by enrolled producers with the enactment of Chapter 2016-1, Laws of Florida. That legislation directed OAWP to formalize the Implementation Verification (IV) Program into rules. In December 2016, OAWP published a notice of rule development. In July 2017, draft rule language was distributed and presented at a public workshop. This draft language provided the structure for a statewide uniform implementation verification system, including assessments of the status of implementation, compliance assistance to aid producers in achieving full implementation, and referral to DEP for producers who are not implementing BMPs. The IV rule was final as of November 1, 2017, (Chapter 5M-1, F.A.C.). 
G.6	Beyond BMPs
Beyond enrolling producers in the FDACS BMP Program and verifying implementation, FDACS will work with DEP to improve the data used to estimate agricultural land uses in the springshed. FDACS will also work with producers to implement a suite of agricultural projects and research agricultural technologies on properties where they are deemed technically feasible and if funding is made available. Acreages provided by FDACS are preliminary estimates that are the maximum acreages that will be evaluated and refined over time. 
As presented here, these projects are based on planning-level information. Actual implementation would require funding as well as more detailed design based on specific information, such as actual applicable acreages and willing landowners. Table G-6 summarizes these efforts. It is important to note that the research projects listed in the table are being conducted in the Suwannee River Basin. At some future point, the findings of these studies may be applicable to the Weeki Wachee BMAP.

[bookmark: _Toc505866896][bookmark: _Toc512092936][bookmark: _Toc514421457]Table G-6. Beyond BMP implementation
	Category
	Name
	Description

	Practices
	Precision Irrigation
	Deployment of equipment, procedures, and training to improve location, volume, and timing of irrigation to match crop needs more precisely.

	Practices
	Soil Moisture Probes
	Deployment, training, technical support, and use of soil moisture probes to manage irrigation systems.

	Practices
	Cover Crops
	Planting of cover crops between production cycles to increase soil organic content, improve nutrient retention, and reduce erosion.

	Research
	Bioreactors
	Bioreactors/denitrification walls and onsite capture and reuse of high-N water.

	Research
	Rotational Production
	Conversion of conventional production operations to planned rotational production incorporating grass and cover crops. May include cattle.

	Research
	Soil Moisture Sensor Deployment and Calibration
	Installation, training, monitoring, and research on use of electronic soil moisture sensors, including correlations to nutrient movement through the root zone.

	Research
	Controlled Release Fertilizer
	Application of new and developing fertilizer products that become available to crops via dissolution over longer periods in the growing season.

	Research
	Reuse of High Nutrient Value Water Sources
	Study of potential sources of high nutrient value water, potential beneficial reuse sites, legal and regulatory obstacles, and costs.






[bookmark: _Toc514419766]Appendix H. Future Growth Strategies of Local Jurisdictions
[bookmark: _Toc505866897][bookmark: _Toc512092937][bookmark: _Toc514421463]Table H-1. Future growth strategies of local jurisdictions
	Local Jurisdiction
	Strategy Name
	Description
	Strategy Type
	Status

	Pasco County
	Ecological Corridors Ordinance
	Ordinance 16-13 was adopted on June 21, 2016, which amended the land development code to designate seven ecological corridors to maintain a contiguous network of wildlife habitat between existing public lands.
	Ordinance
	Completed

	Pasco County
	Conservation Element Policy 1.6.1
	Pasco County shall continue to require mandatory setbacks around the Anclote, Hillsborough, Pithlachascotee, and Withlacoochee Rivers; Outstanding Florida Waters; Classified Shellfish Harvesting Areas; and post development wetlands; i.e., wetland mitigation and natural wetlands.
	Comprehensive Plan
	Completed

	Pasco County
	Conservation Element Policy 1.6.16
	Pasco County shall require, during the site plan review process, where feasible, consideration of the maintenance of groundwater infiltration through the use of site Best Management Practices.
	Comprehensive Plan
	Completed

	Pasco County
	Public Facilities Element Policy SEW 3.1.4
	Pasco County shall require connection to a central sanitary sewer system for all proposed projects within Pasco County, when available, as set forth in the guidelines of the Availability Determination Matrix, Table 10-1A.
	Comprehensive Plan
	Completed

	Pasco County
	Public Facilities Element Policy SEW 3.1.11
	Pasco County shall require connection of all central sewer facilities to regional systems.
	Comprehensive Plan
	Completed

	Pasco County
	Public Facilities Element Policy SEW 3.2.1
	Pasco County shall replace smaller package plants with regional sewage treatment plants (or enlarge existing plants) by 2025.
	Comprehensive Plan
	Completed

	Pasco County
	Public Facilities Element Policy SEW 3.3.1
	Pasco County shall require use of reclaimed water for landscape irrigation and nonpotable use where available and permitted by the Florida Department of Environmental Protection and required by the County Code of Ordinances, with a priority for use of reclaimed water to new residential users or other users determined to provide an adequate offset of potable-water usage.
	Comprehensive Plan
	Completed

	Pasco County
	Public Facilities Element Policy SEW 3.3.4
	Pasco County shall develop a reclaimed water system for irrigation of parks; golf courses; cemeteries; large agricultural, commercial, or governmental complexes; and other potential reclaimed water customers.
	Comprehensive Plan
	Completed

	Pasco County
	Public Facilities Element Policy SEW 3.5.4
	Pasco County will evaluate extending wastewater treatment facilities to areas within close proximity of existing County utilities. Special attention shall be paid to areas that are determined to have a high concentration of septic systems. Connection to the County system will be based upon the County Health Department's evaluation of septic system problems for those areas that are related to siting, inspection, and maintenance considerations and based upon available funding provided by the individual applicant.
	Comprehensive Plan
	Completed

	Pasco County
	Public Facilities Element Objective DGR 6.1
	Provide protections for high aquifer-recharge areas.
	Comprehensive Plan
	Completed

	Pasco County
	Public Facilities Element Objective DGR 6.2
	Develop and adopt, by 2007, a comprehensive stormwater management ordinance, including Best Management Practices.
	Comprehensive Plan
	Completed

	City of Brooksville
	Stormwater Management 
Ordinance
	The City will establish and implement BMPs for all activities, operations, and/or facilities within the city which may cause or contribute to pollution or contamination of storm water, the storm drainage system, or waters of the U.S.
	Ordinance
	Completed

	City of Brooksville
	Conservation Element Policy 2-2
	The City shall consider entering into agreement with Hernando County to establish BMPs for the protection of surface and groundwater quality of water basins within Peck Sink, Blue Sink, and Byster Lake.
	Comprehensive Plan
	Planned

	City of Brooksville
	Conservation Element Policy 3-1
	Require all development in the city connect to city sewer service, where and when available.

	Comprehensive Plan
	Completed

	City of Brooksville
	Future Land Use Element Policy 2-4
	High density and intensity growth shall not be permitted in conservation areas, or those areas best suited for continued low density and intensity development.
	Comprehensive Plan
	Completed

	City of Brooksville
	Future Land Use Element Policy 2-9
	Require central sewer and sewer systems for new urban developments, which are designed to be compatible with future public utility systems.
	Comprehensive Plan
	Completed

	Hernando County
	Riverine Buffer Ordinance
	Regulates land use within 75 feet of rivers, streams, and wetlands. Addresses septic systems, wastewater treatment systems, petroleum products, solid waste, and agricultural waste
	Ordinance
	Completed

	Hernando County
	Low Impact Drainage
	New strategies for low impact drainage standards and initiatives.
	Comprehensive Plan
	Planned

	Hernando County
	Ecological Linkages
	New strategies for prioritizing ecological linkage conservation as one means of recharge and groundwater conservation.
	Comprehensive Plan
	Planned

	Hernando County
	Aquifer Recharge
	Update strategies to protect high recharge areas and karst areas.
	Comprehensive Plan
	Planned

	Hernando County
	Aquifer Protection
	Update strategies to protect groundwater through appropriate design of stormwater, sewage treatment, golf course facilities, and landscaping.
	Comprehensive Plan
	Planned

	Hernando County
	Aquifer Protection
	New strategies for coordination on minimum flows and levels for springs and surface waters.
	Comprehensive Plan
	Planned

	Hernando County
	Surface Water Protection
	Update strategies to continue the County's riverine ordinance.
	Comprehensive Plan
	Planned

	Hernando County
	Erosion Control
	Update strategies for erosion control and minimization of sedimentation.
	Comprehensive Plan
	Planned

	Hernando County
	Habitat Mitigation
	New strategies that require mitigation of loss of large natural communities.
	Comprehensive Plan
	Planned

	Hernando County
	Future Land Use Element Policy 1.01T(6)
	Water and sewer planning conducted by the County will utilize a public participation process.
	Comprehensive Plan
	Completed

	Hernando County
	Sanitary Sewer Element Policy 4.01A(6)
	Wastewater service plans developed and updated hereunder, along with the adopted Capital Improvement Plan, shall be utilized to guide the location and timing of land development requiring wastewater service.
	Comprehensive Plan
	Completed

	Hernando County
	Sanitary Sewer Element Policy 4.01A(7)
	Wastewater facility and service planning conducted by the County will utilize a public participation process.
	Comprehensive Plan
	Completed

	Hernando County
	Sanitary Sewer Element Policy 4.01B(2)
	As part of the Wastewater Service Plan, establish standards to determine when commercial and industrial septic tanks will be required to connect to central services.
	Comprehensive Plan
	Completed

	Hernando County
	Sanitary Sewer Element Policy 4.03A(4)
	Advanced secondary and tertiary treatment should be considered for future permanent sewage treatment plants, particularly those which are located near water bodies or in soils which do not have a defined impermeable clay lens or significantly thick sand layers between the surface and the Floridan aquifer.
	Comprehensive Plan
	Completed

	Hernando County
	Sanitary Sewer Element Policy 4.03B(3)
	Where possible, provide flexibility in public or private facility design to allow for development of reuse systems.
	Comprehensive Plan
	Completed

	Hernando County
	Drainage & Natural Groundwater Aquifer Recharge Element Policy 4.10A(1)
	Develop an aquifer protection program including public education, coordination with appropriate agencies, provision of adequate collection, and disposal facilities in order to limit the amount of contaminants reaching the surficial or Floridan aquifers.
	Comprehensive Plan
	Completed

	Hernando County
	Potable Water Element Policy 4.15B(1)
	Implement a strategy to encourage replacement of potable water use with reclaimed water for irrigation purposes of at least 4.3 MGD by the year 2019.
	Comprehensive Plan
	Completed

	Hernando County
	Coastal Management Element Objective 5.01E
	To protect the water quality and the riverine and native bottom communities of the entire seven-mile length of the Weeki Wachee River and its estuary.
	Comprehensive Plan
	Completed

	Hernando County
	Coastal Management Element Objective 5.01F
	Participate in, or otherwise encourage the purchase of additional lands along the Weeki Wachee River and the associated riverine habitats, the coastal lands through SWFWMD's Save our Rivers Program.
	Comprehensive Plan
	Completed

	Hernando County
	Conservation Element Policy 6.01D(6)
	For those areas located within the Weeki Wachee and Withlacoochee River Protection Areas as mapped in the Future Land Use Element, Land Development Regulations shall be developed which include but are not limited to the following concepts: 
a. Preservation of on-site natural vegetation adjacent to the Weeki Wachee or Withlacoochee Rivers
b. Minimum building setbacks from the banks of the Weeki Wachee or Withlacoochee Rivers
c. On-site drainage design to prevent the flow of untreated stormwater runoff from entering the Weeki Wachee or Withlacoochee Rivers.
	Comprehensive Plan
	Completed

	Hernando County
	Conservation Element Policy 6.01E(3)
	Continue to coordinate with Pasco County on the protection and use of Aripeka Bay.
	Comprehensive Plan
	Completed

	Hernando County
	Conservation Element Policy 6.01E(4)
	Continue to coordinate with the City of Weeki Wachee for the purpose of reviewing and revising agreement on the management, protection and use of the Weeki Wachee River and estuary.
	Comprehensive Plan
	Completed

	Hernando County
	Conservation Element Policy 6.02A(9)
	The County shall require all new golf courses be designed and maintained using the principles developed by the Institute of Food and Agricultural Sciences (IFAS) for Best Management Practices for Florida Golf Courses.
	Comprehensive Plan
	Completed

	Hernando County
	Conservation Element Policy 6.02A(10)
	The County shall establish guidelines for managing existing and future turf and landscapes at all County owned facilities utilizing the educational guidelines of the University of Florida Extension’s Florida Yards & Neighborhoods Program and Best Management Practices. It is the intent of this policy that the County reduce nutrient/pollutant infiltration into ground and surface waters and to encourage best management practices through public education
	Comprehensive Plan
	Completed

	Hernando County
	Conservation Element Policy 6.02C(2)
	Evaluate any development proposal for its effect on the quantity and quality of surface waters which flow into the Gulf of Mexico, including stormwater runoff, erosion and sedimentation, and septic tank discharge.
	Comprehensive Plan
	Completed

	Hernando County
	Conservation Element Policy 6.08A(1)
	Minimum lot sizes for septic fields may be further restricted from the minimum ½ acre in prime aquifer recharge areas, sinkhole areas, areas adjacent to lakes or rivers or areas where soils have severe limitations.
	Comprehensive Plan
	Completed

	Hernando County
	Conservation Element Policy 6.08A(11)
	Development of property shall adhere to green industries Best Management Practices (BMPs), including Integrated Pest Management (IPM) (FDEP & FDEO, 2002. Protecting Florida Springs - Land Use Planning Strategies & Best Management Practices). Florida Yards & Neighborhoods (FYN) education shall be provided for individual lot owners.
	Comprehensive Plan
	Completed
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