Table 1: Provisional Stormwater BMPs
	Standard BMPs
	TP % Reduction
	TN % Reduction
	Data Source

	Off-line Retention 0.25” treatment volume
Off-line Retention 0.50” treatment volume
Off-line Retention 0.75” treatment volume
Off-line Retention 1.00” treatment volume
On-line Retention 0.25” treatment volume
On-line Retention 0.50” treatment volume
On-line Retention 0.75” treatment volume
On-line Retention 1.00” treatment volume
	40
62
75
84
30
52
65
74
	40
62
75
84
30
52
65
74
	Harper, H. & D. Baker. 2007.  Evaluation of Current Stormwater Design Criteria within the State of Florida.

	Wet detention ponds
	Reduction from Figure 13.2 given the project’s residence time
	Reduction from Figure 13.3 given the project’s residence time
	Figures 13.2 and 13.3 in Draft Stormwater Treatment Applicant’s Handbook

	BMP treatment trains using a combination of BMPs
	Use BMP Treatment Train (TT) equation:
BMP TT Efficiency = Eff1 +((1-Eff1)*Eff2)
	Use BMP Treatment Train (TT) equation:
BMP TT Efficiency = Eff1 +((1-Eff1)*Eff2)
	Draft Stormwater Treatment Applicant’s Handbook

	Dry detention
	10
	10
	Harper, H. & D. Baker. 2007.  Evaluation of Current Stormwater Design Criteria within the State of Florida.

	Baffle box
	2.3
	0.5
	Final Report Contract S0236 Effectiveness of Baffle Boxes

	Nutrient baffle box (2nd generation)
	15.5
	19.05
	Final Report Contract S0236 Effectiveness of Baffle Boxes

	Grass swales with swale blocks or raised culverts
	Use on-line retention BMPs above
	Use on-line retention BMPs above
	Evaluation of Harper data

	Grass swales without swale blocks or raised culverts
	50% of value for grass swales with swale blocks or raised culverts
	50% of value for grass swales with swale blocks or raised culverts
	Evaluation of Harper data

	Alum injection
	90
	50
	Evaluation of Harper data

	Stormwater reuse
	Estimate amount water not discharged annually because used for irrigation.
	Estimate amount water not discharged annually because used for irrigation.
	Evaluated on a case-by-case basis

	Stormceptor 
	13
	2
	Final Report Contract S0095 Sanford Stormceptor project

	Continuous deflective separation (CDS) units
	10
	Not applicable
	Final Report Contract WM793 Broadway Outfall Project

	Street sweeping
	Determine the dry weight/volume of material collected annually and multiply by values provided by the Florida Stormwater Association (FSA) University of Florida (UF) municipal separate storm sewer system (MS4) BMP project
	Determine the dry weight/volume of material collected annually and multiply by values to be provided by FSA UF MS4 BMP project
	Final Report of FSA UF MS4 BMP Project

	Catch basin inserts/inlet filters
	Determine the dry weight/volume of material collected annually and multiply by values to be provided by FSA UF MS4 BMP project
	Determine the dry weight/volume of material collected annually and multiply by values to be provided by FSA UF MS4 BMP project
	Final Report of FSA UF MS4 BMP Project

	Septic tank phase out
	Based on values from ArcNLET model
	Based on values from ArcNLET model
	http://people.sc.fsu.edu/~mye/ArcNLET/index.html


Note: The Draft Stormwater Treatment Applicant’s Handbook is located at http://publicfiles.dep.state.fl.us/dwrm/stormwater/stormwater_rule_development/docs/ah_rule_draft_031710.pdf 
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	Provisional BMPs
	TP % Reduction
	TN % Reduction
	Data Source

	Public education
	1-6, depending on extent of program
	1-6, depending on extent of program
	Evaluation of Center for Watershed Protection. 2002. Watershed Treatment Model Version 3.1. See separate calculation spreadsheet.

	Floating islands/ Managed aquatic plant systems (MAPS)
	20
	20
	Chapter 14 Draft Stormwater Treatment Applicant’s Handbook

	Muck removal/ restoration dredging
	Case-by-case depending on the nutrient flux of the muck
	Case-by-case depending on the nutrient flux of the muck
	FDEP Muck Removal Credit Guidance (developed for the Indian River Lagoon BMAPs)

	Aquatic vegetation harvesting
	Based on the total mass of material collected, type of plant(s), and associated nutrient content in the dry material
	Based on the total mass of material collected, type of plant(s), and associated nutrient content in the dry material
	FDEP Removal of Aquatic Vegetation for Nutrient Credits (developed for the Indian River Lagoon BMAPs)



