PSL-07: E-8 Waterway Phase 1 Water Quality Retrofit
Project Summary
The E-8 Waterway is an existing detention outfall for Watershed B that discharges through control structures B-1 and B-2 into the tidal portion of the C-24 canal. This project consisted of baffle boxes, control structure improvements, accumulated sediment removal, and the installation of a stormwater treatment area (STA) to improve water quality by reducing nutrient and sediment discharge into the C-24 Canal and the North Fork. 
Documents Included
· DEP Agreement #S0239 E8 Waterway Project 09.30.05 (Grant assistance agreement)
· Baffle box calculations can be found on page 23 of the PDF.
· Port St. Lucie 112912_Distribution (Excel spreadsheet)
· Reduction credit calculations for all Port St. Lucie projects
· Each project has its own tab with data and calculations.
· 070601-4_StaffRpt_159047 (permit)
· All information typical of a SFWMD Environmental Resource Standard General Permit (general conditions, special conditions, notice of rights, project evaluation, related concerns)
· Permit is written for more work than just this specific project.
· [bookmark: _GoBack]Operational information can be found on pages 6 through 8 of the PDF.
