S-01: Poppleton Creek – Phase II and III
Project Summary
This project consists of stormwater improvements in the 271-acre Poppleton Creek Basin which discharges into St. Lucie River South and is primarily urban. It involves an inline wet detention pond that is enhanced with extensive wetland plantings and provides treatment of TSS, nutrients, heavy metals, and debris. Its design provides 7.9 ac-ft of storage which equates to 0.35 inches of treatment across the basin. The pond was built with 48.85 ac-ft of permanent pool volume.
[bookmark: _GoBack]Documents Included
· Stuart_112912_Distribution (Excel spreadsheet)
· Reduction credit calculations for all Stuart projects
· Each project has its own tab with data and calculations.
· Wet detention calculations for Poppleton Creek (residence time, TN efficiency, and TP efficiency) are on the ‘Wet Detention Calcs’ tab.
· S0278-poppleton-creek-fr (Final Report) 
· Specifications on page 10, pollutant loading on page 12.
