SLC-01: Platt’s Creek Stormwater Treatment Facility
Project Summary
This project captures and treat the ‘first flush’ of runoff from the approximately 1,100 acre Platt’s Creek watershed. It is designed to capture the first 0.66 inches of runoff from all storm events. The water that gets pumped into the pond then gets discharged to a wetland mitigation area before flowing into Platt’s Creek downstream.
Documents Included
· 080410-9_446055 (SFWMD permit)
· All information typical of a SFWMD Environmental Resource Standard General Permit (general conditions, special conditions, notice of rights, project evaluation, related concerns)
· Operational information can be found on pages 55 and 56 of the permit PDF.
· [bookmark: _Hlk495400448]St. Lucie County MS4 112912_Distribution (Excel spreadsheet)
· Reduction credit calculations for all St. Lucie County MS4 projects
· Each project has its own tab with data and calculations.
· [bookmark: _GoBack]Wet detention pond residence time, runoff, TN efficiency, TP efficiency, and ppv prov are included.
