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SYLLABUS

Day One – TIER I 		Qualified BMP Installer (QBI)

8:30am – 9:30am		Introduction and Chapter 1 – Erosion and Sediment Control

9:30am – 9:40am  		Break

9:40am – 10:30am		Chapter 2 – Soils 

10:30am – 10:40am		Break

10:40am – 12:00pm 		Chapter 3:	BMPs for Erosion and Sedimentation Control	
		 
12:00pm – 1:00pm		Lunch

1:00pm – 2:30pm		Chapter 4 – BMPs—Vegetation for Erosion Control

2:30pm – 2:45pm	Break

2:45pm – 4:00 pm	Chapter 5 – BMPs for Dewatering	

Note:  Attendees not interested in becoming a Qualified Compliance Inspector are not required to complete the Day Two or the TIER II portion of this class. However, you have only one year from this date to take TIER II without having to repeat TIER I portion.  Thank you for attending this portion.  Also, there is no certificate given for TIER I portion. 

[bookmark: _GoBack]Day Two – TIER II		Qualified Compliance Inspector (QCI) and Exam

8:30am – 9:30am		Chapter 6: Regulations and Statutory Requirements for Erosion Control

9:30am – 9:40am		Break

9:40am – 10:15am		Chapter 7 - The Stormwater Pollution Prevention Plan (SWPPP)

10:15am – 10:35am	Chapter 8 - BMPs for Stormwater Management 

10:35am – 10:45am		Break

10:45am – 11:30am		Chapter 9 – Inspection and Enforcement
				
11:30am – 12:30pm		Proctored Exam - Exams will be graded today.

Please note, you will have one hour to complete this exam. Normally it takes 40 minutes.  This is a closed book exam, with 100 questions. 70% or greater is a passing score.  If you pass, you will receive a qualification certificate which does not require renewal or CEUs. Thank you for attending! 
Universal Soil Loss Equation (USLE) and Corresponding
C-Factors and P-Factors
The Universal Soil Loss Equation  (USLE)
A = R x K x L x S x C x P
· A = Average annual soil loss (tons/acre)
· R = Rainfall erosion index (Rainfall Kinetic Energy)
· K = Soil erodibility factor (soil survey data)
· L = Slope length factor (dimensionless)
· S = Slope gradient factor (dimensionless)
· C = Vegetative cover factor (dimensionless)
· P = Control practices factor (contractor)
Rainfall is the only factor not under your control!









BMPs or Treatments and Corresponding                       C-FACTORS and P-FACTORS
TREATMENT
C-FACTOR
P-FACTOR
E OR S
Bare Soil/Packed and smooth
1.60
1.60

Bare Soil/Roughen
1.00
0.90
S
Sediment Trap or Basin
1.00
0.10 to 0.90
S
Straw Bale
1.00
0.9
S
Silt Fence
1.00
0.6
S
Temporary Vegetation
0.45
1.0
E
Established Vegetation
 >80% Ground Cover
<0.05
1.0
E
Grass Sod
0.01
1.0
E
Rolled Erosion Control Product
0.10 to 0.30
1.0
E
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