STATION ID: _______________	DATE: _______________		TIME (EST): ______________
STATE OF FLORIDA
DEPARTMENT OF ENVIRONMENTAL PROTECTION
SPRINGS SAMPLING FIELD SHEET
Station Information

STATION ID:_________________________       DATE:_________________	  TIME (EST):_______________ (24 hr)           
                                                                                                   (MM/DD/YYYY)                        (Final field measurements; start of sampling)

SPRING NAME:_________________________		VENT ID:_________________________
														
WEATHER CONDITIONS (Circle One)        Clear	             Partly Cloudy	          Cloudy                     Rain


Water Quality Measurements

Secchi Depth: _______________ (meters)	Secchi Visible on Bottom	Yes	 No   (Circle One)

Stage (if available): _______________ (Feet)

Estimated depth in vent from which laboratory samples were collected: ___________ (meters)

Analytes collected for this site are as listed per the container inventory, including QA/QC samples	Yes	No
	
Field Measurements (if field measurement result has to be qualified, enter F next to the value below):
	
	Estimated Depth (meters)
	Meter Id
	Measurement #
	pH (s.u.)
	D.O. (mg/L)
	% D.O.
	Temperature (oC)
	Conductivity (uS/cm)



 (
Was a new 0.45-micron capsule filter used to collect the final metals and nutrients/anions samples?
Yes
 No
   
(Circle One)
Were all appropriate samples preserved within 15 minutes
?
Yes
No
  
Were total nutrient samples preserved with sulfuric acid?
Yes
No
Total volume added _____ (mL)
Final pH ____ (s.u.)
Were filtered nutrient samples preserved with sulfuric acid?
Yes
No
Total volume added _____ (mL)
Final pH ____ (s.u.)
Were total metal samples preserved with nitric acid?
Yes
No
Total volume added _____ (mL)
Final pH ____ (s.u.)
Were filtered metal samples preserved with nitric acid?
Yes
No
Total volume added _____ (mL)
Final pH ____ (s.u.)
(If additional bottles for the nutrient or metal samples were preserved, note volume of acid added and final pH for each one in the Comments)
Were all 
appropriate samples
, in accordance with the container inventory,
 put on wet ice at 4
o
C?
Yes
No
)Sample Preservation













 (
COMMENTS
:
_
____________________________
_______________________________
__________________________________________________________________________
__________________________________________________________________________
__________________________________________________________________________
__________________________________________________________________________
)QA/QC TAKEN?
 (
TIME E 
COLLECTED 
 _
____
   
(Circle One)
                                                                                      
   
  
EQUIPMENT BLANK
 
   
FIELD BLANK TIME E 
COLLECTED 
 _
____
   
(Circle One)
                                                                                      
   
  
EQUIPMENT BLANK
 
   
FIELD BLANK
) 		
	TIME COLLECTED __________

	(Circle One)

	EQUIPMENT BLANK

	FIELD BLANK

Blanks collected in accordance with Springs Initiative Monitoring SOP
 (
Samplers Signatures
 (all team members present)
:
)
Place
Barcode 
Label 
Here
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CHEMICAL STABILITY MONITORING

	#
	TIME
(00:00)
	pH
(s.u.)
	TEMP. (oC)
	SP.  COND
(uS/cm)
	DO
(mg/L)
	% SAT DO (%)
	COMMENTS

	1
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	

	4
	
	
	
	
	
	
	

	5
	
	
	
	
	
	
	

	6
	
	
	
	
	
	
	

	7
	
	
	
	
	
	
	

	8
	
	
	
	
	
	
	

	9
	
	
	
	
	
	
	

	10
	
	
	
	
	
	
	

	11
	
	
	
	
	
	
	

	12
	
	
	
	
	
	
	

	13
	
	
	
	
	
	
	

	14
	
	
	
	
	
	
	

	15
	
	
	
	
	
	
	




Meter Id: _________________________________     Field Measurements Analyzed By: _______ (initials)

	Field Measurements Recorded By: _______ (initials)

The final three measurements will be evaluated for each of the field parameters listed above (only the values in mg/L for DO) to ensure that representative measurements have been collected for a site.  The lowest and highest values for the three measurements must be within 20% when calculating the relative percent difference (RPD).  If these values are not within 20%, the final field measurement value will be qualified as being estimated with an F value qualifier.

	RPD =           (Highest Value – Lowest Value)	 	X 100%           
	(Mean Value of Highest and Lowest Values)
