[image: image1.jpg]EERPWATER

ORIZON

coesls)

ESPONSE ™




[image: image1.jpg]

Bay County Daily Sampling Report
August 5, 2010
The Florida Department of Environmental Protection is collecting and analyzing water, sediment, and oil samples from Florida’s coastal waters in response to the Deepwater Horizon oil spill.  These samples are being collected for a variety of purposes.  There is a delay from when the samples are collected to when the results are reported due to the time that it takes to deliver the samples to the lab and then analyze the samples.  We are striving for a four day turnaround time.  Results will be reported on a daily basis as available.  

New information for Bay County: 

· Week of July 31 thru August 6, 2010 Water quality samples proposed to be collected on Monday & Thursday.

·  Two water samples are planned per collection day.  If oil product is seen in the water, we will sample in proximity to it.  If no oil is seen we will likely sample at beach locations.
· Note: For new water quality result information please see the rows highlighted in yellow below.

The following sampling has been performed in Bay County:

· May 1 – 7, 2010: Baseline sampling occurred at eight sites within St. Andrews Bay and at beach sites (Laguna Beach, St Andrews State Park, and Mexico Beach). All the water samples and seven of the eight sediment samples exhibited no detectable concentrations of petroleum contamination. One sediment sample had trace levels of several petroleum constituents due to proximity to local sources. 

· Table entries that are different from the previous day are highlighted in yellow.
	Date Sampled
	Sampling Information
	Results

	Laguna Beach Access # 85

	7/29/2010
	Water sample
	No petroleum-related contaminants were found

	8/2/2010
	Water sample
	No petroleum-related contaminants were found

	
	
	

	Panama City beach at Coleman Road

	7/29/2010
	Water sample
	No petroleum-related contaminants were found

	Panama City Access #42

	8/2/2010
	Water sample
	No petroleum-related contaminants were found

	
	
	

	
	
	

	
	
	


Table Explanation:

· Water sample – indicates a water sample that was taken, no oil was visible in the water when the sample was taken.

· Sand sample – indicates a sand sample that was taken to evaluate any potential petroleum contamination.  
· 10 cm from visible tar ball/1 meter from visible tar ball – These are types of proximity sampling that means samples were collected at known distances from oil.  This sampling is performed when the oil in the water is sparse enough that a bather might reasonably expect to swim in the water without coming into contact with the oil.  

· Collected for dispersant analysis – These samples are collected to attempt to detect dispersant.  The first priority is to collect the sample in proximity to oil when oil is present.  When oil is not present the second priority is to sample in locations were oil was previously present, the third priority is to collect the sample where no oil contamination is, or ever was, present.  

For additional information, please refer to the DEP Deepwater Horizon website at http://www.dep.state.fl.us/deepwaterhorizon/default.htm
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