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Franklin County Daily Sampling Report
The Florida Department of Environmental Protection is collecting and analyzing water, sediment, and oil samples from Florida’s coastal waters in response to the Deepwater Horizon oil spill.  These samples are being collected for a variety of purposes.  There is a delay from when the samples are collected to when the results are reported due to the time that it takes to deliver the samples to the lab and then analyze the samples.  We are striving for a four day turnaround time.    
New information for July 9, 2010: 

· Proposed – Week of July 9-15.  Sampling is proposed for one day this next week.  This situation will change as conditions warrant.
· Sampling reports will be provided when samples have been taken and there are lab results to report.  
· Note: For new water quality result information please see the rows highlighted in yellow below.  

The following sampling has been performed in Gulf County:

· Sampling occurred at two locations on July 6, at public access beaches in Carabelle and St. George Island. 

	Date Sampled
	Sampling Information
	Results

	Carabelle Public Access Beach

	7/6/2010
	Water sample
	No petroleum-related contaminants were found.

	St. George Island Public Beach Access

	7/6/2010
	Water sample
	No petroleum-related contaminants were found.

	

	
	
	


Table Explanation:

· Water sample – indicates a water sample that was taken, no oil was visible in the water when the sample was taken.

· Sand sample – indicates a sand sample that was taken to evaluate any potential petroleum contamination.  
· 10 cm from visible tar ball/1 meter from visible tar ball – These are types of proximity sampling that means samples were collected at known distances from oil.  This sampling is performed when the oil in the water is sparse enough that a bather might reasonably expect to swim in the water without coming into contact with the oil.  

· Collected for dispersant analysis – These samples are collected to attempt to detect dispersant.  The first priority is to collect the sample in proximity to oil when oil is present.  When oil is not present the second priority is to sample in locations were oil was previously present, the third priority is to collect the sample where no oil contamination is, or ever was, present.  

For additional information, please refer to the DEP Deepwater Horizon website at http://www.dep.state.fl.us/deepwaterhorizon/default.htm
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