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Walton County Daily Report
July 26, 2010
The Florida Department of Environmental Protection is collecting and analyzing water, sediment, and oil samples from Florida’s coastal waters in response to the Deepwater Horizon oil spill.  These samples are being collected for a variety of purposes.  There is a delay from when the samples are collected to when the results are reported due to the time that it takes to deliver the samples to the lab and then analyze the samples.  We are striving for a four day turnaround time.  Results will be reported on a daily basis.  
New information for July 26, 2010: 
Week of July 23 - 29
· Two water samples were collected today in Walton County.  One in Miramar Beach and one in Grayton Beach.  Sampling team observed a lot of algae in the water today, particularly at the Miramar Beach site.
· Proposed – Sampling is proposed to continue this week - 2 water samples on Thursday. 
· If oil product is seen in the water, we will sample in proximity to it.  If no oil is seen we will likely sample in locations such as Miramar Beach, Blue Mountain Beach, and Grayton Beach.   
· Note: For new water quality results information please see the rows highlighted in yellow below.

The following sampling has been performed in Walton County:

	Date Sampled
	Sampling Information
	Results

	NO NEW LAB RESULTS TODAY

	BLUE MOUNTAIN BEACH

	
	
	

	DEER LAKE STATE PARK

	
	
	

	ED WALLINE PARK

	
	
	

	 GRAYTON BEACH STATE PARK

	
	
	

	
	
	

	MIRAMAR BEACH

	
	
	

	
	
	

	SEAGROVE BEACH

	
	
	

	SEASIDE @ CR 395

	 
	
	

	SEASIDE @ WESTERN LAKE DR

	
	
	

	
	
	

	SOUTH WALTON BEACH – DUNE ALLEN
	
	

	
	
	

	
	
	

	ALLEN REGIONAL BEACH ACCESS 
	
	

	
	
	

	SEASIDE BEACH  
	
	

	
	
	


Table Explanation:

· Water sample – indicates a water sample that was taken, no oil was visible in the water when the sample was taken.

· Sand sample – indicates a sand sample that was taken to evaluate any potential petroleum contamination.  
· 10 cm from visible tar ball/1 meter from visible tar ball – These are types of proximity sampling that means samples were collected at known distances from oil.  This sampling is performed when the oil in the water is sparse enough that a bather might reasonably expect to swim in the water without coming into contact with the oil.  

· Collected for dispersant analysis – These samples are collected to attempt to detect dispersant in the water where no oil contamination has been observed.  

For additional information, please refer to the DEP Deepwater Horizon website at http://www.dep.state.fl.us/deepwaterhorizon/default.htm
2

