WALTON COUNTY DAILY SAMPLING REPORT
July 6, 2010
The Florida Department of Environmental Protection is collecting and analyzing water, sediment, and oil samples from Florida’s coastal waters in response to the Deepwater Horizon oil spill.  These samples are being collected for a variety of purposes.  There is a delay from when the samples are collected to when the results are reported due to the time that it takes to deliver the samples to the lab and then analyze the samples.  We are striving for a four day turnaround time.  Results will be reported on a daily basis.  
New information for July 6, 2010: 
· Water samples were collected each day (two per day) on Friday July 2, Saturday July 3, Sunday July 4, Monday July 5 and today, Tuesday July 6.  
· Proposed – Two water samples will be collected on Thursday, July 8.  
· If oil product is seen in the water, we will sample in proximity to it.  If no oil is seen we will likely sample in locations such as Miramar Beach, Blue Mountain Beach, and Grayton Beach.  
· Note: For new water quality results information please see the rows highlighted in yellow below.
The following sampling has been performed in Walton County:
	Date Sampled
	Sampling Information
	Results

	

	BLUE MOUNTAIN BEACH

	
	
	

	DEER LAKE STATE PARK

	
	
	

	ED WALLINE PARK

	
	
	

	 GRAYTON BEACH STATE PARK

	6/28/10 
	3 sediment samples
	Trace levels of petroleum constituents were found

	6/28/10 
	Water sample
	No petroleum constituents were found

	7/02/10 
	Water sample
	No petroleum constituents were found

	MIRAMAR BEACH

	6/28/10
	3 sediment samples
	Trace levels of petroleum constituents were found

	6/28/10
	Water sample
	No petroleum constituents were found

	
	
	

	SEAGROVE BEACH

	
	
	

	SEASIDE @ CR 395

	 
	
	

	SEASIDE @ WESTERN LAKE DR

	
	
	

	
	
	

	SOUTH WALTON BEACH
	
	

	7/02/10
	Water sample
	No petroleum constituents were found



Table Explanation:
· Water sample – indicates a water sample that was taken, no oil was visible in the water when the sample was taken.

· Sand sample – indicates a sand sample that was taken to evaluate any potential petroleum contamination.  

· 10 cm from visible tar ball/1 meter from visible tar ball – These are types of proximity sampling that means samples were collected at known distances from oil.  This sampling is performed when the oil in the water is sparse enough that a bather might reasonably expect to swim in the water without coming into contact with the oil.  

· Collected for dispersant analysis – These samples are collected to attempt to detect dispersant in the water where no oil contamination has been observed.  

None of the results listed above suggest that recreational activities should be restricted; however, the movement of oil product is unpredictable and conditions at a given location can change rapidly. The public should be advised not to go in the water with visible petroleum products.
