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Tar Ball Sampling 
(if tar balls are in water)
X 
=  sample
) (
water
) (
shore
 (beach)
)
 (
Select 
2
 separate
 locations
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(3 from each= 6 total samples)
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            location 2
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 separate
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(3 from each= 6 total samples)
        
location
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Select 
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location in area of NO tar balls
(3 total samples)
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In 
1
 
area of heavy tar balls, do a micro-transect:
(8 total samples)
10 cm away from a tar ball:
X-Rep 1
X-Rep 2
1m away from tar ball area:
X-Rep 1
X-Rep 2
10m away from tar ball area:
 
X-Rep 1
X-Rep 2
20m away from tar ball area:
X-Rep 1
X-Rep 2
)





