EXAXOL

manufacturers of laboratory solutions/standards since 1988
CERTIFICATE OF ANALYSIS
Product: Conductivity Standard, 100 (-mhos  (C1065-100) 
Lot: 171211B                                                 Expires: (1 year)  12/2018
Assay (ppm, M, N, %, etc)
    Actual:  100+/- 0.5%
Contains:   Potassium Chloride, Water: both ACS

Other results: 100  (-mhos  @  25° C


Conductivity changes with temperature as follows:

20C: 91.0
21C: 92.7
22C: 94.5
23C: 96.3
24C: 98.1
25C: 100.0

26C: 101.9
27C: 103.9
28C: 105.8
29C: 107.9
30C: 109.9

TDS= 50.7 ppm KCl
Made in accordance with written standard Good Laboratory Practice Procedures. Volumetric glassware used is strictly Class A per ASTM E288 requirements, maintained in accordance with ASTM E 542.  Analytical balance(s) calibrated periodically using certified Class S NIST weights, and documented.  Thermometers used are NIST calibrated.  Standardized products prepared according to Master Lab Record book, with lot #, batch size, customer , and testing results.  

STORAGE: ambient (15 degC-30 degC) 

Standards used:
NIST: Potassium Chloride KCl 3193
Exaxol:

Joseph E Papa, Sr. Chemist     

EXAXOL CHEMICAL CORP, 14325 60th St N, Clearwater, FL 33760

 Ph: (727) 524-7732  Fax: (727) 532-8221

