EXAXOL

manufacturers of laboratory solutions/standards in 1988 
CERTIFICATE OF ANALYSIS
Product: Conductivity Standard, 10,000 (-mhos  (C-1065-10000)
Lot:   160222C                    
Expires: (1 yr) 03/2017 
Assay (ppm, M, N, %, etc)
Actual:  10,000
Contains: Potassium chloride, water: both ACS

Other results: 10,000  (-mhos  @  25° C (+/- 0.3%) 

Temperature Conversion Factor = 1.850%
Conductivity changes with temperature as follows:

0C: 5375
1C: 5560
2C: 5745
3C: 5930
4C: 6115
5C: 6300
6C: 6485
7C: 6670
8C: 6855
9C: 7040
10C: 7225
11C: 7410

12: 7595
13C: 7780
14C: 7965
15C: 8150
16C: 8335
17C: 8520
18C: 8705
19C: 8890
20C: 9075
21C: 9260
22C: 9445
23C: 9630

24C: 9815
25C: 10000
26C: 10185
27C: 10370
28C: 10555
29C: 10740
30C: 10925
31C: 11110
32C: 11295
33C: 11480
34C: 11665
35C: 11850

TDS= 5,701 ppm KCl

Made in accordance with written standard Good Laboratory Practice Procedures. Volumetric glassware used is strictly Class A per ASTM E288 requirements, maintained in accordance with ASTM E 542.  Analytical balance(s) calibrated periodically using certified Class S NIST weights, and documented.  Thermometers used are NIST calibrated.  Standardized products prepared according to Master Lab Record book, with lot #, batch size, customer , and testing results.  

STORAGE: ambient (15 degC-30 degC) 

Standards used:
NIST: Potassium Chloride KCl 3193
Exaxol:

Joseph E Papa, Sr. Chemist     
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