General
The following information and resources are applicable to all program areas within the DWM.
Download and Install the Latest Version of the ADaPT Software
· ADaPT 9.0.11 Install Package [ZIP file - 70.2 MB]
· Download and read the installation instructions.
· The ADaPT software requires Microsoft Office Access version 2007, 2010 (32-bit only) or 2013 (32-bit only).
· ADaPT 9.0.11 will install and run under MS Access 2016 (32-bit only) or Office 365 with Access (32-bit only);. Please see the Notes on page one of the ADaPT 9.0.11 installation instructions for details
· Update_ADaPT_Instructions.pdf – update to DWM Library and ADaPT valid values, (if the last update or full installation is more than six months ago). 

DWM ADaPT Library of Analytical Methods and Valid Values
· Division of Waste Management Master Library (updated 04/24/2025) - The library contains DWM appropriate analytical methods for matrices and analytes, method required QC elements, and method specific QC element control limits.
· DWM Library Additions - Provides details on the procedure for adding appropriate methods and analytes to the library.
· DWM Library History - Provides a complete list of library modifications and additions.
· Monitoring Testsite Inventory (Right-click and save to local drive.)

Reference Documentation
· ADaPT DWM User Guide ADaPT_DWM_User_Guide_PrintFriendly (working copy subject to change) --> - Contains information on how to install ADaPT, import data, check the data for completeness (and error check), evaluate data QC, evaluate the data against various standards and criteria, and prepare the data for export to upload to DEP Oracle Databases including REDD and WACS. The ADaPT Users Guide also includes reference information along with responsibilities and uses of ADaPT by labs, consultants, permittees and DEP staff.
· ADaPT FAQ
· ADaPT Error Check Guidance
· ADaPT Version History

