Ground Water Parameters
Acreage
Loxahatchee, Palm Beach County, Florida
FDEP, Site Investigation Section


	Sample ID
	Date
	Time
	Volume Purged
(gallons)
	pH
(standard units)
	Temperature
(°C)
	Specific Conductance
(microSiemens/cm)
	Dissolved
Oxygen
(%)
	Dissolved
Oxygen
(mg/L)
	ORP
(millivolts)
	Turbidity 
(NTUs)

	5Z-SID No.1
	08/26/2009
	11:08
11:12
	NA
	7.49
7.34
	24.73
24.57
	2259
2272
	33.0
31.0
	2.73
2.56
	-221.8
-240.8
	0.63
0.36

	5Z-SID No. 2
	08/26/2009
	10:20
10:24
	NA
	7.23
7.23
	24.23
24.20
	2458
2460
	28.2
24.20
	2.35
2.34
	-235.2
-240.2
	3
3

	5Z-SID No. 3
	08/05/2009
08/26/2009
08/26/2009
	14:02
09:47
09:51
	NA
	6.90
7.13
7.11
	23.99
24.18
24.14
	3316
3085
3100
	0.9
26.7
25.9
	0.07
2.23
2.16
	-156.2
-215.9
-223.0
	0.51
4
2

	5Z-SID No. 4
	08/26/2009
	09:24
09:28
	NA
	7.16
7.10
	24.23
24.18
	2932
2962
	31.8
30.0
	2.64
2.50
	-195.3
-209.7
	3
3

	5Z-SID No. 5
	08/26/2009
	08:56
09:00
	NA
	6.66
6.97
	24.37
25.24
	2121
2141
	3.5
2.9
	0.30
0.25
	-185.7
-211.6
	12
4

	5Z-SID P.O.E
	08/26/2009
	11:35
11:39
	NA
	8.55
8.84
	25.54
25.52
	292
286
	92.4
89.7
	7.64
7.29
	458.2
530.9
	0.40
0.39

	5Z-SID Reject Water
	08/26/2009
	11:53
11:57
	NA
	6.33
6.31
	24.92
24.90
	10236
10303
	4.3
5.1
	0.33
0.41
	-167.7
-170.3
	0.57
0.56

	5Z-SID Repump Water
	08/26/2009
	12:31
12:34
	NA
	8.58
8.72
	27.38
27.41
	213
213
	108.2
106.5
	8.59
8.39
	585.2
603.4
	0.66
0.26



