Table 4:  Summary of Analytical Results For Surface Water Samples
The Acreage Community, Loxahatchee, Palm Beach County, Florida
FDEP Site Investigation
	


	Analyte 
	GCTL 
	1Z-16104 93rd Rd N
8/4/2009

	1Z-16231 70th St N
8/4/2009
	1Z-16441 87th Ln N
8/4/2009
	1Z-16441 87th Ln N
8/27/2009
	1Z-16525 Temple Blvd
8/6/2009
	1Z-16758 67th Ct N
8/4/2009
	1Z-17148 Hamlin Blvd
8/4/2009
	1Z-17639 68th St N
8/4/2009

	Gross Alpha
	15 pCi/L
	1.8 
	4.8 
	7.1 
	8.4
	3.5 
	4.6
	6.6
	7.3 

	Aluminum
	200 ug/L (SSO)
	6.5
	ND
	58
	NA
	30
	58
	ND
	8.8

	Arsenic
	10 ug/L
	0.51
	ND
	ND
	NA
	ND
	0.55
	ND
	0.35

	Barium
	2000 ug/L
	22.5
	25.5
	13.8
	NA
	9.6
	39.9
	25.7
	36.6

	Chromium
	100 ug/L
	1.0
	ND
	0.42
	NA
	0.74
	0.32
	ND
	ND

	Copper
	1000 ug/L (SSO)
	1.93
	2.61
	ND
	NA
	2.32
	26.6
	1.48
	4.54

	Lead
	15 ug/L
	0.30
	0.26
	ND
	NA
	ND
	3.93
	ND
	0.85

	NO2/NO3
	10,000 ug/L
	25
	12
	4
	NA
	6
	ND
	8
	ND

	Radium 226/228
	5 pCi/L
	1.0 
	NA
	NA
	0.8
	NA
	NA
	NA
	3.8

	Strontium
	4200 ug/L (MCST)
	594
	1180
	622
	NA
	1210
	835
	787
	420

	1,4-Dioxane
	3.2 ug/L (MCC)
	ND
	ND
	0.43
	NA
	ND
	ND
	ND
	ND

	Titanium
	Not Established
	ND
	ND
	0.50
	NA
	1.4
	0.88
	ND
	ND



ND=Non Detect
NA=Not Analyzed
Yellow Infill=Exceedance of Ground Water Cleanup Target Level
ug/L= micrograms per Liter
pCi/L=picocuries per Liter
SSO=Secondary Standard Organoleptic
MCST=Minimum Criteria Systemic Toxicant
MCC=Minimum Criteria Carcinogen
Primary Standard Unless Otherwise Noted







	Analyte 
	GCTL 
	1Z-17724 60th Ln N 
8/4/2009

	1Z-17724 60th Ln N
8/27/2009
	1Z-17855 83rd Pl N
8/4/2009
	1Z-17895 80th St N
8/4/2009
	1Z-18801 Hamlin Blvd
8/4/2009
	2Z-14072 78th Pl N
8/5/2009
	2Z-14390 Orange Blvd
8/5/2009
	2Z -14692 Tangerine Blvd
8/4/2009

	Gross Alpha
	15 pCi/L
	ND
	3.4
	2.5 
	2.9
	4.7
	2.3 
	1.6 
	15.6

	Aluminum
	200 ug/L (SSO)
	ND
	NA
	ND
	ND
	ND
	ND
	ND
	ND

	Arsenic
	10 ug/L
	ND
	NA
	ND
	0.79
	1.10
	ND
	ND
	1.01

	Barium
	2000 ug/L
	53.8
	NA
	30.1
	31.0
	49.3
	29.1
	20.8
	65.1

	Chromium
	100 ug/L
	ND
	NA
	ND
	ND
	ND
	0.34
	ND
	0.30

	Copper
	1000 ug/L (SSO)
	3.65
	NA
	3.22
	0.89
	13.1
	ND
	ND
	1.02

	Lead
	15 ug/L
	0.30
	NA
	0.25
	ND
	6.37
	ND
	ND
	ND

	NO2/NO3
	10,000 ug/L
	9
	NA
	ND
	ND
	ND
	5
	ND
	6

	Radium 226/228
	5 pCi/L
	NA
	1.3
	NA
	NA
	NA
	NA
	1.0 
	NA

	Strontium
	4200 ug/L (MCST)
	988
	NA
	677
	917
	547
	589
	391
	528




ND=Non Detect
NA=Not Analyzed
Yellow Infill=Exceedance of Ground Water Cleanup Target Level
ug/L= micrograms per Liter
pCi/L=picocuries per Liter
SSO=Secondary Standard Organoleptic
MCST=Minimum Criteria Systemic Toxicant
MCC=Minimum Criteria Carcinogen
Primary Standard Unless Otherwise Noted










	Analyte 
	GCTL 
	2Z-14741 77th Pl N
8/5/2009

	2Z-15163 82nd Ln N
8/5/2009
	2Z-15285 95th Ln N
8/4/2009
	2Z-15365 71st Pl N
8/4/2009
	2Z-15553 63rd Pl N
8/5/2009
	2Z-15670 78th Pl N
8/4/2009 
	2Z -9035 Hall Blvd
8/4/2009

	Gross Alpha
	15 pCi/L
	ND
	ND
	ND
	2.2 
	2.8 
	3.8 
	ND

	Aluminum
	200 ug/L (SSO)
	ND
	ND
	ND
	ND
	ND
	ND
	ND

	Arsenic
	10 ug/L
	ND
	ND
	ND
	0.29
	0.27
	ND
	ND

	Barium
	2000 ug/L
	8.77
	14.9
	42.1
	29.6
	14.3
	28
	36.9

	Chromium
	100 ug/L
	ND
	ND
	ND
	ND
	ND
	0.47
	ND

	Copper
	1000 ug/L (SSO)
	ND
	0.52
	ND
	1.03
	ND
	ND
	4.49

	Lead
	15 ug/L
	ND
	ND
	ND
	ND
	ND
	ND
	0.61

	NO2/NO3
	10,000 ug/L
	ND
	4
	28
	9
	7
	7
	16

	Radium 226/228
	5 pCi/L
	NA
	NA
	NA
	NA
	NA
	NA
	2.2

	Strontium
	4200 ug/L (MCST)
	1080
	795
	748
	515
	848
	786
	1190

	MTBE
	20 ug/L (MCO)
	ND
	ND
	ND
	ND
	0.72
	ND
	ND



ND=Non Detect
NA=Not Analyzed
Yellow Infill=Exceedance of Ground Water Cleanup Target Level
ug/L= micrograms per Liter
pCi/L=picocuries per Liter
SSO=Secondary Standard Organoleptic
MCST=Minimum Criteria Systemic Toxicant
MCC=Minimum Criteria Carcinogen
MCO=Minimum Criteria Organoleptic
Primary Standard Unless Otherwise Noted





	Analyte 
	GCTL 
	3Z-11546 60th St N
8/5/2009

	3Z-11546 60th St N
8/27/2009
	3Z-11843 Tangerine Blvd
8/5/2009
	3Z-11843
Tangerine
Blvd
8/27/2009
	3Z-11855 Keswick Way
8/4/2009
	3Z-12325 87th St N
8/5/2009
	3Z-12754 77th Pl  N
8/5/2009
	3Z- 13048 82nd St N
8/5/2009

	Gross Alpha
	15 pCi/L
	ND
	2.4
	8.9 
	9.0
	2.3 
	1.4 
	ND
	ND

	Aluminum
	200 ug/L (SSO)
	ND
	NA
	ND
	NA
	ND
	31
	7.1
	ND

	Arsenic
	10 ug/L
	0.36
	NA
	1.58
	NA
	ND
	ND
	ND
	ND

	Barium
	2000 ug/L
	27.7
	NA
	92.9
	NA
	16.4
	14.9
	11.3
	10.4

	Chromium
	100 ug/L
	0.47
	NA
	ND
	NA
	0.73
	0.73
	0.79
	0.40

	Copper
	1000 ug/L (SSO)
	ND
	NA
	3.40
	NA
	1.01
	2.09
	7.77
	8.48

	Lead
	15 ug/L
	ND
	NA
	ND
	NA
	ND
	0.38
	0.82
	0.41

	NO2/NO3
	10,000 ug/L
	4
	NA
	5
	NA
	6
	ND
	4
	ND

	Radium 226/228
	5 pCi/L
	NA
	1.6
	NA
	5.6
	0.3
	NA
	NA
	NA

	Strontium
	4200 ug/L (MCST)
	393
	NA
	680
	NA
	730
	436
	335
	889

	1,4-Dioxane
	3.2 ug/L (MCC)
	ND
	NA
	0.34
	NA
	ND
	ND
	ND
	ND




ND=Non Detect
NA=Not Analyzed
Yellow Infill=Exceedance of Ground Water Cleanup Target Level
ug/L= micrograms per Liter
pCi/L=picocuries per Liter
SSO=Secondary Standard Organoleptic
MCST=Minimum Criteria Systemic Toxicant
MCC=Minimum Criteria Carcinogen
Primary Standard Unless Otherwise Noted






	Analyte 
	GCTL 
	3Z-13678 82nd St N
8/5/2009
	3Z-13756 73rd St N
8/5/2009

	3Z-13920 63rd Ln N
8/5/2009
	3Z-7655 Woodmuir Dr
8/5/2009
	4Z-11060 56th Pl N
8/5/2009
	4Z-11499 51st Ct N
8/5/2009
	4Z-11919 Orange Grove Blvd
8/5/2009
	4Z-13355 54th Ln N
8/5/2009

	Gross Alpha
	15 pCi/L
	ND
	2.2
	6.2 
	ND
	ND
	2.7 
	ND
	1.1

	Aluminum
	200 ug/L (SSO)
	ND
	5.6
	6.4
	ND
	7.7
	ND
	ND
	ND

	Arsenic
	10 ug/L
	ND
	ND
	ND
	ND
	0.54
	1.46
	ND
	ND

	Barium
	2000 ug/L
	10.2
	14.9
	33.1
	12.6
	18.8
	27.8
	11.6
	13.0

	Chromium
	100 ug/L
	0.52
	0.62
	0.48
	0.98
	ND
	0.31
	1.7
	1.3

	Copper
	1000 ug/L (SSO)
	0.56
	5.63
	4.61
	2.71
	1.85
	1.58
	ND
	0.67

	Lead
	15 ug/L
	0.20
	0.29
	ND
	0.38
	ND
	ND
	ND
	ND

	NO2/NO3
	10,000 ug/L
	7
	5
	7
	ND
	ND
	5
	5
	8

	Radium 226/228
	5 pCi/L
	NA
	NA
	2.4 
	NA
	0.6 
	NA
	NA
	NA

	Strontium
	4200 ug/L (MCST)
	466
	675
	972
	648
	222
	422
	958
	672

	1,1,2-TCA
	5 ug/L
	ND
	0.22
	ND
	ND
	ND
	ND
	ND
	ND

	1,2-DCA
	3 ug/L
	ND
	0.21
	ND
	ND
	ND
	ND
	ND
	ND




ND=Non Detect
NA=Not Analyzed
Yellow Infill=Exceedance of Ground Water Cleanup Target Level
ug/L= micrograms per Liter
pCi/L=picocuries per Liter
SSO=Secondary Standard Organoleptic
MCST=Minimum Criteria Systemic Toxicant
MCC=Minimum Criteria Carcinogen
Primary Standard Unless Otherwise Noted




	Analyte 
	GCTL 
	4Z-13445 44th PL N
8/5/2009

	4Z-4331 Coconut Blvd
8/6/2009
	4Z-5806 Coconut Blvd
8/5/2009
	4Z-5924 Avocado Blvd
8/5/2009
	4Z-5924 Avocado Blvd
8/26/2009
	5Z-14155 43rd RD N
8/5/2009
	5Z-14155 43rd Rd N
8/27/2009
	5Z-14563 40th St N
8/5/2009

	Gross Alpha
	15 pCi/L
	3.1 
	2.7 
	ND
	1.3
	ND
	6.2
	4.2
	4.5

	Aluminum
	200 ug/L (SSO)
	89
	ND
	ND
	ND
	NA
	26
	NA
	ND

	Arsenic
	10 ug/L
	ND
	4.83
	ND
	ND
	NA
	0.45
	NA
	0.39

	Barium
	2000 ug/L
	6.51
	49.4
	16.0
	18.9
	NA
	44.9
	NA
	45.3

	Chromium
	100 ug/L
	1.2
	ND
	0.57
	0.72
	NA
	0.83
	NA
	ND

	Copper
	1000 ug/L (SSO)
	1.50
	6.01
	2.51
	0.83
	NA
	3.24
	NA
	0.80

	Lead
	15 ug/L
	0.57
	0.31
	ND
	0.21
	NA
	0.23
	NA
	ND

	NO2/NO3
	10,000 ug/L
	7
	5
	21
	5
	NA
	9
	NA
	8

	Radium 226/228
	5 pCi/L
	NA
	NA
	NA
	NA
	0.2
	NA
	2.8
	NA

	Strontium
	4200 ug/L (MCST)
	813
	320
	1080
	683
	NA
	1070
	NA
	562

	Titanium
	Not Established
	5.1
	ND
	ND
	ND
	NA
	1.2
	NA
	ND

	MTBE
	20 ug/L (MCO)
	ND
	ND
	ND
	ND
	NA
	1.5
	NA
	ND




ND=Non Detect
NA=Not Analyzed
Yellow Infill=Exceedance of Ground Water Cleanup Target Level
ug/L= micrograms per Liter
pCi/L=picocuries per Liter
SSO=Secondary Standard Organoleptic
MCST=Minimum Criteria Systemic Toxicant
MCC=Minimum Criteria Carcinogen
MCO=Minimum Criteria Organoleptic
Primary Standard Unless Otherwise Noted





	Analyte 
	GCTL 
	5Z-15530 42nd Rd N
8/27/2009
	5Z-15530 42nd Rd N
9/14/2009
	5Z-15655 42nd Rd N
8/5/2009
	5Z-15962 42nd St N
8/6/2009
	5Z-16280 Sycamore Dr E
8/5/2009
	5Z-16280 Sycamore Dr E
8/27/2009
	6Z-17368 49th St N
8/6/2009

	Gross Alpha
	15 pCi/L
	23.7
	NA
	2.3
	ND
	10.7 
	7.4
	6.5

	Aluminum
	200 ug/L (SSO)
	NA
	ND
	ND
	ND
	ND
	NA
	6.0

	Arsenic
	10 ug/L
	NA
	0.60
	0.26
	ND
	1.43
	NA
	0.36

	Barium
	2000 ug/L
	NA
	119
	10.6
	13.1
	25.6
	NA
	48.7

	Chromium
	100 ug/L
	NA
	ND
	ND
	ND
	ND
	NA
	ND

	Copper
	1000 ug/L (SSO)
	NA
	3.18
	1.31
	12.1
	0.83
	NA
	5.17

	Lead
	15 ug/L
	NA
	0.66
	ND
	3.49
	ND
	NA
	0.87

	NO2/NO3
	10,000 ug/L
	NA
	ND
	5
	ND
	5
	NA
	21

	Radium 226/228
	5 pCi/L
	13.3
	NA
	NA
	NA
	NA
	4.6
	NA

	Strontium
	4200 ug/L (MCST)
	NA
	1050
	1070
	806
	789
	NA
	1040

	Hexazione
	230 ug/L (MCST)
	NA
	ND
	0.31
	ND
	ND
	NA
	ND

	Selenium
	50 ug/L
	ND
	0.31
	ND
	ND
	ND
	ND
	ND



ND=Non Detect
NA=Not Analyzed
Yellow Infill=Exceedance of Ground Water Cleanup Target Level
ug/L= micrograms per Liter
pCi/L=picocuries per Liter
SSO=Secondary Standard Organoleptic
MCST=Minimum Criteria Systemic Toxicant
MCC=Minimum Criteria Carcinogen
Primary Standard Unless Otherwise Noted






	Analyte 
	GCTL 
	6Z-17413 44th Pl N
8/6/2009
	6Z-18768 47th Ct N
8/6/2009
	6Z-18768 47th Ct N
8/27/2009
	6Z-18852 42nd Rd N
8/6/2009
	6Z-18852 42nd Rd N
8/27/2009
	6Z-4091 Mandarin Blvd
8/5/2009

	Gross Alpha
	15 pCi/L
	2.6 
	2.9
	2.7
	6.9 
	9.8
	2.7 

	Aluminum
	200 ug/L (SSO)
	ND
	ND
	NA
	ND
	NA
	ND

	Arsenic
	10 ug/L
	0.50
	0.73
	NA
	1.26
	NA
	0.46

	Barium
	2000 ug/L
	13.0
	19.1
	NA
	38.5
	NA
	17.5

	Chromium
	100 ug/L
	ND
	ND
	NA
	ND
	NA
	ND

	Copper
	1000 ug/L (SSO)
	5.37
	0.62
	NA
	0.67
	NA
	ND

	Lead
	15 ug/L
	0.23
	ND
	NA
	ND
	NA
	ND

	NO2/NO3
	10,000 ug/L
	76
	ND
	NA
	ND
	NA
	7

	Radium 226/228
	5 pCi/L
	NA
	NA
	1.3
	NA
	5.2
	1.7

	Strontium
	4200 ug/L (MCST)
	1220
	487
	NA
	743
	NA
	1410

	Titanium
	Not Established
	0.54
	ND
	NA
	ND
	NA
	ND



ND=Non Detect
NA=Not Analyzed
Yellow Infill=Exceedance of Ground Water Cleanup Target Level
ug/L= micrograms per Liter
pCi/L=picocuries per Liter
SSO=Secondary Standard Organoleptic
MCST=Minimum Criteria Systemic Toxicant
MCC=Minimum Criteria Carcinogen
Primary Standard Unless Otherwise Noted


Table 2: Summary of Analytical Results For Private Wells
The Acreage, Loxahatchee, Palm Beach County, Florida
FDEP Site Investigation

	Analyte 
	GCTL 
	5Z-SID No. 1
(Untreated Water)
8/26/2009
	5Z-SID No. 2
(Untreated Water)
8/26/2009
	5Z-SID No. 3
(Untreated Water)
8/5/2009
	5Z-SID No. 3
(Untreated Water)
8/26/2009
	5Z-SID No. 3 Duplicate
(Untreated Water)
8/26/2009
	5Z-SID No. 4
(Untreated Water)
8/26/2009
	5Z-SID No. 5
(Untreated Water)
8/26/2009

	Gross Alpha
	15 pCi/L
	5.2
	14.7
	15.3
	19.6
	18.5
	17.1
	11.4

	Aluminum
	200 ug/L (SSO)
	NA
	NA
	ND
	NA
	NA
	NA
	NA

	Arsenic
	10 ug/L
	NA
	NA
	0.59
	NA
	NA
	NA
	NA

	Barium
	2000 ug/L
	NA
	NA
	127
	NA
	NA
	NA
	NA

	Chromium
	100 ug/L
	NA
	NA
	0.34
	NA
	NA
	NA
	NA

	Copper
	1000 ug/L
	NA
	NA
	ND
	NA
	NA
	NA
	NA

	Lead
	15 ug/L
	NA
	NA
	ND
	NA
	NA
	NA
	NA

	NO2/NO3
	10,000 ug/L
	NA
	NA
	6
	NA
	NA
	NA
	NA

	Radium 226/228
	5 pCi/L
	3.6
	8.5
	11.1
	10.8
	11.8
	8.9
	2.3

	Strontium
	4200 ug/L
	NA
	NA
	1590
	NA
	NA
	NA
	NA

	Titanium
	Not Established
	NA
	NA
	0.86
	NA
	NA
	NA
	NA



ND=Non Detect
NA=Not Analyzed
AR=Awaiting Results
Yellow Infill=Exceedance of Ground Water Cleanup Target Level
ug/L= micrograms per Liter
pCi/L=picocuries per Liter
SSO=Secondary Standard Organoleptic
MCST=Minimum Criteria Systemic Toxicant
MCC=Minimum Criteria Carcinogen
Primary Standard Unless Otherwise Noted



	Analyte 
	GCTL 
	5Z-SID P.O.E. (Treated Water)
8/26/2009
	5Z-SID Reject Water
(Untreated Water)
8/26/2009
	5Z-SID Repump Water (Treated Water)
8/26/2009

	Gross Alpha
	15 pCi/L
	ND
	68.0
	ND

	Aluminum
	200 ug/L (SSO)
	NA
	NA
	NA

	Arsenic
	10 ug/L
	NA
	NA
	NA

	Barium
	2000 ug/L
	NA
	NA
	NA

	Chromium
	100 ug/L
	NA
	NA
	NA

	Copper
	1000 ug/L
	NA
	NA
	NA

	Lead
	15 ug/L
	NA
	NA
	NA

	NO2/NO3
	10,000 ug/L
	NA
	NA
	NA

	Radium 226/228
	5 pCi/L
	ND
	31.4
	ND

	Strontium
	4200 ug/L
	NA
	NA
	NA

	Titanium
	Not Established
	NA
	NA
	NA



ND=Non Detect
NA=Not Analyzed
AR=Awaiting Results
Yellow Infill=Exceedance of Ground Water Cleanup Target Level
ug/L= micrograms per Liter
pCi/L=picocuries per Liter
SSO=Secondary Standard Organoleptic
MCST=Minimum Criteria Systemic Toxicant
MCC=Minimum Criteria Carcinogen
Primary Standard Unless Otherwise Noted




Table 3: Summary of Analytical Results For Seminole Improvement District Well Field & Water Plant
The Acreage Community, Loxahatchee, Palm Beach County, Florida
FDEP Site Investigation


	Analyte 
	SWCTL 
	5Z-Sid Outfall & Sycamore
8/26/2009
	L8-Tieback
8/26/2009
	M Canal-1
8/26/2009
	M Canal-2
8/26/2009
	M Canal-3
8/26/2009

	Gross Alpha
	15 pCi/L
	1.2
	1.8
	1.8
	1.3
	ND

	Radium 226/228
	5 pCi/L
	0.50
	1.4
	1.1
	0.4
	0.7



ND=Non Detect
NA=Not Analyzed
AR=Awaiting Results
Yellow Infill=Exceedance of Ground Water Cleanup Target Level
ug/L= micrograms per Liter
pCi/L=picocuries per Liter
SSO=Secondary Standard Organoleptic
MCST=Minimum Criteria Systemic Toxicant
MCC=Minimum Criteria Carcinogen
Primary Standard Unless Otherwise Noted


