Table 4:  Summary of Analytical Results for Sodium, Bromodichloromethane, Dibromochloromethane and Iron in Pre and Post Treatment Systems
The Acreage Community, Loxahatchee, Palm Beach County, Florida
FDEP Site Investigation
	


	Analyte 
	GCTL 
(ug/L)
	1-Pre
	1-Post
	2-Pre
	2-Post
	3-Pre
	3-Post
	4-Pre
	4-Post

	Bromodichloromethane
	0.6 (MCC)
	
	
	
	
	
	
	
	

	Dibromochloromethane
	0.4 (MCC)
	
	
	
	
	
	
	
	

	Iron
	300 (SSA)
	
	
	1,010
	400
	
	
	670
	150

	Sodium
	160,000 
	
	256,000
	
	
	
	
	
	

	Manganese
	50 (SSA)
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	



ND=Non Detect
NA=Not Analyzed
Yellow Infill=Exceedance of Ground Water Cleanup Target Level
ug/L= micrograms per Liter
pCi/L=picocuries per Liter
SSA=Secondary Standard Aesthetic
MCST=Minimum Criteria Systemic Toxicant
MCC=Minimum Criteria Carcinogen
Primary Standard Unless Otherwise Noted









	Analyte 
	GCTL
(ug/L) 
	5-Pre
	5-Post
	6-Pre
	6-Post
	7-Pre
	7-Post
	8-Pre
	8-Post

	Bromodichloromethane
	0.6 (MCC)
	
	
	
	
	ND
	0.94
	
	

	Dibromochloromethane
	0.4 (MCC)
	
	
	
	
	
	
	
	

	Iron
	300 (SSA)
	1,181
	39
	2,980
	
	
	
	
	

	Sodium
	160,000 
	
	329,000
	
	
	175,000
	329,000
	
	

	Manganese
	50 (SSA)
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	



ND=Non Detect
NA=Not Analyzed
Yellow Infill=Exceedance of Ground Water Cleanup Target Level
ug/L= micrograms per Liter
pCi/L=picocuries per Liter
SSA=Secondary Standard Aesthetic
MCST=Minimum Criteria Systemic Toxicant
MCC=Minimum  Criteria Carcinogen
Primary Standard Unless Otherwise Noted






	Analyte 
	GCTL 
(ug/L)
	9-Pre
	9-Post
	10-Pre
	10-Post
	11-Pre
	11-Post
	12-Pre
	12-Post

	Bromodichloromethane
	0.6 (MCC)
	
	
	
	
	
	
	
	

	Dibromochloromethane
	0.4 (MCC)
	
	
	
	
	
	
	
	

	Iron
	300 (SSA)
	
	
	640
	
	
	
	3,020
	

	Sodium
	160,000 
	41,200
	217,000
	
	
	17,100
	243,000
	
	

	Manganese
	50 (SSA)
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	



ND=Non Detect
NA=Not Analyzed
Yellow Infill=Exceedance of Ground Water Cleanup Target Level
ug/L= micrograms per Liter
pCi/L=picocuries per Liter
SSA=Secondary Standard Organoleptic
MCST=Minimum Criteria Systemic Toxicant
MCC=Minimum Criteria Carcinogen
Primary Standard Unless Otherwise Noted









	Analyte 
	GCTL 
(ug/L)
	14-Pre
	14-Post
	15-Pre
	15-Post
	16-Pre
	16-Post
	17-Pre
	17-Post

	Bromodichloromethane
	0.6 (MCC)
	
	
	
	0.68
	
	
	
	4.0

	Dibromochloromethane
	0.4 (MCC)
	
	
	
	
	
	
	
	3.0

	Iron
	300 (SSA)
	1,750
	
	1,690
	
	3,230
	
	
	

	Sodium
	160,000
	
	
	58,600
	260,000
	
	
	290,000
	524,000

	Manganese
	50 (SSA)
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	



ND=Non Detect
NA=Not Analyzed
Yellow Infill=Exceedance of Ground Water Cleanup Target Level
ug/L= micrograms per Liter
pCi/L=picocuries per Liter
SSA=Secondary Standard Aesthetic
MCST=Minimum Criteria Systemic Toxicant
MCC=Minimum Criteria Carcinogen
Primary Standard Unless Otherwise Noted









	Analyte 
	GCTL 
(ug/L)
	18-Pre
	18-Post
	19-Pre
	19-Post
	20-Pre
	20-Post
	21-Pre
	21-Post

	Bromodichloromethane
	0.6 (MCC)
	
	
	
	
	
	
	
	

	Dibromochloromethane
	0.4 (MCC)
	
	
	
	
	
	
	
	

	Iron
	300 (SSA)
	980
	230
	
	
	570
	
	12,000
	

	Sodium
	160,000 
	
	
	
	
	141,000
	434,000
	22,500
	180,000

	Manganese
	50 (SSA)
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	



ND=Non Detect
NA=Not Analyzed
Yellow Infill=Exceedance of Ground Water Cleanup Target Level
ug/L= micrograms per Liter
pCi/L=picocuries per Liter
SSA=Secondary Standard Aesthetic
MCST=Minimum Criteria Systemic Toxicant
MCC=Minimum Criteria Carcinogen
Primary Standard Unless Otherwise Noted









	Analyte 
	GCTL 
	22-Pre
	22-Post
	23-Pre
	23-Post
	24-Pre
	24-Post
	25-Pre
	25-Post

	Bromodichloromethane
	0.6 (MCC)
	
	
	
	1.2
	
	0.51
	
	

	Dibromochloromethane
	0.4 (MCC)
	
	
	
	
	
	
	
	

	Iron
	300 (SSA)
	
	1,030
	
	
	
	
	
	

	Sodium
	160,000
	
	424,000
	
	453,000
	
	260,000
	
	267,000

	Manganese
	50 (SSA)
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	



ND=Non Detect
NA=Not Analyzed
Yellow Infill=Exceedance of Ground Water Cleanup Target Level
ug/L= micrograms per Liter
pCi/L=picocuries per Liter
SSA=Secondary Standard Aesthetic
MCST=Minimum Criteria Systemic Toxicant
MCC=Minimum Criteria Carcinogen
Primary Standard Unless Otherwise Noted









	Analyte 
	GCTL 
	26-Pre
	26-Post
	27-Pre
	27-Post
	28-Pre
	28-Post
	29-Pre
	29-Post

	Bromodichloromethane
	0.6 (MCC)
	
	
	
	
	
	
	
	

	Dibromochloromethane
	0.4 (MCC)
	
	
	
	
	
	
	
	

	Iron
	300 (SSA)
	960
	
	2,920
	
	4,190
	
	
	

	Sodium
	160,000
	117,000
	304,000
	
	
	
	
	
	

	Manganese
	50 (SSA)
	
	
	
	35.6
	58.6
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	



ND=Non Detect
NA=Not Analyzed
Yellow Infill=Exceedance of Ground Water Cleanup Target Level
ug/L= micrograms per Liter
pCi/L=picocuries per Liter
SSA=Secondary Standard Aesthetic
MCST=Minimum Criteria Systemic Toxicant
MCC=Minimum Criteria Carcinogen
Primary Standard Unless Otherwise Noted






	Analyte 
	GCTL 
	30-Pre
	30-Post
	31-Pre
	31-Post

	Bromodichloromethane
	0.6 (MCC)
	
	
	
	

	Dibromochloromethane
	0.4 (MCC)
	
	
	
	

	Iron
	300 (SSA)
	
	
	
	

	Sodium
	160,000
	
	
	
	

	Manganese
	50 (SSA)
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	



ND=Non Detect
NA=Not Analyzed
Yellow Infill=Exceedance of Ground Water Cleanup Target Level
ug/L= micrograms per Liter
pCi/L=picocuries per Liter
SSA=Secondary Standard Aesthetic
MCST=Minimum Criteria Systemic Toxicant
MCC=Minimum Criteria Carcinogen
Primary Standard Unless Otherwise Noted


