Beach Sand Review Procedures Vary by Locations of Fill Placement and Fill Volumes
	REVIEW PROCEDURES FOR BEACH SAND COMPATIBILITY

	Fill Location
	Volume
	Permit Type1
And
Reviewer2
	Type Review
	Minimum Number of 
Review Samples Needed
	QA/QC Plan

	
	
	
	
	Excavation 
Material
	Native Material
	

	Beach
	≤200 cy
	FP/FI
	Physical Samples
	1 sample
	1 sample 
	No

	
	>200 cy and <600 cy
	FP/PM
	Physical Samples
	1 sample
	1 sample
	Yes

	
	≥600 cy and <2000 cy
	AP/PM
	Lab reports or mine assays
	2 core borings with 
1 sample per 
soil strata
	1 sample per 
500 feet of beach length
	Yes

	
	≥2000 cy
	AP/CE
	Lab reports or mine assays
	2 core borings with 
1 sample per 
soil strata
	1 sample per 
500 feet of beach length
	Yes

	Dune System
	≤200 cy3
	FP/FI
	Physical Samples
	1 sample
	Visual inspection
	No

	
	>200 cy and <600 cy
	FP/AP/PM
	Physical Samples
	1 sample
	1 sample
	No

	
	≥600 cy and <2000 cy
	AP/PM
	Lab reports or mine assays
	2 core borings with 
1 sample per soil strata
	1 sample per 
1000 feet of beach length
	Yes

	
	≥2000 cy
	AP/CE
	Lab reports or mine assays
	2 core borings with 
1 sample per soil strata
	1 sample per 
1000 feet of beach length
	Yes

	Upland of Dune System
	≤200 cy3
	FP/FI
	Physical Samples
	1 sample
	Visual inspection
	No

	
	>200 cy
	FP/AP/PM
	Physical Samples
	1 sample
	1 sample
	No

	Between ECL and MHWL
	Any Amount
	AP/LOC/CE
	Lab reports or mine assays
	2 core borings with 
1 sample per soil strata
	1 sample per 
500 feet of beach length
	Yes

	Seaward of MHWL
	Beach sand compatibility review and activity authorization handled by the 
Joint Coastal Permitting (JCP) Section

	1Permit Type: 
FP (Field Permit)
AP (Administrative Permit) 
LOC (JCP Letter of Consent)
	3≤200 cy:
For volumes of fill ≤200 cy with placement on or upland of  the dune system, the field inspector’s authorization is further limited by the source of fill, as follows:
1. Source is landward of CCCL, or
2. Source is upland of the dune system and not resulting in >1-foot lower grade elevation.

	2Beach Sand Compatibility Reviewer: 
FI (Field Inspector)
PM (Permit Manager)
CE (Coastal Engineering Staff)
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