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	_______________ (Enter “Reclaimed Water” or “Effluent”, as appropriate.) Limitations
	

Monitoring Requirements
	

	
Parameter
	
Units
	
Max/Min
	
Limit
	
Statistical Basis
	Frequency of Analysis
	
Sample Type
	Monitoring 
Site Number
	
Notes

	Oxygen, dissolved percent saturation
(Applicable to Class I, Class II, Class III, and Class III-limited discharge)
	Percent samples in compliance
	Min
	90
	Monthly Total
	
	
	
	

	Oxygen, dissolved percent saturation
(Applicable to predominately marine Class II, Class III, and Class III-limited discharge)
	Number of exceedances
	Max
Max
	1
1
	Quarterly Total
Annual Total
	
	
	
	




1. No more than 10 percent of the daily average percent dissolved oxygen (DO) saturation values shall be below __________________ (Enter 67 % in the Panhandle West bioregion, 38 % in the Peninsula and Everglades bioregions, or 34 % in the Northeast and Big Bend bioregions.).  To report the “percent samples in compliance,” count the number of daily average values greater than or equal to ____________ (Enter 67% in the Panhandle West bioregion, 38% in the Peninsula and Everglades bioregions, or 34% in the Northeast and Big Bend bioregions.), divide by the total number of daily average values, and multiply by 100% (round to the nearest integer).  (In the table above, reference this condition in the notes column for oxygen, dissolved percent saturation where the discharge is to Class I, Class III, or Class III-limited predominately freshwaters.)[62-302.533(1)(a)]
2. No more than 10 percent of the daily average percent dissolved oxygen (DO) saturation values shall be below 42%.  To report the “percent samples in compliance,” count the number of daily average values greater than or equal to 42%, divide by the total number of daily average values, and multiply by 100% (round to the nearest integer).  (In the table above, reference this condition in the notes column for oxygen, dissolved percent saturation where the discharge is to Class II, Class III, or Class III-limited predominately marine waters.)[62-302.533(2)(a)]
3. The weekly average DO percent saturation shall not be below 51% more than once in any three month period.  To report the “number of exceedances,” count the number of weekly average values greater than or equal to 51% during the three month period.  The weekly average value shall only be counted if samples or readings are taken on 3 or more days during the week.  (In the table above, reference this condition in the notes column for oxygen, dissolved percent saturation where the discharge is to Class II, Class III, or Class III-limited predominately marine waters.)[62-302.533(2)(a)]
4. [bookmark: _GoBack]The monthly average DO percent saturation shall not be below 56% more than once in any twelve month period.  To report the “number of exceedances,” count the number of monthly average values greater than or equal to 56% during the twelve month period.  The monthly average value shall only be counted if samples or readings are taken on 10 or more days during the month.  (In the table above, reference this condition in the notes column for oxygen, dissolved percent saturation where the discharge is to Class II, Class III, or Class III-limited predominately marine waters.)[62-302.533(2)(a)]
