	Appendix A                                                 Entering “Latitude” and “Longitude” coordinates 




A.  Entering “Latitude” and “Longitude” coordinates

When entering coordinates for Latitude and Longitude in either the Discharge Points screen or in any of the Application Sites table, Permit Builder will prompt you with a message if the coordinates you enter are not within the proper ranges.  

Coordinate ranges should be as follows:

· Latitude:  	24 – 31 degrees,  00 – 59 minutes,  00 – 59 seconds.
· Longitude:  	80 – 88 degrees,  00 – 59 minutes,  00 – 59 seconds.
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Latitude and Longitude coordinates fields on the Discharges Tab.
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Latitude and Longitude coordinates fields in an Application Sites table.

Always check the coordinates submitted with the permit application for a facility, with the coordinates that have been entered into WAFR-PA.  If they differ, choose the set of coordinates given in WAFR, as these coordinates have been verified.
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* Domestic Wastewater Program - Windows Internet Explorer

Monitoring Group™: | D_Suface Water v - oot New;/ Existing: ? | Exising

Monitoring Group Description: ? [[Type a description of Monitoring Grour| ( 448 characters remaining )

Permitted Capacity: ?|0250 MGD  Basis for Permitted Capacity: ?| Annual Average Daily Flow

Latitude: (24 P12 f[12 Longitude: ? 0l

outfall Length: ? |20 feet  Depth: 15

Receiving Water Body Class*

Discharge to:
[Acosta Creek
|Airport Canal
|Alzpaha River
|Alapahoochee River
|Allen Mill Pond

Receiving Waters are*: ? | None ofthe Above

Basis for Effiuent Limitation*: ? |Secondary Treatment Non-ocean Discharge ¥/

Disinfection Level*: ? |Basic v

The discharge is a stormwater only discharge.

[ The system is a reuse system.
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Application Site Description / User Name
(463characters remaining.) *

description of PAR-001 here.]

<>

description of ABF-002 here.]

TSNS vy cows Internet Explorer

pre—— ‘ Pleaseenter avals from 24to 31
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description of PAR-002 here.]
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Reclaimed water that fails to meet the criteria in the approved operating protocol(s) shall be directed to:
@ Reiect storage for subseauent additional treatment.
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