AMENDMENT TO FACT SHEET

FOR

FLORIDA DEPARTMENT OF ENVIRONMENTAL PROTECTION

DOMESTIC WASTEWATER FACILITY PERMIT                                                                                                     

	PERMIT NUMBER:
	FL0021857 (Major)

	FACILITY NAME:
	City of Clearwater Marshall Street AWWTF

	FACILITY LOCATION:
	Clearwater

Pinellas County

	NAME OF PERMITTEE:
	City of Clearwater

	PERMIT WRITER:
	Jeff Hilton, P.E.


1.
SYNOPSIS OF APPLICATION

a.
Chronology of Application

	
	Application Date:
	December 6, 2004

	
	Additional Information:
	February 1, 2005

	
	Public Notice Date:
	



b.
Type of Facility


Domestic Wastewater Treatment Plant



Publicly-owned treatment works



Standard Industrial Classification Code: 4952


c.
Facility Capacity

	
	Existing Design Capacity:
	10.0
	MGD
	AADF

	
	Proposed Increase in Design Capacity:
	0
	MGD
	AADF

	
	Proposed Total Design Capacity:
	10.0
	MGD
	AADF


	
	Existing Permitted Capacity:
	10.0
	MGD
	AADF

	
	Proposed Increase in Permitted Capacity:
	0
	MGD
	AADF

	
	Proposed Total Permitted Capacity:
	10.0
	MGD
	AADF



d.
Description of Effluent or Reclaimed Water Discharges (as reported by applicant)
Outfall Serial Number D-001 

Annual Average Daily Flow (mgd): 10.0



pH Range (Standard Units): 6.5 to 8.5

The description of the facility was amended to add the existing 5 MG reclaimed water storage tank.

2.
BASIS FOR EFFLUENT AND RECLAIMED WATER LIMITS AND MONITORING REQUIREMENTS (INCLUDING EFFLUENT MONITORING REQUIREMENTS)
The following table provides amendments to the fact sheet for Part I. A. provisions.

Outfall D-001 (Class III marine water):
	Parameter
	Limit
	Basis
	Rationale

	Whole Effluent Toxicity (Chronic) (***)
	100
	Single Sample Min.
	62-302.530(21) & (62) FAC

	Oxygen, Dissolved  (DO) (MG/L)
	5.0
	Single Sample Max.
	62-320.530(31)


Whole Effluent Toxicity (Chronic) was mistaken left out of the table in the original Fact Sheet.  The limit was added to the table, paragraph 8.b.2. the first sentence was changed to “A NOEC of less than 100% effluent in any routine test or additional test shall constitute a failure of the test.” and the last part of paragraph 8.f.5., “shall be terminated with the conclusion that the test constitutes non-compliance with these permit conditions.” was changed to “shall be terminated with the conclusion that the test failed.”  Additionally, the monitoring frequency has been reduced to Quarterly based on the facility’s completion of at least six valid tests that demonstrate no unacceptable toxicity. 

Based on the Ambient Monitoring results for the last five years the Dissolved Oxygen limit has been revised to 5.0 mg/l.  This limit is still above the State Water Quality Standard of 4.0 mg/l.  Ambient Monitoring will be continued and if the results indicate a reduction in downstream DO in relation to the reference site, the permit may be revised to address this.

Additionally, the sampling location for CBOD, TSS, TN, TP and pH have been moved from the plant site sampling location (EFA-01) to the Outfall sampling location (EFD-01) at the request of the City, on the basis that this location was more representative of the quality of the effluent being discharged. 

Total Residual Chlorine (For Dechlorination) Monitoring Frequency was changed to daily and the sample type to grab at the request of the City, to reflect how the City samples for this parameter. 
This is consistent with the monitoring schedule requirements of 62-601.

Ambient Monitoring: TSS was added to 9.d.(2). 

The following table provides amendments to the fact sheet for Part I. C. provisions.

Other Limitations and Monitoring Requirements:
	Parameter
	Limit
	Basis
	Rationale

	Rainfall (INCHES)
	Report
	Monthly Total 
	BPJ



Clarified that Rainfall should be reported as a monthly total.


Influent sampling frequency was changed to weekly.  This is consistent with other major facilities.

The annual reuse report and reporting of storage were removed from this permit.  These are contained in the City’s Master Reuse Permit.

3.
RESIDUALS MANAGEMENT
Updated pathogen reduction method and added an additional vector attraction reduction method.

12.
APPLICABLE RULES
The following were used as the basis of the permit limitations/conditions:

	a.
FAC refers to various portions of the Florida Administrative Code.

The effective dates of FAC Rule Chapters cited in the table are as follows:

Chapter
Effective Date

62-4
05-01-03

62-160            04-09-02

62-302
05-15-02

62-520
12-09-96

62-522
08-27-01
62-550
05-28-03

62-600
12-24-96

62-601
12-24-96

62-602
02-06-02
62-610
08-08-99

62-620
08-25-03

62-625
01-08-97

62-640
03-30-98

62-650
12-26-96

62-699
07-05-01

b.
FS refers to various portions of the Florida Statutes

c.
CFR refers to various portions of the Code of Federal Regulations, Title 40

d.
BPJ refers to Best Professional Judgment

	


13.
DEPARTMENT CONTACT

Additional information concerning the permit may be obtained during normal business hours from:


Jeff Hilton, P.E.


Program Manager


Department's Southwest District Office


13051 N. Telecom Parkway 

Temple Terrace, FL 33637-0926


Telephone Number: 813-632-7600

Fax Number: 813-632-7662

14.
THE ADMINISTRATIVE RECORD
The administrative record including application, draft permit, fact sheet, amended fact sheet, public notice (after release), comments received and additional information is available for public inspection during normal business hours at the location specified in item 13.

15.
PROPOSED SCHEDULE FOR PERMIT ISSUANCE


	
	Draft permit to Applicant and EPA :
	May 12, 2006

	
	Beginning of Proposed Public Comment Period :
	 

	
	End of Proposed Public Comment Period :
	 

	
	Notice of Agency Action :
	 

	
	Proposed Issuance Date of Permit :
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