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This permit is issued under the provisions of Chapter 403, Florida Statutes, and applicable rules of the Florida Administrative Code and constitutes authorization to discharge to waters of the state under the National Pollution Discharge Elimination System.  The above named permittee is hereby authorized to operate the facilities shown on the application and other documents attached hereto or on file with the Department and made a part hereof and specifically described as follows:
REUSE:

Land Application:  An existing 22.0 MGD 12-Month Average Daily Flow (12MADF) permitted capacity slow-rate public access system (R-001) consisting of a general service area located in Pasco County as defined by the map titled  Pasco County Master Reuse System  Fig. 1, dated December, 2006 as depicted in Attachment 1.  

This permit authorizes installation of all metering and controls as outlined in the process flow diagrams as referenced in Attachment 3 of this permit.

Reclaimed water meeting Part III public access standards is provided by separately permitted Pasco County Utilities operated waste water treatment facilities, as follows:


Deer Park Subregional WWTF – FLA439223 


Embassy Hills WWTF – FLA012735 


Hudson Subregional WWTF – FLA012738 

Land O’ Lakes Subregional WWTF – FLA012731 

Shady Hills Subregional WWTF – FLA012741 

Southeast Subregional WWTF – FLA012737 

Wesley Center Subregional WWTF – FLA016094 

The Permitted Annual Average Daily Flow (AADF) into the Pasco County Master Reuse System for each individual source facility is contained in the corresponding treatment facility permit.

Additional reclaimed water meeting the Part III public access standards may also be provided under agreement from the following source facility outside of the Pasco County Utilities systems:


New Port Richey WWTF – FLA127434 

Effluent quality is continuously monitored at the source wastewater treatment plants for high level disinfection in accordance with each facility’s approved operating protocol.  For all source plants, the on-site and off-site storage is controlled, sequenced, and operated during staffed and unstaffed periods according to procedures set forth in an Operating Protocol established for each source plant in order to assure maximum reliability and safeguards on the quality of the reclaimed water.

REUSE: Part IV Rapid Infiltration Basins as depicted in Attachment 2
Located At Deer Park Subregional WWTF and as depicted in Attachment 2 aerial:

Land Application:  An existing 0.27 MGD 12MADF permitted capacity Part IV rapid-rate land application system (R-002) located at Deer Park Subregional WWTF.   R-002 consists of a four cell RIB of 5.6 acres of bottom surface area.  Reject water from the Deer Park Subregional WWTF may be directed to RIB system R-002 as described above for alternative disposal.

Hudson, Embassy Hills and Northwest RIBs as depicted in Attachment 2 aerial:

Land Application (Hudson site):  An existing 3.0 MGD 12MADF permitted capacity Part IV rapid-rate land application system (R-003).  R-003 consists of a twenty-one cell RIB of 31.5 acres of bottom surface area.  R-003 is located on the north side of Denton Avenue east of the Hudson Subregional WWTF.  Cells 9, 10, and 11 of the RIB system are also utilized for alternative disposal for the Hudson Subregional WWTF.  Reject water from the Hudson Subregional WWTF may be directed to RIB system R-003 as described above for alternative disposal.

Land Application (Embassy Hills site):  An existing 1.5 MGD 12MADF permitted capacity Part IV rapid-rate land application system (R-004).   R-004 consists of a nine cell RIB system of 15.5 acres of bottom surface area.  R-004 is located at the south side of Denton Avenue across from the Hudson Subregional WWTF.

Land Application (Northwest site):  An existing 0.954 MGD 12MADF permitted capacity Part IV rapid-rate land application system (R-005).   R-005 consists of a five cell RIB system 11.71 acres of bottom surface area.  R-005 is located at the south side of Denton Avenue across from the Hudson Subregional WWTF and south of the Embassy Hills RIBs.

Oakley Groves RIB system as depicted in Attachment 2 aerial:

Land Application:  An existing 0.075 MGD 12MADFpermitted capacity Part IV rapid-rate land application system (R-006) located west of Interstate 75 and Wesley Center Subregional WWTF.   R-006 consists of a nineteen cell RIB system of 17.9 acres of bottom surface area.  Up to 0.72 MGD of reclaimed water may be returned from Oakley Groves to Wesley Center Subregional WWTF upstream of filtration for additional treatment to be returned to the PCMRS.  

Fox Hollow RIB system as depicted in Attachment 2 aerial:

Land Application:  An existing 0.663 MGD 12MADF permitted capacity Part IV rapid-rate land application system (R-007).   R-007 consists of a four cell RIB system of 5.4 acres of bottom surface area.  R-007 is located west of the Fox Hollow Elementary School.

Located At Shady Hills Subregional WWTF as depicted in Attachment 2 aerial:

Land Application:  An existing 0.35 MGD 12MADF permitted capacity Part IV rapid-rate land application system (R-008) located at Shady Hills Subregional WWTF.   R-008 consists of a four cell RIB system of 6.28 acres of bottom surface area. 
The entire RIB system has a collective disposal capacity of 6.812 MGD 12MADF permitted capacity.

The following locations, under the control of Pasco County Utilities, provide storage:

	Storage Basin
	Storage Capacity (MG)
	Type of Storage

	Embassy Hills WWTF
	2.0
	Tank

	Hudson WWTF
	2.0
	Tank

	Shady Hills WWTF
	1.5
	Tank

	Deer Park WWTF
	1.5
	Tank

	Land O’ Lakes WWTF
	3.8
	Tank

	Wesley Center WWTF
	6.0
	Tank

	Southeast WWTF
	1.5
	Tank

	Odessa WWTF
	5.0
	Tank

	Handcart Road
	2.0
	Tank

	Handcart Road - Lake Rita
	65.0
	Reservoir

	Land O’ Lakes Reservoir
	114.0
	Reservoir

	Total
	204.3
	


Intermittently discharging stormwater storage ponds for Part III Reclaimed Water:

Reclaimed water is stored in storm water storage lake system STM-01 at D-001, Heritage Springs, which intermittently overflows to the following:   Duck Slough.

Reclaimed water is stored in storm water storage lake system STM-02 at D-002, Seven Springs, which intermittently overflows to the following:  Duck Slough.

Reclaimed water is stored in storm water storage lake system STM-03 at D-003, Lexington Oaks, which intermittently overflows to the following:  North Cypress Creek.

Reclaimed water is stored in storm water storage lake system STM-04 at D-004, Plantation Palms, which intermittently overflows to the following:  Cypress Creek.

Reclaimed water is stored in storm water storage lake system STM-05 at D-005, Hidden Creek, which intermittently overflows to the following:  Lake Zephyr.

Reclaimed water is stored in storm water storage lake system STM-06 at D-006, Silver Oaks, which intermittently overflows to the following:  South Side Branch.

Reclaimed water is stored in storm water storage lake system STM-07 at D-007, Quail Hollow, which intermittently overflows to the following:  Cypress Creek.

Reclaimed water is stored in storm water storage lake system STM-08 at D-008, Saddlebrook, which intermittently overflows to the following:  Trout Creek .

Reclaimed water is stored in storm water storage lake system STM-09A at D-009, Heritage Pines Area 43A, which intermittently overflows to the following:  Hunter Lake Outlet.

Reclaimed water is stored in storm water storage lake system STM-09B at D-009, Heritage Pines Area 4, which intermittently overflows to the following:  Hunter Lake Outlet.

Reclaimed water is stored in storm water storage lake system STM-10 at D-010, Timber Oaks, which intermittently overflows to the following:  Gulf of Mexico.

Reclaimed water is stored in storm water storage lake system STM-11 at D-011, Timber Greens, which intermittently overflows to the following:  Pithlachascotee River.

Reclaimed water is stored in storm water storage lake system STM-12 at D-012, Lake Bernadette, which intermittently overflows to the following:  Indian Creek.

Reclaimed water is stored in storm water storage lake system STM-13 at D-013, Lake Jovita, which intermittently overflows to the following:  Clear Lake Outlet.

Reclaimed water is stored in storm water storage lake system STM-14E at D-014, Beacon Woods East, which intermittently overflows to the following:  Bear Creek.

Reclaimed water is stored in storm water storage lake system STM-14W at D-014, Beacon Woods West, which intermittently overflows to the following:  Bear Creek.

IN ACCORDANCE WITH: The limitations, monitoring requirements and other conditions set forth in Pages 1 through 39 of this permit.

I. RECLAIMED WATER AND EFFLUENT LIMITATIONS AND MONITORING REQUIREMENTS

A.
Reuse and Land Application Systems

1. During the period beginning on the issuance date and lasting through the expiration date of this permit, the permittee is authorized to direct reclaimed water to Reuse System R-001 through R-008.  Such reclaimed water shall be limited and monitored by the permittee as specified below:

	Total System
	
	
	Reclaimed Water Limitations
	Monitoring Requirements
	

	Parameter
	Units
	Max/Min
	Annual

Average
	Monthly

Average
	Weekly

Average
	Single Sample
	Monitoring Frequency
	Sample Type
	Monitoring Location Site Number
	Notes

	Flow (Total Flow, PCMRS)

R-001
	MGD
	Maximum
	22.0

(12MADF)
	Report
	-
	-
	Monthly
	Calculation
	FLW-01
	See Cond.I.A.2


	Total System Inflows
	
	
	Reclaimed Water Limitations
	Monitoring Requirements
	

	Parameter
	Units
	Max/Min
	Annual

Average
	Monthly

Average
	Weekly

Average
	Single Sample
	Monitoring Frequency
	Sample Type
	Monitoring Location Site Number
	Notes

	Flow (Deer Park Subregional WWTF), FLA439223
	MGD
	Maximum
	Report*
	Report
	-
	-
	Monthly
	Calculation
	FLW-02
	See Cond.I.A.3

	Flow (Embassy Hills Subregional WWTF), FLA012735
	MGD
	Maximum
	Report*
	Report
	-
	-
	Continuous
	Meter
	FLW-03
	See Cond.I.A.3

	Flow (Hudson Subregional WWTF), FLA012738
	MGD
	Maximum
	Report*
	Report
	-
	-
	Monthly
	Calculation
	FLW-04
	See Cond.I.A.3

	Flow (Land O’ Lakes Subregional WWTF), FLA012731
	MGD
	Maximum
	Report*
	Report
	-
	-
	Monthly
	Calculation
	FLW-05
	See Cond.I.A.3

	Flow (Shady Hills Subregional WWTF), FLA012741
	MGD
	Maximum
	Report*
	Report
	-
	-
	Monthly
	Calculation
	FLW-06
	See Cond.I.A.3

	Flow (Southeast Subregional WWTF), FLA012737
	MGD
	Maximum
	Report*
	Report
	-
	-
	Monthly
	Calculation
	FLW-07
	See Cond.I.A.3

	Flow, (Wesley Center Subregional WWTF), FLA016094
	MGD
	Maximum
	Report*
	Report
	-
	-
	Continuous
	Meter
	FLW-08
	See Cond.I.A.3

	Flow, (New Port Richey WWTF),

FLA127434
	MGD
	Maximum
	Report*
	Report
	-
	-
	Continuous
	Meter
	FLW-09
	See Cond.I.A.3


*The Permitted Annual Average Daily Flow (AADF) into the Pasco County Master Reuse System for each individual source facility is contained in the corresponding treatment facility permit.

	PCMRS Outflows
	
	
	Reclaimed Water Limitations
	Monitoring Requirements
	

	Parameter
	Units
	Max/Min
	Annual

Average
	Monthly

Average
	Weekly

Average
	Single Sample
	Monitoring Frequency
	Sample Type
	Monitoring Location Site Number
	Notes

	To R-002, (Deer Park RIBs)
	MGD
	Maximum
	Report
	Report
	-
	-
	Continuous
	Meter
	FLW-10
	See Cond.I.A.3

	To R-003, (Hudson RIBs)
	MGD
	Maximum
	Report
	Report
	-
	-
	Continuous
	Meter
	FLW-11
	See Cond.I.A.3

	To R-004, (Embassy Hills RIBs)
	MGD
	Maximum
	Report
	Report
	-
	-
	Continuous
	Meter
	FLW-12
	See Cond.I.A.3

	To R-005, (Northwest RIBs)
	MGD
	Maximum
	Report
	Report
	-
	-
	Continuous
	Meter
	FLW-13
	See Cond.I.A.3

	To R-006, (Oakley Grove RIBs)
	MGD
	Maximum
	Report
	Report
	-
	-
	Continuous
	Meter
	FLW-14
	See Cond.I.A.3

	To R-007, (Fox Hollow RIBs)
	MGD
	Maximum
	Report
	Report
	-
	-
	Continuous
	Meter
	FLW-15
	See Cond.I.A.3

	To R-008, (Shady Hills RIBs)
	MGD
	Maximum
	Report
	Report
	-
	-
	Continuous
	Meter
	FLW-16
	See Cond.I.A.3

	To SE WWTF from PCMRS (Handcart Road)
	MGD
	Maximum
	Report
	Report
	-
	-
	Continuous
	Meter
	FLW-17
	See Cond.I.A.3


	PCMRS Water Quality
	
	
	Reclaimed Water Limitations
	Monitoring Requirements
	

	Parameter
	Units
	Max/Min
	Annual

Average
	Monthly

Average
	Weekly

Average
	Single Sample
	Monitoring Frequency
	Sample Type
	Monitoring Location Site Number
	Notes

	Total Chloride
	MG/L
	Maximum
	-
	Report
	-
	-
	Monthly
	Grab
	EFF-01, EFF-02 & EFF-03
	See Cond.I.A.11

	Total Sodium
	MG/L
	Maximum
	-
	Report
	-
	-
	Monthly
	Grab
	EFF-01, EFF-02 & EFF-03
	See Cond.I.A.11

	Total Dissolved Solids
	MG/L
	Maximum
	-
	Report
	-
	-
	Monthly
	Grab
	EFF-01, EFF-02 & EFF-03
	See Cond.I.A.11


	Rapid Infiltration Basins
	
	
	Reclaimed Water Limitations
	Monitoring Requirements
	

	Parameter
	Units
	Max/Min
	Annual

Average
	Monthly

Average
	Weekly

Average
	Single Sample
	Monitoring Frequency
	Sample Type
	Monitoring Location Site Number
	Notes

	Total R-002, (Deer Park Subregional WWTF RIBs)
	MGD
	Maximum
	0.27

(12MADF)
	Report
	-
	-
	Monthly
	Calculation
	FLW-18
	See Cond.I.A.3

	Total R-003, (Hudson Subregional WWTF RIBs)
	MGD
	Maximum
	3.0

(12MADF)
	Report
	-
	-
	Monthly
	Calculation
	FLW-19
	See Cond.I.A.3

	Total R-004, (Embassy Hills RIBs)
	MGD
	Maximum
	 1.5

(12MADF)
	Report
	-
	-
	Continuous
	Meter
	FLW-12
	See Cond.I.A.3

	Total R-005, (Northwest RIBs)
	MGD
	Maximum
	0.954

(12MADF)
	Report
	-
	-
	Continuous
	Meter
	FLW-13
	See Cond.I.A.3

	Total R-006, (Oakley Grove RIBs)
	MGD
	Maximum
	0.075

((12MADF)
	Report
	-
	-
	Monthly
	Calculation
	FLW-20
	See Cond.I.A.3

	Total R-007, (Fox Hollow RIBs)
	MGD
	Maximum
	0.663

(12MADF)
	Report
	-
	-
	Continuous
	Meter
	FLW-15
	See Cond.I.A.3

	Total R-008, (Shady Hills Subregional WWTF RIBs)
	MGD
	Maximum
	0.35
(12MADF)
	Report
	-
	-
	Monthly
	Calculation
	FLW-21
	See Cond.I.A.3


	R-004 Embassy Hills 
	
	
	Reclaimed Water Limitations
	Monitoring Requirements
	

	Parameter
	Units
	Max/Min
	Annual

Average
	Monthly

Average
	Weekly

Average
	Single Sample
	Monitoring Frequency
	Sample Type
	Monitoring Location Site Number
	Notes

	R-004, (Embassy Hills RIBs)
	MGD
	Maximum
	1.5

(12MADF)
	Report
	-
	-
	Continuous
	Meter
	FLW-12
	See Cond.I.A.3

	Carbonaceous Biochemical Oxygen Demand (5 day)
	MG/L
	Maximum
	-
	-
	-
	15.0
	Weekly
	Grab
	EFF-04
	

	Total Dissolved Solids
	MG/L
	Maximum
	-
	-
	-
	500.0
	Weekly
	Grab
	EFF-04
	

	Sodium
	MG/L
	Maximum
	-
	-
	-
	160.0
	Weekly
	Grab
	EFF-04
	

	Chloride
	MG/L
	Maximum
	-
	-
	-
	250.0
	Weekly
	Grab
	EFF-04
	

	Nitrate (as N)
	MG/L
	Maximum
	-
	-
	-
	10.0
	Weekly
	Grab
	EFF-04
	

	Specific Conductance
	UMHO/CM
	Maximum
	-
	-
	-
	1200
	Weekly
	Grab
	EFF-04
	


	Independent Well Systems

For Individual Users
	
	
	Reclaimed Water Limitations
	
	Monitoring Requirements
	

	
	
	
	Irrigation Water

(Wells)
	
	Reclaimed Water

(PCMRS)
	
	
	
	
	

	Parameter
	Units
	Max/Min
	Monthly

Total
	Daily Average
	Monthly

Total
	Daily Average
	Monitoring Frequency
	Sample Type
	Monitoring Location Site Number
	Notes

	Flow, (Plantation Palms Well)
	MGD
	Maximum
	Report
	Report
	Report
	Report
	Continuous
	Meter
	FLW-22IW

FLW-22RW
	See Cond.I.A.3

	Flow, (Lexington Oaks #2 & #4 Wells)
	MGD
	Maximum
	Report
	Report
	Report
	Report
	Continuous
	Meter
	FLW-23IW

FLW-23RW
	See Cond.I.A.3

	Flow, (Grand Oaks #1 through #5 Wells)
	MGD
	Maximum
	Report
	Report
	Report
	Report
	Continuous
	Meter
	FLW-24IW

FLW-24RW
	See Cond.I.A.3

	Flow, (Oakstead #1 & #2

Wells)
	MGD
	Maximum
	Report
	Report
	Report
	Report
	Continuous
	Meter
	FLW-25IW

FLW-25RW
	See Cond.I.A.3

	Flow, (Heritage Springs Well)
	MGD
	Maximum
	Report
	Report
	Report
	Report
	Continuous
	Meter
	FLW-26IW

FLW-26RW
	See Cond.I.A.3

	Flow, (Heritage Pines Well)
	MGD
	Maximum
	Report
	Report
	Report
	Report
	Continuous
	Meter
	FLW-27IW

FLW-27RW
	See Cond.I.A.3

	Flow, (Saddlebrook

 Well)
	MGD
	Maximum
	Report
	Report
	Report
	Report
	Continuous
	Meter
	FLW-28IW

FLW-28RW
	See Cond.I.A.3

	Flow, (Lake Bernadette Well)
	MGD
	Maximum
	Report
	Report
	Report
	Report
	Continuous
	Meter
	FLW-29IW

FLW-29RW
	See Cond.I.A.3

	Flow, (Silver Oaks

 Well)
	MGD
	Maximum
	Report
	Report
	Report
	Report
	Continuous
	Meter
	FLW-30IW

FLW-30RW
	See Cond.I.A.3

	Flow, (Beacon Woods East Well)
	MGD
	Maximum
	Report
	Report
	Report
	Report
	Continuous
	Meter
	FLW-31IW

FLW-31RW
	See Cond.I.A.3

	Flow, (Quail Hollow

 Well)
	MGD
	Maximum
	Report
	Report
	Report
	Report
	Continuous
	Meter
	FLW-32IW

FLW-32RW
	See Cond.I.A.3

	Flow, (Lake Jovita

 Well)
	MGD
	Maximum
	Report
	Report
	Report
	Report
	Continuous
	Meter
	FLW-33IW

FLW-33RW
	See Cond.I.A.3

	Flow, (Wildcat

 Supplemental Well)
	MGD
	Maximum
	Report
	Report
	Report
	Report
	Continuous
	Meter
	FLW-34IW

FLW-34RW
	See Cond.I.A.3


	Handcart Road Storage System
	
	
	Reclaimed Water Limitations
	Monitoring Requirements
	

	Parameter
	Units
	Max/Min
	Annual

Average
	Monthly

Average
	Max Storage
	Min Storage
	Monitoring Frequency
	Sample Type
	Monitoring Location Site Number
	Notes

	Flow, into Handcart Road Total Storage System (tank included)
	MGD
	Maximum
	Report
	Report
	-
	-
	Daily
	Meter
	FLW-35
	See Cond.I.A.3

	Flow, into Handcart Road Ponds Only
	MGD
	Maximum
	Report
	Report
	-
	-
	Daily
	Meter
	FLW-36
	See Cond.I.A.3

	Flow, out of Handcart Road

Storage System to SE WWTF
	MGD
	Maximum
	Report
	Report
	-
	-
	Daily
	Meter
	FLW-17
	See Cond.I.A.3

	Flow, out of Handcart Rd Storage System into Price / Altman Groves
	MGD
	Maximum
	Report
	Report
	-
	-
	Daily
	Meter
	FLW-37
	See Cond.I.A.3

	Staff Gauge located in Lake Rita*
	Feet
	N/A
	-
	-
	-
	Report*
	Daily
	Gauge*
	OTH-01
	


*The Staff gauge reading shall be taken at the same time as the daily meter readings and recorded on the Part B DMR only.

	Major Residential Systems
	
	
	Reclaimed Water Limitations
	Monitoring Requirements
	

	Parameter
	Units
	Max/Min
	Annual

Average
	Monthly

Average
	Weekly

Average
	Single Sample
	Monitoring Frequency
	Sample Type
	Monitoring Location Site Number
	Notes

	Grand Oaks Subdivision
	MGD
	Maximum
	Report
	Report
	-
	-
	Monthly
	Meter
	FLW-38
	See Cond.I.A.3

	Lake Bernadette Villas
	MGD
	Maximum
	Report
	Report
	-
	-
	Monthly
	Meter
	FLW-39
	See Cond.I.A.3

	Lexington Oaks Subdivision
	MGD
	Maximum
	Report
	Report
	-
	-
	Monthly
	Meter
	FLW-40
	See Cond.I.A.3

	Meadow Pointe Subdivision
	MGD
	Maximum
	Report
	Report
	-
	-
	Monthly
	Meter
	FLW-41
	See Cond.I.A.3

	Oakstead Subdivision
	MGD
	Maximum
	Report
	Report
	-
	-
	Monthly
	Meter
	FLW-42
	See Cond.I.A.3

	Sabal Ridge Subdivision
	MGD
	Maximum
	Report
	Report
	-
	-
	Monthly
	Meter
	FLW-43
	See Cond.I.A.3

	Seven Oaks Subdivision
	MGD
	Maximum
	Report
	Report
	-
	-
	Monthly
	Meter
	FLW-44
	See Cond.I.A.3


	Rain Gauge Data
	
	
	Reclaimed Water Limitations
	Monitoring Requirements
	

	Parameter
	Units
	Max/Min
	Annual

Average
	Monthly

Average
	Weekly

Average
	Single Sample
	Monitoring Frequency
	Sample Type
	Monitoring Location Site Number
	Notes

	Rainfall at (Deer Park Subregional WWTF), FLA439223
	Inches
	Maximum
	Report
	Report
	-
	-
	Continuous

(Daily Reading)
	Rain Gauge
	OTH-DPRG
	

	Rainfall at (Embassy Hills Subregional WWTF), FLA012735
	Inches
	Maximum
	Report
	Report
	-
	-
	Continuous

(Daily Reading)
	Rain Gauge
	OTH-EHRG
	

	Rainfall at (Hudson Subregional WWTF), FLA012738
	Inches
	Maximum
	Report
	Report
	-
	-
	Continuous

(Daily Reading)
	Rain Gauge
	OTH-HDRG
	

	Rainfall at (Land O’ Lakes Subregional WWTF), FLA012731
	Inches
	Maximum
	Report
	Report
	-
	-
	Continuous

(Daily Reading)
	Rain Gauge
	OTH-LLRG
	

	Rainfall at (Shady Hills Subregional WWTF), FLA012741
	Inches
	Maximum
	Report
	Report
	-
	-
	Continuous

(Daily Reading)
	Rain Gauge
	OTH-SHRG
	

	Rainfall at (Southeast Subregional WWTF), FLA012737
	Inches
	Maximum
	Report
	Report
	-
	-
	Continuous

(Daily Reading)
	Rain Gauge
	OTH-SERG
	

	Rainfall at, (Wesley Center Subregional WWTF), FLA016094
	Inches
	Maximum
	Report
	Report
	-
	-
	Continuous

(Daily Reading)
	Rain Gauge
	OTH-WCRG
	


2. Reclaimed water samples shall be taken at the monitoring site locations listed in Permit Condition I. A.  1. and as described below:

The Total Public Access Reuse System (FLW-01) is calculated by the following:

Total System Inflows minus Total System Outflows 

((FLW-02 to FLW-09)  –  ((FLW-10 to FLW-17)

Total Public Access Reuse System
	Monitoring Location 
	Description of Monitoring Location

	FLW-01
	Total flow to R-001, Calculated as described above. 


Inflows to PCMRS
	Monitoring Location 
	Description of Monitoring Location

	FLW-02
	Metered flow from Deer Park Subregional WWTF

	FLW-03
	Metered flow from Embassy Hills Subregional WWTF

	FLW-04
	Metered flow from Hudson Subregional WWTF

	FLW-05
	Metered flow from Land O’ Lakes Subregional WWTF

	FLW-06
	Metered flow from Shady Hills Subregional WWTF

	FLW-07
	Metered flow from Southeast Subregional WWTF

	FLW-08
	Metered flow from Wesley Center Subregional WWTF

	FLW-09
	Metered flow from New Port Richey WWTF


Outflows from PCMRS
	Monitoring Location 
	Description of Monitoring Location

	FLW-10
	Metered flow to Deer Park Subregional WWTF RIBs directly from PCMRS

	FLW-11
	Metered flow to Hudson Subregional WWTF RIBs directly from PCMRS

	FLW-12
	Metered flow to Embassy Hills RIBs directly from PCMRS

	FLW-13
	Metered flow to Northwest RIBs directly from PCMRS

	FLW-14
	Metered flow to Oakley Grove RIBs directly from PCMRS

	FLW-15
	Metered flow to Fox Hollow RIBs directly from PCMRS

	FLW-16
	Metered flow to Shady Hills Subregional WWTF RIBs directly from PCMRS

	FLW-17
	Metered flow back to Southeast Subregional WWTF from the Handcart Road Storage System for re-treatment.


Total Flows to the RIBs
	Monitoring Location 
	Description of Monitoring Location

	FLW-18
	Total flow disposed into Deer Park RIBs 

	FLW-19
	Total flow disposed into Hudson RIBs

	FLW-12
	Total flow disposed into Embassy Hills RIBs

	FLW-13
	Total flow disposed into Northwest RIBs

	FLW-20
	Total flow disposed into Oakley Grove RIBs

	FLW-15
	Total flow disposed into Fox Hollow RIBs

	FLW-21
	Total flow disposed into Shady Hills RIBs


 Wells - Golf Courses
	Monitoring Location 
	Description of Monitoring Location

	FLW-22IW

FLW-22RW
	Flow from Plantation Palms Well

Flow to Plantation Palms from PCMRS

	FLW-23IW

FLW-23RW
	Flow from Lexington Oaks #2 & #4 Wells

Flow to Lexington Oaks from PCMRS

	FLW-24IW

FLW-24RW
	Flow from Grand Oaks #1 through #5 Wells

Flow to Grand Oaks from PCMRS

	FLW-25IW

FLW-25RW
	Flow from Oakstead #1 & #2 Wells

Flow to Oakstead from PCMRS

	FLW-26IW

FLW-26RW
	Flow from Heritage Springs Well

Flow to Heritage Springs from PCMRS

	FLW-27IW

FLW-27RW
	Flow from Heritage Pines Well

Flow to Heritage Pines from PCMRS

	FLW-28IW

FLW-28RW
	Flow from Saddlebrook Well

Flow to Saddlebrook from PCMRS

	FLW-29IW

FLW-29RW
	Flow from Lake Bernadette Well

Flow to Lake Bernadette from PCMRS

	FLW-30IW

FLW-30RW
	Flow from Silver Oaks Well

Flow to Silver Oaks from PCMRS

	FLW-31IW

FLW-31RW
	Flow from Beacon Woods East Well

Flow to Beacon Woods East from PCMRS

	FLW-32IW

FLW-32RW
	Flow from Quail Hollow Well

Flow to Quail Hollow from PCMRS

	FLW-33IW

FLW-33RW
	Flow from Lake Jovita Well

Flow to Lake Jovita from PCMRS

	FLW-34IW

FLW-34RW
	Flow from Wildcat Well

Flow to Wildcat from PCMRS


Handcart Road Storage System (HRSS)
	Monitoring Location 
	Description of Monitoring Location

	FLW-35
	Flow, into Handcart Road Total Storage System (tank included)

	FLW-36
	Flow, into Handcart Road Ponds Only

	FLW-17
	Flow, out of Handcart Road

Storage System to SE WWTF

	FLW-37
	Flow, out of Handcart Rd Storage System into Price / Altman Groves

	OTH-01
	Staff gauge in Lake Rita


Major Residential Systems
	Monitoring Location 
	Description of Monitoring Location

	FLW-38
	Grand Oaks Subdivision Reclaimed Water Demand

	FLW-39
	Lake Bernadette Villas Reclaimed Water Demand

	FLW-40
	Lexington Oaks Subdivision Reclaimed Water Demand

	FLW-41
	Meadow Point Subdivision Reclaimed Water Demand

	FLW-42
	Oakstead Subdivision Reclaimed Water Demand

	FLW-43
	Sabal Ridge Subdivision Reclaimed Water Demand

	FLW-44
	Seven Oaks Subdivision Reclaimed Water Demand


Additional Monitoring

	Monitoring Location 
	Description of Monitoring Location

	EFF-01
	Sampling point for PCMRS reclaimed water located prior to the storage pond for the Heritage Pines Golf Course.

	EFF-02
	Sampling point for PCMRS reclaimed water located prior to the storage pond for the Timber Oaks Golf Course.

	EFF-03
	Sampling point for PCMRS reclaimed water located prior to the discharge system R-003 at Hudson RIBs.

	EFF-04
	Sampling point after the filters at Embassy Hills ponds


Flow calculations are as depicted on the Process Flow Diagrams in Attachment 3

Deer Park Subregional WWTF Flow Monitoring

(as depicted in Attachment 3, DP PFD)

	Monitoring Location 
	Description of Monitoring Location

	FLW-02
	Total flow from Deer Park Subregional WWTF to PCMRS

FLW-02 = DPA – DPB



	FLW-10
	Metered flow from PCMRS directly to Deer Park WWTF RIBs

FLW-10 = DPE

	FLW-18
	Total flow disposed into Deer Park RIBs

FLW-18 = DPB + DPE – DPD    



	FLW-DPTP
	Total Plant flow for Deer Park Subregional WWTF

FLW-DPTP = DPA



	DPA
	Metered plant flow measured upstream of the CCC



	DPB
	Metered flow to Deer Park Subregional RIBs



	DPC
	(internal metering not a part of this permit)

	DPD
	Metered flow from the RIBs to plant lift station



	DPE
	Metered flow from PCMRS directly to Deer Park WWTF RIBs



	OTH-DPRG


	Rain Gauge Located at Deer Park Subregional WWTF


Hudson Subregional WWTF Flow Monitoring

(as depicted in Attachment 3, HD PFD)

	Monitoring Location 
	Description of Monitoring Location

	FLW-04
	Total flow from Hudson Subregional WWTF to PCMRS

FLW-04 = HDA – HDB

	FLW-11
	Total flow from PCMRS to Hudson RIBs  

FLW-11 = HDE

	FLW-19
	Total flow disposed into Hudson RIBs    

FLW-19 = HDB + HDE – HDD

	FLW-HDTP
	Total Plant flow for Hudson Subregional WWTF

FLW-HDTP  = HDA



	HDA
	Flow metered after the CCC and prior to the transfer pump station



	HDB
	Total flow from Hudson Subregional WWTF to Hudson RIBs

	HDC
	(internal metering not apart of this permit)

	HDD
	Metered flow from the RIBs to plant lift station



	HDE
	Metered flow from PCMRS directly to Hudson WWTF RIBs



	OTH-HDRG


	Rain Gauge Located at Hudson Subregional WWTF


Land O’ Lakes Subregional WWTF Flow Monitoring

(as depicted in Attachment 3, LOL PFD)

	Monitoring Location 
	Description of Monitoring Location

	FLW-05
	Total flow from Land O’ Lakes Subregional WWTF to PCMRS

FLW-05= LLA – LLB



	FLW-LLTP
	Total Plant flow for Land O’Lakes Subregional WWTF

FLW-LLTP = LLA



	LLA
	Metered plant flow measured after the CCC



	LLB
	Metered flow of reject water to lined storage pond



	OTH-LLRG


	Rain Gauge Located at Land O’Lakes Subregional WWTF


Shady Hills Subregional WWTF Flow Monitoring

(as depicted in Attachment 3, SH PFD)

	Monitoring Location 
	Description of Monitoring Location

	FLW-06
	Total flow from Shady Hills Subregional WWTF directly to PCMRS

FLW-06= SHC – SHW


	FLW-16
	Flow from PCMRS to Shady Hills RIBs

FLW-16 = SHD

	FLW-21
	Calculated total flow disposed into Shady Hills RIBs   

FLW-21 = SHD

	FLW-SHTP
	Total Plant flow for Shady Hills Subregional WWTF

FLW-SHTP = SHA - SHW


	SHA
	Influent meter prior to headworks

	SHC
	Flow measured after the filters and Prior to Chlorine contact chamber

	SHD
	Flow measured fro PCMRS to Shady Hills RIBs

	SHW
	Metered flow after treatment for filter backwash.

	OTH-SHRG


	Rain Gauge Located at Shady Hills Subregional WWTF


Southeast Pasco Subregional WWTF Flow Monitoring

(as depicted in Attachment 3, SE PFD)

	Monitoring Location 
	Description of Monitoring Location

	FLW-07
	Total flow from Southeast Subregional WWTF directly to PCMRS

FLW-07 = SEA – SEB1



	FLW-17
	Metered flow back to Southeast Subregional WWTF from the Handcart Road Storage System for re-treatment.

FLW-17 = SEE

	FLW-SETP
	Total Plant flow for Southeast Subregional WWTF

FLW-SETP = SEA - SEE



	SEA
	Metered plant flow measured after the CCC



	SEB1
	Reject water to the lined storage pond



	SEE
	Metered flow from PCMRS (Handcart road storage system) to the Southeast Subregional WWTF filters.

	OTH-SERG


	Rain Gauge Located at Southeast Subregional WWTF


Wesley Center Subregional WWTF Flow Monitoring

(as depicted in Attachment 3, WC PFD)

	Monitoring Location 
	Description of Monitoring Location

	FLW-08
	Total flow from Wesley Center Subregional WWTF directly to PCMRS

FLW-08 = WCA – WCB*

*The metered flow at WCB shall only be subtracted off the metered flow at WCA when the facility is in reject for chlorine residual.

	FLW-14
	Metered flow to Oakley Grove RIBs from PCMRS

FLW-14 = WCE

	FLW-20
	Calculated percolation/evaporation flow into Oakley Grove RIBs

FLW-20 = WCE – WCX

	FLW-WCTP
	Total Treatment plant flow (excluding return from Oakley Groves)

FLW-WCTP = WCY 

	WCA
	Metered flow measured after the CCC 



	WCB
	Metered reject flow to lined storage pond.



	WCE
	Metered flow to Oakley Grove RIBs from PCMRS

	WCX
	Metered flow from Oakley Grove RIBs to Wesley Center WWTF filters

	WCY
	Metered influent flow to Wesley Center WWTF

	OTH-WCRG


	Rain Gauge Located at Wesley Center Subregional WWTF


Embassy Hills Subregional WWTF Flow Monitoring

(as depicted in Attachment 3, EH PFD)

	Monitoring Location 
	Description of Monitoring Location

	FLW-03
	Total flow from Embassy Hills Subregional WWTF to PCMRS

FLW-03 = EHB

	FLW-EHTP
	Total Treatment plant flow 
FLW-EHTP = EHA

	FLW-EHRP
	Total flow disposed into the unlined reject pond at Embassy Hills Subregional WWTF

FLW-EHRP = EHA – EHB - EHD

	EHA
	Total plant flow measured after the CCC

	EHB
	Total flow to PCMRS from Embassy Hills Subregional WWTF

	EHC
	(internal metering not apart of this permit)

	EHD
	Flow returned from the reject pond to the WWTF lift station

	OTH-EHRG


	Rain Gauge Located at Embassy Hills Subregional WWTF


New Port Richey WWTF Flow Monitoring

(as depicted in Attachment 3, NPR PFD)

	Monitoring Location 
	Description of Monitoring Location

	FLW-09
	Total flow from New Port Richey WWTF directly to PCMRS.

FLW-09 = FLW-A

	FLW-A
	Metered flow from New Port Richey WWTF to the PCMRS.


Independent RIB Flow Monitoring

(as depicted in Attachment 3, HD PFD)

	Monitoring Location 
	Description of Monitoring Location

	FLW-12
	Total flow disposed into Embassy Hills RIBs

FLW-12 = EHF                                      

	FLW-13
	Total flow disposed into Northwest RIBs

FLW-13 = SHG

	EHF
	Metered flow at Embassy Hills RIBs

	SHG
	Metered flow at Northwest RIBs


Independent RIB Flow Monitoring

(as depicted in Attachment 3, EH PFD)

	Monitoring Location 
	Description of Monitoring Location

	FLW-15
	Total flow disposed into Fox Hollow RIBs

FLW-15 = EHFH                                            

	EHFH
	Metered flow at Fox Hollow RIBs


Handcart Road Storage Flow Monitoring

(as depicted in Attachment 3, SE PFD)

	Monitoring Location 
	Description of Monitoring Location

	FLW-35
	Flow, into Handcart Road Total Storage System (tank included)

FLW-35 = SEG

	FLW-36
	Flow directly into Handcart Road Ponds Only

FLW-36 = SEF

	FLW-17
	Flow, out of Handcart Road Storage System to SE WWTF

FLW-37 = SEE

	FLW-37
	Flow, out of Handcart Rd Storage System to Price / Altman Groves

FLW-38 = SEH

	SEE
	Metered flow from Handcart Road to SE WWTF

	SEF
	Metered flow directly to handcart road storage ponds

	SEG
	Metered total flow into Handcart Road storage system 

	SEH
	Metered flow to Price Altman Groves form Handcart Road.


3. Recording flow meters and totalizers utilized to measure flow shall be calibrated at least annually.  [62-601.200(17) and .500(6)]  

4. The source treatment facilities shall be operated in accordance with all approved operating protocols.  Only reclaimed water that meets the criteria established in the approved operating protocol(s) may be released to system storage or to the reuse system.  Reclaimed water that fails to meet the criteria in the approved operating protocol(s) shall not be introduced into the master reuse system but stored and retreated at the source facility or directed to another permitted reuse system capable of disposing the reject water. The operating protocol(s) shall be reviewed and updated periodically to ensure continuous compliance with the minimum treatment and disinfection requirements.  Updated operating protocols shall be submitted to the Department for review and approval upon revision of the operating protocol(s) and with each permit application.  [62-610.320(6) and 62-610.463(2)]  

5. Parameters which must be monitored as a result of a surface water discharge shall be analyzed using a sufficiently sensitive method in accordance with 40 CFR Part 136.  Parameters which must be monitored as a result of a ground water discharge (i.e., underground injection or land application system) shall be analyzed in accordance with Chapter 62-601, F.A.C. [62-620.610(18)]
6. The permittee shall provide safe access points for obtaining representative influent, reclaimed water, and effluent samples which are required by this permit. [62-601.500(5)]
7. Monitoring requirements under this permit are effective on the first day of the second month following permit issuance.  Until such time, the permittee shall continue to monitor and report in accordance with previously effective permit requirements, if any.  During the period of operation authorized by this permit, the permittee shall complete and submit to the Department Discharge Monitoring Reports (DMRs) in accordance with the frequencies specified by the REPORT type (i.e., monthly, toxicity, quarterly, semiannual, annual, etc.) indicated on the DMR forms attached to this permit.  Monitoring results for each monitoring period shall be submitted in accordance with the associated DMR due dates below.  

	REPORT Type
	Monitoring Period
	Due Date

	Monthly or Toxicity
	first day of month – last day of month
	28th day of following month

	Quarterly
	January 1 - March 31
April 1 – June 30
July 1 – September 30 
October 1 – December 31 
	April 28
July 28
October 28
January 28

	Semiannual
	January 1 – June 30
July 1 – December 31 
	July 28
January 28

	Annual
	January 1 – December 31
	January 28 


DMRs shall be submitted for each required monitoring period including months of no discharge.  The permittee shall make copies of the attached DMR form(s) and shall submit the completed DMR form(s) to the Department postmarked by the twenty-eighth (28th) of the month following the month of operation at the addresses specified below: 

Originals to:

Florida Department of Environmental Protection

Wastewater Compliance Evaluation Section, Mail Station 3551

Twin Towers Office Building

2600 Blair Stone Road

Tallahassee, Florida  32399-2400

Copies to:

Florida Department of Environmental Protection

Domestic Wastewater Program

Southwest District Office

13051 North Telecom Parkway
Temple Terrace, Florida  33637-0926
[62-620.610(18)][62-601.300(1),(2), and (3)]
11. The permittee shall submit an Annual Reuse Report using DEP Form 62-610.300(4)(a)2. on or before January 1 of each year.  [62-610.870(3)]
12. The permittee shall maintain an inventory of storage systems.  The inventory shall be submitted to the Department at least 30 days before reclaimed water will be introduced into any new storage system.  The inventory of storage systems shall be attached to the annual submittal of the Annual Reuse Report.  [62-610.464(5)]
13. Unless specified otherwise in this permit, all reports and other information required by this permit, including 24-hour notifications, shall be submitted to or reported to, as appropriate, the Department's Southwest District Office at the address specified below:

Southwest District Office

13051 N. Telecom Parkway

Temple Terrace, FL  33637-0926

Phone Number - 813-632-7600

FAX Number -   813-632-7662   

Email – DWSWD@DEP.STATE.FL.US

All FAX copies shall be followed by original copies.  All reports and other information shall be signed in accordance with the requirements of Rule 62-620.305, F.A.C.  [62-620.305]
11. The permittee is required to sample for a period of at least 24 months the reclaimed water directed to the Heritage Pines Golf Course, Timber Oaks Golf Course, and the Hudson Subregional WWTF RIBs.  The sampling is required to verify that the reclaimed water is not impacting the groundwater quality for the parameters sodium, chloride, and total dissolved solids.  [62-600.530(4) and 62-522.700(2)] 
12. Discharge of reclaimed water to the lakes listed in the table below for storage of reclaimed water in the   stormwater storage lake systems, D-001 through D-014, shall only occur when the elevation of the water in each lake is less than the corresponding control elevation listed in the table below.  A list of all days during a month on which discharges from each lake to the receiving water body occurred shall be attached to the DMR form.  For each day on which discharge occurred, the approximate number of hours of discharge shall be noted.  [62-610.830(1) and (3)]
	Monitoring Location 
	Name of Storage Lake/Description of Monitoring Location
	Control Elevation (ft. M.S.L.)
	Receiving Water Body

	D-001

STM-01


	Heritage Springs Golf Course Pond


	37.15


	Duck Slough

	D-002

STM-02


	Seven Springs Golf Course Pond


	34.8


	Duck Slough

	D-003

STM-03


	Lexington Oaks Golf Course Pond


	64.91


	Cypress Creek North

	D-004

STM-04


	Plantation Palms Golf Course Pond


	*
	Cypress Creek

	D-005

STM-05


	Hidden Creek Golf Course Pond


	*
	Lake Zephyr

	D-006

STM-06


	Silver Oaks Golf Course Pond


	*
	Southside Branch

	D-007

STM-07


	Quail Hollow Golf Course Pond


	*
	Cypress Creek

	D-008

STM-08


	Saddlebrook Golf Course Pond


	*


	Trout Creek

	D-009

STM-09A

STM-09B


	Heritage Pines Golf Course Pond Area 43A

Heritage Pines Golf Course Pond Area 4


	21.41

23.16


	Hunter Lake Outlet

	D-010

STM-10


	Timber Oaks
	*
	Gulf of Mexico

	D-011

STM-11


	Timber Greens
	*
	Pithlachascotee River

	D-012

STM-12


	Lake Bernadette
	*
	Indian Creek

	D-013

STM-13


	Lake Jovita
	*
	Clear Lake Outlet

	D-014

STM-14E

STM-14W
	Beacon Woods East & West
	*
	Bear Creek


* The storage lake system may not be used to hold Pasco County public access reuse water until a control elevation has been approved and incorporated into the permit.  The permitte shall apply for a minor revision to the permit to include the control elevation.

II.
RESIDUALS MANAGEMENT REQUIREMENTS 

This section is not applicable to this facility.

III.
GROUND WATER REQUIREMENTS

Operational Requirements

1. For the Part III Public Access system, all ground water quality criteria specified in Chapter 62-520, F.A.C., shall be met at the edge of the zone of discharge.  The zone of discharge shall extend horizontally 100 feet from the application site or to user’s site property line, whichever is less, and vertically to the base of the surficial aquifer.  [62-520.200(23)]  [62-522.400 and 62-522.410]  

2. The ground water minimum criteria specified in Rule 62-520.400 F.A.C., shall be met within the zone of discharge.  [62-520.400 and 62-520.420(4)]
3. During the period of operation authorized by this permit, the permittee shall sample ground water in accordance with this permit and the approved ground water monitoring plan prepared in accordance with Rule 62-522.600, F.A.C.  [62-522.600][62-610.463, ]
4. The following monitoring wells shall be sampled in accordance with the monitoring frequencies specified in Permit Condition III.5 for Reuse System R-001 through R-008.  Quarterly sampling must be reasonably spaced to be representative of potentially changing conditions.

Monitoring Wells – Beacon Woods West Golf Course

	Monitoring Well ID
	Alternate Well Name and/or Description of Monitoring Location
	Aquifer Monitored
	New or

Existing

	MWB-34812
	BWSM-1
	Floridan
	existing

	MWB-34815
	BWSI-1
	Surficial
	existing

	MWI-34813
	BWSM-2
	Floridan
	existing

	MWC-34817
	BWSI-2A
	Surficial
	existing

	MWC-34816
	BWSI-4A
	Surficial
	existing

	MWC-36256
	BW-3
	Surficial
	existing


Monitoring Wells – Heritage Pines Golf Course

	Monitoring Well ID
	Alternate Well Name and/or Description of Monitoring Location
	Aquifer Monitored
	New or

Existing

	MWB-35496
	HPGC-1
	Surficial
	existing

	MWI-35497
	HPGC-2
	Surficial
	existing

	MWC-35498
	HPGC-3
	Surficial
	existing

	MWC-35499
	HPGC-4
	Surficial
	existing

	MWC-35500
	HPGC-5
	Surficial
	existing


Monitoring Wells – Silver Oaks Golf Course

	Monitoring Well ID
	Alternate Well Name and/or Description of Monitoring Location
	Aquifer Monitored
	New or

Existing

	MWB-13672
	SO-1
	Surficial
	existing

	MWC-13671
	SO-2
	Surficial
	existing

	MWC-13670
	SO-3 
	Surficial
	existing

	MWC-13669
	SO-4
	Surficial
	existing


Monitoring Wells – Price-Altman Groves

	Monitoring Well ID
	Alternate Well Name and/or Description of Monitoring Location
	Aquifer Monitored
	New or

Existing

	MWB-13647
	PA-1
	Surficial
	existing

	MWC-13646
	PA-2
	Surficial
	existing

	MWC-13645
	PA-3
	Surficial
	existing

	MWC-13643
	PA-5
	Surficial
	existing

	MWC-13642
	PA-6
	Surficial
	existing


Monitoring Wells – Timber Greens Golf Course

	Monitoring Well ID
	Alternate Well Name and/or Description of Monitoring Location
	Aquifer Monitored
	New or

Existing

	MWC-35940
	TG-1
	Surficial
	existing


Monitoring Wells – Seven Springs Golf Course

	Monitoring Well ID
	Alternate Well Name and/or Description of Monitoring Location
	Aquifer Monitored
	New or

Existing

	MWB-13538
	SSMW-1
	Surficial
	existing

	MWI-13536
	SSMW-3
	Surficial
	existing

	MWI-13531
	SSMW-5
	Surficial
	existing

	MWC-13530
	SSMW-6
	Surficial
	existing


Monitoring Wells – Odessa Sprayfield

	Monitoring Well ID
	Alternate Well Name and/or Description of Monitoring Location
	Aquifer Monitored
	New or

Existing

	MWB-01
	OD-4
	Surficial
	existing

	MWI-01
	OD-1
	Surficial
	existing

	MWC-01
	OD-2
	Surficial
	existing

	MWC-02
	OD-5
	Surficial
	existing 

	MWC-03
	OD-6
	Surficial
	existing

	MWC-04
	OD-7
	Surficial
	existing


Monitoring Wells – Quail Hollow Golf Course

	Monitoring Well ID
	Alternate Well Name and/or Description of Monitoring Location
	Aquifer Monitored
	New or

Existing

	MWB-01
	QH-1
	Surficial
	existing

	MWI-01
	QH-2
	Surficial
	existing

	MWC-01
	QH-3
	Surficial
	existing

	MWC-02
	QH-4A
	Surficial
	existing


Monitoring Wells –The Links of Lake Bernadette Golf Course

	Monitoring Well ID
	Alternate Well Name and/or Description of Monitoring Location
	Aquifer Monitored
	New or

Existing

	MWB-13668
	LB-1
	Surficial
	existing

	MWB-13663
	LB-6
	Surficial
	existing

	MWC-13667
	LB-2
	Surficial
	existing

	MWC-13648
	LB-3A
	Surficial
	existing

	MWC-13665
	LB-4
	Surficial
	existing

	MWC-13664
	LB-5
	Surficial
	existing


Monitoring Wells –Hudson RIBs

	Monitoring Well ID
	Alternate Well Name and/or Description of Monitoring Location
	Aquifer Monitored
	New or

Existing

	MWB-01
	HD-6S
	Surficial
	existing

	MWI-01
	HD-2S
	Surficial
	existing

	MWI-02
	HD-3S
	Surficial
	existing

	MWC-01
	HD-5S
	Surficial
	existing

	MWC-02
	HD-8F
	Floridan
	existing

	MWC-03
	HD-9F
	Floridan
	existing

	MWC-04
	HD-10F
	Floridan
	existing

	MWC-05
	HD-12F
	Floridan
	existing


Monitoring Wells – Embassy Hills RIBs

	Monitoring Well ID
	Alternate Well Name and/or Description of Monitoring Location
	Aquifer Monitored
	New or

Existing

	MWB-13627
	EHN-5F
	Floridan
	existing

	MWC-13631
	EHN-3S
	Surficial
	existing

	MWC-13628
	EHN-4S
	Surficial
	existing


Monitoring Wells –Fox Hollow RIBs

	Monitoring Well ID
	Alternate Well Name and/or Description of Monitoring Location
	Aquifer Monitored
	New or

Existing

	MWB-13619
	EXW-1A
	Surficial
	existing

	MWB-13626
	DMW-1
	Floridan
	existing

	MWC-13620
	EXW-3A
	Surficial
	existing

	MWC-13624
	DMW-4
	Floridan
	existing

	MWC-13612
	P-2RA
	Surficial
	existing

	MWC-13611
	P-3RA
	Surficial
	existing


Monitoring Wells –Oakley Groves RIBs

	Monitoring Well ID
	Alternate Well Name and/or Description of Monitoring Location
	Aquifer Monitored
	New or

Existing

	MWB-01
	OG-1
	Surficial
	existing

	MWI-01
	OG-3
	Surficial
	existing

	MWI-02
	OG-4
	Surficial
	existing

	MWI-03
	OG-5
	Surficial
	existing

	MWC-01
	OG-6
	Surficial
	existing

	MWC-02
	OG-8
	Surficial
	existing


Monitoring Wells –Shady Hills RIBs

	Monitoring Well ID
	Alternate Well Name and/or Description of Monitoring Location
	Aquifer Monitored
	New or

Existing

	MWI-01
	SH-1
	Surficial
	existing

	MWI-02
	SH-2
	Surficial
	existing

	MWI-03
	SH-4
	Surficial
	existing

	MWC-01
	SH-3
	Surficial
	existing

	MWC-02
	SH-5A
	Surficial
	existing

	MWC-03
	DMW-1
	Floridan
	existing

	MWC-04
	DMW-2
	Floridan
	existing


Monitoring Wells –Northwest RIBs

	Monitoring Well ID
	Alternate Well Name and/or Description of Monitoring Location
	Aquifer Monitored
	New or

Existing

	MWI-01
	SHR-2
	Surficial
	existing

	MWC-01
	SHR-2A
	Surficial
	existing

	MWC-02
	SHR-3
	Surficial
	existing


Monitoring Wells –Deer Park RIBs

	Monitoring Well ID
	Alternate Well Name and/or Description of Monitoring Location
	Aquifer Monitored
	New or

Existing

	MWB-01
	DP-1A
	Surficial
	existing

	MWI-02
	DP-2
	Surficial
	existing

	MWC-01
	DP-3
	Surficial
	existing


Monitoring Wells –Handcart Road Storage Ponds

	Monitoring Well ID
	Alternate Well Name and/or Description of Monitoring Location
	Aquifer Monitored
	New or

Existing

	MWI-13653
	HCR-2
	Surficial
	existing

	MWI-13650
	HCR-5
	Surficial
	existing

	MWC-13654
	HCR-1
	Surficial
	existing

	MWC-13649
	HCR-6
	Surficial
	existing


MWB = Background;  MWI = Intermediate;  MWC = Compliance
[62-522.600][62-610.463]  

5. The following parameters shall be analyzed for each of the monitoring well(s) identified in Permit Condition(s) III. 4:

	Parameter
	Compliance Well Limit
	Units
	Sample Type
	Monitoring Frequency

	Water Level Relative to NGVD
	Report
	FEET
	In-situ
	Quarterly

	Nitrogen, Nitrate, Total (as N)
	10
	MG/L
	Grab
	Quarterly

	Solids, Total Dissolved (TDS)
	500
	MG/L
	Grab
	Quarterly

	Arsenic, Total Recoverable
	10
	UG/L
	Grab
	Quarterly

	Chloride (as Cl)
	250
	MG/L
	Grab
	Quarterly

	Cadmium, Total Recoverable
	5
	UG/L
	Grab
	Quarterly

	Chromium, Total Recoverable
	100
	UG/L
	Grab
	Quarterly

	Lead, Total Recoverable
	15
	UG/L
	Grab
	Quarterly

	Coliform, Fecal
	4
	#/100ML
	Grab
	Quarterly

	pH*
	6.5 to 8.5
	SU
	In-situ
	Quarterly

	Sulfate, Total
	250
	MG/L
	Grab
	Quarterly

	Turbidity*
	Report
	NTU
	In-situ
	Quarterly

	Sodium, Total Recoverable
	160
	MG/L
	Grab
	Quarterly

	Specific Conductance*
	Report
	UMHO/CM
	In-situ
	Quarterly

	Temperature (C), Water*
	Report
	DEG.C
	In-situ
	Quarterly

	Dissolved Oxygen*
	Report
	MG/L
	In-situ
	Quarterly


* The field parameters shall be sampled per DEP–SOP-001/01, FS 2200 Groundwater Sampling, Figure FS 2200-2 Groundwater Purging Procedure and recorded on Form FD 9000-24, Groundwater Sampling Log (both documents attached to this permit).  The sampling logs shall be submitted with each groundwater Part D DMR. The field parameters to be reported on Part D of GW DMR shall be the last sample recorded on FD 9000-24. 

[62-522.600(11)(b)] [62-601.300(3), 62-601.700, and Figure 3 of 62-601][62-601.300(6)] [62-520.300(9)]
6. If the concentration for any constituent listed in Permit Condition III. 5. in the natural background quality of the ground water is greater than the stated maximum, or in the case of pH is also less than the minimum, the representative natural background quality shall be the prevailing standard.  [62-520.420(2)]  

7. In accordance with Part D of Form 62-620.910(10), water levels shall be recorded before evacuating wells for sample collection.  Elevation references shall include the top of the well casing and land surface at each well site (NGVD allowable) at a precision of plus or minus 0.1 foot.  [62-610.463(3)(a), ]  

8. Ground water monitoring wells shall be purged prior to sampling to obtain representative samples.  [62-601.700(5)]  

9. Analyses shall be conducted on unfiltered samples, unless filtered samples have been approved by the Department's Southwest District Office as being more representative of ground water conditions.  [62-520.300(9)]  

10. Ground water monitoring parameters shall be analyzed in accordance with Chapter 62-601, F.A.C.  [62-620.610(18)]  

11. Ground water monitoring test results shall be submitted on Part D of Form 62-620.910(10). For reuse or land application projects, results shall be submitted with the DMR for each month listed in the following schedule.  The submitted results shall be for each year during the period of operation allowed by this permit in accordance with Permit Condition I.B.9.  [62-522.600(10) and (11)(b)]  [62-601.300(3), 62.601.700, and Figure 3 of 62-601] [62-620.610(18)]  

	SAMPLE PERIOD
	REPORT DUE DATE

	January - March
	April 28

	April - June
	July 28

	July - September
	October 28

	October - December
	January 28


12. If any monitoring well becomes damaged or cannot be sampled for some reason, the permittee shall notify the Department's Southwest District Office immediately and a written report shall follow within seven days detailing the circumstances and remedial measures taken or proposed.   Repair or replacement of monitoring wells shall be approved in advance by the Department's Southwest District Office.  [62-522.600][62-4.070(3)]  

13. The Permittee shall provide verbal notice to the Department's Southwest District Office as soon as practical after discovery of a sinkhole within an area for the management or application of wastewater, wastewater residuals (sludges), or reclaimed water.  The Permittee shall immediately implement measures appropriate to control the entry of contaminants, and shall detail these measures to the Department's Southwest District Office in a written report within 7 days of the sinkhole discovery.  [62-4.070(3)]  

14. All piezometers and wells not part of the approved ground water monitoring plan are to be plugged and abandoned in accordance with Rule 62-532.500(4), F.A.C., unless there is intent for their future use.  [62-532.500(4)]  

IV.
ADDITIONAL REUSE AND LAND APPLICATION REQUIREMENTS

Part III Public Access System(s) (R-001)
1. Use of reclaimed water is authorized within the general service area identified in the map titled Pasco County Master Reuse System, Fig. 1, dated December, 2006.  The following uses of reclaimed water are authorized within this general service area:  Aesthetic Purposes (decorative ponds, pools, and fountains), Athletic Complexes and Parks, Business, Commercial and Industrial Parks, Construction Dust Control, Fire Protection, Golf Courses, Other Landscape Irrigation, Residential Developments, Residential Irrigation, Retail Nurseries, Ferneries, and Sod Farms, Toilet Flushing.  [62-620.630(10)(d)]
2. This reuse system includes the following major users (i.e., using 0.1 MGD or more of reclaimed water):

Golf Course Major Users

	User Name
	Acreage

	Beacon Woods West Golf Course
	100

	Beacon Woods East Golf Course
	170

	Timber Oaks Golf Course
	67

	Seven Springs Golf Course
	153

	Timber Greens Golf Course
	320

	Heritage Springs Golf Course
	129

	Heritage Pines Golf Course
	170

	Silver Oaks Golf Course
	188

	Lake Bernadette Golf Course
	70

	Saddlebrook Golf Course
	40

	Quail Hollow Golf Course
	137

	Lexington Oaks Golf Course
	101

	Plantation Palms Golf Course
	160

	Lake Jovita Golf Course
	357

	Hidden Creek Golf Course
	90


Parks & Schools Major Users

	User Name
	Acreage

	Arthur Engle Park
	40

	Chasco Elementary
	24

	Cotee River Elementary
	17

	Fox Hollow Elementary
	16

	Hudson School Complex
	31

	Mitchell Field
	33

	Schrader Elementary
	26

	Trinity Elementary
	7


Industrial Major Users

	User Name
	Acreage

	Odessa Sprayfield
	71

	Shady Hills Resource Recovery
	80

	Resource Recovery Cooling Tower
	N/A


Agricultural Major Users

	User Name
	Acreage

	EPCO Groves North & South
	341

	Price / Altman Groves
	150

	Tucker Grove North & South
	273

	Wildcat Grove
	147

	Williams Grove (County Owned)
	77


Residential Major Users

	User Name
	Acreage

	Grand Oaks
	25

	Lake Bernadette Villas
	29

	Lexington Oaks
	37

	Longleaf
	19

	Meadow Pointe
	290

	New River Lake
	19

	Northwood
	90

	Oakstead
	44

	Sabal Ridge
	39

	Saddlebrook West
	25

	Seven Oaks
	18

	Stage Coach Village
	67

	Timber Greens
	52


Potential Major Users

	User Name
	Proposed Use

	Bexley
	Residential

	New River
	Residential

	Connerton
	Residential

	Watergrass
	Residential

	Starkey Ranch
	Residential

	Wiregrass
	Residential


[62-610.800(5)][62-620.630(10)(b)]

3. New major users of reclaimed water (i.e., using 0.1 MGD or more) may be added to the reuse system using the general permit described in Rule 62-610.890, F.A.C., if the requirements in this rule are complied with.  Application for use of this general permit shall be made using Form 62-610.300(4)(a)1.  [62-610.890]
4. Cross-connections to the potable water system are prohibited.  [62-610.469(7)]
5. A cross-connection control program shall be implemented and/or remain in effect within the areas where reclaimed water will be provided for use.  [62-610.469(7)] 
6. The permittee shall conduct inspections within the reclaimed water service area to verify proper connections, to minimize illegal cross-connections, and to verify the proper use of reclaimed water.  Inspections are required when a customer first connects to the reuse distribution system.  Subsequent inspections are required as specified in the cross-connection control and inspection program.  [62-610.469(7)(h)]
7. If a cross-connection between the potable and reclaimed water systems is discovered, the permittee shall:

a.
Immediately discontinue potable water and/or reclaimed water service to the affected area.

b.
If the potable water system is contaminated, clear the potable water lines.

c.
Eliminate the cross-connection.

d.
Test the affected area for other possible cross-connections.

e.
Within 24 hours, notify the Southwest District Office's domestic wastewater and drinking water programs.

f.
Within 5 days of discovery of a cross-connection, submit a written report to the Department detailing: a description of the cross-connection, how the cross-connection was discovered, the exact date and time of discovery, approximate time that the cross-connection existed, the location, the cause, steps taken to eliminate the cross-connection, whether reclaimed water was consumed, and reports of possible illness, whether the drinking water system was contaminated and the steps taken to clear the drinking water system, when the cross-connection was eliminated, plan of action for testing for other possible cross-connections in the area, and an evaluation of the cross-connection control and inspection program to ensure that future cross-connections do not occur.  [62-555.350(3) and 62-555.360][62-620.610(20)]

8. Maximum obtainable separation of reclaimed water lines and potable water lines shall be provided and the minimum separation distances specified in Rule 62-610.469(7), F.A.C., shall be provided.  Reuse facilities shall be color coded or marked.  Underground piping which is not manufactured of metal or concrete shall be color coded using Pantone Purple 522C using light stable colorants.  Underground metal and concrete pipe shall be color coded or marked using purple as the predominant color.  [62-610.469(7)]
9. In constructing reclaimed water distribution piping, the permittee shall maintain a 75-foot setback distance from a reclaimed water transmission facility to public water supply wells.  No setback distances are required to other potable water supply wells or to any nonpotable water supply wells.  [62-610.471(3)]
10. A setback distance of 75 feet shall be maintained between the edge of the wetted area and potable water supply wells, unless the utility adopts and enforces an ordinance prohibiting potable water supply wells within the reuse service area.  No setback distances are required to any nonpotable water supply well, to any surface water, to any developed areas, or to any private swimming pools, hot tubs, spas, saunas, picnic tables, barbecue pits, or barbecue grills.  [62-610.471(1), (2), (5), and (7)]
11. Reclaimed water shall not be used to fill swimming pools, hot tubs, or wading pools.  [62-610.469(4)]
12. Low trajectory nozzles, or other means to minimize aerosol formation shall be used within 100 feet from outdoor public eating, drinking, or bathing facilities.  [62-610.471(6)]
13. A setback distance of 100 feet shall be maintained from indoor aesthetic features using reclaimed water to adjacent indoor public eating and drinking facilities.  [62-610.471(8)]
14. The public shall be notified of the use of reclaimed water.  This shall be accomplished by posting of advisory signs in areas where reuse is practiced, notes on scorecards, or other methods.  [62-610.468(2)]
15. All new advisory signs and labels on vaults, service boxes, or compartments that house hose bibbs along with all labels on hose bibbs, valves, and outlets shall bear the words “do not drink” and “no beber” along with the equivalent standard international symbol.  In addition to the words “do not drink” and “no beber,” advisory signs posted at storage ponds and decorative water features shall also bear the words “do not swim” and “no nadar” along with the equivalent standard international symbols.  Existing advisory signs and labels shall be retrofitted, modified, or replaced in order to comply with the revised wording requirements.  For existing advisory signs and labels this retrofit, modification, or replacement shall occur within 365 days after the date of this permit.  For labels on existing vaults, service boxes, or compartments housing hose bibbs this retrofit, modification, or replacement shall occur within 730 days after the date of this permit.  [62-610.468 & 62-610.469]
16. The permittee shall ensure that users of reclaimed water are informed about the origin, nature, and characteristics of reclaimed water; the manner in which reclaimed water can be safely used; and limitations on the use of reclaimed water. Notification is required at the time of initial connection to the reclaimed water distribution system and annually after the reuse system is placed into operation.  A description of on-going public notification activities shall be included in the Annual Reuse Report.  [62-610.468(6)]
17. Routine aquatic weed control and regular maintenance of storage pond embankments and access areas are required.  [62-610.414 & 62-610.464]
18. Overflows from emergency discharge facilities on storage ponds shall be reported as an abnormal event to the Department's Southwest District Office within 24 hours of an occurrence.  The provisions of Rule 62-610.800(9), F.A.C., shall be met.  [62-610.800(9)]
Part IV Rapid-Rate Land Application Systems (R-002 through R-008)

19.
Advisory signs shall be posted around the site boundaries to designate the nature of the project area.  [62-610.518]
20. The annual average hydraulic loading rate to the rapid infiltration basin(s) shall be limited to a maximum as applied to the entire bottom area and as indicated below:  

	Reuse System
	RIB System
	Number of Cells
	Area (Acres)
	Loading Rate (inches/day)
	Disposal Capacity (MGD)

	R-002
	Deer Park
	4
	5.6
	1.77
	0.27

	R-003
	Hudson site
	21
	31.9
	3.46
	3.0

	R-004
	Embassy Hills
	9
	18.0
	3.07
	 1.5

	R-005
	Northwest
	5
	11.7
	3.0
	0.954

	R-006
	Oakley Grove
	19
	 23.8
	0.12
	0.075

	R-007
	Fox Hollow
	4
	5.4
	4.5
	0.663

	R-008
	Shady Hills
	4
	6.28
	2.03
	0.35



[62-610.523(3)]
21. Rapid infiltration basins normally shall be loaded for 1 to 7 days and shall be rested for 5 to 14 days.  Infiltration ponds, basins, or trenches shall be allowed to dry during the resting portion of the cycle.  [62-610.523(4)]
22. Rapid infiltration basins shall be routinely maintained to control vegetation growth and to maintain percolation capability by scarification or removal of deposited solids.  Basin bottoms shall be maintained to be level.  [62-610.523(6) and (7)]
23. Routine aquatic weed control and regular maintenance of storage pond embankments and access areas are required.  [62-610.514 and 62-610.414]
24. Overflows from emergency discharge facilities on storage ponds or on infiltration ponds, basins, or trenches shall be reported as an abnormal event to the Department's Southwest District Office within 24 hours of an occurrence.  The provisions of Rule 62-610.800(9), F.A.C., shall be met.  [62-610.800(9)]
V. OPERATION AND MAINTENANCE REQUIREMENTS

1.
During the period of operation authorized by this permit, the Pasco County Master Reuse System shall be operated under the supervision of an operator certified in accordance with Chapter 62-602, F.A.C.  The PCMRS shall fall under the authority of the Pasco County Utilities’ Operations Division and meet the following operator requirement:

A Class C or higher operator for 40 hours/week.

 [62-620.630(3)] [62-699.310] [62-610.462]
4. The application to renew this permit shall include a detailed operation and maintenance performance report prepared in accordance with Rule 62-600.735, F.A.C.  [62-600.735(1)]
5. The permittee shall maintain the following records and make them available for inspection by the Department as requested.

a.
Records of all compliance monitoring information, including all calibration and maintenance records and all original strip chart recordings for continuous monitoring instrumentation and a copy of the laboratory certification showing the certification number of the laboratory, for at least three years from the date the sample or measurement was taken;

b.
Copies of all reports required by the permit for at least three years from the date the reports was prepared;

c.
Records of all data, including reports and documents, used to complete the application for the permit for at least three years from the date the application was filed;

d.
Monitoring information, including a copy of the laboratory certification showing the laboratory certification number, related to the residuals use and disposal activities for the time period set forth in Chapter 62-640, F.A.C., for at least three years from the date of sampling or measurement;

e.
A copy of the current permit;

f.
A copy of the current operation and maintenance manual as required by Chapter 62-600,. F.A.C.;

g.
A copy of the facility record drawings;

h.
Copies of the licenses of the current certified operators; and 

i.
Copies of  the logs and schedules showing plant operations and equipment maintenance for three years from the date of the logs or schedules.  The logs shall, at a minimum, include identification of the plant; the signature and certification number of the operator(s) and the signature of the person(s) making any entries; date and time in and out; specific operation and maintenance activities; tests performed and samples taken; and major repairs made. The logs shall be maintained on-site in a location accessible to 24-hour inspection, protected from weather damage, and current to the last operation and maintenance performed.


[62-620.350]
VI.
SCHEDULES

1. The permittee shall conduct and implement according to the following schedule:

	Implementation Step
	Completion Date

	1
	All metering and controls as depicted in Attachment 3 (process flow diagrams) shall be installed and operational.
	90 days from issuance of permit.

	2
	Provide appropriate documentation as required in permit condition VIII. 1 before placing any new facilities or unit processes into operation. 
	As required by conditions VIII. 1.

	3
	The permittee shall submit Process Flow Diagrams (PFDs) to the Department to be included in Attachment 3.  The revised PFDs shall depict the flow monitoring as outlined in pages 13 thru 17 of this permit.
	30 days from permit issuance.


 [62-620.320(1) and (2)] [62-4.070(3)]

VII.  INDUSTRIAL PRETREATMENT PROGRAM REQUIREMENTS

This facility is not required to have a pretreatment program at this time.  [62-625.500]
VIII.  OTHER SPECIFIC CONDITIONS

1. After completion of the metering and controls project, the permittee shall complete and submit to the Department DEP Form 62-620.910(12), Notification of Completion of Construction for Domestic Wastewater Facilities to include any deviations from the Process Flow Diagrams in Attachment 3.     [62-620.630(2)] 
2. The permittee shall apply for renewal of this permit at least 180 days before the expiration date of the permit using the appropriate forms listed in Rule 62-620.910, F.A.C., including submittal of the appropriate processing fee set forth in Rule 62-4.050, F.A.C.  The existing permit shall not expire until the Department has taken final action on the application renewal in accordance with the provisions of 62-620.335(3) and (4), F.A.C.  [62-620.335(1)-(4)]
3. Florida water quality criteria and standards shall not be violated as a result of any discharge or land application of reclaimed water or residuals from this facility.  [62-610.850(1)(a) and (2)(a)]
4. In the event that the treatment facilities or equipment no longer function as intended, are no longer safe in terms of public health and safety, or odor, noise, aerosol drift, or lighting adversely affects neighboring developed areas at the levels prohibited by Rule 62-600.400(2)(a), F.A.C., corrective action (which may include additional maintenance or modifications of the permitted facilities) shall be taken by the permittee.  Other corrective action may be required to ensure compliance with rules of the Department.  Additionally, the treatment, management, use or land application of residuals shall not cause a violation of the odor prohibition in Rule 62-296.320(2), F.A.C.  [62-600.410(8) and 62-640.400(6)]
5. The deliberate introduction of stormwater in any amount into collection/transmission systems designed solely for the introduction (and conveyance) of domestic/industrial wastewater; or the deliberate introduction of stormwater into collection/transmission systems designed for the introduction or conveyance of combinations of storm and domestic/industrial wastewater in amounts which may reduce the efficiency of pollutant removal by the treatment plant is prohibited, except as provided by Rule 62-610.472, F.A.C.  [62-604.130(3)]
6. Collection/transmission system overflows shall be reported to the Department in accordance with Permit Condition IX. 20.  [62-604.550]  [62-620.610(20)]
7. The operating authority of a collection/transmission system and the permittee of a treatment plant are prohibited from accepting connections of wastewater discharges which have not received necessary pretreatment or which contain materials or pollutants (other than normal domestic wastewater constituents):

a.
Which may cause fire or explosion hazards; or

b.
Which may cause excessive corrosion or other deterioration of wastewater facilities due to chemical action or pH levels; or

c.
Which are solid or viscous and obstruct flow or otherwise interfere with wastewater facility operations or treatment; or

d.
Which result in the wastewater temperature at the introduction of the treatment plant exceeding 40oC or otherwise inhibiting treatment; or

e.
Which result in the presence of toxic gases, vapors, or fumes that may cause worker health or safety problems.

[62-604.130(5)]
8. The treatment facility, storage ponds, rapid infiltration basins, and/or infiltration trenches shall be enclosed with a fence or otherwise provided with features to discourage the entry of animals and unauthorized persons.  [62-600.400(2)(b)]
9. Screenings and grit removed from the wastewater facilities shall be collected in suitable containers and hauled to a Department approved Class I landfill or to a landfill approved by the Department for receipt/disposal of screenings and grit.  [62-701.300(1)(a)]
10. The permittee shall provide adequate notice to the Department of the following:

a.
Any new introduction of pollutants into the facility from an industrial discharger which would be subject to Chapter 403, F.S., and the requirements of Chapter 62-620, F.A.C. if it were directly discharging those pollutants; and

b.
Any substantial change in the volume or character of pollutants being introduced into that facility by a source which was identified in the permit application and known to be discharging at the time the permit was issued.

Adequate notice shall include information on the quality and quantity of effluent introduced into the facility and any anticipated impact of the change on the quantity or quality of effluent or reclaimed water to be discharged from the facility.

[62-620.625(2)]
IX.
GENERAL CONDITIONS

1.
The terms, conditions, requirements, limitations and restrictions set forth in this permit are binding and enforceable pursuant to Chapter 403, Florida Statutes.  Any permit noncompliance constitutes a violation of Chapter 403, Florida Statutes, and is grounds for enforcement action, permit termination, permit revocation and reissuance, or permit revision.  [62-620.610(1)]

2.
This permit is valid only for the specific processes and operations applied for and indicated in the approved drawings or exhibits.  Any unauthorized deviations from the approved drawings, exhibits, specifications or conditions of this permit constitutes grounds for revocation and enforcement action by the Department.  [62-620.610(2)]
3.
As provided in Subsection 403.087(6), F.S., the issuance of this permit does not convey any vested rights or any exclusive privileges.  Neither does it authorize any injury to public or private property or any invasion of personal rights, nor authorize any infringement of federal, state, or local laws or regulations.  This permit is not a waiver of or approval of any other Department permit or authorization that may be required for other aspects of the total project which are not addressed in this permit.  [62-620.610(3)]
4.
This permit conveys no title to land or water, does not constitute state recognition or acknowledgment of title, and does not constitute authority for the use of submerged lands unless herein provided and the necessary title or leasehold interests have been obtained from the State.  Only the Trustees of the Internal Improvement Trust Fund may express State opinion as to title.  [62-620.610(4)]

5.
This permit does not relieve the permittee from liability and penalties for harm or injury to human health or welfare, animal or plant life, or property caused by the construction or operation of this permitted source; nor does it allow the permittee to cause pollution in contravention of Florida Statutes and Department rules, unless specifically authorized by an order from the Department.  The permittee shall take all reasonable steps to minimize or prevent any discharge, reuse of reclaimed water, or residuals use or disposal in violation of this permit which has a reasonable likelihood of adversely affecting human health or the environment.  It shall not be a defense for a permittee in an enforcement action that it would have been necessary to halt or reduce the permitted activity in order to maintain compliance with the conditions of this permit.  [62-620.610(5)]
6.
If the permittee wishes to continue an activity regulated by this permit after its expiration date, the permittee shall apply for and obtain a new permit.  [62-620.610(6)]
7.
The permittee shall at all times properly operate and maintain the facility and systems of treatment and control, and related appurtenances, that are installed and used by the permittee to achieve compliance with the conditions of this permit.  This provision includes the operation of backup or auxiliary facilities or similar systems when necessary to maintain or achieve compliance with the conditions of the permit.  [62-620.610(7)]

8.
This permit may be modified, revoked and reissued, or terminated for cause.  The filing of a request by the permittee for a permit revision, revocation and reissuance, or termination, or a notification of planned changes or anticipated noncompliance does not stay any permit condition.  [62-620.610(8)]

9.
The permittee, by accepting this permit, specifically agrees to allow authorized Department personnel, including an authorized representative of the Department and authorized EPA personnel, when applicable, upon presentation of credentials or other documents as may be required by law, and at reasonable times, depending upon the nature of the concern being investigated, to:

a.
Enter upon the permittee’s premises where a regulated facility, system, or activity is located or conducted, or where records shall be kept under the conditions of this permit;

b.
Have access to and copy any records that shall be kept under the conditions of this permit;

c.
Inspect the facilities, equipment, practices, or operations regulated or required under this permit; and

d.
Sample or monitor any substances or parameters at any location necessary to assure compliance with this permit or Department rules.


[62-620.610(9)]

10.
In accepting this permit, the permittee understands and agrees that all records, notes, monitoring data, and other information relating to the construction or operation of this permitted source which are submitted to the Department may be used by the Department as evidence in any enforcement case involving the permitted source arising under the Florida Statutes or Department rules, except as such use is proscribed by Section 403.111, Florida Statutes, or Rule 62-620.302, Florida Administrative Code.  Such evidence shall only be used to the extent that it is consistent with the Florida Rules of Civil Procedure and applicable evidentiary rules.  [62-620.610(10)]

11.
When requested by the Department, the permittee shall within a reasonable time provide any information required by law which is needed to determine whether there is cause for revising, revoking and reissuing, or terminating this permit, or to determine compliance with the permit.  The permittee shall also provide to the Department upon request copies of records required by this permit to be kept.  If the permittee becomes aware of relevant facts that were not submitted or were incorrect in the permit application or in any report to the Department, such facts or information shall be promptly submitted or corrections promptly reported to the Department.  [62-620.610(11)]

12.
Unless specifically stated otherwise in Department rules, the permittee, in accepting this permit, agrees to comply with changes in Department rules and Florida Statutes after a reasonable time for compliance; provided, however, the permittee does not waive any other rights granted by Florida Statutes or Department rules.  A reasonable time for compliance with a new or amended surface water quality standard, other than those standards addressed in Rule 62-302.500, F.A.C., shall include a reasonable time to obtain or be denied a mixing zone for the new or amended standard.  [62-620.610(12)]

13.
The permittee, in accepting this permit, agrees to pay the applicable regulatory program and surveillance fee in accordance with Rule 62-4.052, F.A.C.  [62-620.610(13)]

14.
This permit is transferable only upon Department approval in accordance with Rule 62-620.340, F.A.C.  The permittee shall be liable for any noncompliance of the permitted activity until the transfer is approved by the Department.  [62-620.610(14)]

15.
The permittee shall give the Department written notice at least 60 days before inactivation or abandonment of a wastewater facility and shall specify what steps will be taken to safeguard public health and safety during and following inactivation or abandonment.  [62-620.610(15)]

16.
The permittee shall apply for a revision to the Department permit in accordance with Rules 62-620.300 and the Department of Environmental Protection Guide to Wastewater Permitting at least 90 days before construction of any planned substantial modifications to the permitted facility is to commence or with Rule 62-620.325(2) for minor modifications to the permitted facility.  A revised permit shall be obtained before construction begins except as provided in Rule 62-620.300, F.A.C.  [62-620.610(16)]
17.
The permittee shall give advance notice to the Department of any planned changes in the permitted facility or activity which may result in noncompliance with permit requirements.  The permittee shall be responsible for any and all damages which may result from the changes and may be subject to enforcement action by the Department for penalties or revocation of this permit.  The notice shall include the following information:

a.
A description of the anticipated noncompliance;

b.
The period of the anticipated noncompliance, including dates and times; and

c.
Steps being taken to prevent future occurrence of the noncompliance.


[62-620.610(17)]

18.
Sampling and monitoring data shall be collected and analyzed in accordance with Rule 62-4.246, Chapters 62-160 and 62-601, F.A.C., and 40 CFR 136, as appropriate.

a.
Monitoring results shall be reported at the intervals specified elsewhere in this permit and shall be reported on a Discharge Monitoring Report (DMR), DEP Form 62-620.910(10), or as specified elsewhere in the permit.

b.
If the permittee monitors any contaminant more frequently than required by the permit, using Department approved test procedures, the results of this monitoring shall be included in the calculation and reporting of the data submitted in the DMR.

c.
Calculations for all limitations which require averaging of measurements shall use an arithmetic mean unless otherwise specified in this permit.

d.
Except as specifically provided in Rule 62-160.300, F.A.C., any laboratory test required by this permit shall be performed by a laboratory that has been certified by the Department of Health Environmental Laboratory Certification Program (DOH ELCP).  Such certification shall be for the matrix, test method and analyte(s) being measured to comply with this permit.  For domestic wastewater facilities, testing for parameters listed in Rule 62-160.300(4), F.A.C., shall be conducted under the direction of a certified operator.

e. Field activities including on-site tests and sample collection shall follow the applicable standard operating procedures described in DEP-SOP-001/01 adopted by reference in Chapter 62-160, F.A.C.  

f. Alternate field procedures and laboratory methods may be used where they have been approved in accordance with Rules 62-160.220 and 62-160.330, F.A.C.


[62-620.610(18)]
19.
Reports of compliance or noncompliance with, or any progress reports on, interim and final requirements contained in any compliance schedule detailed elsewhere in this permit shall be submitted no later than 14 days following each schedule date.  [62-620.610(19)]

20.
The permittee shall report to the Department any noncompliance which may endanger health or the environment.  Any information shall be provided orally within 24 hours from the time the permittee becomes aware of the circumstances.  A written submission shall also be provided within five days of the time the permittee becomes aware of the circumstances.  The written submission shall contain:  a description of the noncompliance and its cause; the period of noncompliance including exact dates and time, and if the noncompliance has not been corrected, the anticipated time it is expected to continue; and steps taken or planned to reduce, eliminate, and prevent recurrence of the noncompliance.

a.
The following shall be included as information which must be reported within 24 hours under this condition:

1.
Any unanticipated bypass which causes any reclaimed water or effluent to exceed any permit limitation or results in an unpermitted discharge,

2.
Any upset which causes any reclaimed water or the effluent to exceed any limitation in the permit,

3.
Violation of a maximum daily discharge limitation for any of the pollutants specifically listed in the permit for such notice, and

4.
Any unauthorized discharge to surface or ground waters.

b.
Oral reports as required by this subsection shall be provided as follows:

1.
For unauthorized releases or spills of treated or untreated wastewater reported pursuant to subparagraph a.4 that are in excess of 1,000 gallons per incident, or where information indicates that public health or the environment will be endangered, oral reports shall be provided to the Department by calling the STATE WARNING POINT TOLL FREE NUMBER (800) 320-0519, as soon as practical, but no later than 24 hours from the time the permittee becomes aware of the discharge. The permittee, to the extent known, shall provide the following information to the State Warning Point:

a) Name, address, and telephone number of person reporting;

b) Name, address, and telephone number of permittee or responsible person for the discharge; 

c) Date and time of the discharge and status of discharge (ongoing or ceased); 

d) Characteristics of the wastewater spilled or released (untreated or treated, industrial or domestic wastewater);

e) Estimated amount of the discharge;

f) Location or address of the discharge; 

g) Source and cause of the discharge; 

h) Whether the discharge was contained on-site, and cleanup actions taken to date; 

i) Description of area affected by the discharge, including name of water body affected, if any; and  

j) Other persons or agencies contacted.

2.
Oral reports, not otherwise required to be provided pursuant to subparagraph b.1 above,  shall be provided to the Department within 24 hours from the time the permittee becomes aware of the circumstances. 

c.
If the oral report has been received within 24 hours, the noncompliance has been corrected, and the noncompliance did not endanger health or the environment, the Department shall waive the written report.


[62-620.610(20)]

21.
The permittee shall report all instances of noncompliance not reported under Permit Conditions IX. 18. and 19. of this permit at the time monitoring reports are submitted.  This report shall contain the same information required by Permit Condition IX. 20 of this permit.  [62-620.610(21)]

22.
Bypass Provisions.

a.
Bypass is prohibited, and the Department may take enforcement action against a permittee for bypass, unless the permittee affirmatively demonstrates that:

1.
Bypass was unavoidable to prevent loss of life, personal injury, or severe property damage; and 

2.
There were no feasible alternatives to the bypass, such as the use of auxiliary treatment facilities, retention of untreated wastes, or maintenance during normal periods of equipment downtime.  This condition is not satisfied if adequate back-up equipment should have been installed in the exercise of reasonable engineering judgment to prevent a bypass which occurred during normal periods of equipment downtime or preventive maintenance; and

3.
The permittee submitted notices as required under Permit Condition IX. 22. b. of this permit.

b.
If the permittee knows in advance of the need for a bypass, it shall submit prior notice to the Department, if possible at least 10 days before the date of the bypass.  The permittee shall submit notice of an unanticipated bypass within 24 hours of learning about the bypass as required in Permit Condition IX. 20. of this permit.  A notice shall include a description of the bypass and its cause; the period of the bypass, including exact dates and times; if the bypass has not been corrected, the anticipated time it is expected to continue; and the steps taken or planned to reduce, eliminate, and prevent  recurrence of the bypass.

c.
The Department shall approve an anticipated bypass, after considering its adverse effect, if the permittee demonstrates that it will meet the three conditions listed in Permit Condition IX. 22. a. 1. through 3. of this permit.

d.
A permittee may allow any bypass to occur which does not cause reclaimed water or effluent limitations to be exceeded if it is for essential maintenance to assure efficient operation.  These bypasses are not subject to the provisions of Permit Condition IX. 22. a. through c. of this permit.


[62-620.610(22)]

23.
Upset Provisions

a.
A permittee who wishes to establish the affirmative defense of upset shall demonstrate, through properly signed contemporaneous operating logs, or other relevant evidence that:

1.
An upset occurred and that the permittee can identify the cause(s) of the upset;

2.
The permitted facility was at the time being properly operated;

3.
The permittee submitted notice of the upset as required in Permit Condition IX. 20. of this permit; and

4.
The permittee complied with any remedial measures required under Permit Condition IX. 5. of this permit.

b.
In any enforcement proceeding, the permittee seeking to establish the occurrence of an upset has the burden of proof.

c.
Before an enforcement proceeding is instituted, no representation made during the Department review of a claim that noncompliance was caused by an upset is final agency action subject to judicial review.

[62-620.610(23)]
Executed in Hillsborough County, Florida.

STATE OF FLORIDA DEPARTMENT OF ENVIRONMENTAL PROTECTION

____________________________________

Jeffry S. Greenwell, P.E.

Water Facilities Administrator

Southwest District

13051 N. Telecom Parkway

Temple Terrace, FL  33637-0926
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