
ATTACHMENT E

SOLID WASTE CONSTRUCTION AND OPERATIONS REQUIREMENTS
(WACS Facility ID: 45799)

1. General
This site shall be classified as a Class I landfill [Solid Waste Cells SW-1 & SW-2 and Ash Monofill Cells A-1 through A-4] and shall be constructed, operated, closed, monitored and maintained in accordance with all applicable requirements of Chapters 62-4, 62-302, 62-330, 62- 520, 62-550, and 62-701, Florida Administrative Code (F.A.C.) and all applicable requirements of Department rules.
A. Prohibitions. The prohibitions of F.A.C. Rule 62-701.300 shall apply to operations and new structures.
B. Pollution Prevention. The landfill shall be designed, constructed, operated, maintained, closed and monitored throughout its design period to control the movement of waste and waste constituents into the environment so that ground water and surface water quality standards and criteria of Chapters 62-302 and 62-520, F.A.C., will not be violated beyond the zone of discharge specified for the landfill.
C. Access Control. To prevent unauthorized waste disposal, as required by F.A.C. Rule 62-701.500(5), access to and use of the Facility shall be controlled by fencing, gates, or other barriers, as well as signs and Facility personnel.
D. Records Maintenance. As required by F.A.C. Rule 62-701.500(13), records shall be kept of all information used to develop or support the landfill design and any supplemental information provided to DEP pertaining to construction of the landfill. Records pertaining to the operation of the landfill shall be kept for the design period of the landfill. Records of all monitoring information, including calibration and maintenance records, all original chart recordings for continuous monitoring instrumentation, and copies of all reports required by these conditions, shall be kept for at least ten years.  Background water quality records shall be kept for the design period of the landfill.
E. Professional Certifications. Where required by Chapter 471 (P.E.) or Chapter 492 (P.G.), Florida Statutes, applicable portions of supporting documents which are submitted to the Department for public record shall be signed and sealed by the professional(s) who prepared or approved them.
F. Nuisance Conditions. Nuisance conditions shall be controlled by conducting site activities in the manner described in these Conditions of Certification, the operations plan, and applicable Department rules.

2. Construction
The Class I landfill disposal units associated with this site shall be constructed in accordance with all applicable requirements of Chapter 62-701, F.A.C., and in accordance with all applicable requirements of other Department rules.
A. General Construction Requirements. All construction shall be done in accordance with the approved design, drawings, CQA plan, and specifications. The Department shall be notified before any changes, other than minor deviations, to the approved design are implemented in order to determine whether an amendment or modification is required. If an
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amendment or modification is not required, it may be processed in accordance with Section A, Condition XX Procedures for Post-Certification Submittals.
C. Certification of Construction Completion. Upon completion of construction, the engineer of record shall certify to the Department in accordance with Rule 62-701.320(9)(b), F.A.C., that the permitted construction is complete and was done in substantial conformance with the approved construction plans except where minor deviations were necessary. All deviations shall be described in detail and the reasons therefore enumerated. The following documents shall be submitted along with the Certification:
(1) The final report and record drawings showing that the liner system has been installed in substantial conformance with the plans and specifications for the liner system. The record drawings must include the results of the surveys of the liner, base grade and collection pipe slopes.
(2) The final report showing the results of the geomembrane liner leak location survey, if applicable.
(3) Results of testing of geosynthetic and soil components of the liner system.
D. Construction Quality Assurance Plan pursuant to 62-701.400(1), F.A.C.
E. Approval of Certification. The licensee shall not begin using newly constructed Class I disposal unit at the facility until one of the following has occurred: (1) the Department has stated in writing that it has no objection to the certification of construction completion; or (2) at least 30 days have passed since the certification was submitted and the Department has not responded in writing to the certification.

3. Operation
Operation of the associated landfill shall be done in accordance with all applicable portions of Chapter 62-701, F.A.C., including prohibitions, procedures for closing of the landfill, and final cover requirements, or, as provided in the Conditions Section B. Condition I. Department of Environmental Protection, C – Resource Recovery Facility in its entirety. Review shall be performed in accordance with the Conditions Section A. Condition VI. Design and Performance Criteria. The final plans for this Facility shall include provisions for the isolated temporary handling of suspected hazardous, toxic, or infectious wastes.
A. No suspected or known hazardous, toxic, or infectious wastes as defined by applicable Federal, State or local statutes, rules, regulations or ordinances shall be burned or landfilled at the site.
B. Special Wastes. The disposal or management of any "special wastes" shall be in accordance with F.A.C. 62-701.300(8), 62-701.520 and any other applicable Department rules, to protect the public safety, health and welfare. All solid wastes, recovered materials, or residues shall be managed in a manner so as not to constitute a fire or safety hazard or a sanitary nuisance, and shall comply with all applicable local or state regulations.  Recovered resources which may be offered for sale shall comply with applicable regulations of all appropriate state agencies.
C. Landfill Operation Requirements. This Facility shall be operated in accordance with F.A.C. 62-701.500, Landfill Operation Requirements, and the current Department-approved Operations Plan (see attached Appendix I). Changes to the Operations Plan shall be submitted to the Department for review and written approval prior to implementation. The Department shall approve or disapprove requests for minor changes to the Operations Plan within 30 days of such change request. A minor change is defined to include: changes to filling sequence, changes to equipment used, dimensions of the working face, and similar daily operational issues.
D. 

E. Operating Personnel. As required by F.A.C. 62-701.320(15) and 62-701.500(1), at least one operator shall be at the landfill at all times when the landfill receives waste and at least one spotter shall be at the working Face when the landfill receives waste. Copies of the training verifications shall be maintained at the site for the Department’s review.
F. Operation Plan and Operating Record.  The landfill owner and operators shall have an operations plan which meets the requirements of F.A.C. 62-701.500(2). A copy of these Conditions of Certification, operations plan, construction reports and record drawings, and supporting information shall be kept at the Facility at all times for reference and inspections.
The operating record as required by F.A.C. 62-701.500(3) is part of the operations plan and shall also be maintained at the site.
G. Authorized Waste Types. The facility is authorized to manage only the following waste types defined in Rule 62-701.200, F.A.C.:
(1) Fly Ash
(2) Bottom Ash
(3) Ash Residue
(4) Class I Waste
H. Unauthorized Waste Types. The facility is not authorized to accept, process or dispose any waste types not listed in F, above. Any unauthorized waste inadvertently received by the facility shall be managed in accordance with the approved Operation Plan.
I. Landfill Elevation. The final elevation for Ash Monofill A-4 shall not exceed
+122 feet as shown on Sheets C-15 and C-15A of the plan set titled West Pasco Class I Landfill Cell A-4 Construction dated November 2008. The final elevation of Solid Waste Cell SW-2 shall not exceed +101 feet as shown on Figure 7-1, Phasing Plan for Cells SW1 and SW2, of the approved Operation Plan (Appendix I) .
J. Initial Waste Placement. The first layer of waste placed above the liner and leachate collection system shall be a minimum of four feet in compacted thickness and consist of selected wastes containing no large rigid objects that may damage the liner or leachate collection system.
K. Method and Sequence of Filling. The method and sequence of filling shall be in accordance with the current Department-approved Operations Plan.
L. Waste Records. Waste quantity records shall be maintained as required by F.A.C. 62-701.500(4) and submitted to the Department quarterly.
M. Control of Access. Access to, and use of, the Facility shall be controlled as required by F.A.C. 62-701.500(5).
N. Monitoring of Waste. Wastes shall be monitored as required by F.A.C. 62- 701.500(6). No regulated hazardous waste as identified in Chapter 62-730, F.A.C. shall be accepted for disposal at this site. Hazardous waste should be disposed of in accordance with F.A.C. 62-701.300(4) and 62-701.500(6)(b).
O. Working Face and Waste Handling Requirements. All solid waste disposed of in Cells SW-1 and SW-2 area shall be covered as required by F.A.C. 62-701.500(7).  As required by F.A.C. 62-701.500(7)(d), the operator shall minimize the size of the working Face. The working Face of a cell shall be only wide enough to accommodate vehicles discharging waste. Leachate from the working Face shall be managed as described in the approved Operations Plan. Runoff from the landfill will be considered stormwater if the flow passes over only areas with no exposed waste.
(1) Initial cover shall be applied and maintained in accordance with F.A.C. 62-701.500(7)(e), and as described in the approved Operations Plan.
(2) 

(3) Alternate cover materials not identified herein shall be approved by the Department prior to use at the Facility. For those areas where solid waste will be deposited on the working Face within 18 hours, initial cover may consist of a temporary cover or tarpaulin. Waste tires that have been cut into sufficiently small parts, which means that 70 percent of the waste tire material is cut into pieces of 4 square inches or less and 100 percent of the waste tire material is 32 square inches or less and applied in a six (6) inch compacted layer, may be used as initial cover as described in the approved Operations Plan.
(4) Intermediate cover shall be applied and maintained in accordance with
F.A.C. 62-701.500(7)(g).  An intermediate cover of one (1) foot of compacted earth in addition to the six (6) inch initial cover shall be applied within seven (7) days of cell completion at all landfills if final cover or an additional lift is not to be applied within 180 days of cell completion.
P. Final Cover. Portions of the landfill which have been filled with waste to the extent of final closure designed dimensions shall be closed (shall receive final cover) in accordance with F.A.C. 62-701.500(7)(g) and all applicable requirements of Department rules.
Q. Erosion Control. Erosion control measures shall be employed to correct any erosion which exposes waste or causes malfunction of the storm water management system. Such measures shall be implemented within three days of occurrence. If the erosion cannot be corrected within seven days of occurrence, the landfill operator shall notify the Department and propose a correction schedule.
R. Leachate Management. Leachate shall be managed in accordance with the requirements of F.A.C. 62-701.500(8), these conditions of certification, and the current Department-approved Operations Plan.
(1) Leachate storage tanks shall be inspected as required by F.A.C. 62- 701.400(6)(c)9, and inspection results shall be made available to the Department upon request.
(2) Each pump station shall be inspected on a semi-annual basis. Documentation of all inspections shall be kept on file at the Facility.
(3) Leachate generation reports as required by F.A.C. Rule 62-701.500(8) shall be compiled monthly and submitted to the Department quarterly.
(4) A report assessing the effectiveness of the leachate collection and removal system, force mains and gravity pipe lines, leachate storage tank and treatment Facility shall be submitted to the Department at least every five years. As part of the five-year assessment, the entire leachate collection and removal system, force mains and gravity pipelines, shall be visually or video inspected, or pressure tested where possible to verify adequate performance. Components not performing adequately shall be cleaned and/or repaired. Those portions of the tank secondary containment liner which can be readily visually inspected shall be inspected for damage and repaired if necessary. The report shall include the results of the inspection and any corrective measures undertaken to demonstrate adequate performance, signed and sealed by a professional engineer.
S. Landfill Gas Management
(1) Gas Monitoring and Control.
a. Landfills that receive biodegradable wastes shall have a gas management and control system designed to prevent explosions and fires, and to minimize off- site odors, lateral migration of gases and damage to vegetation. A gas management and control system is not necessary until such time as the methane generation rate exceeds the thresholds in 40 CFR 60, Subpart WWW.
b. 

c. Landfill gas shall be monitored to demonstrate compliance with the criteria established in Rule 62-701.530(1)(a), F.A.C. (less than 25% of the lower explosive limit (LEL) for combustible gases in structures and less than 100% of the LEL for combustible gases at or beyond the property boundary).
d. The results of quarterly gas monitoring required by Rule
62-701.530(2)(c), F.A.C., conducted at the locations listed in Specific Condition #F.3., shall be submitted to the Department by the following dates:

Measured During	Report Submitted By
Quarter 1	April 15th of each year
Quarter 2	July 15th of each year
Quarter 3	October 15th of each year
Quarter 4	January 15th of each year

2. Gas Monitoring Locations. The gas monitoring probes installed in proximity to solid waste cells SW-1 and SW-2 shall be sampled at least quarterly for concentrations of combustible gases determined as a percentage of the LEL calibrated to methane, as described in Rule 62-701.530(2), F.A.C.
Monitoring Probe		Location Description
Solid Waste Cell SW-1	GMP-1, GMP-2, GMP-3 and GMP-4

Solid Waste Cell SW-2	GMP-5 and GMP-6  All gas probes are to be clearly labeled and easily visible at all times

3. Gas Remediation. If the results of gas monitoring show that combustible gas concentrations exceed 25% of the LEL calibrated to methane in structures or 100% of the LEL calibrated to methane at the property boundary, the licensee shall immediately take all necessary steps to ensure protection of human health and notify the Department. Within 7 days of detection, a gas remediation plan detailing the nature and extent of the problem and the proposed remedy shall be submitted to the Department for approval. The remedy shall be completed within 60 days of detection unless otherwise approved by the Department.
4. Odor Remediation Plan. The facility shall be operated to control objectionable odors. If objectionable odors are confirmed beyond the property boundary then upon notification by the Department the licensee shall develop and implement an odor remediation plan in accordance with the requirements of Rule 62-701.530(3)(b), F.A.C.
T. Stormwater System Management.  Stormwater shall be managed as required by
F.A.C. 62-701.400(9). The system shall minimize stormwater from entering waste filled areas and avoid the mixing of stormwater with leachate.
U. Record Keeping Requirements
1. Waste Quantity Records. Waste records shall be compiled monthly, and copies shall be provided to the Department no less than annually by February 1st of each year. This information shall be reported to the Department through the DEP Business Portal located at: http://www.fldepportal.com/go.
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3. Estimate of Remaining Life. The licensee shall submit the annual estimate of the remaining life and capacity by March 1st of each year. The report is required by Rule 62-701.500(13)(c), F.A.C. and must be submitted to the District Office and to:
Florida Department of Environmental Protection Solid Waste Section, MS 4565
2600 Blair Stone Road Tallahassee, Florida, 32399-2400 SWPP@dep.state.fl.us
V. Waste Burning. Open burning of solid waste is prohibited except in accordance with F.A.C. 62-701.300(3).
W. Liner Location. The top edge of the geomembrane liner shall be clearly identified in the field to prevent waste disposal and leachate runoff outside the geomembrane liner.

4. Closure Requirements.

A. Prior to initiating closure of a solid waste disposal unit, or part of a solid waste disposal unit, the Licensee shall receive authorization from the Department in one of the following ways.
(1) If the landfill is operating under a Department approved Closure Plan with sufficient detail to provide reasonable assurance of compliance with the closing requirements of Rule 62-701.600, F.A.C., then the Licensee shall notify the Department at least 30 days prior to initiating the closure activities and receive written approval from the Department prior to beginning the work in accordance with the Conditions Section A, Condition XX. Procedures for Post-Certification Submittals.
(2) If the landfill is operating under an approved Closure Plan that requires substantive changes to the closing activities in the permitted Closure Plan, then the Licensee shall request a modification of this license to include sufficient design detail to ensure compliance with the closing requirements of Rule 62-701.600, F.A.C., and shall initiate closing only after the license has been modified in accordance with the Conditions Section A, Condition
XXIII. Modification of Certification.
(3) The Licensee shall submit an application to the Department for a closure permit on Form 62-701.900(1) and shall initiate closure activities only after the permit is issued. The application shall include a Closure Plan made up of the following:
a. A closure design plan;
b. A closure operation plan;
c. A plan for long-term care; and,
d. A demonstration that proof of financial assurance for long-term
care will be provided.

B. Closure Design. All closure construction shall be done in accordance with the approved closure design plan. The Department shall be notified before any changes, other than minor deviations, to the approved closure design are implemented in order to determine whether a modification is required. If require it will be processed in accordance with the Conditions Section A, Condition XXIII. Modification of Certification.
C. 

D. Closure Operation Plan. All closure shall be done in accordance with the approved closure operation plan.

E. Certification of Closure Construction Completion. After closure construction has been completed, the engineer of record shall certify to the Department on Form 62-701.900(2) that the closure is complete and that it was done in accordance with the plans submitted to the Department except where minor deviation was necessary. All deviations shall be described in detail and the reasons therefore enumerated.

5. Financial Assurance and Cost Estimates
A. Financial Assurance Mechanism
The licensee may not receive waste for disposal or storage in any disposal unit for which financial assurance has not been approved. Proof that the financial mechanisms are established and funded in accordance with Rule 62-701.630, F.A.C. shall be submitted to the Department at least sixty (60) days prior to the planned acceptance of solid waste in any disposal unit. When established, the licensee shall maintain, in good standing, the financial assurance mechanisms. Supporting documentation and evidence of increases associated with cost estimate increases shall be submitted within the time frames specified in Rule 62-701.630, F.A.C.

All submittals in response to this specific condition shall be sent to: Florida Department of Environmental Protection
Financial Coordinator - Solid Waste Section 2600 Blair Stone Road, MS 4548
Tallahassee, Florida 32399-2400

B. Cost Estimates.
(1) The licensee shall submit closure cost estimates, including annual adjustments for inflation, in accordance with the requirements of Rule 62-701.630(3) and (4), F.A.C., and 40 CFR Part 264.142(a) using Form 62-701.900(28).
(2) An owner or operator using an escrow account shall submit the annual inflation adjusted estimate(s) between July 1 and September 1. An owner or operator using a letter of credit, guarantee bond, performance bond, financial test, corporate guarantee, trust fund or insurance shall submit the inflation adjusted cost estimate(s) between January 1 and March 1.
(3) A revised closure cost estimate, made by recalculating the total cost of closure or long- term care, in current dollars shall be submitted every 5 years in accordance with 62-701.630(3), F.A.C.
(4) All submittals in response to this specific condition shall be sent to the District Office and a copy to the address identified in this Attachment (Attachment E) 5. Financial Assurance and Cost Estimates, A., or to the following email address: Solid.Waste.Financial.Coordinator@dep.state.fl.us.

6. Beneficial Ash Use Authorization 

A. Beneficial Use Authorization by the Department.  
Section 403.7045(5) of the Florida Statutes authorizes the Department to approve the beneficial use of ash residue when an applicant demonstrates that “no significant threat to public health will result and that applicable Department standards and criteria will not be violated.”  

B. Documents Submitted in Support of Beneficial Use of Ash Residue.  
The following documents have been submitted by the Licensee and reviewed by the Department regarding the beneficial use of bottom ash residue by the Licensee:
(1) “Request for Approval of Standing Beneficial Use Encapsulated Bottom Ash Generated by the Pasco County Resource Recovery Facility”. dated August 14, 2014. 
(2) “Request for Amendment to Approval of Standing Beneficial Use of Encapsulated Bottom Ash Generated by the Pasco County Resource Recovery Facility”, dated October 20, 2016.  
(3)	“Request for Amendment to the Previous Approval of the Standing Beneficial Uses of Bottom Ash Generated by the Pasco County Resource Recovery Facility”, which was included as part of the “Request for Modification to Conditions of Certification”, dated February 6, 2019. 

C. Approval of Beneficial Use of Bottom Ash Residue Generated by the Licensee.  Based on review of the documents listed in Paragraph 6.B. above, the Licensee is hereby authorized to beneficially use bottom ash residue in accordance with Section 403.7045(5), F.S., as follows:  
(1)	Specified Materials:
The following materials (Specified Materials) are allowed for recycling or reuse within Pasco County by, under the direction of the Licensee:
a.	Bottom Ash Residue as defined in Rule 62-701.200(7)(a), F.A.C., from the Pasco County Resource Recovery Facility (Facility), a waste-to-energy facility as defined in Section 403.7061(4), F.S. (bottom ash), andb.	Any product or construction material, including asphalt or concrete, which contains bottom ash residue as referenced herein.

(2)	Required Treatment:
a.	The Specified Materials for recycling and reuse shall be conditioned, by or under the direction of the Licensee, in accordance with the following procedure: 
Prior to recycling and reuse, bottom ash residue will be aged for a minimum period of 3 months.  Aging will be conducted on top of or in a lined Class I landfill cell.  During the entire treatment period, ash piles shall be no greater than 20 feet in height.

(3)	Specified Uses:
a.	The recycling and reuse of the above specified materials are limited to, and only approved for, the following specified uses where the Specified Materials shall be as required herein: (i)	Covered use as a road base course, where bottom ash residue from the Facility has been screened to remove large pieces of waste materials (>3/4 inch), and the road base course will be completely covered by a pavement layer; (ii)	Encapsulated use as a replacement for up to 50%, by weight, of the customarily used aggregate in Portland cement concrete pavement, where bottom ash residue from the Facility has been screened to remove large pieces of waste materials (>3/4 inch) and the fine fraction of the ash (<3/8 inch); 
(iii)	Encapsulated as an aggregate in hot mix asphalt pavement, where bottom ash residue from the Facility has been screened to remove large pieces of waste materials (>3/4 inch) and the fine fraction of the ash (<3/8 inch);
[bookmark: _GoBack](iv)	As a partial coarse aggregate replacement in Portland cement concrete slabs beneath structures; and
(v)	As a structural base course, underlying multi-use paths.

(4)	Recycling and Reuse Conditions:
The Licensee shall implement the recycling and reuse controls specified herein.  The following controls and conditions are binding upon the Licensee and are enforceable under Chapter 403, F.S: 
a.	Bottom ash residue shall be treated by conditioning, prior to recycling and reuse, in accordance with this Authorization.
b.	The Licensee shall not allow recycling, reuse, or disposal of the Specified Materials in any manner inconsistent with the requirements of Chapter 62-701, F.A.C., or this Authorization.
c.	Bottom ash residue shall not be placed within 3 feet of groundwater, or 15 feet of wetlands or natural water bodies, or within 100 feet of a potable well that is being used or might be used for human or livestock water consumption.
d.	When utilized as road base, the placement of the bottom ash residue shall not extend beyond the outside edge of the pavement*.  Bottom ash residue remaining outside the edge of the pavement after construction shall be removed and recycled in a manner consistent with this Authorization or placed in a permitted Class I lined landfill. 
e.	When utilized as road base, placement of the pavement shall be completed as soon as practicable after placement of the bottom ash residue.
f.	When bottom ash residue is utilized as a road base course, only dense‑graded asphalt mixes shall be placed as the overlying pavement layer with a 4-inch or greater as-built thickness, except that for two lane roads designed for lower density traffic loads, an overlying pavement layer with a 2-inch as-built thickness may be used.  
g.	All roadways shall be placed and maintained following generally accepted road construction practices consistent with those utilized in Pasco County at the time of the issuance of the COC modification that incorporates this Authorization. 
h.	When used as structural base for multi-use paths, the placement of the bottom ash residue shall not extend more than six inches beyond the edge of the pavement and shall be completely covered by a compacted soil layer of a thickness of at least one inch, or equal to the thickness of the pavement, whichever is greater.
i.	Bottom ash residue remaining outside this distance after construction shall be removed and recycled in a manner consistent with this Authorization or placed in a permitted Class I lined landfill.
j.	When bottom ash residue is utilized as a structural base layer under a multi-use path, only asphalt or concrete mixes shall be placed as the overlying pavement layer with a one-inch or greater as-built thickness.
k.	When removed from service, asphalt or concrete products containing bottom ash residue as aggregates shall be managed as construction and demolition debris, recycled or reused in a manner consistent with this Authorization, or placed in a permitted Class I lined landfill. 
l.	When removed from service, bottom ash residue that has been used as a base course shall be recycled or reused in a manner allowed under this Authorization or placed in a permitted Class I lined landfill. 
m.	Fugitive dust emissions from the storage, processing, transport or placement of bottom ash residue shall be controlled by wetting.
n.	Bottom ash residue used as an aggregate in asphalt and concrete shall be stored on site at batch plants for a period of no more than 120 hours. Loads shall be covered with a tarp, or a similar protective cover, during transportation and ash will not be transported during periods of inclement weather. Following batching of the concrete or asphalt products, the unused
o.	Bottom ash residue shall be recovered and either used in a subsequent allowed construction project or placed in a Class I lined landfill.
p.	The Licensee shall comply with the following record keeping requirements:
[bookmark: _Hlk2681392](i)	Whenever not the owner, the Licensee shall receive written notice, from the owner or duly authorized agent of the owner (Owner) of the property where the Specified Materials are to be placed, providing the Licensee express authorization for the placement of the Specified Materials, detailing the Owner’s authorized placement dates, placement locations, and the maximum quantities of bottom ash residue that may be recycled or reused, or otherwise placed, on the Owner’s property; 
(ii)	The Licensee may receive such notices from Owner’s electronically;
(iii)	The Licensee shall provide and maintain records detailing the actual placement dates, locations, quantities, the nature of recycling or reuse including the types of associated construction materials (i.e., road base course, concrete pavement, or asphalt pavement) where the Specified Materials were placed, and the dates and disposition whenever any Specified Materials are removed from service;
(iv)	Notices and records shall be maintained in a centralized record storage system accessible from the Facility, and also in association with the particular construction project records for any related road construction project that utilizes the Specified Materials; and
(v)	Such notices and records shall be maintained by the Licensee for a period of not less than 30 years after the removal of the Specified Materials from service. 
q.	Recycling and reuse of the Specified Materials, and associated construction activities, shall be conducted in a manner that does not cause or contribute to violations of state water quality standards.  Performance-based erosion and sediment control best management practices shall be implemented and maintained immediately prior to, during, and after construction as needed to stabilize all disturbed areas, including material storage, staging, and processing areas, to prevent adverse impacts to the water resources and adjacent lands. Erosion and sediment control measures shall be installed and maintained in accordance with the State of Florida Erosion and Sediment Control Designer and Reviewer Manual (Florida Department of Environmental Protection and Florida Department of Transportation June 2007), available at www.dep.state.fl.us/water/wetlands/docs/erp/FLErosionSedimentManual_6_07.pdf, and the Florida Stormwater Erosion and Sedimentation Control Inspector’s Manual (Florida Department of Environmental Protection, Nonpoint Source Management Section, Tallahassee, Florida, July 2008), available at www.dep.state.fl.us/water/nonpoint/docs/erosion/erosion-inspectors-manual.pdf.
r.	The Licensee shall immediately notify the Department in writing upon, or at least within 5 business days of, becoming aware of any condition, test result, or other information indicating that recycling or reuse of the Specified Materials, in accordance with this Authorization, may cause or contribute to violations of state water quality standards.
s.	Upon reasonable notice to the Licensee, Department staff or agents with proper identification shall have permission to enter, inspect, sample and test as the Department may claim needed to verify compliance with the requirements of Chapter 403, F.S., and this Authorization.
t.	Uses other than as specified herein are not approved under this Authorization.  Where bottom ash residue from the Facility, or related materials, may be used or placed in a manner that does not comply with this Authorization, such materials shall be managed as a solid waste subject to the requirements of Chapter 62-701, F.A.C. 


*Pavement is defined as including the paved shoulders
