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(1) 
SECTION 3.  EMISSIONS UNIT SPECIFIC CONDITIONS (DRAFT)
B.  EU Group Description
PERMITTEE
	Company Name
Street Address
City, State and Zip
Authorized Representative:
Name, Title
	Air Permit No. 9999999-99-AC
Permit Expires:  Date
Minor Air Construction Permit
Plant Name
Project Name


Project
This is the final air construction permit, which authorizes Very brief project description.  The proposed work will be conducted at the new/existing Plant Name, which is a Plant Type categorized under Standard Industrial Classification No. XXXX.  The new/existing facility will be/is located in Name County at Address in City, Florida.  The UTM coordinates are Zone XX, XX.XX km East and XXXX.XX km North.  
This final permit is organized into the following sections:  Section 1 (General Information); Section 2 (Administrative Requirements); Section 3 (Emissions Unit Specific Conditions); and Section 4 (Appendices).  Because of the technical nature of the project, the permit contains numerous acronyms and abbreviations, which are defined in Appendix A of Section 4 of this permit.  {Add only to the final permit.} As noted in the Final Determination provided with this final permit, only minor changes and clarifications were made to the draft permit.
STATEMENT OF BASIS
(1) 
(1) 
Letterhead
This air pollution construction permit is issued under the provisions of:  Chapter 403 of the Florida Statutes (F.S.) and Chapters 62-4, 62-204, 62-210, 62-212, 62-296 and 62-297 of the Florida Administrative Code (F.A.C.).  The permittee is authorized to conduct the proposed work in accordance with the conditions of this permit.  This project is subject to the general preconstruction review requirements in Rule 62-212.300, F.A.C. and is not subject to the preconstruction review requirements for major stationary sources in Rule 62-212.400, F.A.C. for the Prevention of Significant Deterioration (PSD) of Air Quality.
{INTENAL NOTE:  Do NOT include the following paragraph regarding an appeal IF a full administrative hearing was held on the project and there a FINAL ORDER was issued by the hearing officer.} 
Upon issuance of this final permit, any party to this order has the right to seek judicial review of it under Section 120.68 of the Florida Statutes by filing a notice of appeal under Rule 9.110 of the Florida Rules of Appellate Procedure with the clerk of the Department of Environmental Protection in the Office of General Counsel (Mail Station #35, 3900 Commonwealth Boulevard, Tallahassee, Florida, 32399-3000) {Local Air Programs will need to replace with their legal support agency} and by filing a copy of the notice of appeal accompanied by the applicable filing fees with the appropriate District Court of Appeal.  The notice must be filed within 30 days after this order is filed with the clerk of the Department.
Executed in City, Florida
(Signature)
DRAFT PERMIT
(DRAFT)
Facility Name	Project No. 9999999-999-AC
Site Name	Project Name
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CERTIFICATE OF SERVICE
The undersigned duly designated deputy agency clerk hereby certifies that this Air Permit package was sent by electronic mail, or a link to these documents made available electronically on a publicly accessible server, with received receipt requested before the close of business on the date indicated below to the following persons.
Authorized Representative, Company, email address
Application Contact, Company, email address
Applicant’s P.E. of Record, Company, email address
As necessary:  Local Air Program Office, email address
R4TitleVFL@epa.gov (Permits that establish synthetic non-Title V limitations. Also, on the email put “Synthetic Minor” in the subject line.)
Interested 3rd Parties Requesting Copies, email address
(For projects of heightened public concern:  county officials, city officials, mayor, etc.)
Ms. Barbara Friday, DEP OPC, barbara.friday@dep.state.fl.us (Only if concurrent with TV)
Ms. Lynn Scearce, DEP OPC, lynn.scearce@dep.state.fl.us (Only if concurrent with TV)
Clerk Stamp
FILING AND ACKNOWLEDGMENT FILED, on this date, pursuant to Section 120.52(7), Florida Statutes, with the designated agency clerk, receipt of which is hereby acknowledged.
(Signature)
(DRAFT)

FACILITY DESCRIPTION
{Provide a detailed facility description.}
The existing facility consists of the following emissions units (EU).
	EU No.
	Emission Unit Description

	
	

	
	

	
	


{If there is no existing facility, delete the above subsection.}
PROPOSED PROJECT
Provide a brief description of the proposed project being permitted.
This project will add and/or modify the following emissions units.
	EU No.
	Emission Unit Description

	
	

	
	

	
	


Facility Regulatory Classification
· The facility is/is not a major source of hazardous air pollutants (HAP).
· The facility operates/does not operate units subject to the acid rain provisions of the Clean Air Act (CAA).
· The facility is/is not a Title V major source of air pollution in accordance with Chapter 62-213, F.A.C.
· [bookmark: _GoBack]The facility is/is not a major stationary source in accordance with Rule 62-212.400, F.A.C. for the PSD of Air Quality.
· [bookmark: _Hlk490667633]The facility does operate units subject to the New Source Performance Standards (NSPS) of Title 40 Part 60 of the Code of Federal Regulations (40 CFR 60).  {Only include if applicable to the facility.}
· The facility does operate units subject to the National Emissions Standards of Hazardous Air Pollutants (NESHAP) of 40 CFR 63. {Only include if applicable to the facility.}


SECTION 1.  GENERAL INFORMATION (DRAFT)

1. Permitting Authority:  The permitting authority for this project is the District Office of the Department of Environmental Protection (Department).  The District/Local Office mailing address is Address, City, Florida Zip.  
2. Compliance Authority:  All documents related to compliance activities such as reports, tests, and notifications shall be submitted to the District/Local Office at:  Address, City, Florida  Zip.
3. Appendices:  The following Appendices are attached as a part of this permit:  Appendix A (Citation Formats and Glossary of Common Terms); Appendix B (General Conditions); Appendix C (Common Conditions); and Appendix D (Common Testing Requirements).  {Include only applicable Appendices.}
4. Applicable Regulations, Forms and Application Procedures:  Unless otherwise specified in this permit, the construction and operation of the subject emissions units shall be in accordance with the capacities and specifications stated in the application.  The facility is subject to all applicable provisions of: Chapter 403, F.S.; and Chapters 62-4, 62-204, 62-210, 62-212, 62-213, 62-296 and 62-297, F.A.C.  Issuance of this permit does not relieve the permittee from compliance with any applicable federal, state, or local permitting or regulations.
5. New or Additional Conditions:  For good cause shown and after notice and an administrative hearing, if requested, the Department may require the permittee to conform to new or additional conditions.  The Department shall allow the permittee a reasonable time to conform to the new or additional conditions, and on application of the permittee, the Department may grant additional time.  [Rule 62-4.080, F.A.C.]
6. Modifications:  The permittee shall notify the Compliance Authority upon commencement of construction.  No new emissions unit shall be constructed and no existing emissions unit shall be modified without obtaining an air construction permit from the Department.  Such permit shall be obtained prior to beginning construction or modification.  [Rules 62-210.300(1) and 62-212.300(1)(a), F.A.C.]
7. Construction and Expiration:  The expiration date shown on the first page of this permit provides time to complete the physical construction activities authorized by this permit, complete any necessary compliance testing, and obtain an operation permit.  Notwithstanding this expiration date, all specific emissions limitations and operating requirements established by this permit shall remain in effect until the facility or emissions unit is permanently shut down.  For good cause, the permittee may request that a permit be extended.  Pursuant to Rule 62-4.080(3), F.A.C., such a request shall be submitted to the Permitting Authority in writing before the permit expires.  [Rules 62-4.070(3) & (4), 62-4.080 & 62-210.300(1), F.A.C.]
8. Source Obligation:
a. At such time that a particular source or modification becomes a major stationary source or major modification (as these terms were defined at the time the source obtained the enforceable limitation) solely by virtue of a relaxation in any enforceable limitation which was established after August 7, 1980, on the capacity of the source or modification otherwise to emit a pollutant, such as a restriction on hours of operation, then the requirements of subsections 62-212.400(4) through (12), F.A.C., shall apply to the source or modification as though construction had not yet commenced on the source or modification.
b. At such time that a particular source or modification becomes a major stationary source or major modification (as these terms were defined at the time the source obtained the enforceable limitation) solely by exceeding its projected actual emissions, then the requirements of subsections 62-212.400(4) through (12), F.A.C., shall apply to the source or modification as though construction had not yet commenced on the source or modification.
[Rule 62-212.400(12), F.A.C.]
9. {Not needed for combined AC/AV projects}Application for Title V Permit:  This permit authorizes construction of the permitted emissions units and initial operation to determine compliance with Department rules.  A Title V air operation permit is required for regular operation of the permitted emissions unit.  The permittee shall apply for a Title V air operation permit at least 90 days prior to expiration of this permit, but no later than 180 days after commencing operation.  To apply for a Title V operation permit, the applicant shall submit the appropriate application form, compliance test results, and such additional information as the Department may by law require.  The application shall be submitted to the appropriate Permitting Authority with copies to the Compliance Authority.  [Rules 62-4.030, 62-4.050 and Chapter 62-213, F.A.C.]
Or
{Not needed for combined AC/AO projects}Application for Air Operating Permit or FESOP:  Subsequent to any construction, reconstruction or modification of a facility or emissions unit authorized by an air construction permit, and demonstration of compliance with the conditions of such air construction permit, the owner or operator of such facility or emissions unit shall obtain an initial air operation permit or revision of an existing air operation permit, whichever is appropriate, in accordance with all applicable provisions of this chapter and Chapter 62-4, F.A.C.  [Rule 62-210.300(2), F.A.C.]
10. {If applicable, move to emission unit section unless the report is for multiple emission units or is facility-wide:}  Actual Emissions Reporting:  This permit is based on an analysis that compared baseline actual emissions with projected actual emissions and avoided the requirements of subsection 62-212.400(4) through (12), F.A.C. for several pollutants.  Therefore, pursuant to Rule 62-212.300(1)(e), F.A.C., the permittee is subject to the following monitoring, reporting and recordkeeping provisions.
a. The permittee shall monitor the emissions of any PSD pollutant that the Department identifies could increase as a result of the construction or modification and that is emitted by any emissions unit that could be affected; and, using the most reliable information available, calculate and maintain a record of the annual emissions, in tons per year on a calendar year basis, for a period of 5 years {change to “10 years” if project increases design capacity or the potential to emit a PSD pollutant} following resumption of regular operations after the change.  Emissions shall be computed in accordance with the provisions in Rule 62-210.370, F.A.C., which are provided in Appendix C of this permit.
b. The permittee shall report to the Department’s permitting and compliance authority within 60 days after the end of each calendar year during the 5-year period {change to “10-year period” if project increases design capacity or potential to emit PSD pollutant} setting out the unit’s annual emissions during the calendar year that preceded submission of the report.  The report shall contain the following:
1) The name, address and telephone number of the owner or operator of the major stationary source;
2) The annual emissions calculations pursuant to the provisions of 62-210.370, F.A.C., which are provided in Appendix C of this permit;
3) If the emissions differ from the preconstruction projection, an explanation as to why there is a difference; and
4) Any other information that the owner or operator wishes to include in the report.
c. The information required to be documented and maintained pursuant to subparagraphs 62-212.300(1)(e)1 and 2, F.A.C., shall be submitted to the Department, which shall make it available for review to the general public.
d. [bookmark: _Hlk490667876]The permittee shall compute and report annual emissions in accordance with Rule 62-210.370(2), F.A.C. as provided by Appendix C of this permit.  For this project, the permittee shall use the following methods in reporting the actual annual add pollutant(s) emissions for the add emissions unit(s):
(1) [bookmark: _Hlk490667951]Example:  The permittee shall use data collected from the CEMS to determine and report the actual annual emissions of NOX and SO2.
(2) Example:  Unless otherwise approved by the Department, the permittee shall use the same emissions factors for reporting the actual annual emissions of VOC as used in the application to establish baseline emissions.  {Permitting Note:  Baseline emission factor for VOC was 0.00214 lb/ton of steam.}
(3) As defined in Rule 62-210.370(2), F.A.C., the permittee shall use a more accurate methodology if it becomes available.
e. [bookmark: _Hlk490668197]Baseline emissions of {Name Pollutants} were determined to be….  If applicable add: The could have accommodated/demand growth emissions of {Name Pollutants} were determined to be…
[Application 9999999-999-AC; and Rules 62-212.300(1)(e) and 62-210.370, F.A.C.]
(1) 
(1) 
SECTION 2.  ADMINISTRATIVE REQUIREMENTS (DRAFT)

This section of the permit addresses the following emissions units.
	EU No.
	Emission Unit Description

	
	Name of Emission Unit.

	
	

	
	


[bookmark: _Hlk490668312]{Brief descriptions of emissions units, fuels, capacity, controls, monitors, stack parameters, etc.}
{Permitting Note:  This/These emission unit(s) is/are regulated under…}
Equipment
1. Equipment Name:  The permittee is authorized to install {Specify}.  [Application No. 9999999-999-AC]
PERFORMANCE RESTRICTIONS
2. Permitted Capacity:  {Specify}  [Rule 62-210.200(PTE), F.A.C.]
3. Authorized Fuel:  {Specify}  [Application No. 9999999-999-AC and Rule 62-210.200(PTE), F.A.C.]
4. Hours of Operation/Restricted Operation:  The hours of operation are not limited (8,760 hours/year).  {Or specify}  [Rules 62-4.070(3) and 62-210.200(PTE), F.A.C.]
EMISSIONS STANDARDS
5. Emissions Standards:
a. {Specify}  [Application No. 9999999-999-AC and Rule 62-296.XXX, F.A.C.]
b. {Specify}  [Application No. 9999999-999-AC and Rule 62-296.XXX, F.A.C.]
TESTING REQUIREMENTS
6. Initial Compliance Tests:  The emissions unit shall be tested to demonstrate initial compliance with the emissions standards for Pollutants.  The initial tests shall be conducted within 60 days after achieving permitted capacity, but not later than 180 days after initial operation of the unit.  [Rules 62-4.070(3) and 62-297.310(8)(b)1, F.A.C.]
7. Annual Compliance Tests:  During each calendar year (January 1st to December 31st), the emissions unit shall be tested to demonstrate compliance with the emissions standards for Pollutants.  [Rule 62-297.310(8)(a)1, F.A.C.]
8. Test Requirements:  The permittee shall notify the Compliance Authority in writing at least 15 days prior to any required tests.  Tests shall be conducted in accordance with the applicable requirements specified in Appendix D (Common Testing Requirements) of this permit.  [Rule 62-297.310(9), F.A.C.]
[bookmark: _Hlk9346819]{Permitting Note:  Air compliance test notifications can now be completed online in the Department’s Business Portal.  To access this online process, go to http://www.fldepportal.com/go/home and sign in (or register if you’re a new user) from the link in the upper right corner of the page.  On the Welcome page select the Submit option, then select Registration/Notification, and then click on Air Compliance Test Notifications.  Once in the process, just carefully read the instructions on each screen (and under the Help tabs) to complete the notification.}
9. Test Methods:  Required tests shall be performed in accordance with the following reference methods.  Only include applicable test methods.
	Method
	Description of Method and Comments

	1-4
	Traverse Points, Velocity and Flow Rate, Gas Analysis, and Moisture Content

	5
	Method for Determining Particulate Matter Emissions

	6C
	Method for Determining Sulfur Dioxide Emissions (Instrumental)

	7E
	Determination of Nitrogen Oxide Emissions from Stationary Sources

	9
	Visual Determination of the Opacity of Emissions from Stationary Sources

	10
	Determination of Carbon Monoxide Emissions from Stationary Sources
{Note:  The method shall be based on a continuous sampling train.}

	19
	Determination of Sulfur Dioxide Removal Efficiency and Particulate Matter, Sulfur Dioxide, and Nitrogen Oxides Emission Rates (Optional F-factor method may be used to determine flow rate and gas analysis to calculate mass emissions in lieu of Methods 1-4.)

	25A
	Method for Determining Gaseous Organic Concentrations (Flame Ionization)


The above methods are described in Appendix A of 40 CFR 60 and are adopted by reference in Rule 62-204.800, F.A.C.  No other methods may be used unless prior written approval is received from the Department.  [Rules 62-204.800, F.A.C.; and Appendix A of 40 CFR 60]
MONITORING REQUIREMENTS
10. {Specify}:  The permittee shall {Specify} 
a. {Specify}  
b. {Specify}  
[Rule 62-4.070(3), F.A.C.]
RECORDS AND REPORTS
11. {If Applicable} Test Reports:  The permittee shall prepare and submit reports for all required tests in accordance with the requirements specified in Appendix D (Common Testing Requirements) of this permit.  For each test run, the report shall also indicate the {List parameters.}.  [Rule 62-297.310(10), F.A.C.]
12. {If Applicable} Operational Data:  The permittee shall {Specify}  [Rule 62-4.070(3), F.A.C.]
(1) 
(1) 
SECTION 3.  EMISSIONS UNIT SPECIFIC CONDITIONS (DRAFT)
A.  EU Group Description

This section of the permit addresses the following emissions units.
	EU No.
	Emission Unit Description

	
	Name of Emission Unit

	
	

	
	


{Brief descriptions of emissions units, fuels, capacity, controls, monitors, stack parameters, etc.}
{Permitting Note:  This emission unit is regulated under…}
Equipment
1. Equipment Name:  The permittee is authorized to install {Specify}.  [Application No. 9999999-999-AC]
PERFORMANCE RESTRICTIONS
2. Permitted Capacity:  {Specify}  [Rule 62-210.200(PTE), F.A.C.]
3. Authorized Fuel:  {Specify}  [Application No. 9999999-999-AC and Rule 62-210.200(PTE), F.A.C.]
4. Hours of Operation/Restricted Operation:  The hours of operation are not limited (8,760 hours/year).  {Or specify}  [Rules 62-4.070(3) and 62-210.200(PTE), F.A.C.]
EMISSIONS STANDARDS
5. Emissions Standards:
a. {Specify}  [Application No. 9999999-999-AC and Rule 62-296.XXX, F.A.C.]
b. {Specify}  [Application No. 9999999-999-AC and Rule 62-296.XXX, F.A.C.]
TESTING REQUIREMENTS
6. Initial Compliance Tests:  The emissions unit shall be tested to demonstrate initial compliance with the emissions standards for Pollutants.  The initial tests shall be conducted within 60 days after achieving permitted capacity, but not later than 180 days after initial operation of the unit.  [Rules 62-4.070(3) and 62-297.310(8)(b)1, F.A.C.]
7. Annual Compliance Tests:  During each calendar year (January 1st to December 31st), the emissions unit shall be tested to demonstrate compliance with the emissions standards for Pollutants.  [Rule 62-297.310(8)(a)1, F.A.C.]
8. Test Requirements:  The permittee shall notify the Compliance Authority in writing at least 15 days prior to any required tests.  Tests shall be conducted in accordance with the applicable requirements specified in Appendix D (Common Testing Requirements) of this permit.  [Rule 62-297.310(9), F.A.C.]
9. Test Methods:  Required tests shall be performed in accordance with the following reference methods.  Only include applicable test methods.
	Method
	Description of Method and Comments

	1-4
	Traverse Points, Velocity and Flow Rate, Gas Analysis, and Moisture Content

	5
	Method for Determining Particulate Matter Emissions

	6C
	Method for Determining Sulfur Dioxide Emissions (Instrumental)

	7E
	Determination of Nitrogen Oxide Emissions from Stationary Sources

	9
	Visual Determination of the Opacity of Emissions from Stationary Sources

	10
	Determination of Carbon Monoxide Emissions from Stationary Sources
{Note:  The method shall be based on a continuous sampling train.}

	19
	Determination of Sulfur Dioxide Removal Efficiency and Particulate Matter, Sulfur Dioxide, and Nitrogen Oxides Emission Rates (Optional F-factor method may be used to determine flow rate and gas analysis to calculate mass emissions in lieu of Methods 1-4.)

	25A
	Method for Determining Gaseous Organic Concentrations (Flame Ionization)


The above methods are described in Appendix A of 40 CFR 60 and are adopted by reference in Rule 62-204.800, F.A.C.  No other methods may be used unless prior written approval is received from the Department.  [Rules 62-204.800, F.A.C.; and Appendix A of 40 CFR 60]
MONITORING REQUIREMENTS
10. {Specify}:  The permittee shall {Specify} 
a. {Specify}  
b. {Specify}  
[Rule 6-24.070(3), F.A.C.]
RECORDS AND REPORTS
11. {If Applicable} Test Reports:  The permittee shall prepare and submit reports for all required tests in accordance with the requirements specified in Appendix D (Common Testing Requirements) of this permit.  For each test run, the report shall also indicate the {List parameters.}.  [Rule 62-297.310(10), F.A.C.]
12. {If Applicable} Operational Data:  The permittee shall {Specify}  [Rule 62-4.070(3), F.A.C.]
