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Geographic Information Systems

GeoData Disclaimer

DEP has not confirmed the accuracy of all the spatial data contained in its databases. Users of this data
should therefore do so at their own risk. In addition, a similar disclaimer should accompany any.
redistribution or reproduction of this data. Data is provided on an "as is" basis. Information about the
availability of specific layers may be obtained by contacting the BIS-GIS section at 850-245-8238/SC 205-
8238. Data will be distributed as WinZip archives of ESRI shapefiles. Metadata documentation is included
with each WinZipped shapefile and is available for every dataset available for download. The primary
means of distribution is via the Department's FTP site, located at

ww.dep state.flus/ais/datadir.ntm. The file names are meant to be as descriptive as possible.
However, if you have difficulty, please consult the directory or contact any of us in the sect

Special accommodations may be made for requestors with limited or no available access to the FTP site. In
those cases, media type will be Smm-tape, CDROM or 3.5 diskette. Tapes may be created in low or medium
density format (2GB, SGB, or 14GB). Applicable media charges may be applied if the medium is not replaced
or provided by the requestor.

All data are provided in the FDEP custom Albers projection in the HPGN datum. The projection parameters.
are as follows:

240000 [7| First Standard Parallel
313000 | | Second Standard Parall
840000 | | Central Meridian
240000 | | Latitude of Origin
400000 | | False Easting (meters)
0 || False Northing (meters)

1f you need to work with the data in a different projection, please see Reprojecting DEP Data.

Currently, data are available as statewide layers, with the exception of landuse/landcover and SSURGO
soils datasets processed from the five Water Management Districts (WMDs). These regional data layers
correspond to WMD boundaries. No customized clipping or joining will be performed.




