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Lower St. Johns River (LSJR) Tributaries
Technical Assessment Team (TAT) Call
August 24, 2017 2:30 PM
Meeting Highlights

Invited Participants:
	JEA 

	City of Jacksonville (COJ)

	Florida Department of Environmental Protection (DEP)

	Florida Department of Transportation (FDOT)

	Florida Department of Health (FDOH) in Duval County

	City of Atlantic Beach 

	City of Neptune Beach 

	City of Jacksonville Beach

	Naval Station (NS) Mayport



When:
Third Thursday of each month

Goals of the Calls:
· Review recent fecal coliform and Escherichia coli (E. coli) sampling results. 
· Review recent source identification (ID) monitoring results.
· Determine the best follow up actions to hits/hot spots.
· Share knowledge among entities about monitoring, eliminating sources, lessons learned, and other topics related to bacteria load reductions. 
Meeting Participants 
Zhan Bennett, FDOH 
Katie Bizub, JEA
Wayne Dickey, Jacksonville Beach
Anita Nash, DEP,
Jeremy Parrish, DEP
Cassidy Reichert, COJ
Laura Savage, Wildwood Consulting
Ginger, FDOH

Meeting Summary
[bookmark: _Hlk491419515]Jeremy Parrish reported the July results for Craig Creek. The results were also reported during last month's TAT call. The results were high, which prompted follow up sampling. The follow up sampling occurred upstream of the hot spot. Downstream was not sampled because of the tidal conditions of the creek. Anita reminded Jeremy to resample the hot spot area as well. This will show if the problem is persistent. Jeremy reported that DEP Northeast District (NED) is still sampling for fecal coliform. He will reach out to Cheryl Swanson at the DEP Lab in Tallahassee, via email, to determine when DEP NED can convert over to the new testing requirements (i.e., E. coli). Anita requested that Jeremy copy her on the email request. 

Anita reported that additional source identification work will be performed at Miller Creek and Hopkins Creek. The pilot study will be complete upon evaluation of this work. Anita asked Jeremy if he coordinated the Hopkins Creek sampling event with the City of Atlantic Beach. Jeremy responded that he called Bobby with the City of Neptune Beach, but has not reached out to Atlantic Beach yet. He noted that he will call Atlantic Beach to confirm their participation. 
 
Anita reported that two new areas will be investigated along Miller Creek. For Hopkins Creek, the investigation has progressed upstream to an underground stormwater system. Investigative work in this area could include dye testing or pipe television (tv) inspection. 

[bookmark: _Hlk491419062]Anita requested that the City of Jacksonville investigate the deteriorated stormwater pipe at Hogan Creek. JEA tried to tv inspect the pipe (Nov. 2016) but because of the pipe's condition it could not be tested. Source identification work in this area indicates raw sewage. 

Wayne Dickey reported that the bacteria count at Tallwood is still high. He resampled the hot spot site as well as downstream and upstream of the hot spot site last week. During this sampling event, Wayne noticed a cloudy white film and smelled sewage. One of the samples he pulled was next to the while film. Anita asked Wayne to check on the previously broken wastewater pipe if the August results come back high- the pipe may have been damaged again. Anita asked Wayne to use these sampling events as source identification training opportunities. Wayne agreed to perform the tasks and noted that he will send the August sample results to Anita as soon as they are available. He also noted that the city cleaned a portion of Hopkins Creek. The creek is now more accessible and more visible. The city also plans to recoat and reline manholes in an older neighborhood. 

Katie Bizub reported the August results for McCoy Creek and Williamson Creek. The fecal coliform results were less than 900 colony-forming units per 100 milliliters (cfu/100mL). She reviewed rainfall conditions prior to and during the sampling events. 

Anita asked Katie if she had any suggestions for sampling closed pipe stormwater systems. Katie recommended tv inspections. Wayne commented that pipes as small as four inches can be tv inspected. Anita asked Zhan Bennett and Ginger if they had any ideas for inspecting closed pipe systems. Ginger stated that the Florida Department of Health (FDOH) performs similar investigations, frequently prompted by complaints. Often times the issues are in heavily populated areas, which makes it difficult to pinpoint a source. Aids such as dye testing are needed to find the source. Anita commented that the source identification work is not specifically focused on septic systems. The work helps narrow down the area of concern(s), which can result in more detailed inspections including areas with both sanitary sewer and septic tanks. 

Anita reported that an area of downtown Atlantic Beach was sampled for human markers. Some of the markers were detected, but not all. She was later informed that a public beach party is held in this area annually. It was noted that the markers identified could be associated with urine and not feces. More samples are scheduled to see if the presence of the markers persists after much stormwater flushing. 

Wrap up and Comments:
Anita concluded the meeting and sent a calendar invitation for the next meeting. The next meeting will be held on September 21, 2017 at 2:30 PM. 

Meeting Adjournment:
The meeting adjourned at 3:06 pm. 

New Action Items:
1. Anita- Request the presence of the City of Atlantic Beach and Naval Air Station Mayport at the monthly TAT calls. 
2. Jeremy- Reach out to Cheryl via email to determine when DEP (NED office) can convert over to the new testing requirements (i.e., E. coli). Copy Anita on the email request.
3. Jeremy- Contact Atlantic Beach to confirm their participation in the Hopkins Creek source identification work. 
4. Anita/Cassidy- Request the City of Jacksonville investigate the deteriorated pipe at Hogans Creek.
5. Wayne- Check on the previously broken wastewater pipe if the August results are high- the pipe may have been damaged again. Use the inspection as a training opportunity. 
6. Wayne- Send the August sample results to Anita as soon as they are available.

Ongoing Action Items: 
1. Monitoring Providers- Conduct follow- up sampling (at the hot spot as well as upstream and downstream of the hot spot) if the following thresholds are exceeded: 4000 cfu/100mL for E. coli, 1300 cfu/100mL for Enterococcus, and results above historical/normal values.
2. Anita- Send two source identification sampling kits to Wayne. 
3. Wayne- Sample upstream and downstream of the sewage discharge once the source identification kits are received. 
4. Monitoring Providers: Record rain conditions during and up to 48 hours prior to a sampling event. 
5. Anita-Schedule a meeting to review the current source identification work and recent positive hits, and estimate a good range for follow up sampling. 
[bookmark: _GoBack]
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