Wekiva BMAP – Project Review Classification Criteria
(used for non-wastewater treatment plant projects)
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	Category
	Definition
	Examples

	Studies
	Project will not impact the watershed and/or springshed to help meet the TMDL.


	Studies

	Low Impact

	Project has low potential impact on the watershed and/or springshed to help meet the TMDL.


	Dry Detention Pond, Inlet Basket, Baffle Boxes, CDS Unit, erosion protection/bank stabilization, sewer pipe repair/reline

	Medium Impact
	Project has medium potential impact on the watershed and/or springshed to help meet the TMDL.

	Wet Detention Ponds, Wetland Rehabilitation, Exfiltration systems, Dry Retention Ponds, Stormwater System Inspections & Maintenance, sewering areas on septic systems

	High Impact
	Project has high potential impact on the watershed and/or springshed to help meet the TMDL.

	Wetlands, Reclaimed Water Storage Ponds




In addition to general ranking of criteria, project specific information was also considered.  The following are types of information that may have changed the impact ranking:

· Surface water projects located in the springshed (where surface water drains to the Ocklawaha Basin) - Where there was no benefit to Wekiva springshed and only benefit to the Ocklawaha surface water shed, the project was removed from consideration in the Wekiva BMAP project list but should be considered for inclusion in the Ocklawaha BMAP.
· Size of project and treatment area (e.g., large drainage area treated, extensive drainage features, extensive linear feet of pipe replaced or repaired) yielded a larger project impact classification.
· Additional components to a project (such as Bold and Gold™) yielded a larger project impact classification
