MC-11: Fern Creek Water Quality Retrofit
Project Summary
[bookmark: _GoBack]The project consists of a wet detention area retrofit stormwater treatment area to serve existing development within the Fern Creek Basin. The 6.4-acre wet detention facility is located within land acquired by Martin County. Surface water runoff is routed into the wet detention flow-through area for water quality treatment prior to discharge back Fern Creek via a connecting channel.
Documents Included
· MC Storm Projects – Detention Volumes (Table)
· Has Elevation, Area, Storage (in acre-feet), Depth, Width, and Length of the project on page 2
· 030929-11_Permit_13819 (SFWMD permit)
· All information typical of a SFWMD Environmental Resource Standard General Permit (general conditions, special conditions, notice of rights, project evaluation, related concerns)
· Operational information can be found on pages 13 and 14 of the permit PDF.
