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Project Summary
Installation of the C-25 Diversion Structure which regulates flow from the NSLRWCD C-44/North Emergency Relief Canal to SFWMD C-25. The C-25 structure can remove runoff from the North St. Lucie Basin under various flow events. In addition, three risers with adjustable gates were installed. These 4 control structures together provide better water quality and more efficient management of water levels. The C-25 Diversion Structure has the capacity to serve approximately 3,795 acres. The 3 other control structures serve approximately 4,000 acres around Canals 52, 53, 54 & 55.
Documents Included
· No supporting documentation.
