A sensitive rapid resolution liquid chromatography–tandem mass spectrometry (RRLC–MS/MS) method, combined with solid-phase extraction, ultrasonic extraction and silica gel cartridge cleanup, was developed for 28 steroids including 4 estrogens (estrone (E1), 17_-estradiol (E2), 17_-ethynyl estradiol (EE2), diethylstilbestrol (DES)), 14 androgens (androsta-1,4-diene-3,17-dione (ADD), 17_-trenbolone, 17_- trenbolone, 4-androstene-3,17-dione, 19-nortestoserone, 17_-boldenone, 17_-boldenone, testosterone (T), epi-androsterone (EADR), methyltestosterone (MT), 4-hydroxy-androst-4-ene-17-dione (4-OHA), 5_-dihydrotestosterone (5_-DHT), androsterone (ADR), stanozolol (S)), 5 progestagens (progesterone (P), ethynyl testosterone (ET), 19-norethindrone, norgestrel, medroxyprogesterone (MP)), and 5 glucocorticoids
(cortisol, cortisone, prednisone, prednisolone, dexamethasone) in surface water, wastewater
[bookmark: _GoBack]and sludge samples. The recoveries of surface water, influents, effluents and sludge samples were 90.6–119.0% (except 5_-DHT was 143%), 44.0–200%, 60.7–123% and 62.6–138%, respectively. The method detection limits for the 28 analytes in surface water, influents, effluents and freeze-dried sludge samples were 0.01–0.24 ng/L, 0.02–1.44 ng/L, 0.01–0.49 ng/L and 0.08–2.06 ng/g, respectively. This method was applied in the determination of the residual steroidal hormones in two surface water of Danshui River, 12 wastewater and 8 sludge samples from two wastewater treatment plants (Meihu and Huiyang WWTPs) in Guangdong (China). Ten analytes were detected in surface water samples with concentrations ranging between 0.4 ng/L (17_-boldenone) and 55.3 ng/L (5_-DHT); twenty analytes in the wastewater samples with concentrations ranging between 0.3 ng/L (P) and 621 ng/L (5_-DHT); and 12 analytes in the sludge samples with concentrations ranging between 1.6 ng/g (E1) and 372 ng/g
(EADR).
