MERRITT’S MILL POND SAMPLING LOCATIONS
Weeks of January 24 & 31, 2012

· Collect surface water samples at 5 designated latitude/longitude locations and 4 spring locations (only if springs are discharging): field, lab, isotopes, Secchi Depth (for surface water stations, only if water is NOT clear to the bottom)…

· In addition to field and lab samples, please describe / sketch algal/benthic plant communities at each site, and take underwater photos, too.
Surface Water Stations (NE – SW):
1) MMP-1: 30˚47’15.4” / 85˚08’41.1”
2) MMP-2 (aka “BLUE SPRINGS N END HWY # 164”): 30˚47’11.4” / 85˚08’56.2”
3) MMP-3 (aka “NWB-LL-1002 MERRITT’S MILL POND”): 30˚47’01.6” / 85˚09’24.7”
4) MMP-4 (aka “Merritt’s Mill Pond Station 3”): 30˚46’07.3” / 85˚10’22.9”
5) MMP-5 (aka “Merritts Mill Pond @ Hwy. 90”): 30˚45’12.5” / 85˚11’33.6”
Spring Stations (NE – SW: sample ONLY if flowing):
6) Shangri-La Spring: 30˚47’24.6” / 85˚08’34.4”
7) Twin Caves Spring: 30˚47’12.9” / 85˚08’41.8”
8) Hole-In-The-Wall Spring: 30˚47’00.2” / 85˚09’22.1”
9) Gator Hole Spring: 30˚46’40.3” / 85˚10’01.7”
Use the FREE FWS boat ramp shown on Garmin Handheld GPS unit (on Hunter Fish Camp Road) to access the Mill Pond.
Gary Maddox: 850-566-4298 (cell)

Mike Nash: 850-591-9664 (cell)
