Differences between DEP and DOH qualifiers:
 

A : doesn't matter, as is a qualifier for biologicals, which we don't track. If you note that there are five instances of 'A' in our database, you will see that they are for samples analyzed at DEP (the DEP analyses can be distinguished by the chemical name, which is in lower case for DEP samples).
 

F:, both are QA issues, slightly different.
 

J: both are QA issues, slightly different.
 

K: both are QA issues, slightly different.
 

O: if the value is zero in our database (over 97% of those with "O" qualifier), the O's mean the same thing (no analysis done). IF the value is nonzero in our database then O means approximate.
 
V: both are contaminated blank QA issues, slightly different
 

W:  In our database, means XYLENE value is sum of three components. In Gwis it means well construction issues.
 

Same:
 

I
T
U
attached is the list of DoH lab qualifiers.
 SampleManager List of RESULT_QUALIFIER records                         Page  1

Generated by : WPRIEST                                                          

Generated on : 19-JAN-2006 05:24:37.00                                          

Identity    : A                                                                

Description : Result based on countable colonies as indicated (TSA only or MEA o

Identity    : B                                                                

Description : Potential lead risk to children; contact Joe Sekerke at 904-488-33

Identity    : C                                                                

Description : Result exceeds Maximum Contaminant Level as in Chap. 62-550 or 520

Identity    : D                                                                

Description : Confirmation test performed beyond holding time; result is suspect

Identity    : E                                                                

Description : Analyte not detected; quality control out of range; result is the 

Identity    : F                                                                

Description : Result exceeds allowable level (Manual for the Cert. of Labs, EPA 

Identity    : G                                                                

 Description : Result based on dissolved ions, i.e., the sample was filtered by 

Identity    : H                                                                

Description : Value exceeds DOH Health Advisory Level.                          

Identity    : I                                                                

Description : Approximate result between MDL and PQL; supporting evidence for id

Identity    : J                                                                

Description : Approximate result; quality control out of range.                 

Identity    : K                                                                

Description : Approximate result; result out of calibrated range of instrument. 

Identity    : L                                                                

Description : Wipe sample included significant particles of debris.             

Identity    : M                                                                

Description : Method approved only as a screen for this analyte.                

Identity    : N                                                                

Description : Analyte not reported due to interference; result is the MDL.      

Identity    : O                                                                

Description : Method not approved for this analyte; result for informational pur

Identity    : P                                                                

Description : No valid trip blank result for this analyte; result is suspect.   

Identity    : Q                                                                

Description : MDL reflects sample dilution due to matrix or interference effects

Identity    : R                                                                

Description : Result exceeds recommended lead level of 0.50% by weight.         

Identity    : S                                                                

Description : Analyte not screened; result value is the MDL.                    

Identity    : T                                                                

Description : Peak detected; supporting evidence for identity; result is the MDL

Identity    : U                                                                

Description : Analyte not detected; result reported is the MDL, if applicable.  

Identity    : V                                                                

Description : Analyte detected in the sample and laboratory reagent blank; resul

Identity    : W                                                                

Description : Result is the sum of three components.                            

Identity    : X                                                                

Description : Analyte detected in both the sample and the trip blank.           

Identity    : Y                                                                

Description : Analysis from improperly preserved sample; result is suspect.     

Identity    : Z                                                                

Description : Zero result with qualifier indicates colonies too numerous to coun

                 --------------------------------

 

On an unrelated note, as I was looking through the data to respond to your question, I noticed that the majority of "real" values with qualifier of "O" were treated finished drinking water samples. I was wondering how a user of this composite database will be able to distinguish these, because if she doesn't, she will be under the impression that the groundwater in Florida is heavily contaminated with trihalomethane products.
