INORGANIC CONTAMINANTS

Introduction to Inorganic Contaminants and Ground Water Quality
Environmental Fate and Transport of Inorganic Contaminants

The priority order of metals for ground water, based on toxicity and occurrence, are in decreasing order:  Lead, arsenic, cadmium, mercury, chromium, thallium, iron, aluminum, zinc, copper, nickel, selenium, silver, manganese, sodium and beryllium.

The priority order of metals for surface water based on occurrence for both the planning and verified lists are in decreasing order:  Lead, copper, iron, chromium, mercury, cadmium, silver, selenium, beryllium, nickel, zinc, arsenic, thallium, aluminum, manganese and sodium.

