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Escambia County Daily Sampling Report  
August 10, 2010

The Florida Department of Environmental Protection is collecting and analyzing water, sediment, and oil samples from Florida’s coastal waters in response to the Deepwater Horizon oil spill.  These samples are being collected for a variety of purposes.  There is a delay from when the samples are collected to when the results are reported due to the time that it takes to deliver the samples to the lab and then analyze the samples.  We are striving for a four day turnaround time.  Results will be reported on a daily basis.  

New Information Week of August 9th – August 13th: 
· Week of August 9nd through August 13, 2010, water quality samples will be collected on Monday and Thursday.   Samples collected Tuesdays in Franklin and Gulf County.  Water samples will be analyzed for PAH’s.  Sampling frequencies may change next week based on beach advisories.
·  Note: For new water quality result information please see information highlighted in yellow below.  
The following sampling was performed in Escambia County:
· Results reported below for 8/5/10 sampling event.

Post Impact Sampling (Reporting results from August 9th through August 13th, 2010):

	Date Sampled
	Sampling Information
	Results

	PENSACOLA BEACH SOUTH OF TRISTAN TOWERS

	6/22/2010 15:49
	Water sample analyzed for dispersant
	No Dioctylsulfosuccinate-Na* was found. *

	PENSACOLA BEACH @ FT.  PICKENS

	8/5/10
	Water Sample
	No petroleum-related contaminants were found.

	PERDIDO KEY-JOHNSON BEACH

	8/5/10
	Water Sample
	No petroleum-related contaminants were found.

	PENSACOLA BEACH EAST OF PIER

	8/5/10
	Water Sample
	No petroleum-related contaminants were found.

	NAVARRE PARK*

	8/5/10
	Water Sample
	No petroleum-related contaminants were found.

	NAVARRE BEACH**

	6/22/2010 14:45
	Water sample analyzed for dispersant
	No Dioctylsulfosuccinate-Na* was found. *


* Of the Corexit dispersant products that were used during the Deepwater Horizon Oil Spill, Dioctylsulfosuccinate-Na is the component that is most likely to persist in the water.
** by lat/longs, area sampled in Escambia County
Table Explanation:
· Water sample – indicates a water sample that was taken, no oil was visible in the water when the sample was taken.

· Sand sample – indicates a sand sample that was taken to evaluate any potential petroleum contamination.  

· “10 cm from visible tar ball”, “1 meter from visible tar ball”, “near oil sheen and/or tar balls” or “Near mousse”– These are types of proximity sampling that means samples were collected at known distances from oil material.  This sampling is performed when the oil in the water is sparse enough that a bather might reasonably expect to swim in the water without coming into contact with the oil.  

· Collected for dispersant analysis – These samples are collected to attempt to detect dispersant.  The first priority is to collect the sample in proximity to oil when oil is present.  When oil is not present the second priority is to sample in locations were oil was previously present.  The third priority is to collect the sample where no oil contamination is, or ever was, present.  

For additional information, please refer to the DEP Deepwater Horizon website at http://www.dep.state.fl.us/deepwaterhorizon/default.htm 
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