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Escambia County Daily Sampling Report  

July 12, 2010

The Florida Department of Environmental Protection is collecting and analyzing water, sediment, and oil samples from Florida’s coastal waters in response to the Deepwater Horizon oil spill.  These samples are being collected for a variety of purposes.  There is a delay from when the samples are collected to when the results are reported due to the time that it takes to deliver the samples to the lab and then analyze the samples.  We are striving for a four day turnaround time.  Results will be reported on a daily basis.  

Proposed Sampling in Escambia County Week of July 11-July 16th: 

· Water samples will be collected on Sunday, Tuesday, and Thursday this week.  
The following sampling was performed in Escambia County:
· Samples collected at four locations on 7/8/10– Pensacola Beach Pier, Navarre Beach Pier, Langdon Beach at Fort Pickens, and at Johnson Beach (near Perdido Key).

Post Impact Sampling (Reporting results from July 8th through July 16th, 2010):

	Date Sampled
	Sampling Information
	Results

	PENSACOLA BEACH PIER

	7/8/10
	Water Sample
	No petroleum-related contaminants were found.

	LANGDON BCH @ FT.PICKENS

	7/8/10
	Water Sample
	No petroleum-related contaminants were found.



	JOHNSON’S BEACH

	7/8/10
	Water sample
	No petroleum-related contaminants were found.

	NAVARRE BEACH PIER *

	7/8/10
	Water sample
	A small amount of a gas/diesel contaminant (naphthalene) was detected. This is not believed to be associated with the Deepwater Horizon oil spill.


*by lat/longs, area sampled in Escambia County

Table Explanation:

· Water sample – indicates a water sample that was taken, no oil was visible in the water when the sample was taken.

· Sand sample – indicates a sand sample that was taken to evaluate any potential petroleum contamination.  

· “10 cm from visible tar ball”, “1 meter from visible tar ball”, “near oil sheen and/or tar balls” or “Near mousse”– These are types of proximity sampling that means samples were collected at known distances from oil material.  This sampling is performed when the oil in the water is sparse enough that a bather might reasonably expect to swim in the water without coming into contact with the oil.  

· Collected for dispersant analysis – These samples are collected to attempt to detect dispersant.  The first priority is to collect the sample in proximity to oil when oil is present.  When oil is not present the second priority is to sample in locations were oil was previously present.  The third priority is to collect the sample where no oil contamination is, or ever was, present.  

For additional information, please refer to the DEP Deepwater Horizon website at http://www.dep.state.fl.us/deepwaterhorizon/default.htm 
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