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Escambia County Daily Sampling Report  

July 19, 2010

The Florida Department of Environmental Protection is collecting and analyzing water, sediment, and oil samples from Florida’s coastal waters in response to the Deepwater Horizon oil spill.  These samples are being collected for a variety of purposes.  There is a delay from when the samples are collected to when the results are reported due to the time that it takes to deliver the samples to the lab and then analyze the samples.  We are striving for a four day turnaround time.  Results will be reported on a daily basis.  

New Information Week of July 18th -July 23rd: 
· Week of July 18th through July 23rd, 2010, water quality samples to be collected on Monday and Thursday of this week.  Samples collected Tuesdays in Franklin and Gulf County.
·  Note: For new water quality result information please see the rows highlighted in yellow below.  
The following sampling was performed in Escambia County:
· Sampling commenced on July 19, 2010.
Post Impact Sampling (Reporting results from July 15th through July 23rd, 2010):

	Date Sampled
	Sampling Information
	Results

	PENSACOLA BEACH FORT PICKENS

	7/15/10
	Water Sample
	No petroleum-related contaminants were found.

	PENSACOLA BEACH @ WALKOVER # 16

	7/15/10
	Water Sample
	No petroleum-related contaminants were found.

	NAVARRE BEACH FISHING PIER *

	7/15/10
	Water sample
	No petroleum-related contaminants were found.

	NAVARRE BEACH WEST*

	7/15/10
	Water Sample
	No petroleum-related contaminants were found.


*by lat/longs, area sampled in Escambia County
Table Explanation:

· Water sample – indicates a water sample that was taken, no oil was visible in the water when the sample was taken.

· Sand sample – indicates a sand sample that was taken to evaluate any potential petroleum contamination.  

· “10 cm from visible tar ball”, “1 meter from visible tar ball”, “near oil sheen and/or tar balls” or “Near mousse”– These are types of proximity sampling that means samples were collected at known distances from oil material.  This sampling is performed when the oil in the water is sparse enough that a bather might reasonably expect to swim in the water without coming into contact with the oil.  

· Collected for dispersant analysis – These samples are collected to attempt to detect dispersant.  The first priority is to collect the sample in proximity to oil when oil is present.  When oil is not present the second priority is to sample in locations were oil was previously present.  The third priority is to collect the sample where no oil contamination is, or ever was, present.  

For additional information, please refer to the DEP Deepwater Horizon website at http://www.dep.state.fl.us/deepwaterhorizon/default.htm 
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