Escambia County Daily Sampling Report  
July 6, 2010

The Florida Department of Environmental Protection is collecting and analyzing water, sediment, and oil samples from Florida’s coastal waters in response to the Deepwater Horizon oil spill.  These samples are being collected for a variety of purposes.  There is a delay from when the samples are collected to when the results are reported due to the time that it takes to deliver the samples to the lab and then analyze the samples.  We are striving for a four day turnaround time.  Results will be reported on a daily basis.  

Sampling in Escambia County Week of July 2-July 8th: 
· Proposed: Two water samples will be collected on Sunday (7/4), Tuesday (7/6), and Thursday (7/8) this week. 

· Planned: Wednesday (7/7) – Sediment samples will be collected in Escambia County. 

The following sampling was performed in Escambia County:
· One sample at Fort Pickens.  An attempt was made at Johnson Beach on Perdido Key (rough, no sample taken).  Orange “stain” on high tide line, tar balls on beach, none visible in H2O.  Cleanup crews present.  Some “oiled” garbage on beach. 
· At sample site in Langdon Beach in State Park, there were large patches of small tar balls at sample site, and a sample was taken  in between tar ball (no edge, no prox sample collected)
· Additional samples were collected on Friday (7/2), Saturday (7/3), and Monday (7/5).


Post Impact Sampling (includes last week results):
	Date Sampled
	Sampling Information
	Results

	Note: sampling was cancelled on June 30 and July 1 due to rough surf conditions

	PENSACOLA BEACH 

	6/28/10
	3 Sediment samples
	Petroleum constituents were found. 

	6/28/10
	Water sample
	Trace levels of petroleum constituents were found

	PENSACOLA BEACH PIER

	6/24/10
	Water sample
	Petroleum-related compounds were detected in water near a tar ball but no health exposure benchmarks were exceeded.

	PENSACOLA BEACH WALKOVER 16

	7/2/10
	Water sample
	Trace levels of petroleum constituents were found

	FORT PICKENS BEACH AREA

	7/2/10
	Water Sample
	Trace levels of petroleum constituents were found

	6/29/10
	Water sample
	Petroleum-related compounds were detected but no health exposure benchmarks were exceeded.

	6/24/10
	Water sample (mousse reported the day before but not visible at time of collection)
	Petroleum-related compounds were detected but no health exposure benchmarks were exceeded.

	6/23/10
	Near mousse
	Petroleum-related compounds were detected but no health exposure benchmarks were exceeded.

	6/23/10
	Water sample
	No petroleum contaminants were found

	GULF ISLAND NATIONAL SEASHORE

	6/25/10
	Sand sample
	Two samples collected: one contained petroleum-related compounds but no health exposure benchmarks were exceeded the other contained no petroleum contaminants.

	6/24/10
	Water sample
	Petroleum-related compounds were detected but no health exposure benchmarks were exceeded.

	JOHNSON’S BEACH

	6/28/10
	Water sample, sand sample
	No petroleum contaminants were found in water.  Results not yet available on sand samples.


	6/24/10
	Water sample
	No petroleum contaminants were found

	Date Sampled
	Sampling Information
	Results

	HAWKSHAW LAGOON

	6/24/10
	Water sample
	Petroleum-related compounds were detected in water near a tar ball but no health exposure benchmarks were exceeded.

	PROJECT GREENSHORES

	6/24/10
	Water sample
	No petroleum contaminants were found

	NAVARRE BEACH

	6/28/10
	Water Sample
	No petroleum constituents were found

	NAVARRE BEACH FISHING PIER

	7/2/2010
	Water sample
	No petroleum constituents were found

	NAVARRE BEACH WEST

	7/2/2010
	Water sample
	No petroleum constituents were found



Table Explanation:
· Water sample – indicates a water sample that was taken, no oil was visible in the water when the sample was taken.

· Sand sample – indicates a sand sample that was taken to evaluate any potential petroleum contamination.  

· “10 cm from visible tar ball”, “1 meter from visible tar ball”, “near oil sheen and/or tar balls” or “Near mousse”– These are types of proximity sampling that means samples were collected at known distances from oil material.  This sampling is performed when the oil in the water is sparse enough that a bather might reasonably expect to swim in the water without coming into contact with the oil.  

· Collected for dispersant analysis – These samples are collected to attempt to detect dispersant.  The first priority is to collect the sample in proximity to oil when oil is present.  When oil is not present the second priority is to sample in locations were oil was previously present.  The third priority is to collect the sample where no oil contamination is, or ever was, present.  

None of the results listed above suggest that recreational activities should be restricted; however, the movement of oil product is unpredictable and conditions at a given location can change rapidly. The public should be advised not to go in the water with visible petroleum products.
